<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>AR</text>
<text>VIN</text>
<text>3.3</text>
<text>FTDI</text>
<text>2</text>
<text>3</text>
<text>4 </text>
<text>5</text>
<text>6 </text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>TX</text>
<text>RX</text>
<text>1</text>
<text>0</text>
<text>A7</text>
<text>A6</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>SCL</text>
<text>MO</text>
<text>RST</text>
<text>GND</text>
<text>3.3</text>
<text>GND</text>
<wire x1="2.032" y1="-1.27" x2="52.5018" y2="-1.143" width="0" layer="20"/>
<wire x1="53.213" y1="-0.4318" x2="53.213" y2="33.4518" width="0" layer="20"/>
<wire x1="2.413" y1="34.29" x2="1.27" y2="33.147" width="0" layer="20"/>
<wire x1="1.27" y1="33.147" x2="1.27" y2="-0.254" width="0" layer="20"/>
<text>GND</text>
<text>REG</text>
<text>VIN</text>
<text>3.3</text>
<text>2</text>
<text>3</text>
<text>4 </text>
<text>5</text>
<text>6 </text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>1</text>
<text>0</text>
<text>A7</text>
<text>A6</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>RST</text>
<text>GND</text>
<text>GND</text>
<text>RTS</text>
<text>RTS</text>
<text>ANT</text>
<text>FLASH</text>
<text>MI</text>
<text>SK</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>SDA</text>
<text>MOTEINO</text>
<text>R4</text>
<text>MEM</text>
<text>RFM12B
XTAL</text>
<text>RFM69
XTAL</text>
<text>LowPowerLab</text>
<text>ATMEGA
328</text>
<text>ANT</text>
<text>VIN</text>
<wire x1="2.413" y1="34.29" x2="52.5018" y2="34.29" width="0" layer="20"/>
<wire x1="53.213" y1="33.4518" x2="52.5018" y2="34.29" width="0" layer="20"/>
<wire x1="52.5018" y1="-1.143" x2="53.213" y2="-0.4318" width="0" layer="20"/>
<wire x1="1.27" y1="-0.254" x2="2.032" y2="-1.27" width="0" layer="20"/>
<text>SP1</text>
<text>SP0</text>
<text>SCL</text>
<text>MI</text>
<text>MO</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<text>G04</text>
<text>G25</text>
<text>G24</text>
<text>G23</text>
<text>G22</text>
<text>G21</text>
<text>G18</text>
<text>G17</text>
<text>Moteino Pi</text>
<text>TX/RX</text>
<text>SPI</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X13">
</package>
<package name="1X06">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="0805-CAP">
</package>
<package name="0603-LED">
</package>
<package name="RFM12B-ANTENNA">
</package>
<package name="SO08WIDE">
</package>
<package name="RFM69W-MINPADS">
</package>
<package name="RFM12B-MINPADS">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE13-2">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
<package name="FE08">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
<package name="FE09-2">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="SparkFun" package="RESONATOR-SMD" value="16 MHz"/>
<element name="IC3" library="linear" package="SOT23" value="MCP1703CB"/>
<element name="ANALOGSIDE" library="SparkFun-Connectors" package="1X13" value="M13"/>
<element name="DIGITALSIDE" library="SparkFun-Connectors" package="1X13" value="M13"/>
<element name="FTDI" library="SparkFun-Connectors" package="1X06" value="FTDI"/>
<element name="ATMEGA328" library="LowPowerLab" package="TQFP32-08" value="ATMega-328"/>
<element name="JP1" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP2" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="+" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="C5" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="VALUE"/>
</element>
<element name="R1" library="LowPowerLab" package="0603-RES" value="10k">
<attribute name="VALUE"/>
</element>
<element name="C1" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="VALUE"/>
</element>
<element name="C4" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="VALUE"/>
</element>
<element name="C2" library="LowPowerLab" package="0603-CAP" value="1u">
<attribute name="VALUE"/>
</element>
<element name="C3" library="LowPowerLab" package="0805-CAP" value="10u"/>
<element name="U$2" library="LowPowerLab" package="0603-LED" value="LED0603"/>
<element name="R2" library="LowPowerLab" package="0603-RES" value="1k5"/>
<element name="U$3" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="U$1" library="LowPowerLab" package="RFM12B-ANTENNA" value="RFM12B_ANTENNA"/>
<element name="U$5" library="LowPowerLab" package="RFM69W-MINPADS" value="RFM69"/>
<element name="U$6" library="LowPowerLab" package="SO08WIDE" value="AT25F512BWIDE_5.3MM"/>
<element name="RFM12B" library="LowPowerLab" package="RFM12B-MINPADS" value="RFM12B_MINPADS"/>
<element name="SV1" library="con-lsta" package="FE13-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ6" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SV2" library="con-lsta" package="FE08" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV3" library="con-lsta" package="FE08" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SV4" library="con-lsta" package="FE09-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="ANALOGSIDE" pad="13"/>
<contactref element="FTDI" pad="1"/>
<contactref element="ATMEGA328" pad="3"/>
<contactref element="ATMEGA328" pad="21"/>
<contactref element="ATMEGA328" pad="5"/>
<contactref element="JP2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$2" pad="MINUS"/>
<contactref element="U$5" pad="GND"/>
<contactref element="U$5" pad="GND"/>
<contactref element="U$6" pad="4"/>
<contactref element="RFM12B" pad="GND"/>
<contactref element="SV1" pad="6"/>
<contactref element="SV2" pad="3"/>
</signal>
<signal name="D10_SS">
<contactref element="DIGITALSIDE" pad="4"/>
<contactref element="ATMEGA328" pad="14"/>
<contactref element="U$5" pad="NSS"/>
<contactref element="RFM12B" pad="SEL"/>
</signal>
<signal name="RST">
<contactref element="DIGITALSIDE" pad="13"/>
<contactref element="ATMEGA328" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="SJ6" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="1"/>
<contactref element="ATMEGA328" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="X1" pad="3"/>
<contactref element="ATMEGA328" pad="8"/>
</signal>
<signal name="AREF">
<contactref element="ATMEGA328" pad="20"/>
<contactref element="JP1" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="PWR">
<contactref element="IC3" pad="3"/>
<contactref element="FTDI" pad="3"/>
<contactref element="ANALOGSIDE" pad="12"/>
<contactref element="C2" pad="1"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="FTDI" pad="6"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC3" pad="2"/>
<contactref element="ATMEGA328" pad="6"/>
<contactref element="ATMEGA328" pad="18"/>
<contactref element="ATMEGA328" pad="4"/>
<contactref element="ANALOGSIDE" pad="11"/>
<contactref element="+" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U$5" pad="VDD"/>
<contactref element="U$5" pad="VDD"/>
<contactref element="U$6" pad="7"/>
<contactref element="U$6" pad="8"/>
<contactref element="U$6" pad="3"/>
<contactref element="RFM12B" pad="VDD"/>
</signal>
<signal name="D9">
<contactref element="DIGITALSIDE" pad="5"/>
<contactref element="ATMEGA328" pad="13"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D8">
<contactref element="DIGITALSIDE" pad="6"/>
<contactref element="ATMEGA328" pad="12"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="D6">
<contactref element="DIGITALSIDE" pad="8"/>
<contactref element="ATMEGA328" pad="10"/>
</signal>
<signal name="D5">
<contactref element="DIGITALSIDE" pad="9"/>
<contactref element="ATMEGA328" pad="9"/>
</signal>
<signal name="D4">
<contactref element="DIGITALSIDE" pad="10"/>
<contactref element="ATMEGA328" pad="2"/>
</signal>
<signal name="D3">
<contactref element="DIGITALSIDE" pad="11"/>
<contactref element="ATMEGA328" pad="1"/>
</signal>
<signal name="D1_TX">
<contactref element="FTDI" pad="5"/>
<contactref element="ATMEGA328" pad="31"/>
<contactref element="ANALOGSIDE" pad="10"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="D0_RX">
<contactref element="FTDI" pad="4"/>
<contactref element="ATMEGA328" pad="30"/>
<contactref element="ANALOGSIDE" pad="9"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="A6">
<contactref element="ANALOGSIDE" pad="7"/>
<contactref element="ATMEGA328" pad="19"/>
</signal>
<signal name="A4_SDA">
<contactref element="ANALOGSIDE" pad="5"/>
<contactref element="ATMEGA328" pad="27"/>
</signal>
<signal name="A3">
<contactref element="ANALOGSIDE" pad="4"/>
<contactref element="ATMEGA328" pad="26"/>
</signal>
<signal name="A2">
<contactref element="ANALOGSIDE" pad="3"/>
<contactref element="ATMEGA328" pad="25"/>
</signal>
<signal name="A1">
<contactref element="ANALOGSIDE" pad="2"/>
<contactref element="ATMEGA328" pad="24"/>
</signal>
<signal name="A0">
<contactref element="ANALOGSIDE" pad="1"/>
<contactref element="ATMEGA328" pad="23"/>
</signal>
<signal name="D2">
<contactref element="DIGITALSIDE" pad="12"/>
<contactref element="ATMEGA328" pad="32"/>
<contactref element="U$5" pad="DIO0"/>
<contactref element="RFM12B" pad="IRQ"/>
</signal>
<signal name="D11_MOSI">
<contactref element="DIGITALSIDE" pad="3"/>
<contactref element="ATMEGA328" pad="15"/>
<contactref element="U$5" pad="MOSI"/>
<contactref element="U$6" pad="5"/>
<contactref element="RFM12B" pad="SDI"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="D12_MISO">
<contactref element="DIGITALSIDE" pad="2"/>
<contactref element="ATMEGA328" pad="16"/>
<contactref element="U$5" pad="MISO"/>
<contactref element="U$6" pad="2"/>
<contactref element="RFM12B" pad="SDO"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="D13_SCK">
<contactref element="DIGITALSIDE" pad="1"/>
<contactref element="ATMEGA328" pad="17"/>
<contactref element="U$5" pad="SCK"/>
<contactref element="U$6" pad="6"/>
<contactref element="RFM12B" pad="SCK"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="A7">
<contactref element="ANALOGSIDE" pad="8"/>
<contactref element="ATMEGA328" pad="22"/>
</signal>
<signal name="A5_SCL">
<contactref element="ANALOGSIDE" pad="6"/>
<contactref element="ATMEGA328" pad="28"/>
</signal>
<signal name="D7">
<contactref element="DIGITALSIDE" pad="7"/>
<contactref element="ATMEGA328" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="PLUS"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$5" pad="ANA"/>
<contactref element="RFM12B" pad="ANT"/>
</signal>
<signal name="RXD">
<contactref element="SV1" pad="10"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="SV1" pad="8"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="SPI1">
<contactref element="SV2" pad="8"/>
<contactref element="SV1" pad="26"/>
</signal>
<signal name="SPI0">
<contactref element="SV1" pad="24"/>
<contactref element="SV2" pad="7"/>
<contactref element="SJ6" pad="1"/>
</signal>
<signal name="SCLK">
<contactref element="SV2" pad="6"/>
<contactref element="SV1" pad="23"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="SV2" pad="5"/>
<contactref element="SV1" pad="21"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="SV2" pad="4"/>
<contactref element="SV1" pad="19"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="SV2" pad="2"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="SV2" pad="1"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="GP04">
<contactref element="SV1" pad="7"/>
<contactref element="SV3" pad="8"/>
</signal>
<signal name="GP17">
<contactref element="SV1" pad="11"/>
<contactref element="SV3" pad="1"/>
</signal>
<signal name="GP21">
<contactref element="SV1" pad="13"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="GP22">
<contactref element="SV1" pad="15"/>
<contactref element="SV3" pad="4"/>
</signal>
<signal name="GP18">
<contactref element="SV1" pad="12"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="GP23">
<contactref element="SV1" pad="16"/>
<contactref element="SV3" pad="5"/>
</signal>
<signal name="GP24">
<contactref element="SV1" pad="18"/>
<contactref element="SV3" pad="6"/>
</signal>
<signal name="GP25">
<contactref element="SV1" pad="22"/>
<contactref element="SV3" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
