(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 155)
    (tracks 3264)
    (zones 0)
    (modules 105)
    (nets 129)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "ONES-CPU-01 Gerbers/"))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /M2)
  (net 3 /VCC)
  (net 4 "Net-(U3-Pad7)")
  (net 5 "Net-(U3-Pad6)")
  (net 6 "Net-(U3-Pad12)")
  (net 7 "Net-(U3-Pad10)")
  (net 8 /ALE)
  (net 9 /PPU-CLK)
  (net 10 /VIDEO)
  (net 11 "Net-(C6-Pad2)")
  (net 12 "Net-(C7-Pad2)")
  (net 13 "Net-(C17-Pad2)")
  (net 14 "Net-(C9-Pad2)")
  (net 15 "Net-(C11-Pad2)")
  (net 16 "Net-(C18-Pad2)")
  (net 17 /EXP-AUDIO-OUT)
  (net 18 "Net-(C20-Pad1)")
  (net 19 "Net-(C23-Pad2)")
  (net 20 /4017-D0)
  (net 21 /4017-D3)
  (net 22 /4017-D4)
  (net 23 /~OE1)
  (net 24 /4016-D0)
  (net 25 /4016-D3)
  (net 26 /4016-D4)
  (net 27 "Net-(C41-Pad2)")
  (net 28 "Net-(C41-Pad1)")
  (net 29 "Net-(C42-Pad2)")
  (net 30 /CPU-CLK)
  (net 31 /SYSTEM-CLK)
  (net 32 /CIC-TO-MB)
  (net 33 /CIC-TO-CART)
  (net 34 "Net-(R1-Pad1)")
  (net 35 /EXP-VIDEO)
  (net 36 /SOUND-2)
  (net 37 /SOUND-1)
  (net 38 "Net-(R5-Pad1)")
  (net 39 /EXP-AUDIO-IN)
  (net 40 /~NMI)
  (net 41 "Net-(R18-Pad2)")
  (net 42 "Net-(R19-Pad2)")
  (net 43 /4016-D2)
  (net 44 /4016-D1)
  (net 45 /~IRQ)
  (net 46 /4017-D2)
  (net 47 /4017-D1)
  (net 48 /PPU-A13)
  (net 49 /CPU-A8)
  (net 50 /CPU-D2)
  (net 51 /CPU-A9)
  (net 52 /CPU-D1)
  (net 53 /CPU-R~W)
  (net 54 /CPU-D0)
  (net 55 /CPU-A0)
  (net 56 /CPU-A10)
  (net 57 /CPU-A1)
  (net 58 /WRAM-~CE)
  (net 59 /CPU-A2)
  (net 60 /CPU-D7)
  (net 61 /CPU-A3)
  (net 62 /CPU-D6)
  (net 63 /CPU-A4)
  (net 64 /CPU-D5)
  (net 65 /CPU-A5)
  (net 66 /CPU-D4)
  (net 67 /CPU-A6)
  (net 68 /CPU-D3)
  (net 69 /CPU-A7)
  (net 70 /PPU-A1)
  (net 71 /PPU-A0)
  (net 72 /PPU-D0)
  (net 73 /PPU-A7)
  (net 74 /PPU-D2)
  (net 75 /PPU-D7)
  (net 76 /PPU-A2)
  (net 77 /PPU-D5)
  (net 78 /PPU-A4)
  (net 79 /PPU-A5)
  (net 80 /PPU-D4)
  (net 81 /PPU-A3)
  (net 82 /PPU-D6)
  (net 83 /PPU-D3)
  (net 84 /PPU-A6)
  (net 85 /PPU-D1)
  (net 86 /CPU-A15)
  (net 87 /PPU-~CE)
  (net 88 "Net-(U3-Pad1)")
  (net 89 /CPU-A14)
  (net 90 /CPU-A13)
  (net 91 /~ROMSEL)
  (net 92 /PPU-A8)
  (net 93 /PPU-A9)
  (net 94 /PPU-~WE)
  (net 95 /PPU-~RD)
  (net 96 /VRAM-A10)
  (net 97 /VRAM-~CE)
  (net 98 /PPU-A10)
  (net 99 /PPU-A11)
  (net 100 /PPU-A12)
  (net 101 /~RST)
  (net 102 "Net-(Q1-Pad3)")
  (net 103 /OUT-1)
  (net 104 /OUT-2)
  (net 105 /CPU-A12)
  (net 106 /CPU-A11)
  (net 107 "Net-(U7-Pad7)")
  (net 108 "Net-(U8-Pad7)")
  (net 109 /PPU-~A13)
  (net 110 "Net-(U10-Pad6)")
  (net 111 /CIC-CLK)
  (net 112 "Net-(U10-Pad5)")
  (net 113 /CIC-RST)
  (net 114 /+9V)
  (net 115 /AUDIO)
  (net 116 /EXP-0)
  (net 117 /EXP-1)
  (net 118 /EXP-2)
  (net 119 /EXP-3)
  (net 120 /EXP-4)
  (net 121 /EXP-9)
  (net 122 /EXP-7)
  (net 123 /EXP-6)
  (net 124 /EXP-5)
  (net 125 /EXP-8)
  (net 126 "Net-(P2-Pad46)")
  (net 127 /~OE2)
  (net 128 /OUT-0)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+9V)
    (add_net /4016-D0)
    (add_net /4016-D1)
    (add_net /4016-D2)
    (add_net /4016-D3)
    (add_net /4016-D4)
    (add_net /4017-D0)
    (add_net /4017-D1)
    (add_net /4017-D2)
    (add_net /4017-D3)
    (add_net /4017-D4)
    (add_net /ALE)
    (add_net /AUDIO)
    (add_net /CIC-CLK)
    (add_net /CIC-RST)
    (add_net /CIC-TO-CART)
    (add_net /CIC-TO-MB)
    (add_net /CPU-A0)
    (add_net /CPU-A1)
    (add_net /CPU-A10)
    (add_net /CPU-A11)
    (add_net /CPU-A12)
    (add_net /CPU-A13)
    (add_net /CPU-A14)
    (add_net /CPU-A15)
    (add_net /CPU-A2)
    (add_net /CPU-A3)
    (add_net /CPU-A4)
    (add_net /CPU-A5)
    (add_net /CPU-A6)
    (add_net /CPU-A7)
    (add_net /CPU-A8)
    (add_net /CPU-A9)
    (add_net /CPU-CLK)
    (add_net /CPU-D0)
    (add_net /CPU-D1)
    (add_net /CPU-D2)
    (add_net /CPU-D3)
    (add_net /CPU-D4)
    (add_net /CPU-D5)
    (add_net /CPU-D6)
    (add_net /CPU-D7)
    (add_net /CPU-R~W)
    (add_net /EXP-0)
    (add_net /EXP-1)
    (add_net /EXP-2)
    (add_net /EXP-3)
    (add_net /EXP-4)
    (add_net /EXP-5)
    (add_net /EXP-6)
    (add_net /EXP-7)
    (add_net /EXP-8)
    (add_net /EXP-9)
    (add_net /EXP-AUDIO-IN)
    (add_net /EXP-AUDIO-OUT)
    (add_net /EXP-VIDEO)
    (add_net /GND)
    (add_net /M2)
    (add_net /OUT-0)
    (add_net /OUT-1)
    (add_net /OUT-2)
    (add_net /PPU-A0)
    (add_net /PPU-A1)
    (add_net /PPU-A10)
    (add_net /PPU-A11)
    (add_net /PPU-A12)
    (add_net /PPU-A13)
    (add_net /PPU-A2)
    (add_net /PPU-A3)
    (add_net /PPU-A4)
    (add_net /PPU-A5)
    (add_net /PPU-A6)
    (add_net /PPU-A7)
    (add_net /PPU-A8)
    (add_net /PPU-A9)
    (add_net /PPU-CLK)
    (add_net /PPU-D0)
    (add_net /PPU-D1)
    (add_net /PPU-D2)
    (add_net /PPU-D3)
    (add_net /PPU-D4)
    (add_net /PPU-D5)
    (add_net /PPU-D6)
    (add_net /PPU-D7)
    (add_net /PPU-~A13)
    (add_net /PPU-~CE)
    (add_net /PPU-~RD)
    (add_net /PPU-~WE)
    (add_net /SOUND-1)
    (add_net /SOUND-2)
    (add_net /SYSTEM-CLK)
    (add_net /VCC)
    (add_net /VIDEO)
    (add_net /VRAM-A10)
    (add_net /VRAM-~CE)
    (add_net /WRAM-~CE)
    (add_net /~IRQ)
    (add_net /~NMI)
    (add_net /~OE1)
    (add_net /~OE2)
    (add_net /~ROMSEL)
    (add_net /~RST)
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C41-Pad2)")
    (add_net "Net-(C42-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(P2-Pad46)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(U10-Pad5)")
    (add_net "Net-(U10-Pad6)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U7-Pad7)")
    (add_net "Net-(U8-Pad7)")
  )
  (module Package_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5A02E8C5)
    (at 18.475 -42.2 90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U6 (at 7.62 -2.33 90) (layer F.SilkS))
    (fp_text value "RP2A03 CPU" (at 7.62 50.59 90) (layer F.Fab))
    (fp_text user %R (at 7.62 24.13 90) (layer F.Fab))
    (pad 40 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 39 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /CPU-A15))
    (pad 38 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /OUT-1))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 /CPU-A14))
    (pad 37 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 /OUT-2))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 /CPU-A13))
    (pad 36 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 /CPU-A12))
    (pad 35 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 /CPU-A11))
    (pad 34 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /CPU-R~W))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /CPU-A10))
    (pad 33 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /~NMI))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /CPU-A9))
    (pad 32 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /~IRQ))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /CPU-A8))
    (pad 31 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /M2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 /CPU-A7))
    (pad 30 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /CPU-A6))
    (pad 29 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /CPU-CLK))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /CPU-A5))
    (pad 28 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /CPU-D0))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /CPU-A4))
    (pad 27 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /CPU-D1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /CPU-A3))
    (pad 26 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /CPU-D2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /CPU-A2))
    (pad 25 thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /CPU-D3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /CPU-A1))
    (pad 24 thru_hole oval (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /CPU-D4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /CPU-A0))
    (pad 23 thru_hole oval (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /CPU-D5))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /~RST))
    (pad 22 thru_hole oval (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /CPU-D6))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /SOUND-2))
    (pad 21 thru_hole oval (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /CPU-D7))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /SOUND-1))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Symbol_13.4x12mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 80.6 -68.65)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value " " (at 0.75 0) (layer F.Fab) hide)
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 145.625 -24.575 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C9 (at 1.25 -3.75) (layer F.SilkS))
    (fp_text value 2.2uF (at 1.175 -5.275) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-24_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 94.475 -19.5 90)
    (descr "24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value "6116 (VRAM)" (at 3.81 30.27 90) (layer F.Fab))
    (fp_text user %R (at 3.725 21.825 90) (layer F.Fab))
    (pad 24 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 23 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /PPU-A8))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /PPU-D2))
    (pad 22 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /PPU-A9))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /PPU-D1))
    (pad 21 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /PPU-~WE))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 /PPU-D0))
    (pad 20 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 /PPU-~RD))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 /PPU-A0))
    (pad 19 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 /VRAM-A10))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 /PPU-A1))
    (pad 18 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /VRAM-~CE))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 /PPU-A2))
    (pad 17 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /PPU-D7))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 /PPU-A3))
    (pad 16 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 /PPU-D6))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 /PPU-A4))
    (pad 15 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /PPU-D5))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 /PPU-A5))
    (pad 14 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 /PPU-D4))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 /PPU-A6))
    (pad 13 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /PPU-D3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 /PPU-A7))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 131.75 -26.675 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 5.41 0 90) (layer F.SilkS))
    (fp_text value ? (at 5.08 2.12 90) (layer F.Fab))
    (fp_text user %R (at 5.38 0 90) (layer F.Fab))
    (fp_text user K (at 0 -1.8 90) (layer F.Fab))
    (fp_text user " " (at 11.875 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /CIC-TO-CART))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 35.25 -98.65 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C43 (at 1.25 -2.3) (layer F.SilkS))
    (fp_text value 51pF (at 1.25 2.3) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C41-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NESRE:NES_Edge_Connector (layer F.Cu) (tedit 5DAD00C1)
    (at 20.075 -11.725)
    (fp_text reference P1 (at 13.525 -0.025) (layer F.SilkS))
    (fp_text value "72-Pin Connector" (at 13.725 -0.825) (layer F.Fab))
    (pad 1 smd rect (at 17.75 6.25) (size 3 9) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 20.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 106 /CPU-A11))
    (pad 3 smd rect (at 23.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 56 /CPU-A10))
    (pad 4 smd rect (at 25.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 51 /CPU-A9))
    (pad 5 smd rect (at 28.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 49 /CPU-A8))
    (pad 6 smd rect (at 30.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 69 /CPU-A7))
    (pad 7 smd rect (at 33.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 67 /CPU-A6))
    (pad 8 smd rect (at 35.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 65 /CPU-A5))
    (pad 9 smd rect (at 38.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 63 /CPU-A4))
    (pad 10 smd rect (at 40.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 61 /CPU-A3))
    (pad 11 smd rect (at 43.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 59 /CPU-A2))
    (pad 12 smd rect (at 45.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 57 /CPU-A1))
    (pad 13 smd rect (at 48.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 55 /CPU-A0))
    (pad 14 smd rect (at 50.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 53 /CPU-R~W))
    (pad 15 smd rect (at 53.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 45 /~IRQ))
    (pad 16 smd rect (at 55.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 116 /EXP-0))
    (pad 17 smd rect (at 58.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 117 /EXP-1))
    (pad 18 smd rect (at 60.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 118 /EXP-2))
    (pad 19 smd rect (at 63.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 119 /EXP-3))
    (pad 20 smd rect (at 65.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 120 /EXP-4))
    (pad 21 smd rect (at 68.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 95 /PPU-~RD))
    (pad 22 smd rect (at 70.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 96 /VRAM-A10))
    (pad 23 smd rect (at 73.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 84 /PPU-A6))
    (pad 24 smd rect (at 75.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 79 /PPU-A5))
    (pad 25 smd rect (at 78.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 78 /PPU-A4))
    (pad 26 smd rect (at 80.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 81 /PPU-A3))
    (pad 27 smd rect (at 83.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 76 /PPU-A2))
    (pad 28 smd rect (at 85.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 70 /PPU-A1))
    (pad 29 smd rect (at 88.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 71 /PPU-A0))
    (pad 30 smd rect (at 90.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 72 /PPU-D0))
    (pad 31 smd rect (at 93.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 85 /PPU-D1))
    (pad 32 smd rect (at 95.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 74 /PPU-D2))
    (pad 33 smd rect (at 98.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 83 /PPU-D3))
    (pad 34 smd rect (at 100.75 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 33 /CIC-TO-CART))
    (pad 35 smd rect (at 103.25 6.25) (size 2 9) (layers F.Cu F.Paste F.Mask)
      (net 32 /CIC-TO-MB))
    (pad 36 smd rect (at 106.25 6.25) (size 3 9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC))
    (pad 64 smd rect (at 85.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 100 /PPU-A12))
    (pad 65 smd rect (at 88.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 48 /PPU-A13))
    (pad 66 smd rect (at 90.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 75 /PPU-D7))
    (pad 67 smd rect (at 93.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 82 /PPU-D6))
    (pad 63 smd rect (at 83.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 98 /PPU-A10))
    (pad 58 smd rect (at 70.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 109 /PPU-~A13))
    (pad 60 smd rect (at 75.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 92 /PPU-A8))
    (pad 59 smd rect (at 73.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 73 /PPU-A7))
    (pad 61 smd rect (at 78.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 93 /PPU-A9))
    (pad 62 smd rect (at 80.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 99 /PPU-A11))
    (pad 37 smd rect (at 17.75 6.25) (size 3 9) (layers B.Cu B.Paste B.Mask)
      (net 31 /SYSTEM-CLK))
    (pad 38 smd rect (at 20.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 2 /M2))
    (pad 39 smd rect (at 23.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 105 /CPU-A12))
    (pad 40 smd rect (at 25.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 90 /CPU-A13))
    (pad 53 smd rect (at 58.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 122 /EXP-7))
    (pad 51 smd rect (at 53.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 121 /EXP-9))
    (pad 52 smd rect (at 55.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 125 /EXP-8))
    (pad 42 smd rect (at 30.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 60 /CPU-D7))
    (pad 47 smd rect (at 43.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 50 /CPU-D2))
    (pad 56 smd rect (at 65.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 94 /PPU-~WE))
    (pad 43 smd rect (at 33.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 62 /CPU-D6))
    (pad 45 smd rect (at 38.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 66 /CPU-D4))
    (pad 50 smd rect (at 50.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 91 /~ROMSEL))
    (pad 46 smd rect (at 40.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 68 /CPU-D3))
    (pad 49 smd rect (at 48.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 54 /CPU-D0))
    (pad 55 smd rect (at 63.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 124 /EXP-5))
    (pad 48 smd rect (at 45.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 52 /CPU-D1))
    (pad 44 smd rect (at 35.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 64 /CPU-D5))
    (pad 41 smd rect (at 28.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 89 /CPU-A14))
    (pad 54 smd rect (at 60.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 123 /EXP-6))
    (pad 57 smd rect (at 68.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 97 /VRAM-~CE))
    (pad 68 smd rect (at 95.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 77 /PPU-D5))
    (pad 69 smd rect (at 98.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 80 /PPU-D4))
    (pad 70 smd rect (at 100.75 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 113 /CIC-RST))
    (pad 71 smd rect (at 103.25 6.25) (size 2 9) (layers B.Cu B.Paste B.Mask)
      (net 111 /CIC-CLK))
    (pad 72 smd rect (at 106.25 6.25) (size 3 9) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 19.35 -85.5 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C44 (at 4.875 -0.05) (layer F.SilkS))
    (fp_text value 220pF (at 0.95 -2) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /CPU-CLK))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /SYSTEM-CLK))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 84.75 -41.25 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C39 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 137.25 -26.675 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.16 0 90) (layer F.SilkS))
    (fp_text value ? (at 5.08 2.12 90) (layer F.Fab))
    (fp_text user %R (at 5.38 0 90) (layer F.Fab))
    (fp_text user K (at 11.9 -0.075 90) (layer F.Fab))
    (fp_text user " " (at 0 -1.8 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CIC-TO-MB))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 24.2 -93)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C42 (at 4.875 -1.5) (layer F.SilkS))
    (fp_text value 15pF (at 5.325 -0.1) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C42-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 74.75 -22 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C22 (at 2.5 -0.025 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 33.5 -79.502)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C45 (at -2.725 0.077) (layer F.SilkS))
    (fp_text value 51pF (at 5.75 -0.023) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /PPU-CLK))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C42-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 94.5007 -39.497 90)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74HC373 (at 3.81 25.19 90) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43 90) (layer F.Fab))
    (pad 20 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 19 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 /PPU-A7))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 /PPU-A0))
    (pad 18 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /PPU-D7))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 /PPU-D0))
    (pad 17 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /PPU-D5))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /PPU-D2))
    (pad 16 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 /PPU-A5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 /PPU-A2))
    (pad 15 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 /PPU-A3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 /PPU-A4))
    (pad 14 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /PPU-D3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 /PPU-D4))
    (pad 13 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /PPU-D1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 /PPU-D6))
    (pad 12 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 /PPU-A1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 /PPU-A6))
    (pad 11 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /ALE))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 47.5 -99 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C41 (at 1.25 -2.25 90) (layer F.SilkS))
    (fp_text value 18pF (at 1.25 2.25 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C41-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C41-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 73 -53.5 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C32 (at 2.5 0.05 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 24.2189 -81.2038 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (fp_text reference C46 (at 2.5189 -0.1038) (layer F.SilkS))
    (fp_text value 100nF (at 2.6939 -2.0538) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 20.0279 -60.706 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C13 (at 2.5279 0.044) (layer F.SilkS))
    (fp_text value 10nF (at -3.7021 0.024) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-24_W7.62mm (layer F.Cu) (tedit 5DD765D1)
    (at 38.7 -22 90)
    (descr "24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value "6116 (WRAM)" (at 3.81 30.27 90) (layer F.Fab))
    (fp_text user %R (at 3.81 13.97 90) (layer F.Fab))
    (pad 24 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 23 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /CPU-A8))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /CPU-D2))
    (pad 22 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /CPU-A9))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /CPU-D1))
    (pad 21 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /CPU-R~W))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /CPU-D0))
    (pad 20 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /CPU-A0))
    (pad 19 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /CPU-A10))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /CPU-A1))
    (pad 18 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /WRAM-~CE))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /CPU-A2))
    (pad 17 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /CPU-D7))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /CPU-A3))
    (pad 16 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /CPU-D6))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /CPU-A4))
    (pad 15 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /CPU-D5))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /CPU-A5))
    (pad 14 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /CPU-D4))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /CPU-A6))
    (pad 13 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /CPU-D3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 /CPU-A7))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 20.0279 -64.1985 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C25 (at 2.5 -0.1985) (layer F.SilkS))
    (fp_text value "(Unused)" (at 9.7779 0.0015) (layer F.Fab))
    (fp_text user %R (at 2.5 -0.1985) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 132 -34.5 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U10 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value CIC (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(U10-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(U10-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 /CIC-RST))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R18-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /~RST))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 181.575 -85.025 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor")
    (fp_text reference BC1 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 103-25 (at 2.375 2.4 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D6.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 187.5028 -85.79866 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C27 (at 1.3028 -1.92366) (layer F.SilkS))
    (fp_text value " " (at -16.2222 11.10134) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5DE2FD10)
    (at 171.8 -45.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference FC1 (at 5.06 0 90) (layer F.SilkS))
    (fp_text value 39uH (at 5.07 -2.42 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 /AUDIO))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /EXP-AUDIO-OUT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 160.55 -99.25 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C38 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.625 -2.175 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP7 (layer F.Cu) (tedit 5A14249F)
    (at 170.44 -93.15 180)
    (descr "7-pin Resistor SIP pack")
    (tags R)
    (fp_text reference DA1 (at 8.64 2.5) (layer F.SilkS))
    (fp_text value DAN601 (at -4.41 0) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /4016-D4))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /4016-D3))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /4016-D0))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-126-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 155.45 -71.75)
    (descr "TO-126-3, Vertical, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf")
    (tags "TO-126-3 Vertical RM 2.54mm")
    (fp_text reference Q1 (at 7.88 -0.28) (layer F.SilkS))
    (fp_text value 2SA937 (at -4.46 -0.14) (layer F.SilkS))
    (fp_text user %R (at 7.9 -0.3) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 35 /EXP-VIDEO))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-126-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 164.8 -109 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C36 (at 5.25 -0.025 90) (layer F.SilkS))
    (fp_text value " " (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /4016-D3))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP7 (layer F.Cu) (tedit 5A14249F)
    (at 170.45 -79.875 180)
    (descr "7-pin Resistor SIP pack")
    (tags R)
    (fp_text reference DA3 (at 18.425 0) (layer F.SilkS))
    (fp_text value DAN601 (at -4.825 0.05) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /4017-D4))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /4017-D3))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /4017-D0))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP7 (layer F.Cu) (tedit 5A14249F)
    (at 170.44 -89.65 180)
    (descr "7-pin Resistor SIP pack")
    (tags R)
    (fp_text reference DA2 (at 8.89 -2.4) (layer F.SilkS))
    (fp_text value UPA64H (at -4.71 -0.05) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /4016-D4))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /4016-D3))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /4016-D0))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 167.3 -109 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C35 (at 5.325 0.025 90) (layer F.SilkS))
    (fp_text value " " (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /4016-D0))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 169.8 -109 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C34 (at 5.4 0 90) (layer F.SilkS))
    (fp_text value " " (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 172.3 -109 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C33 (at 5.425 -0.05 90) (layer F.SilkS))
    (fp_text value " " (at 1.25 2.05 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP7 (layer F.Cu) (tedit 5A14249F)
    (at 170.45 -76.35 180)
    (descr "7-pin Resistor SIP pack")
    (tags R)
    (fp_text reference DA4 (at 18.45 0.025) (layer F.SilkS))
    (fp_text value UPA64H (at -5.025 -0.025) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /4017-D4))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /4017-D3))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /4017-D0))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 153.35 -32 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 1M (at 12.5 0.05 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 187.49836 -95.79864 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C31 (at 4.92336 0.20136) (layer F.SilkS))
    (fp_text value " " (at -14.30164 3.20136) (layer F.Fab))
    (fp_text user %R (at 1.27336 -0.02364) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /4017-D4))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 187.49772 -90.79992 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C29 (at 4.89772 0.05008) (layer F.SilkS))
    (fp_text value " " (at -15.57728 11.37508) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /4017-D0))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 168.3 -45.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference FC2 (at 5.06 0.05 90) (layer F.SilkS))
    (fp_text value Ferrite_Coil (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /VIDEO))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /EXP-VIDEO))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 162.3 -109 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C37 (at 1.075 2.175 90) (layer F.SilkS))
    (fp_text value "330pF x5" (at 1.025 -15.25 180) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /4016-D4))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 145.9 -90.35 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C40 (at 2.5 0) (layer F.SilkS))
    (fp_text value 10nF (at 7.975 0.025) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 184.55 -45.25 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C12 (at 2.5 0) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 /+9V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 163.55 -62.75)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C20 (at 1.3 -1.65) (layer F.SilkS))
    (fp_text value 51pF (at 1.45 1.3) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /EXP-AUDIO-OUT))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177.55 -51.75)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C14 (at 2.45 -0.05) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 184.55 -42.25 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C11 (at 2.5 0.05) (layer F.SilkS))
    (fp_text value 10nF (at 2.65 -2.525) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177.55 -56.75)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C15 (at 2.5 0.05) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 /+9V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 143.3 -30.5 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (fp_text reference C8 (at 2.5 -0.05) (layer F.SilkS))
    (fp_text value 100nF (at 2.225 2.05) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 157.05 -42.2 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C7 (at -2.525 1.45 90) (layer F.SilkS))
    (fp_text value Unused (at -4.1 -0.1 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177.55 -61.75)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C16 (at 2.45 -0.05) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.45 -0.075) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 157.05 -32.75 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C6 (at -3.275 2.8 90) (layer F.SilkS))
    (fp_text value Unused (at -3.175 4.275 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 156.05 -62.75)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C21 (at 1.25 -1.7) (layer F.SilkS))
    (fp_text value 220pF (at 1.525 1.425) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C20-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 191.275 -79.975 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C26 (at 2.5 -0.05) (layer F.SilkS))
    (fp_text value 10nF (at 2.45 -2.4) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 166.8 -28.75 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C5 (at 1.15 -2.075) (layer F.SilkS))
    (fp_text value 330pF (at 1.25 2.25) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /VIDEO))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 153.05 -24.5 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.375 -3.65) (layer F.SilkS))
    (fp_text value 100uF (at 1.275 -5.2) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 154.35 -101.6 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor")
    (fp_text reference BC2 (at 2.55 0.05 90) (layer F.SilkS))
    (fp_text value 103-25 (at 2.35 -2.15 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D6.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 147.3 -54.75 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C24 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 10nF (at -2.675 -0.025 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177.6 -71.75)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C18 (at 2.5 0) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C18-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 172.55 -54.75 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C19 (at 2.45 0.1 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 177.6 -66.75)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C17 (at 2.45 -0.05) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 152.625 -52.225 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U9 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74LS04 (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R1-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 /PPU-~A13))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(U10-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /PPU-A13))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C20-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 /CIC-CLK))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /EXP-AUDIO-OUT))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R1-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /~RST))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R1-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R5-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 146.89 -29.35)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R17 (at 5.06 0) (layer F.SilkS))
    (fp_text value 2.2K (at 0.86 -2.125) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 155.89 -66.7)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.01 0) (layer F.SilkS))
    (fp_text value 47K (at 8.36 -2.325) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /EXP-AUDIO-OUT))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 16.9926 -26.025 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.225 0.0074 90) (layer F.SilkS))
    (fp_text value 100 (at 4.725 -2.6176 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /SOUND-1))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 57.875 -66.275)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.08 0.05) (layer F.SilkS))
    (fp_text value 12K (at -3.075 0) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C23-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /SOUND-2))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal (layer F.Cu) (tedit 5B7745C6)
    (at 191.3 -85 90)
    (descr "JST PH series connector, S7B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference P5 (at 6 -2.55 90) (layer F.SilkS))
    (fp_text value "Controller Input" (at 6 7.45 90) (layer F.Fab))
    (fp_text user %R (at 6 2.5 90) (layer F.Fab))
    (pad 7 thru_hole oval (at 12 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 /4017-D4))
    (pad 6 thru_hole oval (at 10 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 /4017-D3))
    (pad 5 thru_hole oval (at 8 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 /4017-D0))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 128.1 -93 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U7 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value "40H368 (CI)" (at 4.15 -4.425 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /CPU-D2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /4016-D0))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /4016-D2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /CPU-D0))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /CPU-D3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /4016-D1))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /4016-D3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /CPU-D1))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /CPU-D4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /4016-D4))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(U7-Pad7)"))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 172.3 -48.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.1 -0.05) (layer F.SilkS))
    (fp_text value 510 (at 5.08 2.37) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /EXP-VIDEO))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 187.47486 -88.30056 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C28 (at 4.92486 -0.07556) (layer F.SilkS))
    (fp_text value " " (at -15.17514 14.87444) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-126-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 24 -98.65)
    (descr "TO-126-3, Vertical, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf")
    (tags "TO-126-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 2.45 -4.625) (layer F.SilkS))
    (fp_text value 2SC2021 (at 2.575 -3.05) (layer F.SilkS))
    (fp_text user %R (at 2.475 -4.625) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(C41-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C42-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-126-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 128.1 -80.1 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U8 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value "40H368 (CII)" (at 3.8 -4.5 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(U8-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /4017-D4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /CPU-D4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /CPU-D1))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /4017-D3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /4017-D1))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /CPU-D3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /CPU-D0))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /4017-D2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /4017-D0))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /CPU-D2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal (layer F.Cu) (tedit 5B7745C6)
    (at 174.1 -114.25 180)
    (descr "JST PH series connector, S7B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference P4 (at 6 -2.55) (layer F.SilkS))
    (fp_text value "Controller Input" (at 6 7.45) (layer F.Fab))
    (fp_text user %R (at 6 2.5) (layer F.Fab))
    (pad 7 thru_hole oval (at 12 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 26 /4016-D4))
    (pad 6 thru_hole oval (at 10 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 /4016-D3))
    (pad 5 thru_hole oval (at 8 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 4 thru_hole oval (at 6 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 /4016-D0))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Resonator_muRata_CSTLSxxxG-3Pin_W8.0mm_H3.0mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 161.05 -35 90)
    (descr "Ceramic Resomator/Filter Murata CSTLSxxxG, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/timingdevice/ceralock/p17e.ashx, length*width=8.0x3.0mm^2 package, package length=8.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter CSTLSxxxG")
    (fp_text reference X2 (at 2.5 -2.7 90) (layer F.SilkS))
    (fp_text value 4MHz (at 2.5 2.7 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Resonator_muRata_CSTLSxxxG-3Pin_W8.0mm_H3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 149.5 -101.425 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 5.05 0 90) (layer F.SilkS))
    (fp_text value Unused (at 5.075 -2.15 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 169.8 -62.75 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.15 0 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C18-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 21 -26.04 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.225 0.05 90) (layer F.SilkS))
    (fp_text value 100 (at 5.08 2.37 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /SOUND-2))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 187.49772 -93.30182 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C30 (at 4.87272 -0.07682) (layer F.SilkS))
    (fp_text value "330pF x5" (at 1.49772 4.89818) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /4017-D3))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NESRE:TestPoint_Pad_1.5x1.5mmAlt (layer F.Cu) (tedit 5E1677A2)
    (at 21 -39.1 180)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference "" (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value " " (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 36 /SOUND-2))
  )
  (module NESRE:TestPoint_Pad_1.5x1.5mmAlt (layer F.Cu) (tedit 5E1677A8)
    (at 17.45 -39.1)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference " " (at 0 -1.648) (layer F.SilkS))
    (fp_text value " " (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 37 /SOUND-1))
  )
  (module NESRE:DIP-24_W7.62mmSingleRow (layer F.Cu) (tedit 5DEEFED0)
    (at 38.7 -29.625 90)
    (descr "24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference " " (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 3.81 30.27 90) (layer F.Fab))
    (fp_text user %R (at 3.81 13.97 90) (layer F.Fab))
    (pad 13 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /CPU-D3))
    (pad 14 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /CPU-D4))
    (pad 15 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /CPU-D5))
    (pad 16 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /CPU-D6))
    (pad 17 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /CPU-D7))
    (pad 18 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /WRAM-~CE))
    (pad 19 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /CPU-A10))
    (pad 20 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 21 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /CPU-R~W))
    (pad 22 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /CPU-A9))
    (pad 23 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /CPU-A8))
    (pad 24 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5A02E8C5)
    (at 94.5 -55 90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U5 (at 7.62 -2.33 90) (layer F.SilkS))
    (fp_text value "RP2C02 PPU" (at 7.625 50.59 90) (layer F.Fab))
    (fp_text user %R (at 7.62 24.13 90) (layer F.Fab))
    (pad 40 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 39 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /ALE))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /~NMI))
    (pad 38 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 /PPU-D0))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /PPU-CLK))
    (pad 37 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /PPU-D1))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 36 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /PPU-D2))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 35 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /PPU-D3))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 34 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 /PPU-D4))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 33 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /PPU-D5))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /PPU-~CE))
    (pad 32 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 /PPU-D6))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /CPU-A0))
    (pad 31 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /PPU-D7))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /CPU-A1))
    (pad 30 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /PPU-A8))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /CPU-A2))
    (pad 29 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /PPU-A9))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /CPU-D7))
    (pad 28 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 /PPU-A10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /CPU-D6))
    (pad 27 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 /PPU-A11))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /CPU-D5))
    (pad 26 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 /PPU-A12))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /CPU-D4))
    (pad 25 thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /PPU-A13))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /CPU-D3))
    (pad 24 thru_hole oval (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 /PPU-~RD))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /CPU-D2))
    (pad 23 thru_hole oval (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /PPU-~WE))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /CPU-D1))
    (pad 22 thru_hole oval (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /~RST))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /CPU-D0))
    (pad 21 thru_hole oval (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /CPU-R~W))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 171.8 -26.75 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 220pF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 /AUDIO))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 151.5 -64.75 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C23 (at 1.275 -3.1) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 3.75) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C23-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NESRE:DIP-24_W7.62mmSingleRow (layer F.Cu) (tedit 5DEEFED0)
    (at 94.475 -27.1 90)
    (descr "24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference " " (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value " " (at 3.81 30.27 90) (layer F.Fab))
    (fp_text user %R (at 3.81 13.97 90) (layer F.Fab))
    (pad 13 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /PPU-D3))
    (pad 14 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 /PPU-D4))
    (pad 15 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /PPU-D5))
    (pad 16 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 /PPU-D6))
    (pad 17 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /PPU-D7))
    (pad 18 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /VRAM-~CE))
    (pad 19 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 /VRAM-A10))
    (pad 20 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 /PPU-~RD))
    (pad 21 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /PPU-~WE))
    (pad 22 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /PPU-A9))
    (pad 23 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /PPU-A8))
    (pad 24 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NESRE:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal_OverLapping (layer F.Cu) (tedit 5DEEFE10)
    (at 76.59116 -95.504)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R16 (at 5.08 0.029) (layer F.SilkS))
    (fp_text value Unused (at 5.10884 -2.496) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer F.Cu) (tedit 5E1677F1)
    (at 139 -45.45)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference " " (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint_Pad_1.0x1.0mm (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 101 /~RST))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5DF58A7B)
    (at 76.6 -92.25)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 5.05 0) (layer F.SilkS))
    (fp_text value 100K (at 5.08 2.37) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 /EXP-6))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /EXP-AUDIO-IN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 16.85 -87.9 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 5.1 0.05 90) (layer F.SilkS))
    (fp_text value 1.2K (at 5 -2.375 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /CPU-CLK))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-126-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 23.375 -87.925)
    (descr "TO-126-3, Vertical, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf")
    (tags "TO-126-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 5.275 -2.875) (layer F.SilkS))
    (fp_text value 2SC2021 (at 2.35 3.85) (layer F.SilkS))
    (fp_text user %R (at 5.25 -2.875) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C42-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 31 /SYSTEM-CLK))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-126-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 34.25 -83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5.1 0 90) (layer F.SilkS))
    (fp_text value 1.2K (at 5.1 -2.15 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C42-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 29.6799 -25.9969 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.5031 0.0701 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 57.875 -72.55)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 5.075 0.025) (layer F.SilkS))
    (fp_text value 20K (at -3.075 0.05) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C23-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /EXP-AUDIO-IN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP5 (layer F.Cu) (tedit 5A14249F)
    (at 66.41 -61.75 180)
    (descr "5-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RA2 (at 10.585 -2.15) (layer F.SilkS))
    (fp_text value "4 x 6.8K" (at 5.135 -2) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /PPU-A13))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5DE60888)
    (at 37.35 -93.175 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 5.175 0.05 90) (layer F.SilkS))
    (fp_text value 220K (at 5.075 -2.3 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C41-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C42-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 127.65 -20.25 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 10nF (at -3.85 0.025 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 20.05 -87.89 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 5.1 -0.05 90) (layer F.SilkS))
    (fp_text value 510 (at 5.08 2.37 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /SYSTEM-CLK))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 123.75 -37 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C10 (at 2.5 0.05 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 140 -16.5 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R18 (at 5 0 90) (layer F.SilkS))
    (fp_text value 1K (at -2.2 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R18-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CIC-TO-MB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 57.875 -69.425)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 0.05) (layer F.SilkS))
    (fp_text value 20K (at -3.1 -0.15) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C23-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /SOUND-1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-U_Horizontal_1EP_style2 (layer F.Cu) (tedit 5DF31710)
    (at 58.45 -94.275 90)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystal")
    (fp_text reference X1 (at -2.1 -2.05) (layer F.SilkS))
    (fp_text value "21.477272 MHz" (at 10.175 8.5) (layer F.Fab))
    (fp_text user %R (at 2.45 7.625 90) (layer F.Fab))
    (pad 3 thru_hole rect (at 8.35 9.25 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole rect (at -3.45 9.25 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at 2.45 9.25 90) (size 11 13.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 4.9 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C41-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C42-Pad2)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-U_Horizontal_1EP_style2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 134.5 -16.5 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R19 (at 5.25 0 90) (layer F.SilkS))
    (fp_text value 1K (at -2.2 -0.075 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R19-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /CIC-TO-CART))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 18.2 -68.3 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74HC139 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U3-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /M2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U3-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /CPU-A15))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /PPU-~CE))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U3-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /WRAM-~CE))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(U3-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 /CPU-A14))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U3-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 /CPU-A13))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 /~ROMSEL))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(U3-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP13 (layer F.Cu) (tedit 5A14249F)
    (at 117.23 -95.5 180)
    (descr "13-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RA1 (at 0.98 -2.7) (layer F.SilkS))
    (fp_text value "12 x 10K" (at 16.51 2.4) (layer F.SilkS))
    (fp_text user %R (at 15.24 0) (layer F.Fab))
    (pad 13 thru_hole oval (at 30.48 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /~NMI))
    (pad 12 thru_hole oval (at 27.94 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /4016-D2))
    (pad 11 thru_hole oval (at 25.4 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /4016-D4))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /4016-D3))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /4016-D0))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /4016-D1))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /~IRQ))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /4017-D2))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /4017-D3))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /4017-D4))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /4017-D0))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /4017-D1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP13.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NESRE:PowerReset-switch-In (layer F.Cu) (tedit 5D97CC0C)
    (at 186.3 -74.25 270)
    (fp_text reference P6 (at 3.725 -3.2 90) (layer F.SilkS))
    (fp_text value "PWR/RST IN" (at 3.325 -5.6 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 0 0) (size 3.25 3.25) (drill 1.65) (layers *.Cu *.Mask)
      (net 16 "Net-(C18-Pad2)"))
    (pad 4 thru_hole circle (at 5 0) (size 3.25 3.25) (drill 1.65) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad2)"))
    (pad 3 thru_hole circle (at 10 0) (size 3.25 3.25) (drill 1.65) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 2 thru_hole circle (at 15 0) (size 3.25 3.25) (drill 1.65) (layers *.Cu *.Mask)
      (net 114 /+9V))
    (pad 1 thru_hole circle (at 22.5 0) (size 3.25 3.25) (drill 1.65) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
  )
  (module NESRE:TrimmerCap-THT (layer F.Cu) (tedit 5D9666E8)
    (at 40.45 -93.15 90)
    (fp_text reference TC1 (at 2.8 1.925 90) (layer F.SilkS))
    (fp_text value 30pF (at 2.925 -1.35 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5.75 2 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(C41-Pad1)"))
    (pad 1 thru_hole circle (at 0 2 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(C41-Pad2)"))
  )
  (module NESRE:EXP_Header (layer F.Cu) (tedit 5D965D3D)
    (at 52.808 -86)
    (fp_text reference P2 (at -2.683 6.625) (layer F.SilkS))
    (fp_text value EXP-Connector (at -2.733 -3.875) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.615 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /~NMI))
    (pad 5 thru_hole circle (at 10.155 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /CPU-A15))
    (pad 6 thru_hole circle (at 12.7 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 /EXP-9))
    (pad 1 thru_hole circle (at -0.008 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 2 thru_hole circle (at 2.532 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole circle (at 5.076 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /EXP-AUDIO-IN))
    (pad 8 thru_hole circle (at 17.775 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 /EXP-7))
    (pad 9 thru_hole circle (at 20.318 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 /EXP-6))
    (pad 14 thru_hole circle (at 33.016 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /~IRQ))
    (pad 13 thru_hole circle (at 30.476 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /4016-D3))
    (pad 20 thru_hole circle (at 48.254 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /4017-D1))
    (pad 23 thru_hole circle (at 55.878 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 /+9V))
    (pad 12 thru_hole circle (at 27.937 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /4016-D1))
    (pad 21 thru_hole circle (at 50.798 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /EXP-VIDEO))
    (pad 22 thru_hole circle (at 53.338 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /EXP-AUDIO-OUT))
    (pad 17 thru_hole circle (at 40.64 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 10 thru_hole circle (at 22.858 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 /EXP-5))
    (pad 16 thru_hole circle (at 38.095 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /4017-D3))
    (pad 18 thru_hole circle (at 43.175 6.501) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /4017-D4))
    (pad 19 thru_hole circle (at 45.715 6.503) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /4017-D0))
    (pad 24 thru_hole circle (at 58.416 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 /CIC-CLK))
    (pad 11 thru_hole circle (at 25.397 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 /~OE2))
    (pad 7 thru_hole circle (at 15.235 6.498) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 /EXP-8))
    (pad 15 thru_hole circle (at 35.555 6.498) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /4017-D2))
    (pad 25 thru_hole circle (at 58.421 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /CPU-D7))
    (pad 26 thru_hole circle (at 55.883 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /CPU-D6))
    (pad 27 thru_hole circle (at 53.343 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /CPU-D5))
    (pad 28 thru_hole circle (at 50.803 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /CPU-D4))
    (pad 29 thru_hole circle (at 48.259 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /CPU-D3))
    (pad 30 thru_hole circle (at 45.72 0.003) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /CPU-D2))
    (pad 31 thru_hole circle (at 43.18 0.001) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /CPU-D1))
    (pad 32 thru_hole circle (at 40.645 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /CPU-D0))
    (pad 33 thru_hole circle (at 38.1 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /4016-D2))
    (pad 34 thru_hole circle (at 35.56 -0.002) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (pad 35 thru_hole circle (at 33.021 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /4016-D0))
    (pad 36 thru_hole circle (at 30.481 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /4016-D4))
    (pad 37 thru_hole circle (at 27.942 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~OE1))
    (pad 38 thru_hole circle (at 25.402 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 /EXP-4))
    (pad 39 thru_hole circle (at 22.863 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 /EXP-3))
    (pad 40 thru_hole circle (at 20.323 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 /EXP-2))
    (pad 41 thru_hole circle (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 /EXP-1))
    (pad 42 thru_hole circle (at 15.24 -0.002) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 /EXP-0))
    (pad 43 thru_hole circle (at 12.705 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /OUT-0))
    (pad 44 thru_hole circle (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /OUT-1))
    (pad 45 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 /OUT-2))
    (pad 46 thru_hole circle (at 5.081 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(P2-Pad46)"))
    (pad 47 thru_hole circle (at 2.537 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 48 thru_hole circle (at -0.003 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VCC))
  )
  (module NESRE:Mod_RF (layer F.Cu) (tedit 5E431874)
    (at 166.146 -20.956)
    (fp_text reference P3 (at 0.314 5.086) (layer F.SilkS))
    (fp_text value MOD-RF (at 6.224 -1.314) (layer F.Fab))
    (pad 9 thru_hole oval (at 22.344 -2.275 90) (size 4.25 9.25) (drill oval 1.16 5.62) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 8 thru_hole oval (at 22.344 16.575 90) (size 4.25 9.25) (drill oval 1.16 5.62) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 7 thru_hole oval (at -6.23 15.9) (size 4.25 9.25) (drill oval 1.16 5.12) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 6 thru_hole oval (at -6.23 5.1) (size 4.25 9.25) (drill oval 1.16 5.12) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 5 thru_hole circle (at 16 2.156) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 4 thru_hole circle (at 12 2.156) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 114 /+9V))
    (pad 3 thru_hole circle (at 8 2.156) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 2 thru_hole circle (at 4 2.156) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 115 /AUDIO))
    (pad 1 thru_hole circle (at 0 2.156) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 /VIDEO))
  )
  (gr_text Unused (at 24.15 -64.2) (layer F.SilkS))
  (gr_text ONES-CPU-01 (at 106.35 -50.65) (layer F.SilkS))
  (gr_text "RST test point" (at 139.2 -47.175) (layer F.SilkS))
  (gr_text "U5        PPU" (at 113.6 -52.825) (layer F.SilkS))
  (gr_text "U4                   SRAM (VRAM)\n" (at 109.1 -17.375) (layer F.SilkS))
  (gr_text "OSHW\nOpen-Source Hardware" (at 80.55 -61.35) (layer F.SilkS))
  (gr_text "SRAM (VRAM)\n" (at 108.45 -23.25) (layer F.SilkS))
  (gr_text 2019 (at 80.65 -58.9) (layer F.SilkS))
  (gr_text "U6      CPU" (at 40.175 -60) (layer F.SilkS))
  (gr_text "SRAM (WRAM)" (at 52.625 -25.775) (layer F.SilkS))
  (gr_text "U1                   SRAM (WRAM)\n" (at 55.05 -19.375) (layer F.SilkS))
  (gr_text Redherring32 (at 121.3 -73.45) (layer F.SilkS))
  (gr_text 5 (at 188.875 -75.825) (layer F.SilkS))
  (gr_text 25 (at 113.55 -87.2) (layer F.SilkS))
  (gr_text "E  C  B" (at 25.75 -85.75) (layer F.SilkS))
  (gr_text 24 (at 113.55 -77.425) (layer B.SilkS))
  (gr_text MOD-RF (at 172.31 -22.55) (layer F.SilkS))
  (gr_text Cartridge-Connector (at 33.15 -13.5) (layer F.SilkS))
  (gr_text "E  C  B" (at 26.55 -96.475) (layer F.SilkS))
  (gr_text 1 (at 51.2 -77.075) (layer B.SilkS))
  (gr_text "21.477272 MHz" (at 66.95 -104.44) (layer F.SilkS))
  (gr_text 5 (at 181.75 -21.33) (layer F.SilkS))
  (gr_text 1 (at 191.325 -82.175) (layer F.SilkS))
  (gr_text 1 (at 188.8 -49.3) (layer F.SilkS))
  (gr_text 1 (at 164.74 -21.31) (layer F.SilkS))
  (gr_text 48 (at 51.075 -87.725) (layer F.SilkS))
  (gr_text 1 (at 177.4 -114.325) (layer F.SilkS))
  (gr_text RP2C02 (at 117.68 -62.44) (layer F.SilkS))
  (gr_text RP2A03 (at 41.54 -49.85) (layer F.SilkS))
  (gr_text 40H368 (at 137.16 -96.52) (layer F.SilkS))
  (gr_text 1 (at 36.35 -10.95) (layer F.SilkS))
  (gr_text 36 (at 127.575 -10.975) (layer F.SilkS))
  (gr_text 74HC139 (at 27.25 -72.1) (layer F.SilkS))
  (gr_text 74HCU04 (at 160.02 -55.88) (layer F.SilkS))
  (gr_text 25 (at 113.5 -87.175) (layer B.SilkS))
  (gr_text 72 (at 127.625 -10.925) (layer B.SilkS))
  (gr_text 40H368 (at 137.16 -83.82) (layer F.SilkS))
  (gr_text 7 (at 191.325 -100.325) (layer F.SilkS))
  (gr_text "Stereo L" (at 26.1 -39.075) (layer B.SilkS))
  (gr_text 37 (at 36.3 -10.825) (layer B.SilkS))
  (gr_text "Stereo R" (at 12.675 -39.05) (layer B.SilkS))
  (gr_text 48 (at 51.2 -87.55) (layer B.SilkS))
  (gr_text 74HC373 (at 106.57 -43.16) (layer F.SilkS))
  (gr_text "EXP-Audio Enable" (at 94.825 -92.35) (layer F.SilkS))
  (gr_text "E  C  B" (at 157.99 -69.58) (layer F.SilkS))
  (gr_text 1 (at 51.275 -77.3) (layer F.SilkS))
  (gr_text 7 (at 158.575 -114.225) (layer F.SilkS))
  (gr_text 24 (at 113.475 -77.4) (layer F.SilkS))
  (gr_text "EXP-Connector\n" (at 50.075 -89.875) (layer F.SilkS))
  (gr_circle (center 12 -82.75) (end 13 -82.75) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 183.3 -112.75) (end 184.36 -112.75) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 152.099 -112.425) (end 153.874 -112.425) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 115.803 -82.791) (end 117.363 -82.791) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 12.225 -112.425) (end 14 -112.425) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 49.3 -83) (end 51.36 -83) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 188.25 -112.425) (end 190.025 -112.425) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0 -98.75) (end 0.025 -96.875) (angle -89.26363163) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 0 -98.75) (end 1.875 -98.75) (angle -89.23610154) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 195.046 -77.497) (end 195.021 -77.997) (angle -86.10737296) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.275 -78) (end 196.275 -118.725) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.275023 -77.000624) (end 196.275 -49.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 195.045456 -77.506001) (end 194.545456 -77.506001) (angle -87.13660569) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.277296 -48.500516) (end 196.275 -44.85) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 195.052015 -48.997) (end 195.020015 -49.501) (angle -86.36704926) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 195.046681 -48.999485) (end 194.546681 -48.999485) (angle -87.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.024998 -100.624833) (end 0.025 -118.725) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15.975 -118.725) (end 0.025 -118.725) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.125 -118.725) (end 148.125 -115.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15.975 -118.725) (end 15.975 -115.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15.975 -115.775) (end 148.125 -115.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 193.275 -44.85) (end 196.275 -44.85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.125 -118.725) (end 196.275 -118.725) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.276 -77.997) (end 195.025 -77.997) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.277 -49.5) (end 195.024 -49.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.277 -48.5) (end 195.024 -48.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.275 -77.005) (end 195.024 -77.006) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 17.097 -4.939) (end 18.907 -4.939) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 147.157 -4.939) (end 148.967 -4.939) (layer Edge.Cuts) (width 0.12))
  (gr_circle (center 4.698 -4.901) (end 6.758 -4.901) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 0.025 -96.875) (end 0.025 -0.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.2 -0.025) (end 140.2 -10.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.775 -0.025) (end 128.775 -10.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 24.975 -0.025) (end 24.975 -10.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 24.975 -10.025) (end 35.375 -10.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 35.375 -0.025) (end 128.775 -0.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.025 -0.025) (end 24.975 -0.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.775 -10.025) (end 140.2 -10.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 35.375 -0.025) (end 35.375 -10.025) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 188.55 -33.775) (end 190.150195 -33.775) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 140.2 -0.025) (end 193.275 -0.025) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 180.303 -4.901) (end 182.363 -4.901) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 193.275 -0.025) (end 193.275 -44.85) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.775 -82.5) (xy 147.825 -84.45) (xy 147.825 -91.1) (xy 147.825 -93.175) (xy 148.325 -93.675)
        (xy 150.1 -93.675) (xy 150.9 -92.875) (xy 150.9 -90.325) (xy 151.25 -89.975) (xy 151.25 -82.475)
        (xy 149.8 -82.475) (xy 149.8 -82.45)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16 -115.8) (xy 148.1 -115.8) (xy 148.1 -118.75) (xy 196.3 -118.75) (xy 196.3 -44.825)
        (xy 193.3 -44.825) (xy 193.3 0) (xy 140.175 0) (xy 140.175 -10) (xy 127.825 -10)
        (xy 127.825 -0.975) (xy 124.825 -0.975) (xy 124.825 -9.975) (xy 125.45 -9.975) (xy 125.45 -12.3)
        (xy 128.375 -15.225) (xy 130.925 -15.225) (xy 130.925 -19.45) (xy 124.6 -19.45) (xy 124.6 -20.775)
        (xy 70.6 -20.775) (xy 70.175 -21.2) (xy 65.85 -21.2) (xy 65.85 -23.325) (xy 46.275 -23.325)
        (xy 44.125 -25.475) (xy 28.875 -25.475) (xy 27.475 -26.875) (xy 25.225 -26.925) (xy 21.725 -25.2)
        (xy 13.925 -25.2) (xy 13.925 -13.725) (xy 26.725 -13.725) (xy 27.075 -13.375) (xy 34.275 -13.375)
        (xy 34.275 -10) (xy 25 -10) (xy 25 0) (xy 0 0) (xy 0 -118.75)
        (xy 16 -118.75)
      )
    )
    (polygon
      (pts
        (xy 130.9 -58.6) (xy 130.1 -57.8) (xy 105.425 -57.8) (xy 104.7 -58.125) (xy 88.65 -58.1)
        (xy 87.875 -57.325) (xy 79.375 -57.325) (xy 72.2 -50.15) (xy 56.25 -50.15) (xy 54.45 -48.35)
        (xy 47.575 -48.35) (xy 45.825 -50.1) (xy 37.85 -50.1) (xy 37.35 -50.6) (xy 33.275 -50.6)
        (xy 32 -49.325) (xy 24.6 -49.325) (xy 23.75 -50.175) (xy 23.025 -50.175) (xy 21.275 -48.425)
        (xy 19.025 -48.425) (xy 17.65 -47.05) (xy 16.3125 -47.05) (xy 15.925 -46.725) (xy 15.65 -46.45)
        (xy 15.025 -46.2) (xy 14.975 -35.375) (xy 12.8 -35.375) (xy 12.8 -28.4) (xy 30.65 -28.4)
        (xy 32.25 -26.8) (xy 45.175 -26.8) (xy 45.55 -26.425) (xy 72.45 -26.425) (xy 73.425 -25.45)
        (xy 84.075 -25.45) (xy 86.475 -23.05) (xy 108.825 -23.05) (xy 109.6375 -23.425) (xy 132.875 -23.4)
        (xy 132.875 -19.775) (xy 132.55 -19.45) (xy 132.55 -15.2) (xy 136.45 -15.2) (xy 136.45 -17.275)
        (xy 138.05 -17.275) (xy 138.05 -15.275) (xy 141.5 -15.275) (xy 141.5 -23.225) (xy 146.625 -23.225)
        (xy 146.625 -26.475) (xy 143.6 -26.475) (xy 142.05 -28.025) (xy 136.825 -28.025) (xy 134.925 -29.925)
        (xy 123.8 -29.925) (xy 123.8 -36.05) (xy 123.325 -36.05) (xy 120.65 -38.725) (xy 116.55 -38.725)
        (xy 116.55 -40.825) (xy 95.425 -40.825) (xy 95.425 -38.6) (xy 92.35 -38.6) (xy 92.35 -36.85)
        (xy 92.55 -35.6) (xy 88.925 -31.975) (xy 76.075 -31.975) (xy 76.075 -33.25) (xy 79.675 -33.25)
        (xy 83.9 -37.475) (xy 83.9 -42.5) (xy 84.075 -42.7) (xy 84.275 -42.9) (xy 91.5 -42.9)
        (xy 91.925 -42.475) (xy 94 -42.475) (xy 94.375 -42.85) (xy 119.325 -42.85) (xy 122 -40.175)
        (xy 127.4 -40.175) (xy 128.6 -38.975) (xy 151.425 -38.975) (xy 151.425 -30.775) (xy 148.75 -30.775)
        (xy 148.75 -35.825) (xy 130.6 -35.825) (xy 128.6 -33.825) (xy 128.6 -31.425) (xy 135.525 -31.425)
        (xy 137.75 -29.2) (xy 142.525 -29.225) (xy 144.075 -27.525) (xy 147.275 -27.525) (xy 148 -28.25)
        (xy 158.4 -28.25) (xy 158.4 -32) (xy 156.2 -32) (xy 156.2 -33.65) (xy 162.375 -33.65)
        (xy 162.375 -36.65) (xy 162.325 -38.325) (xy 162.32983 -38.624518) (xy 162.375 -41.425) (xy 157.15 -41.425)
        (xy 156.625 -41.775) (xy 156.2 -42.175) (xy 156.2 -44.375) (xy 146.975 -44.375) (xy 145.8 -45.55)
        (xy 140.25 -45.55) (xy 139.425 -46.375) (xy 138.75 -46.375) (xy 137.475 -45.1) (xy 133.575 -45.1)
        (xy 133.575 -48.4) (xy 145.7 -48.4) (xy 148.525 -44.9) (xy 152.875 -44.9) (xy 153.825 -45.85)
        (xy 166.825 -45.85) (xy 166.825 -43.425) (xy 178.175 -43.425) (xy 178.175 -40.675) (xy 181.425 -40.675)
        (xy 181.425 -48.675) (xy 174.075 -48.675) (xy 174.075 -50.65) (xy 172.025 -52.7) (xy 168.6 -52.7)
        (xy 168.6 -51.325) (xy 167.025 -51.325) (xy 167.025 -54.3) (xy 161.325 -54.3) (xy 160.9 -54.725)
        (xy 149.25 -54.725) (xy 148.45 -53.925) (xy 146.4 -53.925) (xy 146.4 -55.425) (xy 144.6 -57.225)
        (xy 139.75 -57.225) (xy 138.05 -57.25) (xy 136.8 -58.6)
      )
    )
    (polygon
      (pts
        (xy 164.6425 -20.296) (xy 164.125 -20.275) (xy 163.475 -19.975) (xy 162.75 -18.975) (xy 162.7 -18.8)
        (xy 162.65 -18.325) (xy 162.75 -17.75) (xy 162.8 -17.55) (xy 162.95 -17.3) (xy 163.125 -17.025)
        (xy 163.375 -16.8) (xy 163.625 -16.6) (xy 164.025 -16.425) (xy 164.46 -16.272) (xy 180.71 -16.272)
        (xy 181.2 -16.4) (xy 181.6 -16.575) (xy 181.925 -16.775) (xy 182.125 -16.975) (xy 182.3 -17.2)
        (xy 182.475 -17.45) (xy 182.575 -17.775) (xy 182.65 -18.15) (xy 182.65 -18.65) (xy 182.575 -18.975)
        (xy 182.45 -19.275) (xy 182.325 -19.475) (xy 182.2 -19.625) (xy 181.95 -19.9) (xy 181.65 -20.1)
        (xy 181.3 -20.25) (xy 180.6675 -20.296)
      )
    )
    (polygon
      (pts
        (xy 167 -36.35) (xy 167 -33.75) (xy 170.5 -33.75) (xy 170.5 -30.45) (xy 173.1 -30.45)
        (xy 173.1 -36.35)
      )
    )
    (polygon
      (pts
        (xy 184.825 -53.875) (xy 184 -53.05) (xy 181.975 -53.05) (xy 181.4 -52.475) (xy 181.4 -51.15)
        (xy 182.125 -50.425) (xy 184.025 -50.425) (xy 184.925 -49.525) (xy 187.0875 -49.525) (xy 188.5125 -50.95)
        (xy 188.5375 -52.5) (xy 187.1625 -53.875)
      )
    )
    (polygon
      (pts
        (xy 49.75 -104.325) (xy 45.825 -100.4) (xy 45.825 -95.325) (xy 47.675 -93.475) (xy 47.675 -88.55)
        (xy 40.475 -88.55) (xy 39.575 -87.65) (xy 33.5 -87.65) (xy 32.675 -86.675) (xy 32.675 -80.525)
        (xy 29.4 -80.525) (xy 29.4 -78.95) (xy 19 -78.95) (xy 16.85 -76.8) (xy 16.85 -72.125)
        (xy 19.4 -72.125) (xy 20.575 -73.3) (xy 27.525 -73.3) (xy 29.15 -71.675) (xy 31.725 -71.675)
        (xy 32.375 -72.325) (xy 36.375 -72.325) (xy 38.225 -70.95) (xy 44.05 -70.95) (xy 44.85 -70.15)
        (xy 47.375 -70.15) (xy 47.375 -68.725) (xy 46.125 -68.725) (xy 45.475 -68.075) (xy 36.675 -68.075)
        (xy 35.175 -69.575) (xy 16.875 -69.575) (xy 16.875 -65.25) (xy 20.825 -65.25) (xy 20.825 -59.525)
        (xy 16.325 -59.525) (xy 16.325 -53.525) (xy 70.55 -53.525) (xy 77.2 -60.175) (xy 89.125 -60.175)
        (xy 89.975 -59.325) (xy 123.175 -59.325) (xy 126.15 -62.3) (xy 136.2 -62.3) (xy 139.1 -59.025)
        (xy 144.45 -59.025) (xy 148.525 -55.325) (xy 149.525 -55.325) (xy 149.525 -55.45) (xy 149.5625 -55.325)
        (xy 157.2875 -55.325) (xy 157.725 -55.7) (xy 172.15 -55.7) (xy 174.375 -55.675) (xy 175.725 -57.025)
        (xy 175.425 -98.4) (xy 154.225 -98.3) (xy 151.45 -98.325) (xy 151.075 -97.55) (xy 147.15 -97.55)
        (xy 147.175 -101.825) (xy 144.625 -101.825) (xy 142.575 -103.875) (xy 120.975 -103.875) (xy 118.175 -101.075)
        (xy 82.35 -101.075) (xy 82.35 -104.2) (xy 74.4 -104.2) (xy 70.1 -99.9) (xy 66.975 -99.9)
        (xy 62.55 -104.325)
      )
    )
    (polygon
      (pts
        (xy 185.375 -76.4) (xy 181.25 -72.275) (xy 181.25 -55.45) (xy 182.9625 -55.45) (xy 184.5375 -57.025)
        (xy 187.275 -57) (xy 188.525 -58.25) (xy 188.425 -74.975) (xy 187 -76.4)
      )
    )
    (polygon
      (pts
        (xy 190.65 -98.1) (xy 189.65 -97.1) (xy 187.1 -97.1) (xy 186.2 -96.2) (xy 186.2 -81.35)
        (xy 184.95 -79.975) (xy 186.4 -78.5) (xy 187.85 -80.175) (xy 189.9 -82.7) (xy 189.9 -85.9)
        (xy 192.675 -85.9) (xy 192.675 -97.325) (xy 191.9 -98.1)
      )
    )
    (polygon
      (pts
        (xy 16.15 -89.3) (xy 16.15 -84.175) (xy 21.325 -84.175) (xy 21.325 -86.5) (xy 29.075 -86.5)
        (xy 29.075 -89.3)
      )
    )
    (polygon
      (pts
        (xy 32.95 -94.475) (xy 32.95 -91.85) (xy 38.3 -91.85) (xy 38.3 -94.475)
      )
    )
    (polygon
      (pts
        (xy 25.15 -100.05) (xy 25.15 -97.25) (xy 30.5 -97.25) (xy 30.5 -100.05)
      )
    )
    (polygon
      (pts
        (xy 161.5 -115.625) (xy 158.7 -112.825) (xy 158.7 -102.925) (xy 161.875 -102.925) (xy 161.875 -107.7)
        (xy 172.6 -107.7) (xy 173.625 -108.725) (xy 173.625 -110.3) (xy 168.075 -110.3) (xy 168.075 -112.825)
        (xy 173.2 -112.825) (xy 173.2 -115.625)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15.65 -19.8) (xy 21.55 -19.8) (xy 22.325 -19.025) (xy 52.325 -19.025) (xy 52.7 -18.625)
        (xy 53.1 -18.625) (xy 53.675 -18.475) (xy 62.375 -18.475) (xy 64.925 -15.925) (xy 76.55 -15.925)
        (xy 76.55 -19.825) (xy 82.775 -19.825) (xy 83.175 -19.425) (xy 83.175 -15.925) (xy 84.025 -15.075)
        (xy 88.95 -15.075) (xy 89.775 -15.9) (xy 100.375 -15.9) (xy 101.675 -14.6) (xy 102.575 -14.6)
        (xy 103.2 -15.225) (xy 113.075 -15.225) (xy 113.075 -17.925) (xy 130.3 -17.925) (xy 130.3 -15.75)
        (xy 128.05 -15.75) (xy 125.15 -12.775) (xy 92.95 -12.775) (xy 92.45 -12.275) (xy 48 -12.275)
        (xy 47.175 -13.1) (xy 40.4 -13.1) (xy 37.8 -15.7) (xy 36.925 -16.575) (xy 26.275 -16.575)
        (xy 25.35 -15.65) (xy 15.65 -15.65)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15.624706 -115.842449) (xy 147.724706 -115.842449) (xy 147.724706 -118.842449) (xy 195.949706 -118.842449) (xy 195.949706 -44.867449)
        (xy 192.999706 -44.867449) (xy 193.025 0) (xy 139.749706 -0.067449) (xy 139.749706 -10.017449) (xy 129.446 -10.102)
        (xy 129.449706 -12.592449) (xy 131.924706 -15.067449) (xy 154.474706 -15.067449) (xy 154.474706 -17.267449) (xy 162.699706 -25.492449)
        (xy 163.625 -29.25) (xy 165.125 -29.1) (xy 164.799706 -22.467449) (xy 162.4 -20) (xy 162.2 -19.725)
        (xy 162.025 -19.275) (xy 161.9 -18.85) (xy 161.875 -18.65) (xy 161.85 -18.425) (xy 161.85 -18.275)
        (xy 161.9 -17.775) (xy 161.975 -17.475) (xy 162.075 -17.2) (xy 162.175 -17.025) (xy 162.25 -16.875)
        (xy 162.5 -16.525) (xy 162.9 -16.125) (xy 163.375 -15.825) (xy 163.8 -15.65) (xy 164.075 -15.575)
        (xy 164.4 -15.475) (xy 164.649999 -15.42489) (xy 181.474706 -15.417449) (xy 181.775 -15.425) (xy 181.949706 -15.5)
        (xy 182.25 -15.65) (xy 182.625 -15.9) (xy 182.95 -16.217449) (xy 183.075 -16.359044) (xy 183.35 -16.754949)
        (xy 183.575 -17.179949) (xy 183.724706 -17.748527) (xy 183.774706 -17.998527) (xy 183.799706 -18.192449) (xy 183.799706 -18.592449)
        (xy 183.774706 -18.792449) (xy 183.749706 -18.967449) (xy 183.724706 -19.092449) (xy 183.699706 -19.192449) (xy 183.674706 -19.267449)
        (xy 183.649706 -19.367449) (xy 183.499706 -19.742449) (xy 183.374706 -19.967449) (xy 183.099706 -20.367449) (xy 182.999706 -20.492449)
        (xy 182.824706 -20.667449) (xy 182.724706 -20.742449) (xy 182.649706 -20.817449) (xy 182.549706 -20.892449) (xy 182.174706 -21.142449)
        (xy 182.174706 -46.917449) (xy 183.649706 -48.392449) (xy 188.049706 -48.392449) (xy 188.624706 -48.967449) (xy 188.624706 -74.842449)
        (xy 187.374706 -76.092449) (xy 172.924706 -76.067449) (xy 171.724706 -77.642449) (xy 154.274706 -77.692449) (xy 154.249706 -74.967449)
        (xy 167.324706 -74.967449) (xy 167.849706 -74.442449) (xy 167.849706 -71.842449) (xy 168.474706 -71.217449) (xy 170.949706 -71.217449)
        (xy 172.824706 -73.092449) (xy 179.824706 -73.092449) (xy 180.424706 -72.492449) (xy 180.424706 -65.367449) (xy 179.799706 -64.742449)
        (xy 172.799706 -64.742449) (xy 171.999706 -64.167449) (xy 157.174706 -64.167449) (xy 156.399706 -63.442449) (xy 156.399706 -61.342449)
        (xy 150.399706 -61.342449) (xy 150.399706 -62.492449) (xy 151.249706 -63.017449) (xy 152.399706 -63.017449) (xy 152.399706 -65.417449)
        (xy 150.424706 -67.392449) (xy 150.424706 -74.892449) (xy 148.724706 -74.892449) (xy 146.849706 -73.017449) (xy 146.849706 -68.567449)
        (xy 145.499706 -67.392449) (xy 145.499706 -58.367449) (xy 146.299706 -57.667449) (xy 147.574706 -56.392449) (xy 147.574706 -46.492449)
        (xy 150.949706 -46.492449) (xy 151.549706 -47.092449) (xy 151.549706 -48.392449) (xy 150.675 -49.95) (xy 150.725 -50.5)
        (xy 151.174706 -50.267449) (xy 152.574706 -48.867449) (xy 152.574706 -45.167449) (xy 151.249706 -43.842449) (xy 146.324706 -43.967449)
        (xy 145.099706 -43.429949) (xy 145.099706 -36.354949) (xy 143.899706 -36.354949) (xy 143.899706 -49.129949) (xy 144.699706 -50.217449)
        (xy 144.687206 -56.829949) (xy 144.5625 -63.0625) (xy 144.1375 -63.2875) (xy 143.325 -63.0125) (xy 143.175 -62.5875)
        (xy 143.15 -62.325) (xy 143.699706 -60.992449) (xy 143.699706 -51.442449) (xy 143.099706 -50.217449) (xy 143.099706 -36.367449)
        (xy 141.549706 -36.367449) (xy 141.549706 -37.767449) (xy 139.524706 -39.417449) (xy 135.749706 -39.417449) (xy 133.624706 -41.467449)
        (xy 133.624706 -47.867449) (xy 126.85 -54.092449) (xy 126.875 -68.05) (xy 131.574706 -68.017449) (xy 131.574706 -55.967449)
        (xy 133.949706 -55.967449) (xy 133.949706 -68.342449) (xy 134.099706 -68.292449) (xy 136.074706 -66.317449) (xy 136.024706 -66.217449)
        (xy 136.024706 -54.217449) (xy 135.174706 -53.367449) (xy 135.174706 -51.617449) (xy 137.924706 -48.867449) (xy 137.924706 -44.017449)
        (xy 140.249706 -44.017449) (xy 140.249706 -52.167449) (xy 141.624706 -53.542449) (xy 141.624706 -66.142449) (xy 144.849706 -69.367449)
        (xy 144.849706 -73.142449) (xy 148.574706 -76.867449) (xy 148.574706 -78.717449) (xy 146.674706 -78.717449) (xy 141.649706 -73.692449)
        (xy 139.174706 -73.692449) (xy 139.174706 -71.692449) (xy 127.574706 -71.692449) (xy 127.574706 -76.367449) (xy 128.874706 -77.667449)
        (xy 139.975 -77.675) (xy 139.975 -81.175) (xy 141.625 -81.167449) (xy 141.625 -78.792449) (xy 144.724706 -78.792449)
        (xy 144.724706 -84.467449) (xy 146.649706 -86.392449) (xy 146.649706 -88.842449) (xy 144.724706 -90.767449) (xy 144.724706 -96.992449)
        (xy 147.599706 -99.867449) (xy 150.774706 -99.867449) (xy 151.974706 -98.379949) (xy 152.024706 -94.617449) (xy 152.474706 -94.267449)
        (xy 156.274375 -94.276537) (xy 156.274706 -91.892449) (xy 171.699706 -91.817449) (xy 172.099706 -106.854949) (xy 173.774706 -108.417449)
        (xy 173.774706 -109.617449) (xy 173.374706 -110.317449) (xy 173.374706 -113.917449) (xy 172.799706 -115.617449) (xy 161.449706 -115.617449)
        (xy 160.649706 -114.892449) (xy 160.624706 -106.567449) (xy 158.699706 -104.804949) (xy 123.824706 -104.567449) (xy 123.274706 -103.867449)
        (xy 76.174706 -103.867449) (xy 75.35 -102.95) (xy 75.27593 -89.047033) (xy 75.143 -88.966) (xy 74.972 -88.817449)
        (xy 62.124706 -88.817449) (xy 60.724706 -87.417449) (xy 56.549706 -87.417449) (xy 56.5375 -84.7) (xy 58.3625 -84.7)
        (xy 58.374706 -80.7) (xy 56.499706 -80.7) (xy 56.499706 -76.167449) (xy 55.199706 -74.867449) (xy 49.474706 -74.867449)
        (xy 48.799706 -75.542449) (xy 45.624706 -75.542449) (xy 44.974706 -74.892449) (xy 44.974706 -71.167449) (xy 46.874706 -69.267449)
        (xy 46.874706 -61.542449) (xy 44.8 -58.825) (xy 44.8 -50.075) (xy 43.624706 -49.817449) (xy 43.624706 -43.817449)
        (xy 39.099706 -43.817449) (xy 39.099706 -49.042449) (xy 43 -52.25) (xy 43 -76.15) (xy 44.374706 -78.217449)
        (xy 49.649706 -78.217449) (xy 50.299706 -77.567449) (xy 52.999706 -77.567449) (xy 54.325 -78.2375) (xy 54.325 -90.1125)
        (xy 55.099706 -91.542449) (xy 58.799706 -91.542449) (xy 60.05 -92.55) (xy 60 -100.125) (xy 55.874706 -103.867449)
        (xy 12.275 -103.925) (xy 12.274706 -102.742449) (xy 12.274706 -75.592449) (xy 11.725 -75) (xy 11.65 -14.95)
        (xy 12.049706 -14.242449) (xy 33.649706 -14.242449) (xy 35.499706 -12.392449) (xy 38.099706 -12.392449) (xy 39.024706 -11.467449)
        (xy 39.024706 -0.992449) (xy 36.332 -0.994842) (xy 36.332 -10.095158) (xy 24.599706 -10.092449) (xy 24.599706 -0.092449)
        (xy -0.350294 -0.092449) (xy -0.350294 -118.842449) (xy 15.624706 -118.842449)
      )
    )
    (polygon
      (pts
        (xy 190.75 -98.075) (xy 190.3 -97.8) (xy 186.45 -97.8) (xy 186.075 -97.425) (xy 186.075 -94.95)
        (xy 180.75 -94.95) (xy 172.5 -87.525) (xy 159.65 -87.525) (xy 153.95 -81.825) (xy 153.95 -78.55)
        (xy 169.2 -78.55) (xy 169.2 -81.1) (xy 171.6 -81.1) (xy 171.575 -78.55) (xy 172.05 -78.25)
        (xy 186.675 -78.25) (xy 190.25 -81.825) (xy 190.25 -83.75) (xy 189.45 -84.55) (xy 189.45 -85.275)
        (xy 189.975 -85.8) (xy 192.45 -85.8) (xy 192.65 -86) (xy 192.65 -97.25) (xy 191.825 -98.075)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C17-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.443429 -70.443429) (xy 183.368429 -68.368429) (xy 182.318429 -66.543429) (xy 182.318429 -65.443429) (xy 181.643429 -64.768429)
        (xy 181.618429 -64.043429) (xy 181.618429 -64.018429) (xy 183.068429 -64.018429) (xy 187.793429 -68.743429) (xy 185.793429 -70.743429)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.625 -103.575) (xy 81.625 -98.45) (xy 74.875 -98.45) (xy 70.075 -93.65) (xy 65.55 -93.65)
        (xy 61.25 -89.35) (xy 55.375 -89.35) (xy 53.65 -87.625) (xy 53.65 -78.35) (xy 51.6 -76.3)
        (xy 47.8 -76.3) (xy 43.325 -80.775) (xy 39.675 -80.775) (xy 39.675 -86.6) (xy 40.925 -87.85)
        (xy 49.1 -87.85) (xy 50.55 -89.3) (xy 50.55 -102.3) (xy 51.25 -103) (xy 62.8 -103)
        (xy 66.4 -99.4) (xy 70.55 -99.4) (xy 74.975 -103.575)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.596403 -69.346403) (xy 26.596403 -71.346403) (xy 23.996403 -73.946403) (xy 22.096403 -73.946403) (xy 22.096403 -77.471403)
        (xy 22.171403 -77.596403) (xy 29.021403 -77.596403) (xy 29.696403 -76.921403) (xy 30.346403 -77.571403) (xy 31.471403 -77.571403)
        (xy 32.196403 -76.846403) (xy 32.896403 -77.546403) (xy 34.071403 -77.546403) (xy 34.771403 -76.846403) (xy 35.471403 -77.546403)
        (xy 36.596403 -77.546403) (xy 37.121403 -77.021403) (xy 37.121403 -74.496403) (xy 36.45 -73.9375) (xy 36.45 -71.4625)
        (xy 35.15 -70) (xy 35.15 -67.9) (xy 36.8 -67.9375) (xy 37.301799 -70.5625) (xy 37.898202 -73.221403)
        (xy 38.671403 -74.496403) (xy 38.671403 -77.021403) (xy 37.321403 -78.371403) (xy 29.021403 -78.371403) (xy 25.146403 -82.246403)
        (xy 23.296403 -82.246403) (xy 19.321403 -78.271403) (xy 19.321403 -69.346403)
      )
    )
  )
  (zone (net 114) (net_name /+9V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.05 -53.5125) (xy 180.05 -44.9875) (xy 179.925 -44.575) (xy 178.4 -43.85) (xy 178.075 -43.2)
        (xy 178.075 -41.475) (xy 179.525 -39.65) (xy 179.371 -22.671) (xy 179 -20.475) (xy 179.4 -18)
        (xy 176.9 -18.05) (xy 176.5 -19.96) (xy 177.5945 -23.74125) (xy 177.65 -38.725) (xy 176.6 -40.925)
        (xy 176.6 -41.45) (xy 176.6 -48.575) (xy 178.5 -50.475) (xy 178.5 -56.85) (xy 179.725 -58.075)
        (xy 181.5 -58.075) (xy 181.925 -58.2) (xy 182.7 -58.2) (xy 184.5 -59.95) (xy 187.025 -60.7375)
        (xy 187.625 -59.9125) (xy 188 -57.325) (xy 185.675 -54.75) (xy 181.225 -54.75)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.625 -106.425) (xy 165.625 -104.625) (xy 167.225 -103.025) (xy 167.225 -101.35) (xy 166.45 -100.575)
        (xy 163.825 -100.55) (xy 163.825 -103.2) (xy 164.2 -103.575) (xy 164.2 -106.425)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.029975 -54.1) (xy 154.025 -56.2) (xy 151.275 -56.2) (xy 151.279975 -54.1)
      )
    )
  )
  (zone (net 29) (net_name "Net-(C42-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25.65 -98.275) (xy 25.6125 -93.2125) (xy 27.499413 -91) (xy 27.500588 -89.80017) (xy 27.45 -88.35)
        (xy 27.65 -87.55) (xy 27.9 -87.55) (xy 36.25 -87.725) (xy 36.55 -82.6) (xy 38.15 -82.75)
        (xy 38.1 -83.3875) (xy 37.825 -87.6625) (xy 44.425 -87.675) (xy 50.8 -94.05) (xy 56.975 -94.05)
        (xy 58.1 -93.55) (xy 59.15 -94.7) (xy 58.55 -95.075) (xy 57.425 -96.2) (xy 50.1 -96.2)
        (xy 44.95 -91.1) (xy 35.525 -91.1) (xy 34.95 -91.675) (xy 34.95 -92.45) (xy 35.1 -93.05)
        (xy 35 -93.55) (xy 34.875 -93.75) (xy 34.525 -94.025) (xy 33.9625 -94.2) (xy 33.55 -94.2)
        (xy 28.05 -94.2) (xy 27.35 -94.575) (xy 27.35 -98.275)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.05 -73.9) (xy 27.05 -73.225) (xy 31.025 -69.8) (xy 34.325 -69.8) (xy 34.3 -71.225)
        (xy 34.95 -71.875) (xy 34.95 -73.95) (xy 32.425 -73.95) (xy 32.175 -73.95) (xy 32.175 -72.025)
        (xy 29.85 -72.025) (xy 29.85 -73.9)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.3 -55.675) (xy 47.95 -55.7) (xy 47.95 -47.925) (xy 46.15 -46.125) (xy 46.15 -44.175)
        (xy 48.825 -44.175) (xy 48.825 -46.45) (xy 49.525 -47.15) (xy 51.275 -47.15) (xy 51.275 -44.175)
        (xy 54.025 -44.175) (xy 54.025 -47.325) (xy 55.3 -48.6)
      )
    )
  )
  (zone (net 28) (net_name "Net-(C41-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.3625 -99.775) (xy 57.25 -99.575) (xy 58.4 -99.925) (xy 59.175 -98.95) (xy 57.85 -98.125)
        (xy 42.85 -98.125) (xy 41.975 -98.45) (xy 41.975 -99.175) (xy 42.375 -99.875) (xy 43.325 -99.875)
        (xy 44.4875 -99.775)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.589085 -103.35) (xy 13.125 -103.325) (xy 12.925 -75.35) (xy 12.225 -74.675) (xy 12.425 -18.275)
        (xy 21.639085 -18.2) (xy 21.639085 -20.225) (xy 15.239085 -20.225) (xy 14.639085 -20.825) (xy 14.639085 -39.15)
        (xy 15.889085 -40.4) (xy 15.889085 -48.6) (xy 19.014085 -51.725) (xy 19.014085 -58.175) (xy 16.913293 -60.175)
        (xy 16.986708 -75.175) (xy 18.475 -75.125) (xy 18.475 -76.725) (xy 17.125 -76.725) (xy 17.1 -80.425)
        (xy 19.6 -80.425) (xy 19.825 -80.575) (xy 20.075 -80.9) (xy 20.075 -81.55) (xy 18.339085 -82.975)
        (xy 17.064085 -82.975) (xy 15.839085 -84.2) (xy 15.85 -89.975) (xy 24.95 -89.925) (xy 24.95 -86.175)
        (xy 29.139085 -82.1) (xy 34.889085 -82.1) (xy 34.889085 -86.2) (xy 26.9 -86.2) (xy 26.95 -89.95)
        (xy 25.875 -91.475) (xy 25.675 -91.725) (xy 25.35 -91.9) (xy 22.214085 -91.9) (xy 22.214085 -96.325)
        (xy 15.889085 -96.325) (xy 15.889085 -100.625) (xy 54.614085 -100.625) (xy 54.614085 -103.35)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13.725 -33.2) (xy 21.025 -33.2) (xy 22.575 -31.65) (xy 31.175 -31.65) (xy 34.675 -28.25)
        (xy 37.875 -28.25) (xy 37.9 -30.4) (xy 39.475 -30.4) (xy 39.475 -28.125) (xy 67.425 -28.125)
        (xy 70.575 -31.275) (xy 84.75 -31.275) (xy 86 -30.025) (xy 86 -26.85) (xy 87.175 -25.675)
        (xy 107.925 -25.675) (xy 108.375 -26.125) (xy 128.475 -26.125) (xy 128.475 -24.45) (xy 108.9 -24.45)
        (xy 108.4 -23.95) (xy 86.5 -23.95) (xy 84.425 -26.05) (xy 73.75 -26.05) (xy 72.775 -27.025)
        (xy 45.8 -27) (xy 45.475 -27.35) (xy 32.775 -27.35) (xy 31.025 -28.95) (xy 13.775 -28.95)
      )
    )
  )
  (zone (net 16) (net_name "Net-(C18-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.688232 -74.875) (xy 186.313232 -74.875) (xy 186.4 -72.7) (xy 181.688232 -71.525)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.825 -9.6) (xy 124.825 -9.975) (xy 125.2 -9.975) (xy 125.8 -10.575) (xy 125.819 -12.289)
        (xy 126.88825 -13.25025) (xy 127.02175 -13.68175) (xy 127.25 -14.025) (xy 127.237 -16.706) (xy 127.333 -16.864)
        (xy 127.508 -16.96) (xy 127.775 -16.975) (xy 130.625 -21.0625) (xy 130.625 -21.55) (xy 126.9375 -25.3125)
        (xy 127.8 -26.125) (xy 128.825 -25.25) (xy 141.325 -25.25) (xy 141.325 -23.4) (xy 144 -23.4)
        (xy 144 -25.95) (xy 141 -28.95) (xy 141 -31.825) (xy 139.575 -31.825) (xy 138.85 -32.55)
        (xy 138.85 -36.725) (xy 131.9 -36.725) (xy 131.175 -37.45) (xy 131.175 -48.35) (xy 131.7 -48.35)
        (xy 132.975 -47.075) (xy 132.975 -40.9) (xy 135.1 -38.775) (xy 139.15 -38.775) (xy 140.425 -37.5)
        (xy 140.425 -34.025) (xy 141.55 -32.9) (xy 150.775 -32.9) (xy 150.775 -36.375) (xy 150.3 -36.85)
        (xy 147.75 -36.85) (xy 145.725 -38.875) (xy 145.725 -40.8) (xy 151.675 -40.8) (xy 151.675 -39.95)
        (xy 151.45 -39.95) (xy 151.45 -31.625) (xy 152.375 -30.7) (xy 156.225 -30.7) (xy 156.225 -28.7)
        (xy 157.875 -28.7) (xy 158.175 -30.7) (xy 158.175 -37.525) (xy 155.275 -37.525) (xy 155.275 -38.325)
        (xy 159.375 -38.325) (xy 159.375 -33.275) (xy 161.4 -33.275) (xy 162.9 -34.775) (xy 162.9 -43.275)
        (xy 163.65 -44.025) (xy 172.175 -44.025) (xy 172.925 -44.775) (xy 172.925 -46.925) (xy 171.65 -48.2)
        (xy 171.65 -51.8) (xy 173.525 -53.675) (xy 173.525 -56.05) (xy 172.3 -57.275) (xy 172.3 -60.35)
        (xy 172.3 -60.65) (xy 180.15 -60.65) (xy 180.775 -60.65) (xy 185.7 -65.575) (xy 187.45 -63.825)
        (xy 182.325 -58.7) (xy 177.1 -58.7) (xy 176.075 -57.675) (xy 176.075 -40.175) (xy 176.521 -38.436)
        (xy 176.585 -24.531) (xy 175.34 -19.71) (xy 175.45 -17.9) (xy 172.8 -18.1) (xy 173.375 -23.85)
        (xy 173.525 -25.3) (xy 173.5 -27.05) (xy 173.5 -36.075) (xy 172 -37.575) (xy 166.525 -37.575)
        (xy 165.675 -36.725) (xy 165.675 -32.925) (xy 161.975 -29.225) (xy 161.975 -26.45) (xy 159.8 -24.275)
        (xy 157.525 -24.275) (xy 157.05 -23.8) (xy 157.05 -23.325) (xy 153.425 -19.7) (xy 153.425 -15.95)
        (xy 143.275 -15.95) (xy 141.25 -17.975) (xy 131.15 -17.975) (xy 130.375 -17.2) (xy 130.364 -14.649)
        (xy 128.8 -13.1) (xy 128.784 -11.447) (xy 127.625 -9.625)
      )
    )
  )
  (zone (net 15) (net_name "Net-(C11-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184 -53.625) (xy 184.95 -53.625) (xy 186.875 -50.225) (xy 183.725 -50.225) (xy 180.55 -47.05)
        (xy 180.75 -52.45) (xy 181.7 -53.625) (xy 184.025 -53.625) (xy 183.925 -53.625)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.5 -53.1) (xy 125.5 -45.45) (xy 126.825 -44.125) (xy 126.825 -35.25) (xy 128.2 -33.875)
        (xy 128.875 -33.875) (xy 128.875 -48.075) (xy 128.275 -48.675) (xy 128.275 -51.75) (xy 126.875 -53.15)
        (xy 126.275 -53.875) (xy 125.95 -53.875)
      )
    )
  )
  (zone (net 31) (net_name /SYSTEM-CLK) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.35 -89.35) (xy 23.525 -89.3) (xy 23.525 -88.475) (xy 23.5 -87.925) (xy 20.965568 -84.95)
        (xy 19.3 -84.95)
      )
    )
  )
  (zone (net 17) (net_name /EXP-AUDIO-OUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.403537 -62.65) (xy 166.778537 -62.65) (xy 168.85 -61.45) (xy 164.05 -61.45) (xy 165.253537 -62.65)
        (xy 165.378537 -62.65)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.925 -42.425) (xy 156.9 -40.975) (xy 155.8125 -42.475) (xy 155.7375 -51.075) (xy 156.825 -51.05)
        (xy 167.125 -51.05) (xy 167.075 -54.53835) (xy 156.775 -54.53835) (xy 156.325 -55.35) (xy 156.325 -58.6)
        (xy 167.675 -58.56335) (xy 168.7 -57.9375) (xy 168.7 -50.8625) (xy 167.675 -49.85) (xy 161.275 -49.85)
        (xy 160.875 -49.45) (xy 160.675 -48.15) (xy 161.3 -47.225) (xy 164.4 -47.225) (xy 166.374 -45.569)
        (xy 166.375 -44.55) (xy 163.25 -44.55) (xy 161.225 -42.675) (xy 160.975 -42.46335)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.02327 -57.3) (xy 173.99827 -56.275) (xy 157.57327 -56.275) (xy 157.1 -56.025) (xy 148.6 -56.025)
        (xy 144.59827 -59.775) (xy 139.99827 -59.775) (xy 138.82327 -60.95) (xy 138.82327 -62.75) (xy 138.625 -63.1)
        (xy 138.425 -63.35) (xy 125.37327 -63.35) (xy 122.47327 -60.45) (xy 92.29827 -60.45) (xy 90.9625 -61.775)
        (xy 88.8875 -61.775) (xy 87.87327 -60.75) (xy 76.82327 -60.75) (xy 70.22327 -54.15) (xy 17.32327 -54.15)
        (xy 17.32327 -58.25) (xy 19.248412 -58.25) (xy 19.24827 -56) (xy 69.575 -55.930245) (xy 72.125 -58.355245)
        (xy 72.19827 -61.75) (xy 73.62327 -63.175) (xy 73.62327 -69) (xy 74.69827 -70.075) (xy 83.87327 -70.075)
        (xy 85.57327 -68.375) (xy 90.225 -68.375) (xy 90.59827 -67.85) (xy 93.075 -67.85) (xy 93.69827 -68.375)
        (xy 93.69827 -71.075) (xy 95.32327 -71.075) (xy 95.32327 -67.3) (xy 95.325 -62.05) (xy 95.725 -61.525)
        (xy 120.82327 -61.525) (xy 121.49827 -62.2) (xy 121.49827 -68.475) (xy 122.09827 -69.075) (xy 139.99827 -69.075)
        (xy 143.24827 -65.825) (xy 143.24827 -61.75) (xy 143.62327 -61.375) (xy 146.39827 -61.375) (xy 146.72327 -61.05)
        (xy 148.12327 -61.05) (xy 148.84827 -60.325) (xy 148.84827 -58.35) (xy 149.07327 -58.125) (xy 167.84827 -58.125)
        (xy 171.32327 -61.6) (xy 171.32327 -74.95) (xy 169.67327 -76.6) (xy 171.97327 -78.9) (xy 171.97327 -81.9)
        (xy 171.24827 -82.625) (xy 167.14827 -82.625) (xy 166.69827 -83.075) (xy 162.39827 -83.075) (xy 162.39827 -84.125)
        (xy 167.84827 -84.125) (xy 171.77327 -88.05) (xy 171.77327 -95.25) (xy 160.44827 -95.25) (xy 160.14827 -94.95)
        (xy 153.77327 -94.95) (xy 152.47327 -96.25) (xy 152.475 -97.7) (xy 174.7 -97.7)
      )
    )
    (polygon
      (pts
        (xy 84.6 -65.45) (xy 84.6 -63.65) (xy 90.95 -63.65) (xy 90.95 -65.45)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.675 -34.35) (xy 79.175 -34.35) (xy 83.125 -38.3) (xy 83.125 -43.65) (xy 88.475 -43.65)
        (xy 91.55 -46.2) (xy 91.975 -46.2) (xy 94.0375 -46.2) (xy 95.7125 -44.525) (xy 119.3 -44.525)
        (xy 120.675 -45.9) (xy 126.525 -45.9) (xy 127.225 -45.2) (xy 131.675 -45.2) (xy 131.675 -47.975)
        (xy 127.9 -47.975) (xy 127.45 -48.425) (xy 120.825 -48.425) (xy 118.075 -45.675) (xy 96.9125 -45.6625)
        (xy 94.6375 -47.9375) (xy 82.6 -47.95) (xy 74.675 -40.025)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.6 -93.4) (xy 51.3125 -93.4) (xy 48.725 -91.025) (xy 48.725 -87.75) (xy 51.925 -84.55)
        (xy 51.925 -79.475) (xy 53.375 -79.475) (xy 53.375 -91.55) (xy 53.95 -92.125) (xy 54.6 -92.325)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.272236 -97.143587) (xy 76.272236 -102.493587) (xy 77.097236 -103.318587) (xy 124.047236 -103.318587) (xy 124.672236 -103.943587)
        (xy 158.422236 -103.943587) (xy 160.125 -104.9) (xy 160.7125 -104.875) (xy 161.275 -104) (xy 161.25 -103.643587)
        (xy 161.022236 -102.493587) (xy 158.497236 -99.968587) (xy 158.497236 -94.893587) (xy 152.622236 -94.893587) (xy 152.622236 -99.343587)
        (xy 151.397236 -100.568587) (xy 148.247236 -100.568587) (xy 146.972236 -101.843587) (xy 128.597236 -101.843587) (xy 128.597236 -100.018587)
        (xy 126.697236 -98.018587) (xy 126.697236 -91.793587) (xy 128.597236 -89.893587) (xy 128.597236 -83.368587) (xy 126.722236 -81.493587)
        (xy 126.722236 -71.918587) (xy 120.947236 -71.918587) (xy 115.075 -77.8) (xy 115.072236 -79.068587) (xy 123.972236 -79.068587)
        (xy 125.222236 -80.318587) (xy 125.222236 -82.768587) (xy 126.447236 -84.118587) (xy 126.447236 -86.618587) (xy 123.347236 -89.718587)
        (xy 123.347236 -92.918587) (xy 122 -93.05) (xy 122.05 -94.3) (xy 123.297236 -94.243587) (xy 123.297236 -97.493587)
        (xy 122.747236 -98.043587) (xy 89.672236 -97.968587) (xy 89.047236 -98.568587) (xy 88.997236 -98.568587) (xy 84.147236 -98.568587)
        (xy 78.384 -94.687) (xy 78.3185 -94.588) (xy 76.3935 -94.588)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.2 -82.225) (xy 186.95 -82.225) (xy 186.95 -80.3) (xy 186.35 -79.3) (xy 185.55 -78.85)
        (xy 172.225 -78.85)
      )
    )
  )
  (zone (net 27) (net_name "Net-(C41-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.4 -98.725) (xy 33.725 -98.725) (xy 33.725 -96.775) (xy 38.05 -96.775) (xy 40 -94.825)
        (xy 44.9 -94.825) (xy 47.075 -97) (xy 48.15 -95.925) (xy 44.025 -91.8) (xy 38.175 -91.8)
        (xy 35.3 -94.85) (xy 28.375 -94.85) (xy 28.375 -98.725)
      )
    )
  )
  (zone (net 3) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.25 -68.05) (xy 121.65 -68.025) (xy 121.65 -61.425) (xy 125.4 -57.725) (xy 125.925 -57.6)
        (xy 126.225 -58.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.84298 -88.1) (xy 171.79298 -88.1) (xy 171.79298 -90.75) (xy 164.06798 -90.75) (xy 164.06798 -88.375)
        (xy 161.56798 -88.375) (xy 161.56798 -90.75) (xy 153.84298 -90.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16 -115.8) (xy 148.1 -115.8) (xy 148.1 -118.75) (xy 161.7 -118.75) (xy 161.7 -115.6)
        (xy 160.65 -114.65) (xy 158.7 -108.7) (xy 158.7 -104.75) (xy 123.9 -104.55) (xy 123.25 -103.85)
        (xy 12.25 -103.85) (xy 12.3 -75.55) (xy 11.75 -75) (xy 11.703914 -26.524997) (xy 11.7 -26.45)
        (xy 11.7 -24.25) (xy 11.8 -14.55) (xy 11.8 -14.4) (xy 11.8 -14.3) (xy 16.35 -14.3)
        (xy 16.85 -14.3) (xy 17.25 -14.3) (xy 17.35 -14.3) (xy 17.505691 -14.299954) (xy 25 -14.3)
        (xy 25 0) (xy 0 0) (xy 0 -118.75) (xy 16 -118.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.3 -118.75) (xy 196.3 -99.5) (xy 180.85 -99.5) (xy 180.85 -94.95) (xy 171.8 -94.95)
        (xy 171.8 -104.9) (xy 181.65 -104.75) (xy 181.65 -114.85) (xy 178.35 -114.825) (xy 178.35 -118.475)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6.8 0) (xy 0 0) (xy 0 -118.75) (xy 6.8 -118.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.3 -44.85) (xy 193.35 -44.85) (xy 193.3 0) (xy 154.9 0) (xy 154.9 -17.75)
        (xy 156.45 -19.25) (xy 158.1 -20.85) (xy 163.3 -20.85) (xy 162.4 -19.95) (xy 161.95 -19.1)
        (xy 162.1 -17.65) (xy 162.15 -17.1) (xy 162.4 -16.65) (xy 162.85 -16.2) (xy 163.35 -15.9)
        (xy 163.9 -15.65) (xy 164.65 -15.45) (xy 168.15 -15.45) (xy 173.05 -15.4) (xy 178 -15.4)
        (xy 180.6 -15.4) (xy 181.85 -15.5) (xy 182.7 -15.9) (xy 183.6 -17.1) (xy 184.25 -18.8)
        (xy 183.45 -20.8) (xy 183.05 -40.9) (xy 186.2 -40.9) (xy 186.2 -48.5) (xy 196.3 -48.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.3 -44.8) (xy 193.35 -44.8) (xy 193.35 0) (xy 174.1 0) (xy 174.1 -16.3)
        (xy 177.05 -16.3) (xy 180.65 -16.3) (xy 183.35 -17.3) (xy 184.25 -18.75) (xy 183.55 -20.15)
        (xy 182.25 -20.9) (xy 177.05 -20.9) (xy 177.05 -38.05) (xy 187.5 -38.05) (xy 187.5 -48.5)
        (xy 196.3 -48.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.35 -99) (xy 180.15 -99) (xy 180.15 -87.35) (xy 177.4 -87.35) (xy 177.4 -118.75)
        (xy 196.3 -118.75)
      )
    )
  )
)
