(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "GAppleII HexConn Adapter")
    (date "2024-01-02")
    (rev "0.1")
    (company "https://github.com/kobbler248/GAppleII")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers")
    )
  )
  (net 0 "")
  (net 1 "/GND")
  (net 2 "/PH0")
  (net 3 "/PH1")
  (net 4 "/DIR")
  (net 5 "/PH3")
  (net 6 "/WGATE")
  (net 7 "/5VDC")
  (net 8 "/DRVEN")
  (net 9 "/RDATA")
  (net 10 "/WDATA")
  (net 11 "/WPT")
  (net 12 "unconnected-(J2-Pad4)")
  (net 13 "unconnected-(J1-Pad34)")
  (net 14 "unconnected-(J1-Pad26)")
  (net 15 "unconnected-(J1-Pad16)")
  (net 16 "unconnected-(J1-Pad14)")
  (net 17 "unconnected-(J1-Pad12)")
  (net 18 "unconnected-(J1-Pad8)")
  (net 19 "unconnected-(J1-Pad6)")
  (net 20 "unconnected-(J1-Pad5)")
  (net 21 "unconnected-(J1-Pad4)")
  (net 22 "unconnected-(J1-Pad3)")
  (net 23 "unconnected-(J1-Pad2)")
  (net 24 "unconnected-(P3-Pad19)")
  (net 25 "unconnected-(P3-Pad17)")
  (net 26 "unconnected-(P3-Pad15)")
  (net 27 "unconnected-(P3-Pad13)")
  (net 28 "unconnected-(P3-Pad9)")
  (net 29 "/5VDC{slash}SEL")
  (footprint "Connector_IDC:IDC-Header_2x17_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 120.015 100.33 90)
    (descr "Through hole IDC box header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x17 2.54mm double row")
    (property "Sheetfile" "AppleDiskII2GotekHcX.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 6.985 -3.175 90) (layer "F.SilkS"))
    (fp_text value "Gotek Floppy Interface" (at -1.27 20.32) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 20.32) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 1 "/GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/DRVEN") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/DIR") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/PH3") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/WDATA") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/WGATE") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J1-Pad26)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole circle (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/WPT") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/RDATA") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/5VDC{slash}SEL") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole circle (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J1-Pad34)") (pinfunction "Pin_34") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x17_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 151.765 90.17)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "AppleDiskII2GotekHcX.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P4" (at -2.54 -0.635 90) (layer "F.SilkS"))
    (fp_text value "Gotek UART" (at -1.905 1.27 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/PH0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/PH1") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 163.185 90.805 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "AppleDiskII2GotekHcX.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -2.54 0.665 90) (layer "B.SilkS"))
    (fp_text value "Gotek Pwr" (at -1.905 -5.07) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/5VDC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5EAC9A07)
    (at 121.285 90.805 -90)
    (descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
    (property "Sheetfile" "AppleDiskII2GotekHcX.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P3" (at 6.985 4.445 90) (layer "B.SilkS"))
    (fp_text value "Apple Disk II Interface" (at -1.905 -11.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -11.43) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 1 "/GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/PH0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/PH1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/DIR") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/PH3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(P3-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/WGATE") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/5VDC") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/5VDC{slash}SEL") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(P3-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/DRVEN") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(P3-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/RDATA") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(P3-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/WDATA") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(P3-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/WPT") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Symbol_6.7x6mm_SilkScreen" (layer "B.Cu")
    (tedit 6594B789)
    (at 158.115 94.615 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Symbol_6.7x6mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (gr_arc (start 115.57 88.265) (mid 115.941974 87.366974) (end 116.84 86.995) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 163.83 86.995) (mid 164.728026 87.366974) (end 165.1 88.265) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 116.84 104.14) (mid 115.941974 103.768026) (end 115.57 102.87) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.84 104.14) (end 163.83 104.14) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 163.83 86.995) (end 116.84 86.995) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 115.57 88.265) (end 115.57 102.87) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 165.1 88.265) (end 165.1 102.87) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 165.1 102.87) (mid 164.728026 103.768026) (end 163.83 104.14) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Adapts from the Apple Disk II Interface\nto the Gotek Floppy Emu w/HxC Firmware." (at 133.35 102.87) (layer "B.SilkS"))
  (gr_text "a kobbler248 design" (at 158.115 95.25) (layer "B.SilkS"))
  (gr_text "GAppleII HexConn Adapter v0.1" (at 164.465 102.87) (layer "B.SilkS"))
  (gr_text "Docs: http://tinyurl.com/HxC2001-AppleII\nDesign: https://github.com/kobbler248/GAppleII/" (at 116.205 88.265) (layer "F.SilkS"))
)
