<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="27.5" y1="12" x2="6.5" y2="12" width="0" layer="20"/>
<wire x1="6.5" y1="12" x2="4" y2="9.5" width="0" layer="20" curve="90"/>
<wire x1="4" y1="9.5" x2="3" y2="8.5" width="0" layer="20" curve="-90"/>
<wire x1="3" y1="8.5" x2="2.5" y2="8.5" width="0" layer="20"/>
<wire x1="2.5" y1="8.5" x2="0" y2="6" width="0" layer="20" curve="90"/>
<wire x1="0" y1="6" x2="2.5" y2="3.5" width="0" layer="20" curve="90"/>
<wire x1="2.5" y1="3.5" x2="3" y2="3.5" width="0" layer="20"/>
<wire x1="3" y1="3.5" x2="4" y2="2.5" width="0" layer="20" curve="-90"/>
<wire x1="4" y1="2.5" x2="6.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="6.5" y1="0" x2="27.5" y2="0" width="0" layer="20"/>
<wire x1="27.5" y1="0" x2="30" y2="2.5" width="0" layer="20" curve="90"/>
<wire x1="30" y1="2.5" x2="31" y2="3.5" width="0" layer="20" curve="-90"/>
<wire x1="31" y1="3.5" x2="31.5" y2="3.5" width="0" layer="20"/>
<wire x1="31.5" y1="3.5" x2="34" y2="6" width="0" layer="20" curve="90"/>
<wire x1="34" y1="6" x2="31.5" y2="8.5" width="0" layer="20" curve="90"/>
<wire x1="31.5" y1="8.5" x2="31" y2="8.5" width="0" layer="20"/>
<wire x1="31" y1="8.5" x2="30" y2="9.5" width="0" layer="20" curve="-90"/>
<wire x1="30" y1="9.5" x2="27.5" y2="12" width="0" layer="20" curve="90"/>
<hole x="2.5" y="6" drill="2.8"/>
<hole x="31.5" y="6" drill="2.8"/>
<text>i c 4 Port</text>
<text>2</text>
<text>&gt;VERSION</text>
<text>by
schizobovine
&lt;sean@yak.net&gt;</text>
</plain>
<libraries>
<library name="a_parts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
<package name="JST-4-PH-VERT-PTH-CENTERED-I2C">
</package>
<package name="OSHWLOGO_TINY_SILKONLY">
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="CC-BY-SA-4.0-NO-URL">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v1.0"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="a_parts" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value="v1.0"/>
<attribute name="DESIGNER" value="sean@yak.net"/>
</element>
<element name="I2C1" library="a_parts" package="JST-4-PH-VERT-PTH-CENTERED-I2C" value="M04-I2CJST-4-PH-VERT-CENTERED-I2C"/>
<element name="I2C2" library="a_parts" package="JST-4-PH-VERT-PTH-CENTERED-I2C" value="M04-I2CJST-4-PH-VERT-CENTERED-I2C"/>
<element name="I2C3" library="a_parts" package="JST-4-PH-VERT-PTH-CENTERED-I2C" value="M04-I2CJST-4-PH-VERT-CENTERED-I2C"/>
<element name="U$1" library="a_parts" package="OSHWLOGO_TINY_SILKONLY" value=""/>
<element name="R1" library="a_parts" package="R0805" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a_parts" package="R0805" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C4" library="a_parts" package="JST-4-PH-VERT-PTH-CENTERED-I2C" value="M04-I2CJST-4-PH-VERT-CENTERED-I2C"/>
<element name="U$2" library="a_parts" package="CC-BY-SA-4.0-NO-URL" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="I2C1" pad="1"/>
<contactref element="I2C2" pad="1"/>
<contactref element="I2C3" pad="1"/>
<contactref element="I2C4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="I2C1" pad="2"/>
<contactref element="I2C2" pad="2"/>
<contactref element="I2C3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="I2C4" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="I2C1" pad="3"/>
<contactref element="I2C2" pad="3"/>
<contactref element="I2C3" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="I2C4" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="I2C1" pad="4"/>
<contactref element="I2C2" pad="4"/>
<contactref element="I2C3" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="I2C4" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
