(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 154 100)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "sig01")
	(net 3 "sig02")
	(net 4 "sig03")
	(net 5 "unconnected-(U1-Pad42)")
	(net 6 "sig23")
	(net 7 "sig14")
	(net 8 "sig27")
	(net 9 "sig07")
	(net 10 "sig08")
	(net 11 "sig10")
	(net 12 "sig16")
	(net 13 "unconnected-(U1-Pad61)")
	(net 14 "sig24")
	(net 15 "unconnected-(U1-Pad40)")
	(net 16 "sig09")
	(net 17 "sig13")
	(net 18 "unconnected-(U1-Pad41)")
	(net 19 "unconnected-(U1-Pad62)")
	(net 20 "sig26")
	(net 21 "unconnected-(U1-Pad20)")
	(net 22 "sig31")
	(net 23 "sig29")
	(net 24 "unconnected-(U1-Pad19)")
	(net 25 "sig15")
	(net 26 "sig28")
	(net 27 "sig32")
	(net 28 "unconnected-(U1-Pad39)")
	(net 29 "sig12")
	(net 30 "sig30")
	(net 31 "sig11")
	(net 32 "sig25")
	(net 33 "sig04")
	(net 34 "sig05")
	(net 35 "sig06")
	(net 36 "sig17")
	(net 37 "sig18")
	(net 38 "sig19")
	(net 39 "sig20")
	(net 40 "sig21")
	(net 41 "sig22")
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 137.8 89.196152 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S29"
			(at 0 -2.003848 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "sig29")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 126 88)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at 2 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 148.796151 117)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S1"
			(at 0.403849 -2.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "sig01")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 146.600001 85.196152 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S31"
			(at 0 -2.003848 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "sig31")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 149.6 80)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S32"
			(at -1.2 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "sig32")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 117.2 101.946411 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S8"
			(at 0.8 -0.053589 270)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 2.05 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "sig08")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 122.39615 94.999997 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S10"
			(at -0.00385 -2.200003 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "sig10")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 148.796152 82.999999 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S16"
			(at -0.003848 -2.200001 270)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 2.05 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "sig16")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 140.8 116 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S19"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "sig19")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 134.8 110)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S4"
			(at 0 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "sig04")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 123.2 107.946411 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S23"
			(at 0 -1.998 270)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 2.05 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "sig23")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 123.199999 91.999998)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S26"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "sig26")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 120.2 97.19615 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S25"
			(at 1.4 -0.00385 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "sig25")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 117.2 92)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at 2 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 129 107.203848)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S22"
			(at -0.01436 -2.003848 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "sig22")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 132 112.4 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S21"
			(at 0 -1.998 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "sig21")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 131.196152 109.4)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S5"
			(at 0.003848 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "sig05")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 117.2 98 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S9"
			(at 0.8 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "sig09")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 143.6 114)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S2"
			(at 0 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "sig02")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 126 94 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S11"
			(at 0 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "sig11")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 134.8 84 90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at 1.6 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 139.996152 113)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S3"
			(at 0.003848 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "sig03")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 117.2 107.946411 -90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at 1.653589 -2 270)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 2.05 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 140.8 84)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S30"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "sig30")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 132 88)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S28"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "sig28")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 134.8 90 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S13"
			(at 0 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "sig13")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 120.2 102.8 -90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S24"
			(at 0 1.4 270)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 2.05 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "sig24")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 129 93.196152 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S27"
			(at 0 -2.003848 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "sig27")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 131.196151 91 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S12"
			(at -0.003849 -2.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "sig12")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:ERF8-040-EM2"
		(layer "F.Cu")
		(at 154 100)
		(property "Reference" "U1"
			(at -2.15 -17 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ERF8-ERM8-040-DV"
			(at -3.1 -5.35 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0.05 1.2 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0.05 1.2 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr through_hole)
		(fp_text user "F"
			(at -1.5 -15.25 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd rect
			(at 0 -15.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at 0 -15.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0 -14.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "sig16")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 -14.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "sig32")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0 -14)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "5")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at 0 -14)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "6")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at 0 -13.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "sig15")
			(pinfunction "7")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 0 -13.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "sig31")
			(pinfunction "8")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 0 -12.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "9")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at 0 -12.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "10")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at 0 -11.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "sig14")
			(pinfunction "11")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 0 -11.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "sig30")
			(pinfunction "12")
			(pintype "unspecified")
		)
		(pad "13" smd rect
			(at 0 -10.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "13")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 0 -10.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "14")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 0 -10)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "sig13")
			(pinfunction "15")
			(pintype "unspecified")
		)
		(pad "16" smd rect
			(at 0 -10)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "sig29")
			(pinfunction "16")
			(pintype "unspecified")
		)
		(pad "17" smd rect
			(at 0 -9.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "17")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at 0 -9.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "18")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at 0 -8.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(U1-Pad19)")
			(pinfunction "19")
			(pintype "unspecified+no_connect")
		)
		(pad "20" smd rect
			(at 0 -8.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "unconnected-(U1-Pad20)")
			(pinfunction "20")
			(pintype "unspecified+no_connect")
		)
		(pad "21" smd rect
			(at 0 -7.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "21")
			(pintype "power_in")
		)
		(pad "22" smd rect
			(at 0 -7.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "22")
			(pintype "power_in")
		)
		(pad "23" smd rect
			(at 0 -6.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "sig12")
			(pinfunction "23")
			(pintype "unspecified")
		)
		(pad "24" smd rect
			(at 0 -6.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "sig28")
			(pinfunction "24")
			(pintype "unspecified")
		)
		(pad "25" smd rect
			(at 0 -6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "25")
			(pintype "power_in")
		)
		(pad "26" smd rect
			(at 0 -6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "26")
			(pintype "power_in")
		)
		(pad "27" smd rect
			(at 0 -5.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "sig11")
			(pinfunction "27")
			(pintype "unspecified")
		)
		(pad "28" smd rect
			(at 0 -5.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "sig27")
			(pinfunction "28")
			(pintype "unspecified")
		)
		(pad "29" smd rect
			(at 0 -4.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "29")
			(pintype "power_in")
		)
		(pad "30" smd rect
			(at 0 -4.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "30")
			(pintype "power_in")
		)
		(pad "31" smd rect
			(at 0 -3.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "sig10")
			(pinfunction "31")
			(pintype "unspecified")
		)
		(pad "32" smd rect
			(at 0 -3.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "sig26")
			(pinfunction "32")
			(pintype "unspecified")
		)
		(pad "33" smd rect
			(at 0 -2.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "33")
			(pintype "power_in")
		)
		(pad "34" smd rect
			(at 0 -2.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "34")
			(pintype "power_in")
		)
		(pad "35" smd rect
			(at 0 -2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "sig09")
			(pinfunction "35")
			(pintype "unspecified")
		)
		(pad "36" smd rect
			(at 0 -2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "sig25")
			(pinfunction "36")
			(pintype "unspecified")
		)
		(pad "37" smd rect
			(at 0 -1.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "37")
			(pintype "power_in")
		)
		(pad "38" smd rect
			(at 0 -1.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "38")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at 0 -0.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(U1-Pad39)")
			(pinfunction "39")
			(pintype "unspecified+no_connect")
		)
		(pad "40" smd rect
			(at 0 -0.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "unconnected-(U1-Pad40)")
			(pinfunction "40")
			(pintype "unspecified+no_connect")
		)
		(pad "41" smd rect
			(at 0 0.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(U1-Pad41)")
			(pinfunction "41")
			(pintype "unspecified+no_connect")
		)
		(pad "42" smd rect
			(at 0 0.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "unconnected-(U1-Pad42)")
			(pinfunction "42")
			(pintype "unspecified+no_connect")
		)
		(pad "43" smd rect
			(at 0 1.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "43")
			(pintype "power_in")
		)
		(pad "44" smd rect
			(at 0 1.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "44")
			(pintype "power_in")
		)
		(pad "45" smd rect
			(at 0 2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "sig08")
			(pinfunction "45")
			(pintype "unspecified")
			(padstack
				(mode front_inner_back)
				(layer "Inner"
					(shape rect)
					(size 2 0.5)
					(thermal_bridge_angle 45)
					(zone_connect -1)
				)
				(layer "B.Cu"
					(shape rect)
					(size 2 0.5)
					(thermal_bridge_angle 45)
					(zone_connect -1)
				)
			)
		)
		(pad "46" smd rect
			(at 0 2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "sig24")
			(pinfunction "46")
			(pintype "unspecified")
		)
		(pad "47" smd rect
			(at 0 2.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "47")
			(pintype "power_in")
		)
		(pad "48" smd rect
			(at 0 2.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "48")
			(pintype "power_in")
		)
		(pad "49" smd rect
			(at 0 3.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "sig07")
			(pinfunction "49")
			(pintype "unspecified")
		)
		(pad "50" smd rect
			(at 0 3.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "sig23")
			(pinfunction "50")
			(pintype "unspecified")
		)
		(pad "51" smd rect
			(at 0 4.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "51")
			(pintype "power_in")
		)
		(pad "52" smd rect
			(at 0 4.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "52")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 0 5.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "sig06")
			(pinfunction "53")
			(pintype "unspecified")
		)
		(pad "54" smd rect
			(at 0 5.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 41 "sig22")
			(pinfunction "54")
			(pintype "unspecified")
		)
		(pad "55" smd rect
			(at 0 6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "55")
			(pintype "power_in")
		)
		(pad "56" smd rect
			(at 0 6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "56")
			(pintype "power_in")
		)
		(pad "57" smd rect
			(at 0 6.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "sig05")
			(pinfunction "57")
			(pintype "unspecified")
		)
		(pad "58" smd rect
			(at 0 6.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 40 "sig21")
			(pinfunction "58")
			(pintype "unspecified")
		)
		(pad "59" smd rect
			(at 0 7.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "59")
			(pintype "power_in")
		)
		(pad "60" smd rect
			(at 0 7.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "60")
			(pintype "power_in")
		)
		(pad "61" smd rect
			(at 0 8.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(U1-Pad61)")
			(pinfunction "61")
			(pintype "unspecified+no_connect")
		)
		(pad "62" smd rect
			(at 0 8.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "unconnected-(U1-Pad62)")
			(pinfunction "62")
			(pintype "unspecified+no_connect")
		)
		(pad "63" smd rect
			(at 0 9.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "63")
			(pintype "power_in")
		)
		(pad "64" smd rect
			(at 0 9.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "64")
			(pintype "power_in")
		)
		(pad "65" smd rect
			(at 0 10)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "sig04")
			(pinfunction "65")
			(pintype "unspecified")
		)
		(pad "66" smd rect
			(at 0 10)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 39 "sig20")
			(pinfunction "66")
			(pintype "unspecified")
		)
		(pad "67" smd rect
			(at 0 10.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "67")
			(pintype "power_in")
		)
		(pad "68" smd rect
			(at 0 10.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "68")
			(pintype "power_in")
		)
		(pad "69" smd rect
			(at 0 11.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "sig03")
			(pinfunction "69")
			(pintype "unspecified")
		)
		(pad "70" smd rect
			(at 0 11.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "sig19")
			(pinfunction "70")
			(pintype "unspecified")
		)
		(pad "71" smd rect
			(at 0 12.4)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "71")
			(pintype "power_in")
		)
		(pad "72" smd rect
			(at 0 12.4)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "72")
			(pintype "power_in")
		)
		(pad "73" smd rect
			(at 0 13.2)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "sig02")
			(pinfunction "73")
			(pintype "unspecified")
		)
		(pad "74" smd rect
			(at 0 13.2)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "sig18")
			(pinfunction "74")
			(pintype "unspecified")
		)
		(pad "75" smd rect
			(at 0 14)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "75")
			(pintype "power_in")
		)
		(pad "76" smd rect
			(at 0 14)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "76")
			(pintype "power_in")
		)
		(pad "77" smd rect
			(at 0 14.8)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "sig01")
			(pinfunction "77")
			(pintype "unspecified")
		)
		(pad "78" smd rect
			(at 0 14.8)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "sig17")
			(pinfunction "78")
			(pintype "unspecified")
		)
		(pad "79" smd rect
			(at 0 15.6)
			(size 2 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "79")
			(pintype "power_in")
		)
		(pad "80" smd rect
			(at 0 15.6)
			(size 2 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "80")
			(pintype "power_in")
		)
		(pad "G1" thru_hole rect
			(at 0.25 20.5 180)
			(size 3.5 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "G1")
			(pintype "power_in")
		)
		(pad "G2" thru_hole rect
			(at 0.25 -20.5 180)
			(size 3.5 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "G2")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 139.996152 87 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S14"
			(at 0 -2.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "sig14")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 126 106.4)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S6"
			(at -0.01436 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "sig06")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 122.396152 104.946411 -90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S7"
			(at -1.746411 -0.003848 270)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 2.05 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "sig07")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 137.8 110.803848)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S20"
			(at -0.01436 -2.003848 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "sig20")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 146.600031 114.8)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S18"
			(at 0 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "sig18")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 149.6 120 -90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S17"
			(at 1.2 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "sig17")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 134.8 116 -90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at 2.4 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 143.600033 119.924944 -90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at 1.675056 -1.599967 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "F.Cu")
		(at 126 112.4 -90)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at 1.6 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "B.Cu")
		(at 143.6 80 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "GND"
			(at -2 1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.05 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Library:TestPoint_scope-probe_08mm"
		(layer "B.Cu")
		(at 143.6 86)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "S15"
			(at 0 2 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 -2.05 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "smerf8-tp.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 2 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4224 1.4224)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "sig15")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 115.6 109.826272)
		(end 139.51248 123.330587)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 156.501374 122.637455)
		(mid 156.219992 123.317886)
		(end 155.539779 123.599793)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.249532 83.061469)
		(end 152.126197 82.938135)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155.539779 123.599793)
		(end 140.4 123.599307)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.249532 83.061469)
		(end 156.125923 83.062961)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.126197 82.938135)
		(end 152.125408 82.062452)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 140.4 76.4)
		(end 155.539779 76.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.501374 122.637455)
		(end 156.495089 83.432128)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.125408 82.062452)
		(end 153.625815 80.562541)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 140.4 123.599307)
		(mid 139.936346 123.530654)
		(end 139.51248 123.330587)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.512481 76.66872)
		(end 115.6 90.174087)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.6 109.826272)
		(mid 115.348504 109.557181)
		(end 115.25719 109.200359)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 155.539779 76.4)
		(mid 156.219993 76.681908)
		(end 156.501375 77.362339)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.25719 90.8)
		(mid 115.348505 90.443179)
		(end 115.6 90.174087)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.498192 80.563038)
		(end 156.123925 80.937847)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.00004 80.562056)
		(end 154.375619 80.93766)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.25719 90.8)
		(end 115.25719 109.200359)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.375619 80.93766)
		(end 156.123925 80.937847)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.495089 83.432128)
		(end 156.125923 83.062962)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 139.51248 76.66872)
		(mid 139.936346 76.468653)
		(end 140.4 76.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.499921 80.563038)
		(end 156.501375 77.368533)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.625815 80.562541)
		(end 154.00004 80.562056)
		(layer "Edge.Cuts")
	)
	(gr_text "TP Triangle IDL_25_05\n(Aug. 2025, CD)"
		(at 151.52 100.02 90)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.25)
		)
		(polygon
			(pts
				(xy 67.6 147.4) (xy 172.4 147.4) (xy 172.4 24.2) (xy 67.6 24.2)
			)
		)
	)
	(embedded_fonts no)
)
