<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="27" width="0" layer="20"/>
<wire x1="0" y1="27" x2="36" y2="27" width="0" layer="20"/>
<wire x1="36" y1="27" x2="36" y2="24" width="0" layer="20"/>
<wire x1="36" y1="24" x2="46" y2="24" width="0" layer="20"/>
<wire x1="46" y1="24" x2="46" y2="3" width="0" layer="20"/>
<wire x1="46" y1="3" x2="36" y2="3" width="0" layer="20"/>
<wire x1="36" y1="3" x2="36" y2="0" width="0" layer="20"/>
<wire x1="36" y1="0" x2="0" y2="0" width="0" layer="20"/>
<hole x="6" y="13.5" drill="3"/>
<hole x="42" y="20" drill="3"/>
<hole x="42" y="7" drill="3"/>
<wire x1="6.5" y1="23.5" x2="33.5" y2="23.5" width="1.5" layer="46"/>
<wire x1="7.25" y1="18.75" x2="34" y2="18.75" width="3" layer="46"/>
<wire x1="11" y1="13.25" x2="34" y2="13.25" width="3" layer="46"/>
<text>230V</text>
<text>PE</text>
<text>FAN+</text>
<text>FAN-</text>
<text>GND</text>
<text>TC</text>
<text>REED</text>
<text>Youyue 858D+
Wand Board r1</text>
<text>230V</text>
<text>http://github.com/maugsburger</text>
<text>HEATER</text>
<text>HEATER</text>
<text></text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="grafiken">
<packages>
<package name="SCHAF-7">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$6" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$7" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$8" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$9" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="FAN-" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$11" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$13" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$14" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$15" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$16" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$17" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$18" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$19" library="testpad" package="P1-13" value="">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="grafiken" package="SCHAF-7" value=""/>
</elements>
<signals>
<signal name="L1">
<contactref element="E$3" pad="TP"/>
<contactref element="E$1" pad="TP"/>
</signal>
<signal name="L2">
<contactref element="E$5" pad="TP"/>
<contactref element="E$4" pad="TP"/>
</signal>
<signal name="PE">
<contactref element="E$7" pad="TP"/>
<contactref element="E$6" pad="TP"/>
</signal>
<signal name="FAN+">
<contactref element="E$9" pad="TP"/>
<contactref element="E$8" pad="TP"/>
</signal>
<signal name="SE+">
<contactref element="E$14" pad="TP"/>
<contactref element="E$13" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="E$15" pad="TP"/>
<contactref element="E$17" pad="TP"/>
<contactref element="E$16" pad="TP"/>
</signal>
<signal name="VIB">
<contactref element="E$19" pad="TP"/>
<contactref element="E$18" pad="TP"/>
</signal>
<signal name="FAN-">
<contactref element="E$11" pad="TP"/>
<contactref element="FAN-" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
