<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="71.1075" y2="0" width="0" layer="20"/>
<wire x1="71.1075" y1="0" x2="71.1075" y2="23.5175" width="0" layer="20"/>
<wire x1="71.1075" y1="23.5175" x2="0" y2="23.5175" width="0" layer="20"/>
<wire x1="0" y1="23.5175" x2="0" y2="0" width="0" layer="20"/>
<text>RXD</text>
<text>TXD</text>
<text>Facedancer21</text>
<text>TravisGoodspeed&lt;travis@tnbelt.com&gt;</text>
<text>+1.865.471.8519</text>
<text>http://goodfet.sf.net/</text>
<text>MSP430F2618</text>
<text>RXD</text>
<text>TXD</text>
<text>+49.152.23.90.76.92</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="TI_MSP430_v13">
<packages>
<package name="PM/PAG64">
<description>*** TI: PM *** JEDEC: S-PQFP-G64 *** 64 PINS ***</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-5MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0603" value="0.1µF">
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun" package="SSOP28DB" value="FT232RL-BASICSSOP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RXLED" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TXLED" library="led" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="TI_MSP430_v13" package="PM/PAG64" value="F261X---PM64">
<attribute name="NAME"/>
</element>
<element name="CN1" library="adafruit" package="USB-MINIB" value="HOST">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="crystal" package="HC49UP" value="12MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN2" library="adafruit" package="USB-MINIB" value="TARGET">
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0603" value="18pF">
<attribute name="NAME"/>
</element>
<element name="C7" library="rcl" package="C0603" value="18pF">
<attribute name="NAME"/>
</element>
<element name="U4" library="SparkFun-DigitalIC" package="TQFP32-5MM" value="MAX3421ESMD">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="CN3" library="SparkFun-Connectors" package="USB-A-S" value="USB-A-S"/>
<element name="C4" library="rcl" package="C0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="!CS">
<contactref element="U1" pad="44"/>
<contactref element="U4" pad="14"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="45"/>
<contactref element="U4" pad="16"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="46"/>
<contactref element="U4" pad="15"/>
</signal>
<signal name="SCLK">
<contactref element="U1" pad="47"/>
<contactref element="U4" pad="13"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="U2" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="23"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="U1" pad="33"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="TXD">
<contactref element="U1" pad="32"/>
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="62"/>
<contactref element="LED1" pad="C"/>
<contactref element="U2" pad="26"/>
<contactref element="U2" pad="25"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="21"/>
<contactref element="C2" pad="1"/>
<contactref element="CN1" pad="GND"/>
<contactref element="CN2" pad="GND"/>
<contactref element="C3" pad="1"/>
<contactref element="CN2" pad="GND"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="CN3" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="U4" pad="19"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="22"/>
<contactref element="RXLED" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="23"/>
<contactref element="TXLED" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="RXLED" pad="A"/>
<contactref element="TXLED" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="!RST">
<contactref element="U1" pad="26"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="36"/>
<contactref element="U4" pad="18"/>
</signal>
<signal name="RTS">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="57"/>
</signal>
<signal name="DTR">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="5VCC">
<contactref element="U2" pad="20"/>
<contactref element="CN1" pad="VBUS"/>
<contactref element="CN3" pad="VBUS"/>
</signal>
<signal name="USBDM">
<contactref element="U2" pad="16"/>
<contactref element="CN1" pad="D-"/>
</signal>
<signal name="USBDP">
<contactref element="U2" pad="15"/>
<contactref element="CN1" pad="D+"/>
</signal>
<signal name="VBCOMP">
<contactref element="CN2" pad="VBUS"/>
<contactref element="C3" pad="2"/>
<contactref element="U4" pad="22"/>
</signal>
<signal name="GPX">
<contactref element="U4" pad="17"/>
<contactref element="U1" pad="43"/>
</signal>
<signal name="D-">
<contactref element="CN3" pad="D-"/>
<contactref element="CN2" pad="D-"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="D+">
<contactref element="CN3" pad="D+"/>
<contactref element="CN2" pad="D+"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="X0">
<contactref element="U4" pad="25"/>
<contactref element="Q1" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="X1">
<contactref element="U4" pad="24"/>
<contactref element="Q1" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="DPLUS">
<contactref element="U4" pad="21"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="DMINUS">
<contactref element="U4" pad="20"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
