(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 160)
    (zones 0)
    (modules 2)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.85)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /!CS0)
  (net 2 /A2)
  (net 3 /A1)
  (net 4 /A0)
  (net 5 /!CS1)
  (net 6 /!RD)
  (net 7 /!WR)
  (net 8 /!RESET)
  (net 9 GND)
  (net 10 +5V)
  (net 11 "Net-(J2-Pad49)")
  (net 12 "Net-(J2-Pad48)")
  (net 13 "Net-(J2-Pad47)")
  (net 14 "Net-(J2-Pad46)")
  (net 15 "Net-(J2-Pad43)")
  (net 16 "Net-(J2-Pad42)")
  (net 17 "Net-(J2-Pad40)")
  (net 18 "Net-(J2-Pad33)")
  (net 19 "Net-(J2-Pad31)")
  (net 20 "Net-(J2-Pad30)")
  (net 21 "Net-(J2-Pad29)")
  (net 22 "Net-(J2-Pad28)")
  (net 23 "Net-(J2-Pad27)")
  (net 24 "Net-(J2-Pad26)")
  (net 25 "Net-(J2-Pad25)")
  (net 26 "Net-(J2-Pad24)")
  (net 27 /D6)
  (net 28 /D7)
  (net 29 /D4)
  (net 30 /D5)
  (net 31 /D2)
  (net 32 /D3)
  (net 33 /D0)
  (net 34 /D1)
  (net 35 /IRQ)
  (net 36 /LED)
  (net 37 "Net-(J1-Pad33)")
  (net 38 "Net-(J1-Pad34)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.25)
    (add_net /!CS0)
    (add_net /!CS1)
    (add_net /!RD)
    (add_net /!RESET)
    (add_net /!WR)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /IRQ)
    (add_net /LED)
    (add_net GND)
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad42)")
    (add_net "Net-(J2-Pad43)")
    (add_net "Net-(J2-Pad46)")
    (add_net "Net-(J2-Pad47)")
    (add_net "Net-(J2-Pad48)")
    (add_net "Net-(J2-Pad49)")
  )
  (net_class power ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.25)
    (add_net +5V)
  )
  (module "SateCard footprints:CF_proto" (layer F.Cu) (tedit 5C05C648)
    (at 145.46 103.054999 90)
    (fp_text reference J2 (at 8.054999 2.54 180) (layer F.SilkS))
    (fp_text value CF-CARD (at 13.054999 -22.46 180) (layer F.Fab))
    (fp_text user "CN0022 CompactFlash Adapter Board" (at 2.54 2.54) (layer F.SilkS))
    (fp_text user 50 (at 7.62 33.02 90) (layer F.SilkS))
    (fp_text user 25 (at -2.54 33.02 90) (layer F.SilkS))
    (fp_text user 26 (at 7.62 -27.94 90) (layer F.SilkS))
    (fp_text user 1 (at -2.54 -27.94 90) (layer F.SilkS))
    (pad 50 thru_hole circle (at 10.08 33.02 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 49 thru_hole circle (at 10.08 30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad49)"))
    (pad 48 thru_hole circle (at 10.08 27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad48)"))
    (pad 47 thru_hole circle (at 10.08 25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad47)"))
    (pad 46 thru_hole circle (at 10.08 22.86 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad46)"))
    (pad 45 thru_hole circle (at 10.08 20.32 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /LED))
    (pad 44 thru_hole circle (at 10.08 17.78 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 43 thru_hole circle (at 10.08 15.24 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad43)"))
    (pad 42 thru_hole circle (at 10.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad42)"))
    (pad 41 thru_hole circle (at 10.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /!RESET))
    (pad 40 thru_hole circle (at 10.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad40)"))
    (pad 39 thru_hole circle (at 10.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 38 thru_hole circle (at 10.08 2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 37 thru_hole circle (at 10.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /IRQ))
    (pad 36 thru_hole circle (at 10.08 -2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 35 thru_hole circle (at 10.08 -5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /!WR))
    (pad 34 thru_hole circle (at 10.08 -7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /!RD))
    (pad 33 thru_hole circle (at 10.08 -10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad33)"))
    (pad 32 thru_hole circle (at 10.08 -12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /!CS1))
    (pad 31 thru_hole circle (at 10.08 -15.24 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad31)"))
    (pad 30 thru_hole circle (at 10.08 -17.78 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad30)"))
    (pad 29 thru_hole circle (at 10.08 -20.32 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad29)"))
    (pad 28 thru_hole circle (at 10.08 -22.86 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad28)"))
    (pad 27 thru_hole circle (at 10.08 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad27)"))
    (pad 26 thru_hole circle (at 10.08 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad26)"))
    (pad 25 thru_hole circle (at -5.08 33.02 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad25)"))
    (pad 24 thru_hole circle (at -5.08 30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad24)"))
    (pad 23 thru_hole circle (at -5.08 27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /D2))
    (pad 22 thru_hole circle (at -5.08 25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /D1))
    (pad 21 thru_hole circle (at -5.08 22.86 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /D0))
    (pad 20 thru_hole circle (at -5.08 20.32 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /A0))
    (pad 19 thru_hole circle (at -5.08 17.78 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /A1))
    (pad 18 thru_hole circle (at -5.08 15.24 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A2))
    (pad 17 thru_hole circle (at -5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 16 thru_hole circle (at -5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 15 thru_hole circle (at -5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 14 thru_hole circle (at -5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 13 thru_hole circle (at -5.08 2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 12 thru_hole circle (at -5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 11 thru_hole circle (at -5.08 -2.54 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 10 thru_hole circle (at -5.08 -5.08 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 9 thru_hole circle (at -5.08 -7.62 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 8 thru_hole circle (at -5.08 -10.16 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 7 thru_hole circle (at -5.08 -12.7 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /!CS0))
    (pad 6 thru_hole circle (at -5.08 -15.24 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /D7))
    (pad 5 thru_hole circle (at -5.08 -17.78 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /D6))
    (pad 4 thru_hole circle (at -5.08 -20.32 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /D5))
    (pad 3 thru_hole circle (at -5.08 -22.86 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /D4))
    (pad 2 thru_hole circle (at -5.08 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /D3))
    (pad 1 thru_hole circle (at -5.08 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 GND))
  )
  (module "SateCard footprints:SV_Ext" (layer B.Cu) (tedit 5BEA0FFB)
    (at 148.06525 85 270)
    (fp_text reference J1 (at 3 -15.93475) (layer B.SilkS))
    (fp_text value SatellaviewEXT (at 0 0.5) (layer B.Fab))
    (fp_text user 1 (at -2 20 270) (layer B.SilkS))
    (fp_text user 2 (at 2 20 270) (layer B.SilkS))
    (fp_text user 37 (at -2 -20 270) (layer B.SilkS))
    (fp_text user 38 (at 2 -20 270) (layer B.SilkS))
    (fp_text user "Satellaview EXT" (at 3 0.06525 unlocked) (layer B.SilkS))
    (pad 1 thru_hole circle (at -1 18.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1 18.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 3 thru_hole circle (at -1 16.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 1 16.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -1 14.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1 14.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 7 thru_hole circle (at -1 12.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 1 12.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -1 10.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 1 10.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -1 8.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 /D6))
    (pad 12 thru_hole circle (at 1 8.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 /D7))
    (pad 13 thru_hole circle (at -1 6.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /D4))
    (pad 14 thru_hole circle (at 1 6.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 /D5))
    (pad 15 thru_hole circle (at -1 4.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 /D2))
    (pad 16 thru_hole circle (at 1 4.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 /D3))
    (pad 17 thru_hole circle (at -1 2.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 /D0))
    (pad 18 thru_hole circle (at 1 2.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 /D1))
    (pad 19 thru_hole circle (at -1 0.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /!WR))
    (pad 20 thru_hole circle (at 1 0.06525 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at -1 -1.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /!RD))
    (pad 22 thru_hole circle (at 1 -1.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -1 -3.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 /IRQ))
    (pad 24 thru_hole circle (at 1 -3.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at -1 -5.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 /A1))
    (pad 26 thru_hole circle (at 1 -5.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -1 -7.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 /A0))
    (pad 28 thru_hole circle (at 1 -7.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /A2))
    (pad 29 thru_hole circle (at -1 -9.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 /!CS0))
    (pad 30 thru_hole circle (at 1 -9.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /!CS1))
    (pad 31 thru_hole circle (at -1 -11.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 /LED))
    (pad 32 thru_hole circle (at 1 -11.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /!RESET))
    (pad 33 thru_hole circle (at -1 -13.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad33)"))
    (pad 34 thru_hole circle (at 1 -13.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad34)"))
    (pad 35 thru_hole circle (at -1 -15.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 1 -15.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 37 thru_hole circle (at -1 -17.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 1 -17.93475 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_2x19_P2.00mm_Vertical.wrl
      (offset (xyz 1 18 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text https://github.com/devinacker/satecard (at 156 106) (layer B.SilkS))
  (gr_line (start 180 81) (end 116 81) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 180 111) (end 180 81) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 116 111) (end 180 111) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 116 81) (end 116 111) (layer Edge.Cuts) (width 0.2))
  (gr_text "SateCard CF Adapter" (at 117 89) (layer F.SilkS))
  (gr_text "Rev 1.2 Feb 2019" (at 179 89) (layer F.SilkS))
  (zone (net 9) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116 81) (xy 116 111) (xy 180 111) (xy 180 81)
      )
    )
  )
  (zone (net 9) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116 81) (xy 116 111) (xy 180 111) (xy 180 81)
      )
    )
  )
)
