<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="41.275" y2="0" width="0" layer="20"/>
<wire x1="41.275" y1="0" x2="43.815" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="43.815" y1="2.54" x2="43.815" y2="74.434" width="0" layer="20"/>
<wire x1="43.815" y1="74.434" x2="41.275" y2="76.974" width="0" layer="20" curve="90"/>
<wire x1="41.275" y1="76.974" x2="2.54" y2="76.974" width="0" layer="20"/>
<wire x1="2.54" y1="76.974" x2="0" y2="74.434" width="0" layer="20" curve="90"/>
<wire x1="0" y1="74.434" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<text>BrewPi D32 Pro
AIO Board v0.1
@thorrak says hi</text>
<text>D32:
13 - OneWire
25 - Heat
26 - Cool
34 - Door</text>
<text>RJ-45:
3 - 3V/5V
4 - OneWire
5 - Ground
6 - Door</text>
<text>GROUND</text>
<text>COOL</text>
<text>HEAT</text>
<text>3V3</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>3V3</text>
<text>5V</text>
<text>SEL</text>
<text>5V</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
</plain>
<libraries>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-tycoelectronics">
<description>&lt;b&gt;Tyco Electronics Connector&lt;/b&gt;&lt;p&gt;
http://catalog.tycoelectronics.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RJ45-NO-SHIELD-NOLINE">
<description>&lt;b&gt;RJ45 Low Profile&lt;/b&gt; No Shield&lt;p&gt;
For all RJ45 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Donnie">
<packages>
<package name="HDR-4_VERT">
</package>
<package name="CAP_PTH-2.54">
</package>
<package name="D32_PRO_NO-BATT">
</package>
<package name="HDR-2_VERT">
</package>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="SMD-1206">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2W">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Box Header">
<packages>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X" library="con-wago-500" package="W237-102" value="5V_IN">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-tycoelectronics" package="RJ45-NO-SHIELD-NOLINE" value="RJ45-8X">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RJ45-8X"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6101"/>
</element>
<element name="R1" library="Donnie" package="SMD-1206" value="2k2Ω">
<attribute name="NAME"/>
</element>
<element name="U$2" library="holes" package="3,0" value=""/>
<element name="U$4" library="holes" package="3,0" value=""/>
<element name="U$3" library="Donnie" package="D32_PRO_NO-BATT" value="WEMOS-D32D32_PRO_NO-BATT"/>
<element name="U$1" library="holes" package="3,0" value=""/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="2k2Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="RELAY" library="Donnie" package="HDR-4_VERT" value=" ">
<attribute name="NAME"/>
</element>
<element name="C1" library="Donnie" package="SMD-1206" value="1.0μF">
<attribute name="NAME"/>
</element>
<element name="C2" library="Donnie" package="SMD-1206" value="0.1μF">
<attribute name="NAME"/>
</element>
<element name="C3" library="Donnie" package="CAP_PTH-2.54" value="1.0μF">
<attribute name="NAME"/>
</element>
<element name="C4" library="Donnie" package="CAP_PTH-2.54" value="0.1μF">
<attribute name="NAME"/>
</element>
<element name="C5" library="Donnie" package="SMD-1206" value="1.0μF">
<attribute name="NAME"/>
</element>
<element name="C6" library="Donnie" package="SMD-1206" value="0.1μF">
<attribute name="NAME"/>
</element>
<element name="C7" library="Donnie" package="CAP_PTH-2.54" value="1.0μF">
<attribute name="NAME"/>
</element>
<element name="C8" library="Donnie" package="CAP_PTH-2.54" value="0.1μF">
<attribute name="NAME"/>
</element>
<element name="U$5" library="Donnie" package="HDR-2_VERT" value="POWER">
<attribute name="VALUE"/>
</element>
<element name="OW_VSEL" library="Donnie" package="JP2" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="34"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ_2W" value="">
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="21"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-small-signal" package="SOT23" value="BSS123">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="21"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Donnie" package="SMD-1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Donnie" package="SMD-1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Donnie" package="SMD-1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Donnie" package="SMD-1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TFT" library="Box Header" package="MA05-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="LCD" library="Donnie" package="HDR-4_VERT" value=" ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="GND"/>
<contactref element="U$3" pad="GND2"/>
<contactref element="J1" pad="5"/>
<contactref element="X" pad="2"/>
<contactref element="RELAY" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U$5" pad="2"/>
<contactref element="TFT" pad="3"/>
<contactref element="LCD" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="U$3" pad="VBUS"/>
<contactref element="X" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U$5" pad="1"/>
<contactref element="OW_VSEL" pad="1"/>
<contactref element="SJ1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="TFT" pad="1"/>
<contactref element="LCD" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$3" pad="VCC"/>
<contactref element="RELAY" pad="4"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="OW_VSEL" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="SJ1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="DOOR">
<contactref element="J1" pad="6"/>
<contactref element="U$3" pad="IO34"/>
</signal>
<signal name="COOL">
<contactref element="U$3" pad="IO26"/>
<contactref element="RELAY" pad="2"/>
</signal>
<signal name="HEAT">
<contactref element="U$3" pad="IO25"/>
<contactref element="RELAY" pad="3"/>
</signal>
<signal name="1WIRE">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="U$3" pad="IO13"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="OW_VSEL" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="5V_SCL">
<contactref element="Q1" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="5V_SDA">
<contactref element="Q2" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U$3" pad="IO21"/>
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U$3" pad="IO22"/>
<contactref element="Q1" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="LED">
<contactref element="U$3" pad="IO32"/>
<contactref element="TFT" pad="6"/>
</signal>
<signal name="RESET">
<contactref element="U$3" pad="IO33"/>
<contactref element="TFT" pad="7"/>
</signal>
<signal name="DC">
<contactref element="U$3" pad="IO27"/>
<contactref element="TFT" pad="9"/>
</signal>
<signal name="CS">
<contactref element="U$3" pad="IO14"/>
<contactref element="TFT" pad="5"/>
</signal>
<signal name="T_CS">
<contactref element="U$3" pad="IO12"/>
<contactref element="TFT" pad="10"/>
</signal>
<signal name="MOSI">
<contactref element="U$3" pad="IO23"/>
<contactref element="TFT" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$3" pad="IO19"/>
<contactref element="TFT" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U$3" pad="IO18"/>
<contactref element="TFT" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
