(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x0000000_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/A")
	(net 3 "/B")
	(net 4 "/X")
	(net 5 "/Y")
	(footprint "SophLibraryv2:SKEYAJA010"
		(layer "F.Cu")
		(at 122.25 72.244)
		(property "Reference" "J2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SKEYAJA010"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "SophLibraryv2:SKEYAJA010"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "BTNBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -4.5 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/B")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/B")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4.5 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 4 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155.5 69)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.1mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 2.1)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "SophLibraryv2:SKEYAJA010"
		(layer "F.Cu")
		(at 136.25 81.244)
		(property "Reference" "J3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SKEYAJA010"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "SophLibraryv2:SKEYAJA010"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "BTNBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -4.5 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/X")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/X")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4.5 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 4 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "SophLibraryv2:SKEYAJA010"
		(layer "F.Cu")
		(at 149 72.5)
		(property "Reference" "J4"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SKEYAJA010"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "SophLibraryv2:SKEYAJA010"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "BTNBoard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -4.5 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Y")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Y")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4.5 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 4 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "SophLibraryv2:bb"
		(layer "F.Cu")
		(at 119 92.5)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SophLibraryv2:bb"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 124.5 93.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.1mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 2.1)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 155 93.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.1mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 2.1)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "SophLibraryv2:SKEYAJA010"
		(layer "F.Cu")
		(at 136 62.5)
		(property "Reference" "J1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SKEYAJA010"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "SophLibraryv2:SKEYAJA010"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "BTNBoard.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -4.5 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 7.5)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4.5 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 4 12)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_2.1mm"
		(layer "F.Cu")
		(at 116.5 69)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" "REF**"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.1mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 2.1)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Connector_FFC-FPC:Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal"
		(layer "B.Cu")
		(at 146.1 90.85 90)
		(descr "Hirose FH12, FFC/FPC connector, FH12-6S-0.5SH, 6 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
		(tags "connector Hirose FH12 horizontal")
		(property "Reference" "J5"
			(at 0 3.7 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x06_Pin"
			(at 0 -5.6 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_FFC-FPC:Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "BTNBoard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.7 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.25 1.85 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "/A")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 1.85 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "/B")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.25 1.85 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "/X")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.25 1.85 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "/Y")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.75 1.85 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.25 1.85 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -3.15 -1.4 90)
			(size 1.8 2.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
		)
		(pad "MP" smd rect
			(at 3.15 -1.4 90)
			(size 1.8 2.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 159 67)
		(end 159 65.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113 66.5)
		(end 113 65.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113 66.5)
		(end 113 98)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159 98)
		(end 159 67)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113 65.5)
		(end 159 65.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113 98)
		(end 159 98)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113 65.5) (xy 113 98) (xy 159 98) (xy 159 65.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113 65.5) (xy 113 98) (xy 159 98) (xy 159 65.5)
			)
		)
	)
)
