(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 239)
    (zones 0)
    (modules 49)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.6)
    (user_trace_width 1.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 23.67 24.67)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /MOD_POS)
  (net 2 /MOD_NEG)
  (net 3 "Net-(J7-Pad1)")
  (net 4 "Net-(J8-Pad1)")
  (net 5 "Net-(J10-Pad1)")
  (net 6 "Net-(J11-Pad1)")
  (net 7 /SH_NEG)
  (net 8 /SH_POS)
  (net 9 "Net-(R1-Pad1)")
  (net 10 "Net-(R1-Pad2)")
  (net 11 "Net-(R2-Pad1)")
  (net 12 "Net-(R21-Pad2)")
  (net 13 "Net-(R22-Pad2)")
  (net 14 "Net-(R4-Pad2)")
  (net 15 "Net-(R23-Pad2)")
  (net 16 "Net-(R24-Pad2)")
  (net 17 "Net-(R25-Pad2)")
  (net 18 "Net-(R7-Pad2)")
  (net 19 "Net-(R26-Pad2)")
  (net 20 "Net-(R27-Pad2)")
  (net 21 "Net-(R10-Pad1)")
  (net 22 "Net-(R10-Pad2)")
  (net 23 "Net-(R11-Pad1)")
  (net 24 "Net-(R12-Pad1)")
  (net 25 "Net-(R13-Pad2)")
  (net 26 "Net-(R13-Pad1)")
  (net 27 "Net-(R14-Pad1)")
  (net 28 "Net-(R15-Pad1)")
  (net 29 "Net-(R20-Pad1)")
  (net 30 "Net-(R23-Pad1)")
  (net 31 "Net-(R26-Pad1)")
  (net 32 "Net-(R29-Pad1)")
  (net 33 "Net-(R32-Pad1)")
  (net 34 "Net-(J1-Pad2)")
  (net 35 "Net-(J2-Pad2)")
  (net 36 "Net-(J4-Pad2)")
  (net 37 "Net-(J5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MOD_NEG)
    (add_net /MOD_POS)
    (add_net /SH_NEG)
    (add_net /SH_POS)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R32-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R7-Pad2)")
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 241.67 28.67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 241.67 49.67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 147.67 28.67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 147.67 49.67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 67.67 28.67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 67.67 49.67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 40.67 34.67)
    (fp_text reference J1 (at -4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 1 /MOD_POS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 83.67 34.67)
    (fp_text reference J2 (at -4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 126.67 34.67)
    (fp_text reference J3 (at -4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOD_NEG))
    (pad 1 smd rect (at -1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 169.67 34.67)
    (fp_text reference J4 (at -4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J4-Pad2)"))
    (pad 1 smd rect (at -1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 1 /MOD_POS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 212.67 34.67)
    (fp_text reference J5 (at -4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J5-Pad2)"))
    (pad 1 smd rect (at -1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 255.67 34.67)
    (fp_text reference J6 (at -4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOD_NEG))
    (pad 1 smd rect (at -1.27 0) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 40.67 43.67 180)
    (fp_text reference J7 (at 4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 1 /MOD_POS))
    (pad 1 smd rect (at -1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 83.67 43.67 180)
    (fp_text reference J8 (at 4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J7-Pad1)"))
    (pad 1 smd rect (at -1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 126.67 43.67 180)
    (fp_text reference J9 (at 4 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J8-Pad1)"))
    (pad 1 smd rect (at -1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOD_NEG))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 169.67 43.67 180)
    (fp_text reference J10 (at 4.5 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 1 /MOD_POS))
    (pad 1 smd rect (at -1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 212.67 43.67 180)
    (fp_text reference J11 (at 4.5 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J10-Pad1)"))
    (pad 1 smd rect (at -1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module unl_silab:GEC02SBSN-M89 (layer F.Cu) (tedit 5E30B6C4)
    (at 255.67 43.67 180)
    (fp_text reference J12 (at 4.5 -8) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J11-Pad1)"))
    (pad 1 smd rect (at -1.27 0 180) (size 1.27 3) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOD_NEG))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (offset (xyz -1.2 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x05_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 5A19A425)
    (at 28.67 39.17 180)
    (descr "surface-mounted straight socket strip, 2x05, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Surface mounted socket strip SMD 2x05 2.54mm double row")
    (attr smd)
    (fp_text reference J13 (at 0 -7.85) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0 7.85) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at 2.52 -5.08 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOD_NEG))
    (pad 2 smd rect (at -2.52 -5.08 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /MOD_POS))
    (pad 3 smd rect (at 2.52 -2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOD_NEG))
    (pad 4 smd rect (at -2.52 -2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /MOD_POS))
    (pad 5 smd rect (at 2.52 0 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOD_NEG))
    (pad 6 smd rect (at -2.52 0 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /MOD_POS))
    (pad 7 smd rect (at 2.52 2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /SH_NEG))
    (pad 8 smd rect (at -2.52 2.54 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /SH_POS))
    (pad 9 smd rect (at 2.52 5.08 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /SH_NEG))
    (pad 10 smd rect (at -2.52 5.08 180) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /SH_POS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (offset (xyz -1.3 5 0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 61.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 70.67 41.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 10 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 11 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 52.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 7 /SH_NEG))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 12 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 103.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 13 "Net-(R22-Pad2)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 14 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 112.67 41.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 14 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 15 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 94.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 16 "Net-(R24-Pad2)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 7 /SH_NEG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 146.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 17 "Net-(R25-Pad2)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 18 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 155.67 41.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 18 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 19 "Net-(R26-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 20 "Net-(R27-Pad2)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 7 /SH_NEG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 191.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 21 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 22 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 200.67 41.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 22 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 23 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 182.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 24 "Net-(R12-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 7 /SH_NEG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 234.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 25 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 26 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 243.67 41.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 27 "Net-(R14-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 25 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 225.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 7 /SH_NEG))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 28 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 52.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 9 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 8 /SH_POS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 70.67 36.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 29 "Net-(R20-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 11 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 61.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 12 "Net-(R21-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 29 "Net-(R20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 94.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 13 "Net-(R22-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 8 /SH_POS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 112.67 36.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 30 "Net-(R23-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 15 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 103.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 16 "Net-(R24-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 30 "Net-(R23-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 17 "Net-(R25-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 8 /SH_POS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 155.67 36.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R26 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 31 "Net-(R26-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 19 "Net-(R26-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 146.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R27 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 20 "Net-(R27-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 31 "Net-(R26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 182.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R28 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 21 "Net-(R10-Pad1)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 8 /SH_POS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 200.67 36.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R29 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 32 "Net-(R29-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 23 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 191.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R30 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 24 "Net-(R12-Pad1)"))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 32 "Net-(R29-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 225.67 41.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R31 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 8 /SH_POS))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 26 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 243.67 36.67)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R32 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 27 "Net-(R14-Pad1)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 33 "Net-(R32-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 234.67 36.67 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R33 (at 0 3) (layer F.SilkS))
    (fp_text value 226 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 33 "Net-(R32-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.163934)
      (net 28 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 27 (width 0.15) (layer Dwgs.User)
    (gr_text "27.000 mm" (at 277.47 39.17 90) (layer Dwgs.User))
    (feature1 (pts (xy 273.67 25.67) (xy 276.756421 25.67)))
    (feature2 (pts (xy 273.67 52.67) (xy 276.756421 52.67)))
    (crossbar (pts (xy 276.17 52.67) (xy 276.17 25.67)))
    (arrow1a (pts (xy 276.17 25.67) (xy 276.756421 26.796504)))
    (arrow1b (pts (xy 276.17 25.67) (xy 275.583579 26.796504)))
    (arrow2a (pts (xy 276.17 52.67) (xy 276.756421 51.543496)))
    (arrow2b (pts (xy 276.17 52.67) (xy 275.583579 51.543496)))
  )
  (dimension 250 (width 0.15) (layer Dwgs.User)
    (gr_text "250.000 mm" (at 148.67 58.97) (layer Dwgs.User))
    (feature1 (pts (xy 23.67 52.67) (xy 23.67 58.256421)))
    (feature2 (pts (xy 273.67 52.67) (xy 273.67 58.256421)))
    (crossbar (pts (xy 273.67 57.67) (xy 23.67 57.67)))
    (arrow1a (pts (xy 23.67 57.67) (xy 24.796504 57.083579)))
    (arrow1b (pts (xy 23.67 57.67) (xy 24.796504 58.256421)))
    (arrow2a (pts (xy 273.67 57.67) (xy 272.543496 57.083579)))
    (arrow2b (pts (xy 273.67 57.67) (xy 272.543496 58.256421)))
  )
  (gr_line (start 23.67 25.67) (end 273.67 25.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 273.67 52.67) (end 273.67 25.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 23.67 52.67) (end 273.67 52.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 23.67 25.67) (end 23.67 52.67) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name /MOD_POS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.17 49.67) (xy 158.17 49.67) (xy 165.67 42.17) (xy 169.17 42.17)
      )
    )
  )
  (zone (net 1) (net_name /MOD_POS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.17 49.67) (xy 33.17 49.67) (xy 29.17 45.67) (xy 29.17 38.17) (xy 33.67 38.17)
        (xy 33.67 42.17) (xy 40.17 42.17)
      )
    )
  )
  (zone (net 1) (net_name /MOD_POS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.17 28.67) (xy 158.17 28.67) (xy 165.67 36.17) (xy 169.17 36.17)
      )
    )
  )
  (zone (net 1) (net_name /MOD_POS) (layer In1.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.17 49.67) (xy 158.17 49.67) (xy 158.17 41.67) (xy 40.67 41.67) (xy 40.67 49.67)
        (xy 33.17 49.67) (xy 29.17 45.67) (xy 29.17 28.67) (xy 48.67 28.67) (xy 48.67 36.17)
        (xy 158.17 36.17) (xy 158.17 28.67) (xy 169.17 28.67)
      )
    )
  )
  (zone (net 2) (net_name /MOD_NEG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.17 49.67) (xy 138.17 49.67) (xy 130.67 42.17) (xy 127.17 42.17)
      )
    )
  )
  (zone (net 2) (net_name /MOD_NEG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 256.17 49.67) (xy 267.17 49.67) (xy 259.67 42.17) (xy 256.17 42.17)
      )
    )
  )
  (zone (net 2) (net_name /MOD_NEG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.17 28.67) (xy 138.17 28.67) (xy 130.67 36.17) (xy 127.17 36.17)
      )
    )
  )
  (zone (net 2) (net_name /MOD_NEG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 256.17 28.67) (xy 267.17 28.67) (xy 259.67 36.17) (xy 256.17 36.17)
      )
    )
  )
  (zone (net 2) (net_name /MOD_NEG) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 273.17 52.17) (xy 24.17 52.17) (xy 24.17 26.17) (xy 273.17 26.17)
      )
    )
  )
  (zone (net 2) (net_name /MOD_NEG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.17 45.67) (xy 34.67 52.17) (xy 24.17 52.17) (xy 24.17 38.17) (xy 28.17 38.17)
      )
    )
  )
  (zone (net 1) (net_name /MOD_POS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.17 32.67) (xy 44.17 32.67) (xy 48.17 28.67) (xy 38.17 28.67) (xy 38.17 36.17)
        (xy 40.17 36.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 273.17 52.17) (xy 24.17 52.17) (xy 24.17 26.17) (xy 273.17 26.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 273.17 52.17) (xy 24.17 52.17) (xy 24.17 26.17) (xy 273.17 26.17)
      )
    )
  )
)
