(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 76)
    (zones 0)
    (modules 41)
    (nets 14)
  )
  (page USLetter)
  (title_block
    (title "Dyna PAS Power Supply Board")
    (date 2020-03-21)
    (company "SDS Labs")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 1.905)
    (user_trace_width 2.54)
    (user_trace_width 3.175)
    (user_trace_width 3.81)
    (trace_clearance 0.2)
    (zone_clearance 1.27)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 8.255 8.255)
    (pad_drill 4.7625)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(F1-Pad2)")
  (net 13 "Net-(F1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5E77C81C)
    (at 138.049 88.011)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill0.8mm (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.255 8.255) (drill 4.7625) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E77BE92)
    (at 123.063 70.104 270)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.651 5.207) (layer F.SilkS))
    (fp_text value "47uf 450v" (at 4.191 -0.127) (layer B.SilkS))
    (fp_text user %R (at 1.651 7.239) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E77BE6A)
    (at 153.797 69.977 270)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C2 (at 2.032 4.445) (layer F.SilkS))
    (fp_text value "47uf 450v" (at 4.064 -0.381) (layer B.SilkS))
    (fp_text user %R (at 2.032 6.731) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E77BE7D)
    (at 123.063 107.442 90)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.143 -4.445 180) (layer F.SilkS))
    (fp_text value "47uf 450v" (at 4.318 0.381 180) (layer B.SilkS))
    (fp_text user %R (at 1.143 -6.858 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 90) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5E77BE9C)
    (at 153.924 107.442 90)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C4 (at 1.016 -4.572 180) (layer F.SilkS))
    (fp_text value "47uf 450v" (at 4.064 0 180) (layer B.SilkS))
    (fp_text user %R (at 1.016 -7.239 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0 90) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D13.0mm_P5.00mm (layer F.Cu) (tedit 5E77C141)
    (at 101.346 105.664 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor")
    (fp_text reference C5 (at 0.381 3.302) (layer F.SilkS))
    (fp_text value "1800uf 25V" (at 2.413 -0.381) (layer B.SilkS))
    (fp_text user %R (at 0.381 3.302) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D13.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D13.0mm_P5.00mm (layer F.Cu) (tedit 5E77C12A)
    (at 101.346 82.423 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor")
    (fp_text reference C6 (at 0.254 3.429) (layer F.SilkS))
    (fp_text value "1800uf 25V" (at 2.54 0) (layer B.SilkS))
    (fp_text user %R (at 0.254 3.429) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D13.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L18.0mm_W5.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 5E77BED2)
    (at 115.316 120.142)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 5mm Capacitor")
    (fp_text reference C7 (at 8.128 0.127) (layer F.SilkS))
    (fp_text value "0.1uf 630v" (at 7.366 0) (layer B.SilkS))
    (fp_text user %R (at 5.969 0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 15 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W5.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L18.0mm_W5.0mm_P15.00mm_FKS3_FKP3 (layer F.Cu) (tedit 5E77BEC0)
    (at 161.177 120.142 180)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 5mm Capacitor")
    (fp_text reference C8 (at 6.745 0 180) (layer F.SilkS))
    (fp_text value "0.1uf 630v" (at 7.38 0.127 180) (layer B.SilkS))
    (fp_text user %R (at 9.158 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 15 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W5.0mm_P15.00mm_FKS3_FKP3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5E77C0AE)
    (at 112.395 59.944 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.461 0 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.207 -0.127 180) (layer B.SilkS))
    (fp_text user K (at 0 -2.1 180) (layer F.SilkS))
    (fp_text user K (at 0 -2.1 180) (layer F.Fab))
    (fp_text user %R (at 5.47 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5E77C0BF)
    (at 112.395 56.134 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 5.461 0 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.207 -0.127 180) (layer B.SilkS))
    (fp_text user %R (at 5.47 0 180) (layer F.Fab))
    (fp_text user K (at 0 -2.1 180) (layer F.Fab))
    (fp_text user K (at 0 -2.1 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5E77C15A)
    (at 91.44 76.581 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at 5.461 0 270) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.207 0 270) (layer B.SilkS))
    (fp_text user %R (at 5.47 0 270) (layer F.Fab))
    (fp_text user K (at 0 -2.1 270) (layer F.Fab))
    (fp_text user K (at 0 -2.1 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5E77C164)
    (at 91.44 103.632 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D4 (at 5.461 0 270) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.207 0 270) (layer B.SilkS))
    (fp_text user K (at 0 -2.1 270) (layer F.SilkS))
    (fp_text user K (at 0 -2.1 270) (layer F.Fab))
    (fp_text user %R (at 5.47 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuseholder_Cylinder-5x20mm_Bulgin_FX0456_Vertical_Closed (layer F.Cu) (tedit 5E77C028)
    (at 180.387 93.9 90)
    (descr "Fuseholder, 5x20, closed, vertical, Bulgin, FX0456")
    (tags "Fuseholder 5x20 closed vertical Bulgin FX0456 Sicherungshalter ")
    (fp_text reference F1 (at 12.747 -2.46 180) (layer F.SilkS))
    (fp_text value Fuse (at 5.508 -7.667 90) (layer F.SilkS))
    (fp_text user %R (at 12.747 -4.492 180) (layer F.Fab))
    (fp_text user S (at 8.38 2.67 90) (layer F.Fab))
    (fp_text user F (at 1.78 -2.29 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 3 3) (drill 1.35) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.35) (layers *.Cu *.Mask)
      (net 13 "Net-(F1-Pad1)"))
    (pad "" np_thru_hole circle (at 10.08 -5 90) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.08 -5 90) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.08 5 90) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.08 5 90) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Bulgin_FX0456_Vertical_Closed.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C272)
    (at 91.44 93.218)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J1 (at -1.651 -3.429) (layer F.SilkS))
    (fp_text value Blue (at 1.016 -3.429) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C280)
    (at 106.68 93.218)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J2 (at 2.921 -1.905) (layer F.SilkS))
    (fp_text value Blue (at 2.286 -3.429) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C277)
    (at 95.25 96.139)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J3 (at 2.667 -1.778) (layer F.SilkS))
    (fp_text value Lamp (at 1.143 -3.429) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C285)
    (at 102.87 96.139)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J4 (at -3.048 2.032) (layer F.SilkS))
    (fp_text value Lamp (at -1.143 -3.429) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C27C)
    (at 91.44 98.806)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J5 (at 2.413 2.667) (layer F.SilkS))
    (fp_text value Rect (at 4.191 1.524) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C289)
    (at 106.68 98.806)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J6 (at 2.667 -1.905) (layer F.SilkS))
    (fp_text value Rect (at -4.445 1.397) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5AEE5ED2)
    (at 102.108 75.184)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J7 (at -3.937 -0.127) (layer F.SilkS))
    (fp_text value "PC-5 (18)" (at 1.905 -6.858 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C297)
    (at 107.696 117.856)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J8 (at 1.651 2.921) (layer F.SilkS))
    (fp_text value "PC-5 (19)" (at 3.683 1.143 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5AEE5ED2)
    (at 107.696 75.184)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J9 (at 1.143 3.556) (layer F.SilkS))
    (fp_text value "PC-6 (15)" (at 1.397 -6.985 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C293)
    (at 102.108 117.856)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J10 (at -1.397 3.048) (layer F.SilkS))
    (fp_text value "PC-6 (14)" (at -3.81 1.143 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C0E2)
    (at 92.329 65.786 180)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J11 (at 0.889 -3.81 180) (layer F.SilkS))
    (fp_text value "Red (B+)" (at -0.635 3.683 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C0E8)
    (at 98.171 65.786)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J12 (at 0.508 -3.556) (layer F.SilkS))
    (fp_text value "Red (B+)" (at 0 3.81) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C084)
    (at 123.063 57.658)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J13 (at -4.699 -0.127) (layer F.SilkS))
    (fp_text value "12AX4 (Cath)" (at 0.254 -4.318) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77BFEA)
    (at 170.815 61.976)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J14 (at 4.572 -0.381) (layer F.SilkS))
    (fp_text value "PC-5 (16)" (at 4.064 -3.81) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77BF58)
    (at 170.688 115.062)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J15 (at 4.445 0) (layer F.SilkS))
    (fp_text value "PC-6 (16)" (at 3.175 3.683) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C04F)
    (at 137.668 117.602)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J16 (at 0 -3.81) (layer F.SilkS))
    (fp_text value GND (at 0 3.81) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77C00B)
    (at 180.467 74.93)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J17 (at 4.191 -0.254) (layer F.SilkS))
    (fp_text value Line (at 0 -4.064) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5E77BFF2)
    (at 180.467 102.489)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J18 (at 4.699 0) (layer F.SilkS))
    (fp_text value Line (at 0.127 3.683) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 13 "Net-(F1-Pad1)"))
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E77C070)
    (at 146.05 57.658 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R1 (at 6.858 0.254 180) (layer F.SilkS))
    (fp_text value "10K 1W" (at 7.747 0.127 180) (layer B.SilkS))
    (fp_text user %R (at 9.271 0.254 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E77BF03)
    (at 170.688 66.421 270)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R2 (at 5.969 -0.127 270) (layer F.SilkS))
    (fp_text value "10K 1W" (at 7.62 -0.127 270) (layer B.SilkS))
    (fp_text user %R (at 8.763 -0.127 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E77BEF5)
    (at 170.688 110.363 90)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R3 (at 6.731 0 90) (layer F.SilkS))
    (fp_text value "47K 1W" (at 7.874 0.127 90) (layer B.SilkS))
    (fp_text user %R (at 9.271 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5E77BFB6)
    (at 183.007 55.88)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill0.8mm (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad e thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.7625) (layers *.Cu *.Mask))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5E77BF78)
    (at 183.007 120.269)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill0.8mm (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.7625) (layers *.Cu *.Mask))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5E77BFBE)
    (at 93.218 120.269)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill0.8mm (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.7625) (layers *.Cu *.Mask))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5E77BFB0)
    (at 93.218 55.88)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill0.8mm (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.715 5.715) (drill 4.7625) (layers *.Cu *.Mask))
  )
  (module sdsLogos:sdsLabs-large-fSilk (layer F.Cu) (tedit 5A94A1E6)
    (at 159.385 56.769)
    (fp_text reference G*** (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -5.08) (layer F.SilkS) hide)
  )
  (module sdsLogos:sdsLabs-large-bSilk (layer F.Cu) (tedit 5A94A1E6)
    (at 137.922 97.536)
    (fp_text reference G*** (at 0 -7.62) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 -5.08) (layer B.SilkS) hide)
  )
  (gr_text "PS\nCapboard" (at 180.467 110.363) (layer F.SilkS))
  (gr_text "Dyna\nPAS" (at 180.721 65.405) (layer F.SilkS))
  (gr_circle (center 138.049 88.011) (end 140.43025 88.011) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.325 124.587) (end 88.9 124.587) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 187.325 51.562) (end 187.325 124.587) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 88.9 51.562) (end 187.325 51.562) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 88.9 124.587) (end 88.9 51.562) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.27))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.635) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 88.9 124.587) (xy 88.9 51.562) (xy 187.325 51.562) (xy 187.325 124.587)
      )
    )
  )
)
