(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 49)
    (zones 0)
    (modules 6)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(AE1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(R1-Pad1)")
  (net 4 +5V)
  (net 5 "Net-(RTX1-Pad4)")
  (net 6 "Net-(RTX1-Pad5)")
  (net 7 "Net-(RTX1-Pad6)")
  (net 8 "Net-(RTX1-Pad9)")
  (net 9 +3V3)
  (net 10 "Net-(U1-PadD14)")
  (net 11 "Net-(U1-PadD15)")
  (net 12 "Net-(U1-PadD19)")
  (net 13 "Net-(U1-PadD22)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(RTX1-Pad4)")
    (add_net "Net-(RTX1-Pad5)")
    (add_net "Net-(RTX1-Pad6)")
    (add_net "Net-(RTX1-Pad9)")
    (add_net "Net-(U1-PadD14)")
    (add_net "Net-(U1-PadD15)")
    (add_net "Net-(U1-PadD19)")
    (add_net "Net-(U1-PadD22)")
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5D9496BD)
    (at 133.604 69.85 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 16.002 -4.826 180) (layer F.SilkS))
    (fp_text value 10k (at -2.794 0 180) (layer F.SilkS))
    (fp_text user %R (at -11.176 -0.508 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5D9496B6)
    (at 128.604 66.548)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C1 (at -11.002 5.334) (layer F.SilkS))
    (fp_text value 100nf (at 8.556 0) (layer F.SilkS))
    (fp_text user %R (at -11.256 1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usrlib:robotdyn_mega_pro (layer F.Cu) (tedit 5D94964D)
    (at 139.013001 91.261001)
    (fp_text reference U1 (at 16.51 -27.94) (layer F.SilkS))
    (fp_text value avr_mega_pro (at -11.43 -27.94) (layer F.Fab))
    (pad GND thru_hole circle (at -17.78 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad GND thru_hole circle (at -15.24 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5V thru_hole circle (at -17.78 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 5V thru_hole circle (at -15.24 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 3V3 thru_hole circle (at -17.78 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad 3V3 thru_hole circle (at -15.24 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad D14 thru_hole circle (at -15.24 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-PadD14)"))
    (pad D15 thru_hole circle (at -17.78 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-PadD15)"))
    (pad D19 thru_hole circle (at -17.78 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-PadD19)"))
    (pad D18 thru_hole circle (at -15.24 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D23 thru_hole circle (at -17.78 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D22 thru_hole circle (at -15.24 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-PadD22)"))
    (pad D35 thru_hole circle (at 15.24 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A9 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A5 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A12 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A15 thru_hole circle (at 15.24 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A10 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A4 thru_hole circle (at 17.78 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D36 thru_hole circle (at 17.78 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D33 thru_hole circle (at 15.24 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A8 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D32 thru_hole circle (at 17.78 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A14 thru_hole circle (at 17.78 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A11 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D37 thru_hole circle (at 15.24 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D34 thru_hole circle (at 17.78 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A7 thru_hole circle (at 15.24 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A13 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A6 thru_hole circle (at 17.78 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D39 thru_hole circle (at 15.24 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D44 thru_hole circle (at 17.78 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D41 thru_hole circle (at 15.24 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D42 thru_hole circle (at 17.78 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D38 thru_hole circle (at 17.78 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D46 thru_hole circle (at 17.78 25.4) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D40 thru_hole circle (at 17.78 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D43 thru_hole circle (at 15.24 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D45 thru_hole circle (at 15.24 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad D47 thru_hole circle (at 15.24 25.4) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad I4 thru_hole circle (at -2.54 25.4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad I6 thru_hole circle (at -5.08 25.4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad I1 thru_hole circle (at 0 22.86 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad I5 thru_hole circle (at -5.08 22.86 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad I2 thru_hole circle (at 0 25.4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad I3 thru_hole circle (at -2.54 22.86 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A1 thru_hole circle (at 15.24 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A3 thru_hole circle (at 15.24 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A2 thru_hole circle (at 17.78 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad A0 thru_hole circle (at 17.78 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module usrlib:lvl_shift (layer F.Cu) (tedit 5D9496D5)
    (at 140.208 105.918)
    (fp_text reference U2 (at 8.89 15.24) (layer F.SilkS))
    (fp_text value lvl_shift (at 4.572 7.366) (layer F.SilkS))
    (pad H1 thru_hole circle (at -6.35 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(RTX1-Pad9)"))
    (pad H2 thru_hole circle (at -3.81 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(RTX1-Pad6)"))
    (pad 5V thru_hole circle (at -1.27 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad GND thru_hole circle (at 1.27 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad H3 thru_hole circle (at 3.81 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(RTX1-Pad5)"))
    (pad H4 thru_hole circle (at 6.35 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(RTX1-Pad4)"))
    (pad L4 thru_hole circle (at 6.35 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-PadD14)"))
    (pad L3 thru_hole circle (at 3.81 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-PadD15)"))
    (pad GND thru_hole circle (at 1.27 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3V3 thru_hole circle (at -1.27 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad L2 thru_hole circle (at -3.81 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-PadD22)"))
    (pad L1 thru_hole circle (at -6.35 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-PadD19)"))
  )
  (module "usrlib:Aurel RTX MID 5v" (layer F.Cu) (tedit 5D68EA2A)
    (at 139.954 75.946 180)
    (fp_text reference RTX1 (at -14.732 0.254 180) (layer F.SilkS))
    (fp_text value RTX-MID (at -0.762 3.556 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -11.43 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(AE1-Pad1)"))
    (pad 2 thru_hole circle (at -8.89 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -3.81 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(RTX1-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(RTX1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(RTX1-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 6.35 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(R1-Pad1)"))
    (pad 9 thru_hole circle (at 8.89 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(RTX1-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +5V))
  )
  (module Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal (layer F.Cu) (tedit 5A1B666F)
    (at 151.384 69.284 270)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference AE1 (at -1.5 7 270) (layer F.SilkS))
    (fp_text value Antenna_Shield (at -1.212 -8.128 270) (layer F.Fab))
    (fp_text user %R (at -1.5 7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 270) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AE1-Pad1)"))
    (pad 2 smd rect (at -1.72 -4.38 270) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.72 4.38 270) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.72 -4.38 270) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.72 4.38 270) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 270) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 270) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 -4.38 270) (size 0.95 0.46) (layers F.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 4.38 270) (size 0.95 0.46) (layers F.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 -4.38 270) (size 0.95 0.46) (layers B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 4.38 270) (size 0.95 0.46) (layers B.Cu)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 157.988 64.516) (end 119.888 64.516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.988 117.856) (end 157.988 64.516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.888 117.856) (end 157.988 117.856) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.888 64.516) (end 119.888 117.856) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.888 64.516) (xy 119.888 117.856) (xy 157.988 117.856) (xy 157.988 64.516)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.888 64.516) (xy 119.888 117.856) (xy 157.988 117.856) (xy 157.988 64.516)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.510541 64.516) (xy 136.652 100.33) (xy 157.988 100.33) (xy 157.846541 64.516)
      )
    )
  )
)
