<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="16.51" x2="0" y2="0" width="0.3048" layer="20"/>
<wire x1="0" y1="0" x2="43.18" y2="0" width="0.3048" layer="20"/>
<wire x1="43.18" y1="0" x2="43.18" y2="16.51" width="0.3048" layer="20"/>
<wire x1="0" y1="16.51" x2="43.18" y2="16.51" width="0.3048" layer="20"/>
<text>LED</text>
<text>LO</text>
<text>HI</text>
<text>G</text>
<text>G</text>
<text>HERN LORD OF THE TREES</text>
</plain>
<libraries>
<library name="BTS5014SDA">
<packages>
<package name="TO114P998X235-6_5N-V">
<description>Original name &lt;b&gt;TO114P998X235-6_5N-V&lt;/b&gt;&lt;p&gt;
Max Component Height - 2.35mm</description>
</package>
</packages>
</library>
<library name="TB">
<packages>
<package name="TB_2.5MM_006P_AST04106">
</package>
</packages>
</library>
<library name="MN_PARTS_062920">
<packages>
<package name="C0805_ST0">
<description>SMD Package 0805 (metric 2012). Footprint STANDARD ST0 - Maximum Clearance between SMDs. 
Chip standard dimensions: L0.079" x W0.049" (L2.00mm x W1.25mm). 
SMD size 0.047" x 0.060" (1.1938mm x 1.524mm). 
SMD coordinates X = +/- 0.0435" (+/- 1.1049mm). 
Clearance between SMDs 0.040" (1.016mm). 
Package outline dimensions L0.148" x W0.074" (3.7592mm x 1.8796mm).</description>
</package>
<package name="CONN_TB-3POS-P5.08MM-1PIN_ICUSA_AO127-3P-5.08*2">
<description>Terminal Block, 3 position, 1 pin per position. LS 5.08mm (0.200"). Low Profile. TB Footprint fits International Connect AO127-03P-5,08 and CIXI Kaifeng KF127-03P-5,08. Modular (Stackable).
Terminal block dimensions: L15.24mm (0.600") x W8.4mm (0.335") x H10.02mm (0.400"), Pitch 5.08mm (0.200").
Pin dimensions 0.85mm x 0.55mm (0.0335" x 0.022").
Pad1 is OCT, others are RND. Pads dia 2.286mm (0.090"), Pads drill 1.219mm (0.048").
Clearance between pads 2.794mm (0.110").

International Connect AO127-03P-5,08 and CIXI Kaifeng KF127-03P-5,08 additional mechanical specs
Wire gauge 26AWG - 14AWG;
Torque 4.5 in.lb (0.55 Nm);
Screw M2.4 / Philips</description>
</package>
</packages>
</library>
<library name="MN_MECH_072017">
<packages>
<package name="MNTHL#2_DR100-CLRT130-CLRB130">
<description>Mounting hole for #2 screw / plastic pin, Diameters: Pin 0.095", Drill 0.100", Clearance from pin only: top 0.130", bottom 0.130". No screw head and no stand-off clearances</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="BTS5014SDA" package="TO114P998X235-6_5N-V" value="BTS5014SDA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="BTS5014SDA" package="TO114P998X235-6_5N-V" value="BTS5014SDA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="TB" package="TB_2.5MM_006P_AST04106" value="TB_2.5MM_006P_AST04106">
<attribute name="DESC" value="Terminal Block, 6Pos 2pin each, Spring Clamp, THH Package Pitch 2.5mm, METZ ST04106DDNN"/>
<attribute name="PN" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="MN_PARTS_062920" package="C0805_ST0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="MN_MECH_072017" package="MNTHL#2_DR100-CLRT130-CLRB130" value=""/>
<element name="U$2" library="MN_MECH_072017" package="MNTHL#2_DR100-CLRT130-CLRB130" value=""/>
<element name="TB1" library="MN_PARTS_062920" package="CONN_TB-3POS-P5.08MM-1PIN_ICUSA_AO127-3P-5.08*2" value="CONN_TB-3POS-1PIN_P21L600-W335-H400-LS200/PD1OCT-PDSRND/PDS_DI090_DR048/FOL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="TB1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="TB1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="J5" pad="P$2"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="P$3"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="P$5"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="2"/>
<contactref element="J5" pad="6"/>
<contactref element="J5" pad="P$6"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="2"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="P$4"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="6"/>
<contactref element="TB1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
