(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Spectrum Analyzer +15V / -15V Supply")
    (date "2022-06-15")
    (rev "0.1")
    (company "Andy McCann KA3KAF and Doug McCann KA3KAG")
    (comment 2 "Audiophile's Project Source Book, Fig 7-8")
    (comment 3 "G. Randy Slone")
    (comment 4 "Orginal Design by:")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 75.946 138.684)
    (pcbplotparams
      (layerselection 0x0000020_7ffffffe)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits false)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "15v-supply-models/")
    )
  )
  (net 0 "")
  (net 1 "/+15 REGULATED")
  (net 2 "GND")
  (net 3 "/-15 REGULATED")
  (net 4 "/7815 IN")
  (net 5 "/TRAN OUT1")
  (net 6 "/7915 IN")
  (net 7 "/TRAN OUT2")
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 79.756 135)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H905" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "15v-supply:C_Rect_L6.0mm_W3.5mm_P3.5mm_QYX1H103JTP3TA" (layer "F.Cu")
    (tedit 0)
    (at 115.316 66.04 -90)
    (descr "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (tags "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C909" (at 1.524 3.048 90 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 2 4.35 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 3 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "/TRAN OUT2") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/7915 IN") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/CAP_QYX_3P5X6X8P5_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.574 135)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H903" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "15v-supply:C_Rect_L6.0mm_W3.5mm_P3.5mm_QYX1H103JTP3TA" (layer "F.Cu")
    (tedit 0)
    (at 103.637 53.876 -90)
    (descr "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (tags "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C906" (at 2.004 2.799 90 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 2 4.35 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 3 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/7815 IN") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/TRAN OUT1") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/CAP_QYX_3P5X6X8P5_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 79.756 52)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H902" (at -0.498 4.642) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "15v-supply:terminal-block-691103110003" (layer "F.Cu")
    (tedit 62AA5A7D)
    (at 90.678 57.404 -90)
    (descr "<b>WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular<br></b>Max Height = 8.4mm , Pitch 3.5mm ,  3 Pins")
    (property "DATASHEET-URL" "https://www.we-online.com/catalog/datasheet/691103110003.pdf")
    (property "IR-UL" "10A")
    (property "MOUNT" "THT")
    (property "PART-NUMBER" "691103110003")
    (property "PINS" "3")
    (property "PITCH" "3.5mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Terminal Block")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (property "TYPE" "Horizontal")
    (property "VALUE" "691103110003")
    (property "WIRE" "26 to 16 (AWG) 0.129 to 1.31 (mm²)")
    (property "WORKING-VOLTAGE-UL" "125V(AC)")
    (attr through_hole)
    (fp_text reference "J901" (at -1.016 5.08 90) (layer "F.SilkS"))
    (fp_text value "Terminal Block" (at 0 4.865 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -3.5 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "/TRAN OUT1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.5 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "/TRAN OUT2") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/691103110003_1.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/691103110003_1.wrl"
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 98.044 60.198 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "15v-supply-spice/1n5060.lib")
    (property "Spice_Model" "1N5060")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D901" (at 4.318 -2.47 90) (layer "F.SilkS"))
    (fp_text value "1n5060" (at 3.81 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.2 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "/TRAN OUT1") (pinfunction "Cathode") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "/7815 IN") (pinfunction "Anode") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/1N5060-SOD-57_BYT62-BY203.stp" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.574 51.816)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H901" (at 0.03 4.388) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.474 71.882 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "15v-supply-spice/1n5060.lib")
    (property "Spice_Model" "1N5060")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D904" (at 4.064 -2.54 90) (layer "F.SilkS"))
    (fp_text value "1n5060" (at 3.81 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.2 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "/7915 IN") (pinfunction "Cathode") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "/TRAN OUT2") (pinfunction "Anode") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "15v-supply:6800u-UVR1H682MRD6" (layer "F.Cu")
    (tedit 0)
    (at 130.048 88.9)
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C911" (at 6.096 -13.716) (layer "F.SilkS"))
    (fp_text value "6800u" (at 6.2484 -2.032) (layer "F.SilkS"))
    (fp_text user "*" (at 2.54 2.032) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 6.096 2.032) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 12.4968 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 6 "/7915 IN") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/6800u-U1-BBB_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "15v-supply:6800u-UVR1H682MRD6" (layer "F.Cu")
    (tedit 0)
    (at 97.536 88.9)
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C902" (at 6.35 -13.462) (layer "F.SilkS"))
    (fp_text value "6800u" (at 6.2484 -2.032) (layer "F.SilkS"))
    (fp_text user "*" (at 2.54 2.032) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 6.096 2.032) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 "/+15 REGULATED") (pintype "passive"))
    (pad "2" thru_hole circle (at 12.4968 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/6800u-U1-BBB_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 121.158 124.46 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R902" (at 6.35 -2.72 90) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 6.35 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/-15 REGULATED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "15v-supply:6800u-UVR1H682MRD6" (layer "F.Cu")
    (tedit 0)
    (at 131.064 116.078)
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C910" (at 5.588 13.97) (layer "F.SilkS"))
    (fp_text value "6800u" (at 6.2484 -2.032) (layer "F.SilkS"))
    (fp_text user "*" (at 2.54 2.032) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 6.096 2.032) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 "/7815 IN") (pintype "passive"))
    (pad "2" thru_hole circle (at 12.4968 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/6800u-U1-BBB_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "15v-supply:C_Rect_L6.0mm_W3.5mm_P3.5mm_QYX1H103JTP3TA" (layer "F.Cu")
    (tedit 0)
    (at 103.891 66.068 -90)
    (descr "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (tags "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C907" (at 1.75 3.053 90 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 2 4.35 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 3 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/TRAN OUT1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/7915 IN") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/CAP_QYX_3P5X6X8P5_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 119.1909 102.616)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C904" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "6.8u" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/+15 REGULATED") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 98.044 71.882 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "15v-supply-spice/1n5060.lib")
    (property "Spice_Model" "1N5060")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D902" (at 4.318 -2.47 90) (layer "F.SilkS"))
    (fp_text value "1n5060" (at 3.81 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.2 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "/7915 IN") (pinfunction "Cathode") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "/TRAN OUT1") (pinfunction "Anode") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 119.9529 131.318)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C905" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "6.8u" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/-15 REGULATED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 120.396 95.504 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R901" (at 6.35 -2.72 90) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 6.35 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "/+15 REGULATED") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabUp" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 80.01 109.728)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "15v-supply-spice/regulators.lib")
    (property "Spice_Model" "LM7915")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "2 1 3")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U902" (at 2.54 20.58) (layer "F.SilkS"))
    (fp_text value "LM7915" (at 2.54 -2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 20.58) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 2.54 16.66) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "/7915 IN") (pinfunction "VI") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "/-15 REGULATED") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabUp.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "15v-supply:terminal-block-691103110003" (layer "F.Cu")
    (tedit 62AA5A7D)
    (at 122.936 57.658 90)
    (descr "<b>WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular<br></b>Max Height = 8.4mm , Pitch 3.5mm ,  3 Pins")
    (property "DATASHEET-URL" "https://www.we-online.com/catalog/datasheet/691103110003.pdf")
    (property "IR-UL" "10A")
    (property "MOUNT" "THT")
    (property "PART-NUMBER" "691103110003")
    (property "PINS" "3")
    (property "PITCH" "3.5mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Terminal Block")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (property "TYPE" "Horizontal")
    (property "VALUE" "691103110003")
    (property "WIRE" "26 to 16 (AWG) 0.129 to 1.31 (mm²)")
    (property "WORKING-VOLTAGE-UL" "125V(AC)")
    (attr through_hole)
    (fp_text reference "J902" (at 0 -4.635 90) (layer "F.SilkS"))
    (fp_text value "Terminal Block" (at 4.12 4.865 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -3.5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "/+15 REGULATED") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.5 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "/-15 REGULATED") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/691103110003_1.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/691103110003_1.wrl"
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.474 60.198 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "15v-supply-spice/1n5060.lib")
    (property "Spice_Model" "1N5060")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D903" (at 4.318 -2.47 90) (layer "F.SilkS"))
    (fp_text value "1n5060" (at 3.81 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.2 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "/TRAN OUT2") (pinfunction "Cathode") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "/7815 IN") (pinfunction "Anode") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabUp" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 80.01 77.384)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "15v-supply-spice/regulators.lib")
    (property "Spice_Model" "LM7815")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U901" (at 2.54 20.58) (layer "F.SilkS"))
    (fp_text value "LM7815" (at 2.54 -2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 20.58) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 2.54 16.66) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "/7815 IN") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "/+15 REGULATED") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabUp.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "15v-supply:C_Rect_L6.0mm_W3.5mm_P3.5mm_QYX1H103JTP3TA" (layer "F.Cu")
    (tedit 0)
    (at 115.067 53.848 -90)
    (descr "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (tags "C, Rect series, pin pitch=3.50mm, , length*width=6*3.5mm^2, Capacitor")
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C908" (at 1.778 2.794 90 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 2 4.35 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 3 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/7815 IN") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "/TRAN OUT2") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/CAP_QYX_3P5X6X8P5_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "15v-supply:6800u-UVR1H682MRD6" (layer "F.Cu")
    (tedit 0)
    (at 98.0871 116.332)
    (property "Sheetfile" "15v-supply.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C903" (at 6.3069 14.224) (layer "F.SilkS"))
    (fp_text value "6800u" (at 6.2484 -2.032) (layer "F.SilkS"))
    (fp_text user "*" (at 2.54 2.032) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 6.096 2.032) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 12.4968 0) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 3 "/-15 REGULATED") (pintype "passive"))
    (model "${KIPRJMOD}/15v-supply-models/15v-supply-3D/6800u-U1-BBB_NCH.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 75.946 48.26) (end 151.13 138.684) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Andy McCann KA3KAF and Doug McCann KA3KAG" (at 112.776 136.144) (layer "F.SilkS"))
  (gr_text "Spectrum Analyzer: \n15V Dual Supply \nRev 0.0" (at 119.634 69.342) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.13 138.684)
        (xy 75.946 138.684)
        (xy 75.946 48.26)
        (xy 151.13 48.26)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.384 138.684)
        (xy 75.946 138.684)
        (xy 75.946 48.26)
        (xy 151.384 48.26)
      )
    )
  )
)
