(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/VCC")
	(net 2 "/SWDIO_TMS")
	(net 3 "unconnected-(J1-Pin_8-Pad8)")
	(net 4 "/Reset")
	(net 5 "/GND")
	(net 6 "unconnected-(J1-Pin_1-Pad1)")
	(net 7 "/SWO_TDO")
	(net 8 "unconnected-(J1-Pin_7-Pad7)")
	(net 9 "/TDI")
	(net 10 "/SWDCK{slash}TCK")
	(net 11 "unconnected-(J2-Pin_9-Pad9)")
	(net 12 "unconnected-(J2-Pin_7-Pad7)")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 144.925 89.2875 90)
		(descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 2.54mm double row")
		(property "Reference" "J2"
			(at 1.27 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Arm10Pin"
			(at 1.27 12.49 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "STLinkMinie_DebugAdapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SWDIO_TMS")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/SWDCK{slash}TCK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SWO_TDO")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J2-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/TDI")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J2-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/Reset")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCBEdge:STLinkV3Minie_Edge"
		(layer "F.Cu")
		(at 150 95.5 180)
		(property "Reference" "J1"
			(at 0 1.25 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STLinkEdge"
			(at 0.15 -9.1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "PCBEdge:STLinkV3Minie_Edge"
			(at 0.15 -11.2 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x05, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "STLinkMinie_DebugAdapter.kicad_sch")
		(fp_line
			(start -5 -4.5)
			(end 5 -4.5)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at -0.05 -6.8 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole rect
			(at 1 -2.95 180)
			(size 0.6 3.1)
			(drill oval 0.6 3.1)
			(layers "Dwgs.User")
		)
		(pad "1" connect rect
			(at 4 -2 180)
			(size 1 4)
			(layers "F.Cu" "F.Mask")
			(net 6 "unconnected-(J1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" connect rect
			(at 2 -2 180)
			(size 1 4)
			(layers "F.Cu" "F.Mask")
			(net 9 "/TDI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" connect rect
			(at 0 -2 180)
			(size 1 4)
			(layers "F.Cu" "F.Mask")
			(net 2 "/SWDIO_TMS")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" connect rect
			(at -2 -2 180)
			(size 1 4)
			(layers "F.Cu" "F.Mask")
			(net 10 "/SWDCK{slash}TCK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" connect rect
			(at -4 -2 180)
			(size 1 4)
			(layers "F.Cu" "F.Mask")
			(net 7 "/SWO_TDO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" connect rect
			(at 4 -2 180)
			(size 1 4)
			(layers "B.Cu" "B.Mask")
			(net 5 "/GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" connect rect
			(at 2 -2 180)
			(size 1 4)
			(layers "B.Cu" "B.Mask")
			(net 8 "unconnected-(J1-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" connect rect
			(at 0 -2 180)
			(size 1 4)
			(layers "B.Cu" "B.Mask")
			(net 3 "unconnected-(J1-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" connect rect
			(at -2 -2 180)
			(size 1 4)
			(layers "B.Cu" "B.Mask")
			(net 4 "/Reset")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" connect rect
			(at -4 -2 180)
			(size 1 4)
			(layers "B.Cu" "B.Mask")
			(net 1 "/VCC")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
	)
	(gr_line
		(start 155 100)
		(end 157.5 100)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145 100)
		(end 142.5 100)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.5 100)
		(end 157.5 84.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142.5 84.5)
		(end 142.5 100)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.5 84.5)
		(end 142.5 84.5)
		(layer "Edge.Cuts")
	)
)
