(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 78)
    (no_connects 1)
    (area 107.754707 73.21012 134.756661 102.513402)
    (thickness 1.6)
    (drawings 5)
    (tracks 366)
    (zones 0)
    (modules 30)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x01008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(L1-Pad2)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 "Net-(C8-Pad2)")
  (net 7 "Net-(AE1-Pad1)")
  (net 8 SCL)
  (net 9 SDA)
  (net 10 "Net-(C10-Pad2)")
  (net 11 ACC_INT)
  (net 12 "Net-(D1-Pad2)")
  (net 13 SWCLK)
  (net 14 SWDIO)
  (net 15 RESET)
  (net 16 LED)
  (net 17 "Net-(U1-Pad3)")
  (net 18 "Net-(U1-Pad4)")
  (net 19 "Net-(U1-Pad24)")
  (net 20 "Net-(U1-Pad23)")
  (net 21 "Net-(U1-Pad32)")
  (net 22 "Net-(U1-Pad31)")
  (net 23 "Net-(U1-Pad14)")
  (net 24 "Net-(U1-Pad15)")
  (net 25 "Net-(U1-Pad26)")
  (net 26 "Net-(U1-Pad16)")
  (net 27 "Net-(U2-Pad3)")
  (net 28 BUT)
  (net 29 "Net-(C9-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ACC_INT)
    (add_net BUT)
    (add_net GND)
    (add_net LED)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad3)")
    (add_net RESET)
    (add_net SCL)
    (add_net SDA)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net VDD)
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 133.0706 98.3742 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 2.31648 -0.08128 360) (layer F.SilkS))
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 128.8796 91.4654 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ekoeppen_parts:DFN-6 (layer F.Cu) (tedit 57B0BC89)
    (at 130.048 97.7138)
    (fp_text reference U3 (at 0.1 2.8) (layer F.SilkS))
    (fp_text value SI7006 (at 0 -2.8) (layer F.Fab))
    (pad 7 smd rect (at 0 0) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.45 -1) (size 0.85 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA))
    (pad 2 smd rect (at -1.45 0) (size 0.85 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.45 1) (size 0.85 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.45 1) (size 0.85 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.45 0) (size 0.85 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 6 smd rect (at 1.45 -1) (size 0.85 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
  )
  (module EFR32BG:EFR32BG_QFN32 (layer F.Cu) (tedit 57337471)
    (at 122.069 87.37416)
    (fp_text reference U1 (at -3.88112 -3.36296) (layer F.SilkS))
    (fp_text value EFR32BG_QFN (at -8.7376 -4.0132) (layer F.Fab))
    (pad 1 smd rect (at -2.435 -1.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 13 SWCLK) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 2 smd rect (at -2.435 -1.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 14 SWDIO) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 3 smd rect (at -2.435 -0.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad3)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 4 smd rect (at -2.435 -0.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad4)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 5 smd rect (at -2.435 0.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 6 smd rect (at -2.435 0.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 7 smd rect (at -2.435 1.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 8 smd rect (at -2.435 1.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 15 RESET) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 24 smd rect (at 2.435 -1.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad24)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 23 smd rect (at 2.435 -1.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad23)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 22 smd rect (at 2.435 -0.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 21 smd rect (at 2.435 -0.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 28 BUT) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 20 smd rect (at 2.435 0.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 16 LED) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 19 smd rect (at 2.435 0.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 11 ACC_INT) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 18 smd rect (at 2.435 1.25) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 17 smd rect (at 2.435 1.75) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 9 smd rect (at -1.75 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 32 smd rect (at -1.75 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad32)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 10 smd rect (at -1.25 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 31 smd rect (at -1.25 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad31)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 11 smd rect (at -0.75 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 30 smd rect (at -0.75 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 12 smd rect (at -0.25 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(L1-Pad2)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 29 smd rect (at -0.25 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 13 smd rect (at 0.25 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 28 smd rect (at 0.25 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 14 smd rect (at 0.75 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad14)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 27 smd rect (at 0.75 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 15 smd rect (at 1.25 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad15)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 26 smd rect (at 1.25 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad26)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 16 smd rect (at 1.75 2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad16)") (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 25 smd rect (at 1.75 -2.435 90) (size 0.86 0.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05) (solder_paste_margin -0.01))
    (pad 0 smd rect (at 0 0 90) (size 3.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1) (solder_paste_margin -0.1))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 120.142 82.8548 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 1.10744 -1.31064 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 126.01956 85.22716 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 2.3622 0.12192 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 123.7234 82.8548 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 2.06756 1.34112 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 122.5296 82.846 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 2.94268 1.03632 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 117.8052 87.63 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0.39116 1.29032 180) (layer F.SilkS))
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 121.3104 82.8548 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 2.1844 -0.0508 90) (layer F.SilkS))
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 114.9096 87.4776)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0.55372 -1.34112) (layer F.SilkS))
    (fp_text value C (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 115.0112 92.3036)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at -0.1524 1.4224) (layer F.SilkS))
    (fp_text value C (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 121.29516 94.54388 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 2.86512 -0.09144 180) (layer F.SilkS))
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 121.8438 92.6338 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference L1 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value L_Small (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(L1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:crystal_FA238-TSX3225 (layer F.Cu) (tedit 0)
    (at 116.0448 89.954)
    (descr "crystal Epson Toyocom FA-238 and TSX-3225 series")
    (fp_text reference X1 (at 1.43528 2.50708) (layer F.SilkS))
    (fp_text value CRYSTAL_SMD (at 0.2 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad2)"))
    (pad 3 smd rect (at 1.1 0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 -0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 0))
    )
  )
  (module ekoeppen_parts:DFN-10 (layer F.Cu) (tedit 57B0C47E)
    (at 126.3142 92.7354 180)
    (fp_text reference U2 (at 0.20828 1.98628 180) (layer F.SilkS))
    (fp_text value MMA8652FC (at 0 -2.4 180) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -0.8 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.9 -0.4 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (pad 3 smd rect (at -0.9 0 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -0.9 0.4 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad2)"))
    (pad 5 smd rect (at -0.9 0.8 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 11 ACC_INT))
    (pad 6 smd rect (at 0.9 0.8 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.9 0.4 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 0.9 0 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 9 smd rect (at 0.9 -0.4 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 0.9 -0.8 180) (size 0.6 0.225) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA))
  )
  (module ekoeppen_parts:2450AT43B100 (layer F.Cu) (tedit 57B0CA26)
    (at 114.25428 99.6)
    (fp_text reference AE1 (at 0.22352 -2.41808) (layer F.SilkS))
    (fp_text value Antenna (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 3.5 0) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(AE1-Pad1)"))
    (pad 2 smd rect (at -3.5 0) (size 1 2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -0.83) (size 2.8 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0 0.83) (size 2.8 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 133.2484 95.6056 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -0.34036 1.45288 180) (layer F.SilkS))
    (fp_text value R (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 124.22124 95.1992 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -2.18652 0.18288 270) (layer F.SilkS))
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD)
    (at 111.5314 81.9912 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0.03556 2.04216 90) (layer F.SilkS))
    (fp_text value CP (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 128.78308 94.79788 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 2.5908 -1.81864 180) (layer F.SilkS))
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 55BDE255)
    (at 130.1496 88.52408 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.50952 0.1016 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module ekoeppen_parts:CONN_1x4_1.27mm (layer F.Cu) (tedit 57B214A3)
    (at 112.74044 77.56144 180)
    (fp_text reference P1 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.905 0 180) (size 1.016 1.016) (drill 0.69977) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole circle (at -0.635 0 180) (size 1.016 1.016) (drill 0.69977) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0.635 0 180) (size 1.016 1.016) (drill 0.69977) (layers *.Cu *.Mask)
      (net 13 SWCLK))
    (pad 4 thru_hole circle (at 1.905 0 180) (size 1.016 1.016) (drill 0.69977) (layers *.Cu *.Mask)
      (net 14 SWDIO))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 131.953 82.1182 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.8 180) (layer F.SilkS))
    (fp_text value R (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 BUT))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 128.36652 87.74684 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -0.06604 1.63068 180) (layer F.SilkS))
    (fp_text value R (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 LED))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ekoeppen_parts:BAT-HLD-001-THM (layer B.Cu) (tedit 57B2BE0E)
    (at 121.966401 88.4018 180)
    (fp_text reference BT1 (at 0 -3.81 180) (layer B.SilkS))
    (fp_text value Battery (at 0 3.81 180) (layer B.Fab))
    (pad 1 thru_hole circle (at -10.4 1.5 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole circle (at -10.4 -1.6 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole circle (at 10.4 1.5 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole circle (at 10.4 -1.6 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0 0 180) (size 5 5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 120.50776 98.86188)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference L2 (at -0.14224 -1.23444) (layer F.SilkS))
    (fp_text value L_Small (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(AE1-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 121.99112 99.45624 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference L3 (at 0.07112 -1.37668 270) (layer F.SilkS))
    (fp_text value L_Small (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ekoeppen_parts:SIDE_SWITCH_SMALL (layer F.Cu) (tedit 57B21FD4)
    (at 129.37236 77.31252)
    (fp_text reference SW1 (at 0.18288 3.4798) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3.175) (layer F.Fab))
    (pad 1 smd rect (at -1.65 1.65) (size 1.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.65 1.65) (size 1.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 28 BUT))
    (pad 3 smd rect (at 0 1.65) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 thru_hole rect (at -2.2 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 2.2 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module ekoeppen_parts:SIDE_SWITCH_SMALL (layer F.Cu) (tedit 57B21FD4)
    (at 120.35536 77.31252)
    (fp_text reference SW2 (at -3.64744 3.3528) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 -3.175) (layer F.Fab))
    (pad 1 smd rect (at -1.65 1.65) (size 1.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 15 RESET))
    (pad 2 smd rect (at 1.65 1.65) (size 1.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.65) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 thru_hole rect (at -2.2 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 2.2 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  )
  (gr_text + (at 115.39728 78.6638) (layer F.SilkS))
  (gr_line (start 134.62 101.6) (end 109.22 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 76.2) (end 134.62 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 76.2) (end 134.62 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 101.6) (end 109.22 76.2) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.60984 76.23048) (xy 134.64032 101.5746) (xy 119.24284 101.61016) (xy 119.24284 96.71304) (xy 109.17428 96.71812)
        (xy 109.270776 76.23048)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.23016 76.23048) (xy 109.2708 76.2254) (xy 109.270776 76.23048)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.2454 76.22032) (xy 109.22508 96.72828) (xy 119.24792 96.71304) (xy 119.253 101.6) (xy 134.61492 101.58476)
        (xy 134.60984 76.21524) (xy 109.26572 76.24064)
      )
    )
  )
)
