(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 120)
    (zones 0)
    (modules 15)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 99.9 96.9)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers"))
  )
  (net 0 "")
  (net 1 N_RST)
  (net 2 GND)
  (net 3 TX)
  (net 4 RX)
  (net 5 SWO)
  (net 6 SWCLK)
  (net 7 SWDIO)
  (net 8 "Net-(J1-Pad1)")
  (net 9 +3V3)
  (net 10 "Net-(JP2-Pad2)")
  (net 11 "Net-(JP3-Pad2)")
  (net 12 "Net-(U1-Pad22)")
  (net 13 "Net-(U1-Pad18)")
  (net 14 "Net-(U1-Pad16)")
  (net 15 "Net-(U1-Pad15)")
  (net 16 "Net-(U1-Pad14)")
  (net 17 "Net-(U1-Pad13)")
  (net 18 "Net-(U1-Pad12)")
  (net 19 "Net-(U1-Pad11)")
  (net 20 "Net-(U1-Pad10)")
  (net 21 "Net-(U1-Pad9)")
  (net 22 "Net-(U1-Pad8)")
  (net 23 "Net-(U1-Pad7)")
  (net 24 "Net-(U1-Pad6)")
  (net 25 "Net-(U1-Pad5)")
  (net 26 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net N_RST)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net RX)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net SWO)
    (add_net TX)
  )
  (module gen2-jtag:particle-logo-9mm (layer F.Cu) (tedit 0)
    (at 110.2 91.7)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module gen2-jtag:particle-logo-9mm (layer F.Cu) (tedit 0)
    (at 110.06 89.28)
    (fp_text reference U2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value PARTICLE_LOGO_9MM (at 0.75 0) (layer F.SilkS) hide)
  )
  (module gen2-jtag:PHOTON locked (layer F.Cu) (tedit 5F36C807)
    (at 100 100)
    (fp_text reference U1 (at 5.715 1.143) (layer F.SilkS) hide)
    (fp_text value PHOTON (at 6.35 2.667) (layer F.Fab))
    (fp_text user 24 (at 16.51 -32.004) (layer F.Fab))
    (fp_text user 13 (at 16.51 -4.064) (layer F.Fab))
    (fp_text user 12 (at 2.794 -4.064) (layer F.Fab))
    (fp_text user 1 (at 2.794 -32.004) (layer F.Fab))
    (fp_text user GROUND~PLANE~AND~SIGNAL~KEEP~OUT~RECOMMENDED~ON~ALL~LAYERS (at 3.302 -0.381) (layer F.Fab))
    (fp_text user 13 (at 19.05 -4.064) (layer F.Fab))
    (pad 24 thru_hole circle (at 19.05 -32.258) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad 23 thru_hole circle (at 19.05 -29.718) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N_RST))
    (pad 22 thru_hole circle (at 19.05 -27.178) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad22)"))
    (pad 21 thru_hole circle (at 19.05 -24.638) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole circle (at 19.05 -22.098) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 SWDIO))
    (pad 19 thru_hole circle (at 19.05 -19.558) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 SWCLK))
    (pad 18 thru_hole circle (at 19.05 -17.018) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad18)"))
    (pad 17 thru_hole circle (at 19.05 -14.478) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 SWO))
    (pad 16 thru_hole circle (at 19.05 -11.938) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad16)"))
    (pad 15 thru_hole circle (at 19.05 -9.398) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad15)"))
    (pad 14 thru_hole circle (at 19.05 -6.858) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad14)"))
    (pad 13 thru_hole circle (at 19.05 -4.318) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad13)"))
    (pad 12 thru_hole circle (at 1.27 -4.318) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad12)"))
    (pad 11 thru_hole circle (at 1.27 -6.858) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad11)"))
    (pad 10 thru_hole circle (at 1.27 -9.398) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad10)"))
    (pad 9 thru_hole circle (at 1.27 -11.938) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad9)"))
    (pad 8 thru_hole circle (at 1.27 -14.478) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at 1.27 -17.018) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad7)"))
    (pad 6 thru_hole circle (at 1.27 -19.558) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 -22.098) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 -24.638) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(JP3-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 -27.178) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(JP2-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 -29.718) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.27 -32.258) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad1)"))
  )
  (module gen2-jtag:CONN5X2_1.27 (layer F.Cu) (tedit 5F36C86B)
    (at 110.2 72.7)
    (fp_text reference J1 (at -4.2 3) (layer F.SilkS))
    (fp_text value FTSH-105-01-F-DV-K (at 9.85 -0.58) (layer F.Fab))
    (pad 10 smd rect (at 2.54 -2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 1 N_RST))
    (pad 9 smd rect (at 2.54 2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 1.27 -2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 3 TX))
    (pad 7 smd rect (at 1.27 2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 4 RX))
    (pad 6 smd rect (at 0 -2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 5 SWO))
    (pad 5 smd rect (at 0 2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.27 -2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 6 SWCLK))
    (pad 3 smd rect (at -1.27 2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.54 -2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 7 SWDIO))
    (pad 1 smd rect (at -2.54 2) (size 0.7 2.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 115 85.075 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 2.625 0.1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 N_RST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 115 79.975 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -2.475 -0.1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 N_RST))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 111.8 85.075 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 2.625 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 SWO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 111.8 79.975 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -2.475 0.1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 SWO))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 108.6 85.075 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.625 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 SWCLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 108.6 79.975 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.475 -0.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 SWCLK))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 105.4 85.075 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.625 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 SWDIO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 105.4 79.975 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.475 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at -0.2 -0.5 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 SWDIO))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 104.25 75.3 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (clearance 0.254)
    (attr virtual)
    (fp_text reference JP3 (at -2.9 0) (layer B.SilkS) hide)
    (fp_text value "TX Jumper" (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 11 "Net-(JP3-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 TX) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 104.25 72.8 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (clearance 0.254)
    (attr virtual)
    (fp_text reference JP2 (at -2.9 0) (layer B.SilkS) hide)
    (fp_text value "RX Jumper" (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 10 "Net-(JP2-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 4 RX) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 116.1 67.75 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (clearance 0.254)
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8) (layer B.SilkS) hide)
    (fp_text value "+3.3V Jumper" (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 8 "Net-(J1-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 9 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (gr_text RST (at 113.3 67.4) (layer B.SilkS))
  (gr_text TX (at 104.3 71) (layer B.SilkS))
  (gr_text RX (at 104.4 77.2) (layer B.SilkS))
  (gr_line (start 99.9 96.9) (end 99.9 66.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.4 96.9) (end 99.9 96.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.4 66.4) (end 120.4 96.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.9 66.4) (end 120.4 66.4) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 120.4 96.9) (xy 99.9 96.9) (xy 99.9 66.4) (xy 120.4 66.4)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 120.4 96.9) (xy 99.9 96.9) (xy 99.9 66.4) (xy 120.4 66.4)
      )
    )
  )
)
