(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 14)
    (no_connects 0)
    (area 138.379999 69.799999 153.720001 102.920001)
    (thickness 1.6)
    (drawings 5)
    (tracks 42)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (title_block
    (title "Sensor target GP2y0DxxZ0f")
    (date 2016-11-13)
    (company "RPL HW & SW")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 /Out)
  (net 5 "Net-(R1-Pad1)")
  (net 6 "Net-(U1-Pad1)")
  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class rpl ""
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Out)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net VCC)
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 0)
    (at 148.59 76.2 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 1.25 -3.8 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer B.Cu) (tedit 0)
    (at 148.59 72.39 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 5.1 90) (layer B.SilkS))
    (fp_text value CONN_01X03 (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /Out))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 140.97 80.01 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.05892 -3.50012 270) (layer F.SilkS))
    (fp_text value 4.7 (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
  )
  (module GP2Y0D8xxZ0F-rpl:GP2Y0D8xxZ0F (layer F.Cu) (tedit 56E73616)
    (at 147.32 87.63)
    (fp_text reference U1 (at 0 -8) (layer F.SilkS))
    (fp_text value GP2Y0D8xxZ0F (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.25 -6) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at -3.25 -3) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(R1-Pad1)"))
    (pad 3 thru_hole oval (at -3.25 -1.5) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad1)"))
    (pad 4 thru_hole oval (at -3.25 0) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at -3.25 1.5) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at -3.25 3) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at -3.25 4.5) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 8 thru_hole oval (at 3.25 4.5) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 3.25 3) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 3.25 1.5) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 3.25 0) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 12 thru_hole oval (at 3.25 -1.5) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 13 thru_hole oval (at 3.25 -3) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 /Out))
    (pad 14 thru_hole oval (at 3.25 -6) (size 1.54 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 143.51 76.2 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.25 -2.5 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 140.97 92.71 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 146.05 99.06)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 138.43 93.98) (end 153.67 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.43 102.87) (end 138.43 69.85) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.67 102.87) (end 138.43 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.67 69.85) (end 153.67 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.43 69.85) (end 153.67 69.85) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 102.87) (xy 138.43 102.87) (xy 138.43 69.85) (xy 153.67 69.85) (xy 153.67 102.87)
      )
    )
  )
)
