(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 24)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 R)
  (net 2 G)
  (net 3 B)
  (net 4 A)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A)
    (add_net B)
    (add_net G)
    (add_net R)
  )
  (module "Wiiboy Parts:1.25mm pad" (layer F.Cu) (tedit 5C02D627)
    (at 96.88 62.63)
    (fp_text reference TP1 (at 0 -1 180) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 R))
  )
  (module "Wiiboy Parts:1.25mm pad" (layer F.Cu) (tedit 5C02D627)
    (at 93.58 62.64)
    (fp_text reference TP2 (at 0 -1 180) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 G))
  )
  (module "Wiiboy Parts:1.25mm pad" (layer F.Cu) (tedit 5C02D627)
    (at 95.23 62.64)
    (fp_text reference TP3 (at 0 -1 180) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 B))
  )
  (module "Wiiboy Parts:1.25mm pad" (layer F.Cu) (tedit 5C02D627)
    (at 98.53 62.64)
    (fp_text reference TP4 (at 0 -1 180) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 A))
  )
  (module "Wiiboy Parts:LTST-C19HE1WT" (layer B.Cu) (tedit 5C55BE16)
    (at 96.78 60.57 180)
    (fp_text reference U1 (at -0.01 -1.74 180) (layer B.SilkS))
    (fp_text value LTST-C19HE1WT (at 0 1.55 180) (layer B.Fab))
    (pad 1 smd rect (at -0.43 0.73 180) (size 0.65 0.85) (layers B.Cu B.Paste B.Mask)
      (net 1 R))
    (pad 2 smd rect (at 0.43 0.73 180) (size 0.65 0.85) (layers B.Cu B.Paste B.Mask)
      (net 2 G))
    (pad 3 smd rect (at 0.43 -0.73 180) (size 0.65 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 B))
    (pad 4 smd rect (at -0.43 -0.73 180) (size 0.65 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 A))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5C55BF04)
    (at 91.78 60.57)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 99.49 57.42) (end 89.78 57.42) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.49 63.72) (end 99.49 57.42) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.78 63.72) (end 99.49 63.72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.78 57.42) (end 89.78 63.72) (layer Edge.Cuts) (width 0.15))
  (gr_text G- (at 93.6 61.52) (layer F.SilkS))
  (gr_text B- (at 95.27 61.52) (layer F.SilkS))
  (gr_text R- (at 96.9 61.5) (layer F.SilkS))
  (gr_text V+ (at 98.54 61.52) (layer F.SilkS))
)
