<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-7.62" x2="0" y2="7.62" width="0.06" layer="20"/>
<wire x1="0" y1="7.62" x2="25.4" y2="7.62" width="0.06" layer="20"/>
<wire x1="25.4" y1="7.62" x2="25.4" y2="-7.62" width="0.06" layer="20"/>
<wire x1="25.4" y1="-7.62" x2="0" y2="-7.62" width="0.06" layer="20"/>
<text>5V 5A</text>
<text>Copyright (C) 2015
Herbert Pötzl</text>
<text>Licensed
under CERN
OHL v.1.2</text>
<text>AXIOM Beta
Power Adapter</text>
<text>V0.2
R1.1</text>
<text>BETA POWER ADAPTER
TOP SIDE     V0.2 R1.1</text>
<text>BETA POWER ADAPTER
BOTTOM SIDE  V0.2 R1.1</text>
</plain>
<libraries>
<library name="pico-spox">
<packages>
<package name="PICO-SPOX-5">
</package>
</packages>
</library>
<library name="power_jack">
<packages>
<package name="POWER_JACK_PTH_SLOT">
</package>
</packages>
</library>
<library name="generic-rcl">
<packages>
<package name="0402-B">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_FILLX100_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="pico-spox" package="PICO-SPOX-5" value="PICO-SPOX-5">
<attribute name="NAME"/>
</element>
<element name="X2" library="power_jack" package="POWER_JACK_PTH_SLOT" value="POWER_JACKPTH_SLOT">
<attribute name="NAME"/>
</element>
<element name="R1" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="ohw-logo" package="OSHW_FILLX100_NOTEXT" value="OSHW_LOGO_FILLX0100-NT"/>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="5A"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="1A"/>
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="GND"/>
</signal>
<signal name="VIN">
<contactref element="X1" pad="3A"/>
<contactref element="X1" pad="3"/>
<contactref element="X2" pad="SHUNT"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="BETA_5V">
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="4A"/>
<contactref element="X1" pad="2A"/>
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="PWR"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
