(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 59)
    (zones 0)
    (modules 9)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(LS1-Pad1)")
  (net 3 "Net-(U1-Pad14)")
  (net 4 "Net-(U1-Pad15)")
  (net 5 "Net-(U1-Pad16)")
  (net 6 "Net-(U1-Pad17)")
  (net 7 "Net-(U1-Pad18)")
  (net 8 "Net-(U1-Pad19)")
  (net 9 "Net-(U1-Pad20)")
  (net 10 "Net-(S1-Pad6)")
  (net 11 "Net-(S1-Pad5)")
  (net 12 "Net-(S1-Pad4)")
  (net 13 "Net-(S1-Pad3)")
  (net 14 "Net-(S1-Pad2)")
  (net 15 "Net-(S2-Pad6)")
  (net 16 "Net-(B1-Pad2)")
  (net 17 "Net-(B2-Pad2)")
  (net 18 "Net-(B3-Pad2)")
  (net 19 "Net-(B4-Pad2)")
  (net 20 "Net-(B5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(B1-Pad2)")
    (add_net "Net-(B2-Pad2)")
    (add_net "Net-(B3-Pad2)")
    (add_net "Net-(B4-Pad2)")
    (add_net "Net-(B5-Pad2)")
    (add_net "Net-(LS1-Pad1)")
    (add_net "Net-(S1-Pad2)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(S1-Pad5)")
    (add_net "Net-(S1-Pad6)")
    (add_net "Net-(S2-Pad6)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
  )
  (module Buzzer_Beeper:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 5A030281)
    (at 110.49 73.66 90)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference LS1 (at 3.8 -7.2 90) (layer F.SilkS) hide)
    (fp_text value Piezo (at 3.8 7.4 90) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 90) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 90) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(LS1-Pad1)"))
    (pad 2 thru_hole circle (at 7.6 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Seeeduino XIAO KICAD:Seeeduino XIAO-MOUDLE14P-2.54-21X17.8MM" (layer F.Cu) (tedit 5EA16CE1)
    (at 116.84 91.066621)
    (attr smd)
    (fp_text reference U1 (at 9.3345 -21.7805) (layer F.SilkS))
    (fp_text value SeeeduinoXIAO (at 8.89 -10.795) (layer F.SilkS))
    (pad 14 smd oval (at 16.99768 -18.11782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad14)"))
    (pad 13 smd oval (at 16.99768 -15.57782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd oval (at 16.99768 -13.03782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(S1-Pad2)"))
    (pad 11 smd oval (at 16.99768 -10.49782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(S1-Pad3)"))
    (pad 10 smd oval (at 16.99768 -7.95782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(S1-Pad4)"))
    (pad 9 smd oval (at 16.99768 -5.41782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(S1-Pad5)"))
    (pad 8 smd oval (at 16.99768 -2.87782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(S1-Pad6)"))
    (pad 7 smd oval (at 0.83312 -2.87782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(S2-Pad6)"))
    (pad 6 smd oval (at 0.83312 -5.41782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(B5-Pad2)"))
    (pad 5 smd oval (at 0.83312 -7.95782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(B4-Pad2)"))
    (pad 4 smd oval (at 0.83312 -10.49782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(LS1-Pad1)"))
    (pad 3 smd oval (at 0.83312 -13.03782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(B3-Pad2)"))
    (pad 2 smd oval (at 0.83312 -15.57782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(B2-Pad2)"))
    (pad 1 smd oval (at 0.83312 -18.11782) (size 2.74828 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(B1-Pad2)"))
    (pad 15 smd oval (at 7.7 -1.8 90) (size 2.032 1.016) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad15)"))
    (pad 16 smd oval (at 10.25 -1.8 90) (size 2.032 1.016) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad16)"))
    (pad 17 smd circle (at 7.698803 -18.804187 90) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad17)"))
    (pad 18 smd circle (at 10.238803 -18.804187 90) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad18)"))
    (pad 19 smd circle (at 7.698803 -16.264187 90) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad19)"))
    (pad 20 smd circle (at 10.238803 -16.264187 90) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad20)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 137.795 75.565)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference S1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(S1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(S1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(S1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(S1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.49 78.105 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference B1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(B1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.49 80.645 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference B2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(B2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.49 83.185 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference B3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(B3-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.49 85.725 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference B4 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(B4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.49 88.265 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference B5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(B5-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 140.335 75.565)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference S2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(S1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(S1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(S1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(S2-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "board v1.0" (at 142.494 67.564) (layer F.SilkS))
  (gr_text github.com/monroewilliams/trackball (at 142.24 65.786) (layer F.SilkS))
  (gr_line (start 142.875 64.135) (end 142.875 92.075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.315 64.135) (end 142.875 64.135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.315 92.075) (end 107.315 64.135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.875 92.075) (end 107.315 92.075) (layer Edge.Cuts) (width 0.1))
)
