(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu19.10.1)
  (general
    (thickness 1.6)
    (drawings 27)
    (tracks 10)
    (zones 0)
    (modules 2)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (trace_clearance 0.16)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.16)
    (via_size 0.42)
    (via_drill 0.26)
    (via_min_size 0.42)
    (via_min_drill 0.26)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.02)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.1016)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 127 95.758)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+5V)
  (net 2 /GND)
  (net 3 /RXD)
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.16)
    (via_dia 0.42)
    (via_drill 0.26)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V)
    (add_net /GND)
    (add_net /RXD)
  )
  (module 0_LOCAL:TE-5207826_cut (layer B.Cu) (tedit 5F29E510)
    (at 121.475 94.333 180)
    (descr "9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm")
    (fp_text reference CN1 (at -5.5372 1.7018) (layer B.SilkS) hide)
    (fp_text value DB9_Female (at -5.54 -8.73) (layer B.Fab))
    (fp_text user %R (at -5.54 -1.42) (layer B.Fab))
    (pad 9 thru_hole circle (at -9.695 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (pad 8 thru_hole circle (at -6.925 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -4.155 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 6 thru_hole circle (at -1.385 -2.84 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -11.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -8.31 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -5.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.77 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /RXD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3dmodels/TE-5207826_cut.step
      (offset (xyz -5.528 -1.42 11.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:Socket_Strip_Angled_1x03_Pitch2.54mm (layer F.Cu) (tedit 5F178664)
    (at 136.875 93.233)
    (descr "Through hole angled socket strip, 1x03, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x03 2.54mm single row")
    (fp_text reference CN2 (at -4.38 -2.27) (layer F.SilkS) hide)
    (fp_text value UE27AC54100 (at -4.38 7.35) (layer F.Fab))
    (fp_text user %R (at -4.38 -2.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /RXD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (model ${KIPRJMOD}/3dmodels/PinSocket_1x03_P2.54mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text COVER (at 131.19 99.048) (layer F.SilkS))
  (gr_arc (start 137.225 92.758) (end 139.225 92.758) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 119.5 92.758) (end 119.5 90.758) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 119.5 98.758) (end 117.5 98.758) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 137.225 98.758) (end 137.225 100.758) (angle -90) (layer Edge.Cuts) (width 0.02))
  (gr_text +5v (at 125.1 98.683) (layer F.SilkS))
  (gr_text DATA (at 124.825 95.758) (layer F.SilkS))
  (gr_text GND (at 125.125 92.933) (layer F.SilkS))
  (gr_text BCR (at 118.325 95.783 90) (layer F.SilkS))
  (gr_text BREAKOUT (at 119.675 95.758 90) (layer F.SilkS))
  (gr_text D (at 138.45 95.758) (layer F.SilkS))
  (gr_text + (at 138.5 98.183) (layer F.SilkS))
  (gr_text - (at 138.475 93.158) (layer F.SilkS))
  (gr_line (start 117.5 98.758) (end 117.5 92.758) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 137.225 90.758) (end 119.5 90.758) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 137.225 100.758) (end 119.5 100.758) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 139.225 98.758) (end 139.225 92.758) (layer Edge.Cuts) (width 0.02))
  (gr_text "TE 5207826" (at 127 95.783) (layer B.SilkS))
  (gr_text github.com/bkw777/BCR_Breakout (at 128.425 100.233) (layer B.SilkS))
  (gr_text "DE9F SIDE" (at 127 92.958) (layer B.SilkS))
)
