(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 25)
    (no_connects 0)
    (area 136.124999 93.924999 171.375001 114.075001)
    (thickness 1.6)
    (drawings 17)
    (tracks 165)
    (zones 0)
    (modules 13)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(P2-Pad1)")
  (net 4 "Net-(P2-Pad6)")
  (net 5 "Net-(U1-Pad4)")
  (net 6 "Net-(C1-Pad1)")
  (net 7 "Net-(C2-Pad2)")
  (net 8 "Net-(JP2-Pad1)")
  (net 9 "Net-(JP2-Pad2)")
  (net 10 "Net-(P2-Pad4)")
  (net 11 "Net-(U2-Pad37)")
  (net 12 "Net-(U2-Pad36)")
  (net 13 "Net-(U2-Pad33)")
  (net 14 "Net-(U2-Pad32)")
  (net 15 "Net-(U2-Pad31)")
  (net 16 "Net-(U2-Pad30)")
  (net 17 "Net-(U2-Pad29)")
  (net 18 "Net-(U2-Pad28)")
  (net 19 "Net-(U2-Pad27)")
  (net 20 "Net-(U2-Pad26)")
  (net 21 "Net-(U2-Pad25)")
  (net 22 "Net-(U2-Pad24)")
  (net 23 "Net-(U2-Pad23)")
  (net 24 "Net-(U2-Pad22)")
  (net 25 "Net-(U2-Pad21)")
  (net 26 "Net-(U2-Pad20)")
  (net 27 "Net-(U2-Pad19)")
  (net 28 "Net-(U2-Pad18)")
  (net 29 "Net-(U2-Pad17)")
  (net 30 "Net-(U2-Pad16)")
  (net 31 "Net-(U2-Pad14)")
  (net 32 "Net-(U2-Pad13)")
  (net 33 "Net-(U2-Pad12)")
  (net 34 "Net-(U2-Pad11)")
  (net 35 "Net-(U2-Pad10)")
  (net 36 "Net-(U2-Pad9)")
  (net 37 "Net-(U2-Pad8)")
  (net 38 "Net-(U2-Pad7)")
  (net 39 "Net-(U2-Pad6)")
  (net 40 "Net-(U2-Pad5)")
  (net 41 "Net-(U2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 581B75BC)
    (at 141.9 103 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value LP2985-3.3 (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:0402_CAP (layer F.Cu) (tedit 581B75D0)
    (at 142.3 105.3 180)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference C2 (at 2.1 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 0.635 180) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:0402 (layer F.Cu) (tedit 581B75ED)
    (at 140.2 110.8)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference R1 (at 2.1 0) (layer F.SilkS))
    (fp_text value 1k (at 0 0.635) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0.6477 0) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:SJ_OPEN (layer F.Cu) (tedit 581B75DC)
    (at 142.3 95.5 180)
    (descr "<b>Solder jumper</b>")
    (fp_text reference JP1 (at 0.1 -1.7 180) (layer F.SilkS))
    (fp_text value JUMPER (at 0 1.6 180) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 7 "Net-(C2-Pad2)"))
  )
  (module freetronics_footprints:0402 (layer F.Cu) (tedit 581B75FC)
    (at 140.2 109.5)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference R3 (at 2.1 0) (layer F.SilkS))
    (fp_text value 2k (at 0 0.635) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.6477 0) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57C365A3)
    (at 140.3 108)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.3) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module freetronics_footprints:SJ_OPEN (layer F.Cu) (tedit 581B8A9C)
    (at 140.5 112.6)
    (descr "<b>Solder jumper</b>")
    (fp_text reference JP2 (at 2.8 0) (layer F.SilkS))
    (fp_text value JUMPER (at 0 1.6) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.762 0) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 8 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 9 "Net-(JP2-Pad2)"))
  )
  (module freetronics_footprints:0402 (layer F.Cu) (tedit 581B75E5)
    (at 142.4 107.4 90)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference R4 (at 0 1.3 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0.635 90) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0 90) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.6477 0 90) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:0402_CAP (layer F.Cu) (tedit 581B7773)
    (at 142.3 100.7 180)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference C1 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 0.635 180) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Brain_Duino:Bluetooth_Socket (layer F.Cu) (tedit 57C4247F)
    (at 137.3 97.82)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.22) (layer F.SilkS))
    (fp_text value BLUETOOTH_SOCKET (at -2.5 5.98 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(JP2-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P2-Pad6)"))
  )
  (module Brain_Duino:ESP32-WROOM-V2 (layer F.Cu) (tedit 581BA6F7)
    (at 158.55 104 90)
    (fp_text reference U2 (at 0 4.05 360) (layer F.SilkS))
    (fp_text value ESP32-WROOM (at 5.715 14.224 90) (layer F.Fab))
    (fp_text user "Espressif Systems" (at -6.858 -0.889 180) (layer F.SilkS))
    (fp_text user ESP32-WROOM (at -5.207 0.254 180) (layer F.SilkS))
    (pad 38 smd oval (at -8.75 5.25 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd oval (at -8.75 3.98 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U2-Pad37)"))
    (pad 36 smd oval (at -8.75 2.71 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad36)"))
    (pad 35 smd oval (at -8.75 1.44 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P2-Pad4)"))
    (pad 34 smd oval (at -8.75 0.17 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP2-Pad2)"))
    (pad 33 smd oval (at -8.75 -1.1 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad33)"))
    (pad 32 smd oval (at -8.75 -2.37 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad32)"))
    (pad 31 smd oval (at -8.75 -3.64 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad31)"))
    (pad 30 smd oval (at -8.75 -4.91 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad30)"))
    (pad 29 smd oval (at -8.75 -6.18 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad29)"))
    (pad 28 smd oval (at -8.75 -7.45 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad28)"))
    (pad 27 smd oval (at -8.75 -8.72 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad27)"))
    (pad 26 smd oval (at -8.75 -9.99 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad26)"))
    (pad 25 smd oval (at -8.75 -11.26 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad25)"))
    (pad 24 smd oval (at -5.715 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad24)"))
    (pad 23 smd oval (at -4.445 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad23)"))
    (pad 22 smd oval (at -3.175 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad22)"))
    (pad 21 smd oval (at -1.905 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad21)"))
    (pad 20 smd oval (at -0.635 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad20)"))
    (pad 19 smd oval (at 0.635 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad19)"))
    (pad 18 smd oval (at 1.905 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad18)"))
    (pad 17 smd oval (at 3.175 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad17)"))
    (pad 16 smd oval (at 4.445 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad16)"))
    (pad 15 smd oval (at 5.715 -12.75 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd oval (at 8.75 -11.26 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad14)"))
    (pad 13 smd oval (at 8.75 -9.99 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad13)"))
    (pad 12 smd oval (at 8.75 -8.72 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad12)"))
    (pad 11 smd oval (at 8.75 -7.45 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad11)"))
    (pad 10 smd oval (at 8.75 -6.18 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad10)"))
    (pad 9 smd oval (at 8.75 -4.91 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad9)"))
    (pad 8 smd oval (at 8.75 -3.64 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad8)"))
    (pad 7 smd oval (at 8.75 -2.37 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad7)"))
    (pad 6 smd oval (at 8.75 -1.1 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-Pad6)"))
    (pad 5 smd oval (at 8.75 0.17 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-Pad5)"))
    (pad 4 smd oval (at 8.75 1.44 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad4)"))
    (pad 3 smd oval (at 8.75 2.71 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad2)"))
    (pad 2 smd oval (at 8.75 3.98 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad2)"))
    (pad 1 smd oval (at 8.75 5.25 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at 0.3 -2.45 90) (size 6 6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ESP32.3dshapes/ESP-32S.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module w_logo:Logo_silk_CC-BY-SA_10x4.5mm (layer B.Cu) (tedit 0)
    (at 155.2 106.6 180)
    (descr "CC BY-SA logo, 10x4.5mm")
    (fp_text reference G*** (at 1.9 -0.5 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 1.9 1.7 180) (layer B.SilkS) hide)
  )
  (module freetronics_footprints:LOGO_OSHW_silkscreen_2mm (layer F.Cu) (tedit 0)
    (at 140.1 98)
    (fp_text reference LOGO_OSHW_silkscreen_2mm (at 0 1.05918) (layer F.SilkS) hide)
    (fp_text value val** (at 0 -1.05918) (layer F.SilkS) hide)
  )
  (gr_text TX (at 139.9 105.4) (layer B.SilkS))
  (gr_text RX (at 139.8 108) (layer B.SilkS))
  (gr_text GND (at 139.9 103) (layer B.SilkS))
  (gr_text VCC (at 139.9 100.4) (layer B.SilkS))
  (gr_text "JP2 - for 3.3V RX" (at 144.3 111.1) (layer B.SilkS))
  (gr_text "3 Nov 2016" (at 154.80678 102.102276) (layer B.SilkS))
  (gr_text "ESP32 breakout v0.1" (at 154.80678 96.902276) (layer B.SilkS))
  (gr_text www.brain-duino.com (at 155.2 103.4) (layer B.SilkS))
  (gr_text "Silver Kuusik" (at 154.80678 100.902276) (layer B.SilkS))
  (gr_text "CC-BY-SA 4.0\n" (at 154.80678 99.702276) (layer B.SilkS))
  (gr_text "JP1 - for 3.3V VCC" (at 144.2 109.7) (layer B.SilkS))
  (dimension 20 (width 0.3) (layer Margin)
    (gr_text "20.000 mm" (at 175.85 104 90) (layer Margin))
    (feature1 (pts (xy 171.3 94) (xy 177.2 94)))
    (feature2 (pts (xy 171.3 114) (xy 177.2 114)))
    (crossbar (pts (xy 174.5 114) (xy 174.5 94)))
    (arrow1a (pts (xy 174.5 94) (xy 175.086421 95.126504)))
    (arrow1b (pts (xy 174.5 94) (xy 173.913579 95.126504)))
    (arrow2a (pts (xy 174.5 114) (xy 175.086421 112.873496)))
    (arrow2b (pts (xy 174.5 114) (xy 173.913579 112.873496)))
  )
  (dimension 34 (width 0.3) (layer Margin)
    (gr_text "34.000 mm" (at 154.3 91.253665) (layer Margin))
    (feature1 (pts (xy 171.3 96) (xy 171.3 89.903665)))
    (feature2 (pts (xy 137.3 96) (xy 137.3 89.903665)))
    (crossbar (pts (xy 137.3 92.603665) (xy 171.3 92.603665)))
    (arrow1a (pts (xy 171.3 92.603665) (xy 170.173496 93.190086)))
    (arrow1b (pts (xy 171.3 92.603665) (xy 170.173496 92.017244)))
    (arrow2a (pts (xy 137.3 92.603665) (xy 138.426504 93.190086)))
    (arrow2b (pts (xy 137.3 92.603665) (xy 138.426504 92.017244)))
  )
  (gr_line (start 136.2 114) (end 136.2 94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.3 114) (end 136.2 114) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.3 94) (end 171.3 114) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.2 94) (end 171.3 94) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.3 94) (xy 165.3 94) (xy 165.3 114) (xy 171.3 114)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.3 94) (xy 165.3 94) (xy 165.3 114) (xy 171.3 114)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.3 94) (xy 171.3 114) (xy 136.2 114) (xy 136.2 94)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.3 94) (xy 171.3 114) (xy 136.2 114) (xy 136.2 94)
      )
    )
  )
)
