(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 967)
    (zones 0)
    (modules 85)
    (nets 157)
  )
  (page A4)
  (title_block
    (title "Nixie Clock Top PCB")
    (date 2019-08-15)
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 1.27)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.4 6.4)
    (pad_drill 3.200001)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /HV)
  (net 4 /r1)
  (net 5 /g1)
  (net 6 /b1)
  (net 7 /r2)
  (net 8 /g2)
  (net 9 /b2)
  (net 10 /r3)
  (net 11 /g3)
  (net 12 /b3)
  (net 13 /r4)
  (net 14 /g4)
  (net 15 /b4)
  (net 16 /r5)
  (net 17 /g5)
  (net 18 /b5)
  (net 19 /r6)
  (net 20 /g6)
  (net 21 /b6)
  (net 22 /r7)
  (net 23 /g7)
  (net 24 /b7)
  (net 25 /h7)
  (net 26 /h6)
  (net 27 /h5)
  (net 28 /h4)
  (net 29 /h3)
  (net 30 /h2)
  (net 31 /h1)
  (net 32 /h0)
  (net 33 /m7)
  (net 34 /m6)
  (net 35 /m5)
  (net 36 /m4)
  (net 37 /m3)
  (net 38 /m2)
  (net 39 /m1)
  (net 40 /m0)
  (net 41 /s7)
  (net 42 /s6)
  (net 43 /s5)
  (net 44 /s4)
  (net 45 /s3)
  (net 46 /s2)
  (net 47 /s1)
  (net 48 /s0)
  (net 49 /19b)
  (net 50 /19c)
  (net 51 /19d)
  (net 52 /a1)
  (net 53 "Net-(N1-Pad9)")
  (net 54 "Net-(N1-Pad8)")
  (net 55 "Net-(N1-Pad7)")
  (net 56 "Net-(N1-Pad6)")
  (net 57 "Net-(N1-Pad5)")
  (net 58 "Net-(N1-Pad4)")
  (net 59 "Net-(N1-Pad3)")
  (net 60 "Net-(N1-Pad2)")
  (net 61 "Net-(N1-Pad1)")
  (net 62 "Net-(N1-Pad0)")
  (net 63 /d1)
  (net 64 /a2)
  (net 65 "Net-(N2-Pad9)")
  (net 66 "Net-(N2-Pad8)")
  (net 67 "Net-(N2-Pad7)")
  (net 68 "Net-(N2-Pad6)")
  (net 69 "Net-(N2-Pad5)")
  (net 70 "Net-(N2-Pad4)")
  (net 71 "Net-(N2-Pad3)")
  (net 72 "Net-(N2-Pad2)")
  (net 73 "Net-(N2-Pad1)")
  (net 74 "Net-(N2-Pad0)")
  (net 75 /d2)
  (net 76 /a3)
  (net 77 "Net-(N3-Pad9)")
  (net 78 "Net-(N3-Pad8)")
  (net 79 "Net-(N3-Pad7)")
  (net 80 "Net-(N3-Pad6)")
  (net 81 "Net-(N3-Pad5)")
  (net 82 "Net-(N3-Pad4)")
  (net 83 "Net-(N3-Pad3)")
  (net 84 "Net-(N3-Pad2)")
  (net 85 "Net-(N3-Pad1)")
  (net 86 "Net-(N3-Pad0)")
  (net 87 /d3)
  (net 88 /a4)
  (net 89 "Net-(N4-Pad9)")
  (net 90 "Net-(N4-Pad8)")
  (net 91 "Net-(N4-Pad7)")
  (net 92 "Net-(N4-Pad6)")
  (net 93 "Net-(N4-Pad5)")
  (net 94 "Net-(N4-Pad4)")
  (net 95 "Net-(N4-Pad3)")
  (net 96 "Net-(N4-Pad2)")
  (net 97 "Net-(N4-Pad1)")
  (net 98 "Net-(N4-Pad0)")
  (net 99 /d4)
  (net 100 /a5)
  (net 101 "Net-(N5-Pad9)")
  (net 102 "Net-(N5-Pad8)")
  (net 103 "Net-(N5-Pad7)")
  (net 104 "Net-(N5-Pad6)")
  (net 105 "Net-(N5-Pad5)")
  (net 106 "Net-(N5-Pad4)")
  (net 107 "Net-(N5-Pad3)")
  (net 108 "Net-(N5-Pad2)")
  (net 109 "Net-(N5-Pad1)")
  (net 110 "Net-(N5-Pad0)")
  (net 111 /d5)
  (net 112 /a6)
  (net 113 "Net-(N6-Pad9)")
  (net 114 "Net-(N6-Pad8)")
  (net 115 "Net-(N6-Pad7)")
  (net 116 "Net-(N6-Pad6)")
  (net 117 "Net-(N6-Pad5)")
  (net 118 "Net-(N6-Pad4)")
  (net 119 "Net-(N6-Pad3)")
  (net 120 "Net-(N6-Pad2)")
  (net 121 "Net-(N6-Pad1)")
  (net 122 "Net-(N6-Pad0)")
  (net 123 /d6)
  (net 124 "Net-(N7-Pad14)")
  (net 125 "Net-(N7-Pad12)")
  (net 126 "Net-(N7-Pad11)")
  (net 127 "Net-(N7-Pad10)")
  (net 128 /a7)
  (net 129 "Net-(N7-Pad6)")
  (net 130 "Net-(N7-Pad5)")
  (net 131 "Net-(N7-Pad4)")
  (net 132 "Net-(N7-Pad2)")
  (net 133 "Net-(Q1-Pad2)")
  (net 134 "Net-(Q2-Pad2)")
  (net 135 "Net-(Q3-Pad2)")
  (net 136 "Net-(Q4-Pad2)")
  (net 137 "Net-(Q5-Pad2)")
  (net 138 "Net-(Q6-Pad2)")
  (net 139 "Net-(Q7-Pad2)")
  (net 140 "Net-(Q8-Pad2)")
  (net 141 "Net-(Q9-Pad2)")
  (net 142 "Net-(U7-Pad1)")
  (net 143 "Net-(U7-Pad2)")
  (net 144 +5V)
  (net 145 /r_ctrl)
  (net 146 /g_ctrl)
  (net 147 /b_ctrl)
  (net 148 /d6_ctrl)
  (net 149 /d5_ctrl)
  (net 150 /d4_ctrl)
  (net 151 /d3_ctrl)
  (net 152 /d2_ctrl)
  (net 153 /d1_ctrl)
  (net 154 /r_cath)
  (net 155 /g_cath)
  (net 156 /b_cath)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /19b)
    (add_net /19c)
    (add_net /19d)
    (add_net /b_cath)
    (add_net /b_ctrl)
    (add_net /d1_ctrl)
    (add_net /d2_ctrl)
    (add_net /d3_ctrl)
    (add_net /d4_ctrl)
    (add_net /d5_ctrl)
    (add_net /d6_ctrl)
    (add_net /g_cath)
    (add_net /g_ctrl)
    (add_net /h0)
    (add_net /h1)
    (add_net /h2)
    (add_net /h3)
    (add_net /h4)
    (add_net /h5)
    (add_net /h6)
    (add_net /h7)
    (add_net /m0)
    (add_net /m1)
    (add_net /m2)
    (add_net /m3)
    (add_net /m4)
    (add_net /m5)
    (add_net /m6)
    (add_net /m7)
    (add_net /r_cath)
    (add_net /r_ctrl)
    (add_net /s0)
    (add_net /s1)
    (add_net /s2)
    (add_net /s3)
    (add_net /s4)
    (add_net /s5)
    (add_net /s6)
    (add_net /s7)
    (add_net "Net-(U7-Pad1)")
    (add_net "Net-(U7-Pad2)")
  )
  (net_class HV ""
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /HV)
    (add_net /a1)
    (add_net /a2)
    (add_net /a3)
    (add_net /a4)
    (add_net /a5)
    (add_net /a6)
    (add_net /a7)
    (add_net /d1)
    (add_net /d2)
    (add_net /d3)
    (add_net /d4)
    (add_net /d5)
    (add_net /d6)
    (add_net "Net-(N1-Pad0)")
    (add_net "Net-(N1-Pad1)")
    (add_net "Net-(N1-Pad2)")
    (add_net "Net-(N1-Pad3)")
    (add_net "Net-(N1-Pad4)")
    (add_net "Net-(N1-Pad5)")
    (add_net "Net-(N1-Pad6)")
    (add_net "Net-(N1-Pad7)")
    (add_net "Net-(N1-Pad8)")
    (add_net "Net-(N1-Pad9)")
    (add_net "Net-(N2-Pad0)")
    (add_net "Net-(N2-Pad1)")
    (add_net "Net-(N2-Pad2)")
    (add_net "Net-(N2-Pad3)")
    (add_net "Net-(N2-Pad4)")
    (add_net "Net-(N2-Pad5)")
    (add_net "Net-(N2-Pad6)")
    (add_net "Net-(N2-Pad7)")
    (add_net "Net-(N2-Pad8)")
    (add_net "Net-(N2-Pad9)")
    (add_net "Net-(N3-Pad0)")
    (add_net "Net-(N3-Pad1)")
    (add_net "Net-(N3-Pad2)")
    (add_net "Net-(N3-Pad3)")
    (add_net "Net-(N3-Pad4)")
    (add_net "Net-(N3-Pad5)")
    (add_net "Net-(N3-Pad6)")
    (add_net "Net-(N3-Pad7)")
    (add_net "Net-(N3-Pad8)")
    (add_net "Net-(N3-Pad9)")
    (add_net "Net-(N4-Pad0)")
    (add_net "Net-(N4-Pad1)")
    (add_net "Net-(N4-Pad2)")
    (add_net "Net-(N4-Pad3)")
    (add_net "Net-(N4-Pad4)")
    (add_net "Net-(N4-Pad5)")
    (add_net "Net-(N4-Pad6)")
    (add_net "Net-(N4-Pad7)")
    (add_net "Net-(N4-Pad8)")
    (add_net "Net-(N4-Pad9)")
    (add_net "Net-(N5-Pad0)")
    (add_net "Net-(N5-Pad1)")
    (add_net "Net-(N5-Pad2)")
    (add_net "Net-(N5-Pad3)")
    (add_net "Net-(N5-Pad4)")
    (add_net "Net-(N5-Pad5)")
    (add_net "Net-(N5-Pad6)")
    (add_net "Net-(N5-Pad7)")
    (add_net "Net-(N5-Pad8)")
    (add_net "Net-(N5-Pad9)")
    (add_net "Net-(N6-Pad0)")
    (add_net "Net-(N6-Pad1)")
    (add_net "Net-(N6-Pad2)")
    (add_net "Net-(N6-Pad3)")
    (add_net "Net-(N6-Pad4)")
    (add_net "Net-(N6-Pad5)")
    (add_net "Net-(N6-Pad6)")
    (add_net "Net-(N6-Pad7)")
    (add_net "Net-(N6-Pad8)")
    (add_net "Net-(N6-Pad9)")
    (add_net "Net-(N7-Pad10)")
    (add_net "Net-(N7-Pad11)")
    (add_net "Net-(N7-Pad12)")
    (add_net "Net-(N7-Pad14)")
    (add_net "Net-(N7-Pad2)")
    (add_net "Net-(N7-Pad4)")
    (add_net "Net-(N7-Pad5)")
    (add_net "Net-(N7-Pad6)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q5-Pad2)")
    (add_net "Net-(Q6-Pad2)")
    (add_net "Net-(Q7-Pad2)")
    (add_net "Net-(Q8-Pad2)")
    (add_net "Net-(Q9-Pad2)")
  )
  (net_class LED ""
    (clearance 0.0508)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /b1)
    (add_net /b2)
    (add_net /b3)
    (add_net /b4)
    (add_net /b5)
    (add_net /b6)
    (add_net /b7)
    (add_net /g1)
    (add_net /g2)
    (add_net /g3)
    (add_net /g4)
    (add_net /g5)
    (add_net /g6)
    (add_net /g7)
    (add_net /r1)
    (add_net /r2)
    (add_net /r3)
    (add_net /r4)
    (add_net /r5)
    (add_net /r6)
    (add_net /r7)
  )
  (net_class LV ""
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net VCC)
  )
  (module logos:chinese-signature-5mm (layer F.Cu) (tedit 5D58F63A)
    (at 91.44 80.01)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 55.88 81.28)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 208.28 114.3)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 208.28 81.28)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 55.88 114.3)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 64.23 82.55 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF/300V (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 201.93 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /b7))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /b_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 181.53 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /b_cath))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /b6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 158.75 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /b5))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /b_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 135.81 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /b_cath))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /b4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 113.03 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /b_cath))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /b3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 90.17 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /b2))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /b_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 67.31 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /b_cath))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /b1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixies-us:nixies-us-IN-19 locked (layer F.Cu) (tedit 200000)
    (at 200.66 106.68)
    (attr virtual)
    (fp_text reference N7 (at 8.255 -0.3175 90) (layer F.SilkS))
    (fp_text value IN-19A (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 1.73228 3.7846) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 132 "Net-(N7-Pad2)"))
    (pad 3 thru_hole circle (at 3.22072 2.65176) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask))
    (pad 4 thru_hole circle (at 4.07162 0.98298) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 131 "Net-(N7-Pad4)"))
    (pad 5 thru_hole circle (at 4.11226 -0.88392) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 130 "Net-(N7-Pad5)"))
    (pad 6 thru_hole circle (at 3.33756 -2.58826) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 129 "Net-(N7-Pad6)"))
    (pad 7 thru_hole circle (at 1.90246 -3.78968) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask))
    (pad 8 thru_hole circle (at 0.08636 -4.24688) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 128 /a7))
    (pad 9 thru_hole circle (at -1.74498 -3.87096) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask))
    (pad 10 thru_hole circle (at -3.23342 -2.73558) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 127 "Net-(N7-Pad10)"))
    (pad 11 thru_hole circle (at -4.08178 -1.06934) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 126 "Net-(N7-Pad11)"))
    (pad 12 thru_hole circle (at -4.12496 0.8001) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 125 "Net-(N7-Pad12)"))
    (pad 13 thru_hole circle (at -3.35026 2.50444) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask))
    (pad 14 thru_hole circle (at -1.91262 3.70332) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 124 "Net-(N7-Pad14)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 201.93 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 /g7))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 155 /g_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 119.38 111.76)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value ZVN2110A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 134 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 155 /g_cath))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 165.1 114.935 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 147 /b_ctrl))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(Q3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 121.84 114.935)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 0 1.905) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 146 /g_ctrl))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 99.06 114.935)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 0 1.905) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 145 /r_ctrl))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 189.23 92.71 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R37 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 148 /d6_ctrl))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 141 "Net-(Q9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 166.37 92.71 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R36 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 149 /d5_ctrl))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 138 "Net-(Q6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 143.51 92.71 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R35 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 150 /d4_ctrl))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 140 "Net-(Q8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 120.65 93.345 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R34 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 151 /d3_ctrl))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 137 "Net-(Q5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 97.79 92.71 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R33 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 152 /d2_ctrl))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 139 "Net-(Q7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 74.93 92.79 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R32 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 153 /d1_ctrl))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 136 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 67.945 100.33 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R31 (at 0 1.7) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 52 /a1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 90.725 100.33 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at 0 1.7) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 64 /a2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 113.665 100.33 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at 0 1.7) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 76 /a3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 136.525 100.33 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at 0 1.7) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 88 /a4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 159.305 100.33 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 0 1.7) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 100 /a5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 182.245 100.33 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 0 1.7) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 112 /a6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 196.85 100.965)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 0 1.7) (layer B.SilkS))
    (fp_text value 30k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /HV))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 128 /a7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 148.59 84.455)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 200.66 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 139.065 115.57 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -1.27 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 144 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 60.96 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /r1))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 154 /r_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 181.61 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 /g6))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 155 /g_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 158.67 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.7) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /g5))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 155 /g_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 135.81 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.7) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /g4))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 155 /g_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 113.11 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 1.7) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 /g3))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 155 /g_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 90.17 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 /g2))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 155 /g_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 67.31 113.665 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /g1))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 155 /g_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 198.12 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 /r7))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 154 /r_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 175.26 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /r6))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 154 /r_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 152.4 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 /r5))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 154 /r_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 58E0A804)
    (at 129.54 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 /r4))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 154 /r_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 106.68 114.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 /r3))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 154 /r_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 83.82 114.855 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /r2))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 154 /r_cath))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 177.8 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 154.94 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 132.08 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 109.22 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 86.36 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 63.5 91.44)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 118.11 88.9 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74141 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(N3-Pad0)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(N3-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(N3-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /m5))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(N3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /m6))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(N3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /m4))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(N3-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /m7))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(N3-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(N3-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(N3-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(N3-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm locked (layer F.Cu) (tedit 59650533)
    (at 106.68 81.28 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 148 /d6_ctrl))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 149 /d5_ctrl))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 150 /d4_ctrl))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 151 /d3_ctrl))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 152 /d2_ctrl))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 153 /d1_ctrl))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /19b))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /19c))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /19d))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /s0))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /s1))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /s2))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /s3))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /s4))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /s5))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /s6))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /s7))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /m0))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /m1))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /m2))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /m3))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /m4))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /m5))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /m6))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /m7))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /h0))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /h1))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /h2))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /h3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /h4))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /h5))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /h6))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /h7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 209.55 88.9 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U7 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74141 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(N7-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(N7-Pad12)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(N7-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /19c))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(N7-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /19b))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(N7-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /19d))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(N7-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(N7-Pad11)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 "Net-(U7-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(N7-Pad14)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 "Net-(U7-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 186.69 88.9 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U6 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74141 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(N6-Pad0)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "Net-(N6-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(N6-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /s1))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(N6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /s2))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(N6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /s0))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(N6-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /s3))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(N6-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(N6-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(N6-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(N6-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 163.83 88.9 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U5 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74141 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(N5-Pad0)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(N5-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(N5-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /s5))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(N5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /s6))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(N5-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /s4))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(N5-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /s7))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(N5-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "Net-(N5-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(N5-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(N5-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 140.97 88.9 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74141 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "Net-(N4-Pad0)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(N4-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 "Net-(N4-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /m1))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(N4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /m2))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(N4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /m0))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(N4-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /m3))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(N4-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(N4-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(N4-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(N4-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 95.25 88.9 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74141 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(N2-Pad0)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(N2-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(N2-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /h1))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(N2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /h2))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(N2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /h0))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(N2-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /h3))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(N2-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(N2-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(N2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(N2-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 72.39 88.9 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74141 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(N1-Pad0)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(N1-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(N1-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /h5))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(N1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /h6))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(N1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /h4))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(N1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /h7))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(N1-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(N1-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(N1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(N1-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 191.77 101.6 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q9 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value MPSA42 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 /d6))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(Q9-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 146.05 101.6 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q8 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value MPSA42 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 /d4))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 140 "Net-(Q8-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 100.33 101.6 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q7 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value MPSA42 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /d2))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(Q7-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 168.91 101.6 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q6 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value MPSA42 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 /d5))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(Q6-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 123.19 101.6 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q5 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value MPSA42 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /d3))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 137 "Net-(Q5-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 77.47 101.6 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value MPSA42 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /d1))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 165.1 111.76)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value ZVN2110A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 135 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 156 /b_cath))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 96.52 111.76)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value ZVN2110A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 154 /r_cath))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 133 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module nixies-us:nixies-us-IN-8-2 locked (layer F.Cu) (tedit 200000)
    (at 177.8 106.68 180)
    (attr virtual)
    (fp_text reference N6 (at 9.04748 -0.79248 90) (layer F.SilkS))
    (fp_text value IN-8-2 (at 0 0) (layer F.SilkS) hide)
    (pad . thru_hole circle (at -2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 123 /d6))
    (pad 0 thru_hole circle (at -3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 122 "Net-(N6-Pad0)"))
    (pad 1 thru_hole circle (at 1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 121 "Net-(N6-Pad1)"))
    (pad 2 thru_hole circle (at 3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 120 "Net-(N6-Pad2)"))
    (pad 3 thru_hole circle (at 4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 119 "Net-(N6-Pad3)"))
    (pad 4 thru_hole circle (at 4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 118 "Net-(N6-Pad4)"))
    (pad 5 thru_hole circle (at 2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 117 "Net-(N6-Pad5)"))
    (pad 6 thru_hole circle (at 0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 116 "Net-(N6-Pad6)"))
    (pad 7 thru_hole circle (at -0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 115 "Net-(N6-Pad7)"))
    (pad 8 thru_hole circle (at -4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 114 "Net-(N6-Pad8)"))
    (pad 9 thru_hole circle (at -4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 113 "Net-(N6-Pad9)"))
    (pad A thru_hole circle (at -1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 112 /a6))
  )
  (module nixies-us:nixies-us-IN-8-2 locked (layer F.Cu) (tedit 200000)
    (at 154.94 106.68 180)
    (attr virtual)
    (fp_text reference N5 (at 9.04748 -0.79248 90) (layer F.SilkS))
    (fp_text value IN-8-2 (at 0 0) (layer F.SilkS) hide)
    (pad . thru_hole circle (at -2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 111 /d5))
    (pad 0 thru_hole circle (at -3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 110 "Net-(N5-Pad0)"))
    (pad 1 thru_hole circle (at 1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 109 "Net-(N5-Pad1)"))
    (pad 2 thru_hole circle (at 3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 108 "Net-(N5-Pad2)"))
    (pad 3 thru_hole circle (at 4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 107 "Net-(N5-Pad3)"))
    (pad 4 thru_hole circle (at 4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 106 "Net-(N5-Pad4)"))
    (pad 5 thru_hole circle (at 2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 105 "Net-(N5-Pad5)"))
    (pad 6 thru_hole circle (at 0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 104 "Net-(N5-Pad6)"))
    (pad 7 thru_hole circle (at -0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 103 "Net-(N5-Pad7)"))
    (pad 8 thru_hole circle (at -4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 102 "Net-(N5-Pad8)"))
    (pad 9 thru_hole circle (at -4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 101 "Net-(N5-Pad9)"))
    (pad A thru_hole circle (at -1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 100 /a5))
  )
  (module nixies-us:nixies-us-IN-8-2 locked (layer F.Cu) (tedit 200000)
    (at 132.08 106.68 180)
    (attr virtual)
    (fp_text reference N4 (at 9.04748 -0.79248 90) (layer F.SilkS))
    (fp_text value IN-8-2 (at 0 0) (layer F.SilkS) hide)
    (pad . thru_hole circle (at -2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 99 /d4))
    (pad 0 thru_hole circle (at -3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 98 "Net-(N4-Pad0)"))
    (pad 1 thru_hole circle (at 1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 97 "Net-(N4-Pad1)"))
    (pad 2 thru_hole circle (at 3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 96 "Net-(N4-Pad2)"))
    (pad 3 thru_hole circle (at 4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 95 "Net-(N4-Pad3)"))
    (pad 4 thru_hole circle (at 4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 94 "Net-(N4-Pad4)"))
    (pad 5 thru_hole circle (at 2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 93 "Net-(N4-Pad5)"))
    (pad 6 thru_hole circle (at 0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 92 "Net-(N4-Pad6)"))
    (pad 7 thru_hole circle (at -0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 91 "Net-(N4-Pad7)"))
    (pad 8 thru_hole circle (at -4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 90 "Net-(N4-Pad8)"))
    (pad 9 thru_hole circle (at -4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 89 "Net-(N4-Pad9)"))
    (pad A thru_hole circle (at -1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 88 /a4))
  )
  (module nixies-us:nixies-us-IN-8-2 locked (layer F.Cu) (tedit 200000)
    (at 109.22 106.68 180)
    (attr virtual)
    (fp_text reference N3 (at 9.04748 -0.79248 90) (layer F.SilkS))
    (fp_text value IN-8-2 (at 0 0) (layer F.SilkS) hide)
    (pad . thru_hole circle (at -2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 87 /d3))
    (pad 0 thru_hole circle (at -3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 86 "Net-(N3-Pad0)"))
    (pad 1 thru_hole circle (at 1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 85 "Net-(N3-Pad1)"))
    (pad 2 thru_hole circle (at 3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 84 "Net-(N3-Pad2)"))
    (pad 3 thru_hole circle (at 4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 83 "Net-(N3-Pad3)"))
    (pad 4 thru_hole circle (at 4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 82 "Net-(N3-Pad4)"))
    (pad 5 thru_hole circle (at 2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 81 "Net-(N3-Pad5)"))
    (pad 6 thru_hole circle (at 0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 80 "Net-(N3-Pad6)"))
    (pad 7 thru_hole circle (at -0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 79 "Net-(N3-Pad7)"))
    (pad 8 thru_hole circle (at -4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 78 "Net-(N3-Pad8)"))
    (pad 9 thru_hole circle (at -4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 77 "Net-(N3-Pad9)"))
    (pad A thru_hole circle (at -1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 76 /a3))
  )
  (module nixies-us:nixies-us-IN-8-2 locked (layer F.Cu) (tedit 200000)
    (at 86.36 106.68 180)
    (attr virtual)
    (fp_text reference N2 (at 9.04748 -0.79248 90) (layer F.SilkS))
    (fp_text value IN-8-2 (at 0 0) (layer F.SilkS) hide)
    (pad . thru_hole circle (at -2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 75 /d2))
    (pad 0 thru_hole circle (at -3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 74 "Net-(N2-Pad0)"))
    (pad 1 thru_hole circle (at 1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 73 "Net-(N2-Pad1)"))
    (pad 2 thru_hole circle (at 3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 72 "Net-(N2-Pad2)"))
    (pad 3 thru_hole circle (at 4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 71 "Net-(N2-Pad3)"))
    (pad 4 thru_hole circle (at 4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 70 "Net-(N2-Pad4)"))
    (pad 5 thru_hole circle (at 2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 69 "Net-(N2-Pad5)"))
    (pad 6 thru_hole circle (at 0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 68 "Net-(N2-Pad6)"))
    (pad 7 thru_hole circle (at -0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 67 "Net-(N2-Pad7)"))
    (pad 8 thru_hole circle (at -4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 66 "Net-(N2-Pad8)"))
    (pad 9 thru_hole circle (at -4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 65 "Net-(N2-Pad9)"))
    (pad A thru_hole circle (at -1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 64 /a2))
  )
  (module nixies-us:nixies-us-IN-8-2 locked (layer F.Cu) (tedit 200000)
    (at 63.5 106.68 180)
    (attr virtual)
    (fp_text reference N1 (at 9.04748 -0.79248 90) (layer F.SilkS))
    (fp_text value IN-8-2 (at 0 0) (layer F.SilkS) hide)
    (pad . thru_hole circle (at -2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 63 /d1))
    (pad 0 thru_hole circle (at -3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 62 "Net-(N1-Pad0)"))
    (pad 1 thru_hole circle (at 1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 61 "Net-(N1-Pad1)"))
    (pad 2 thru_hole circle (at 3.74904 2.74828 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 60 "Net-(N1-Pad2)"))
    (pad 3 thru_hole circle (at 4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 59 "Net-(N1-Pad3)"))
    (pad 4 thru_hole circle (at 4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 58 "Net-(N1-Pad4)"))
    (pad 5 thru_hole circle (at 2.99974 -3.49758 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 57 "Net-(N1-Pad5)"))
    (pad 6 thru_hole circle (at 0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 56 "Net-(N1-Pad6)"))
    (pad 7 thru_hole circle (at -0.99822 -4.49834 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 55 "Net-(N1-Pad7)"))
    (pad 8 thru_hole circle (at -4.24942 -1.4986 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 54 "Net-(N1-Pad8)"))
    (pad 9 thru_hole circle (at -4.49834 0.7493 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 53 "Net-(N1-Pad9)"))
    (pad A thru_hole circle (at -1.99898 3.99796 180) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Paste *.Mask)
      (net 52 /a1))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm locked (layer F.Cu) (tedit 59650532)
    (at 66.04 78.74 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /HV))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /HV))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /HV))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 147.32 114.3 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 145 /r_ctrl))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 146 /g_ctrl))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 147 /b_ctrl))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 locked (layer F.Cu) (tedit 587A3A7B)
    (at 198.755 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D7 (at 1.905 3.81) (layer F.SilkS))
    (fp_text value LED_RAGB (at 1.905 3.96) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /b7))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 /g7))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 /r7))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 locked (layer F.Cu) (tedit 587A3A7B)
    (at 175.895 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D6 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value LED_RAGB (at 1.905 3.96) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 /b6))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 /g6))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 /r6))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 locked (layer F.Cu) (tedit 587A3A7B)
    (at 153.035 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D5 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value LED_RAGB (at 1.905 3.96) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 /b5))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 /g5))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 /r5))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 locked (layer F.Cu) (tedit 587A3A7B)
    (at 130.175 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D4 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value LED_RAGB (at 1.905 3.96) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 /b4))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 /g4))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 /r4))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 locked (layer F.Cu) (tedit 587A3A7B)
    (at 107.315 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D3 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value LED_RAGB (at 1.905 3.96) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 /b3))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 /g3))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /r3))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 locked (layer F.Cu) (tedit 587A3A7B)
    (at 84.455 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D2 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value LED_RAGB (at 1.905 3.96) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /b2))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /g2))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /r2))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 locked (layer F.Cu) (tedit 587A3A7B)
    (at 61.595 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D1 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value LED_RAGB (at 1.905 3.96) (layer F.Fab))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /b1))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /g1))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 144 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /r1))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "DANGER!\nHigh voltages (<250Vdc)\nHg vapor in tubes" (at 184.15 80.01) (layer F.SilkS))
  (gr_text "Nixie Clock Top PCB, rev. 1\nTony Zhang, 2019 08 17\n" (at 160.02 80.01) (layer F.SilkS))
  (gr_line (start 213.36 76.2) (end 50.8 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.36 119.38) (end 213.36 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 119.38) (end 213.36 119.38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 76.2) (end 50.8 119.38) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 76.2) (xy 50.8 119.38) (xy 213.36 119.38) (xy 213.36 76.2)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.36 76.2) (xy 213.36 119.38) (xy 50.8 119.38) (xy 50.8 76.2)
      )
    )
  )
  (zone (net 144) (net_name +5V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 97.79) (xy 50.8 119.38) (xy 213.36 119.38) (xy 213.36 97.79)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 76.2) (xy 50.8 92.71) (xy 213.36 92.71) (xy 213.36 76.2)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 76.2) (xy 50.8 119.38) (xy 213.36 119.38) (xy 213.36 76.2)
      )
    )
  )
)
