<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="17.78" y1="52.07" x2="43.18" y2="52.07" width="0" layer="20"/>
<wire x1="43.18" y1="52.07" x2="43.18" y2="31.75" width="0" layer="20"/>
<wire x1="43.18" y1="31.75" x2="17.78" y2="31.75" width="0" layer="20"/>
<wire x1="17.78" y1="31.75" x2="17.78" y2="52.07" width="0" layer="20"/>
<text>VIN</text>
<text>EN</text>
<text>SCL</text>
<text>SDA</text>
<text>INT1</text>
<text>INT2</text>
<text>GND</text>
<text>ADXL345 BOB</text>
<text>16Feb18</text>
<text>v3</text>
</plain>
<libraries>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="ADXL345">
<description>Analog Devices ADXL345 Digital Accelerometer</description>
</package>
<package name="SOT-23(OT)5_LEAD">
<description>5-Lead Plastic Small Outline Transistor (OT) [SOT-23]
From "Microchip Packaging Specification" p 58</description>
</package>
<package name="MSOP_8_LEAD">
<description>Based off of Microchip packaging document. with of pads geometric mean of largest and smallest. Pad extends beyond largest width by 0.03, while centered on 2.2mm&lt;br&gt;
70% cream coverage</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="OST">
<packages>
<package name="OSTVN08">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="ERIC" package="ADXL345" value="ADXL345"/>
<element name="MCP1711T-25I/OTCT-ND_1" library="ERIC" package="SOT-23(OT)5_LEAD" value="MCP1802"/>
<element name="CVDD" library="SparkFun" package="0805" value="100n"/>
<element name="C3" library="SparkFun" package="0805" value="10u"/>
<element name="C4" library="SparkFun" package="0805" value="100n"/>
<element name="C5" library="SparkFun" package="0805" value="100n"/>
<element name="JP1" library="OST" package="OSTVN08" value="M08"/>
<element name="C1" library="SparkFun" package="0805" value="100n"/>
<element name="C2" library="SparkFun" package="0805" value="100n"/>
<element name="U$3" library="ERIC" package="MSOP_8_LEAD" value="PCA9617A"/>
<element name="U$1" library="ERIC" package="MSOP_8_LEAD" value="PCA9617A"/>
<element name="C6" library="SparkFun" package="0805" value="100n"/>
<element name="C7" library="SparkFun" package="0805" value="100n"/>
<element name="U$4" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="U$5" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="U$6" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="U$7" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$2" pad="5"/>
<contactref element="MCP1711T-25I/OTCT-ND_1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="CVDD" pad="2"/>
<contactref element="U$2" pad="12"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="7"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="2V5">
<contactref element="MCP1711T-25I/OTCT-ND_1" pad="5"/>
<contactref element="U$2" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U$2" pad="7"/>
<contactref element="U$2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$3" pad="8"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="8"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="9"/>
<contactref element="U$3" pad="7"/>
</signal>
<signal name="VIN">
<contactref element="MCP1711T-25I/OTCT-ND_1" pad="1"/>
<contactref element="MCP1711T-25I/OTCT-ND_1" pad="3"/>
<contactref element="CVDD" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="13"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="14"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="EN">
<contactref element="U$3" pad="5"/>
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
