(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 25)
    (no_connects 0)
    (area 131.889499 91.249499 139.890501 114.490501)
    (thickness 1.6)
    (drawings 45)
    (tracks 259)
    (zones 0)
    (modules 6)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.381)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.127)
    (pcb_text_size 0.508 0.508)
    (mod_edge_width 0.1524)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.127)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(uC1-Pad25)")
  (net 2 /GND)
  (net 3 /+3.3V)
  (net 4 /P0.7)
  (net 5 /P0.6)
  (net 6 /P0.5)
  (net 7 /P0.4)
  (net 8 /P0.3)
  (net 9 /P0.2)
  (net 10 /P0.1)
  (net 11 /P0.0)
  (net 12 /C2CK)
  (net 13 /C2D)
  (net 14 /P1.6)
  (net 15 /P1.5)
  (net 16 /P1.4)
  (net 17 /P1.3)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3.3V)
    (add_net /C2CK)
    (add_net /C2D)
    (add_net /GND)
    (add_net /P0.0)
    (add_net /P0.1)
    (add_net /P0.2)
    (add_net /P0.3)
    (add_net /P0.4)
    (add_net /P0.5)
    (add_net /P0.6)
    (add_net /P0.7)
    (add_net /P1.3)
    (add_net /P1.4)
    (add_net /P1.5)
    (add_net /P1.6)
    (add_net "Net-(uC1-Pad25)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3302)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 598DF66F)
    (at 137.033 111.125 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference "" (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value "" (at 0 0.254 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /+3.3V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 598DF63D)
    (at 135.001 111.125 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference "" (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value "" (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /+3.3V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 598DF67F)
    (at 135.763 107.569 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference "" (at 0 1.85 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.254 360) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 /C2CK))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /+3.3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 598DE62F)
    (at 135.9916 102.87 135)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference "" (at 0 -3.375 135) (layer F.SilkS))
    (fp_text value "" (at 0 3.375 135) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.95 -0.75 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -1.95 -0.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /+3.3V))
    (pad 4 smd rect (at -1.95 0.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -1.95 0.75 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.95 1.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /C2CK))
    (pad 7 smd rect (at -1.25 1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /C2D))
    (pad 8 smd rect (at -0.75 1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -0.25 1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 0.25 1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /P1.6))
    (pad 11 smd rect (at 0.75 1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /P1.5))
    (pad 12 smd rect (at 1.25 1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /P1.4))
    (pad 13 smd rect (at 1.95 1.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /P1.3))
    (pad 14 smd rect (at 1.95 0.75 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.95 0.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 1.95 -0.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 1.95 -0.75 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /P0.7))
    (pad 18 smd rect (at 1.95 -1.25 135) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /P0.6))
    (pad 19 smd rect (at 1.25 -1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /P0.5))
    (pad 20 smd rect (at 0.75 -1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /P0.4))
    (pad 21 smd rect (at 0.25 -1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /P0.3))
    (pad 22 smd rect (at -0.25 -1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /P0.2))
    (pad 23 smd rect (at -0.75 -1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /P0.1))
    (pad 24 smd rect (at -1.25 -1.95 225) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /P0.0))
    (pad 25 smd rect (at 0.65 0.65 135) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(uC1-Pad25)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65 135) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(uC1-Pad25)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65 135) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(uC1-Pad25)") (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65 135) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(uC1-Pad25)") (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Footprint:Pin_Header_Straight_1x08_Pitch2.54mmEDITED" (layer F.Cu) (tedit 598DE80B)
    (at 139.7 111.76 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value "" (at 0 20.11 180) (layer F.Fab))
    (fp_text user %R (at 2.54 9.144 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /+3.3V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /C2CK))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /C2D))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /P1.6))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /P1.5))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /P1.4))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /P1.3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 -0.015))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Custom Footprint:Pin_Header_Straight_1x08_Pitch2.54mmEDITED" (layer F.Cu) (tedit 598DE80B)
    (at 132.08 93.98)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference "" (at 0 -2.33) (layer F.SilkS))
    (fp_text value "" (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 2.54 9.144 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /P0.7))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0.6))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P0.5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P0.4))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /P0.3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /P0.2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /P0.1))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /P0.0))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 -0.015))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text 1uF (at 137.033 110.998 45) (layer F.SilkS))
  (gr_text 0.1uF (at 135.001 111.125 45) (layer F.SilkS))
  (gr_text < (at 137.033 105.664 315) (layer F.SilkS))
  (gr_text P0.4 (at 133.35 101.6 90) (layer B.SilkS))
  (gr_text P0.3 (at 133.35 104.394 90) (layer B.SilkS))
  (gr_text EFM8SB2-24 (at 135.382 96.012 270) (layer B.SilkS))
  (gr_text GND (at 138.43 111.76 270) (layer B.SilkS))
  (gr_text P0.0 (at 133.35 111.506 270) (layer B.SilkS))
  (gr_text P0.1 (at 133.35 109.22 270) (layer B.SilkS))
  (gr_text P0.2 (at 133.35 106.68 270) (layer B.SilkS))
  (gr_text P0.5 (at 133.35 99.06 270) (layer B.SilkS))
  (gr_text KnightTech (at 136.906 96.266 270) (layer B.SilkS))
  (gr_text P0.6 (at 133.35 96.52 270) (layer B.SilkS))
  (gr_text P0.7 (at 133.35 93.98 270) (layer B.SilkS))
  (gr_text +3.3V (at 138.43 109.22 270) (layer B.SilkS))
  (gr_text C2CK (at 137.922 106.68 45) (layer B.SilkS))
  (gr_text C2D (at 138.43 104.14 270) (layer B.SilkS))
  (gr_text P1.6 (at 138.43 101.6 270) (layer B.SilkS))
  (gr_text P1.5 (at 138.43 99.06 270) (layer B.SilkS))
  (gr_text P1.4 (at 138.43 96.52 270) (layer B.SilkS))
  (gr_text P1.3 (at 138.43 93.98 270) (layer B.SilkS))
  (gr_text P1.3 (at 138.43 93.98 90) (layer F.SilkS))
  (gr_text P1.4 (at 138.43 96.52 90) (layer F.SilkS))
  (gr_text P1.5 (at 138.43 98.552 90) (layer F.SilkS))
  (gr_text P1.6 (at 138.43 100.584 90) (layer F.SilkS))
  (gr_text C2D (at 138.43 104.902 90) (layer F.SilkS))
  (gr_text C2CK (at 137.922 106.68 45) (layer F.SilkS))
  (gr_text +3.3V (at 138.43 109.22 90) (layer F.SilkS))
  (gr_text P0.7 (at 133.35 93.98 90) (layer F.SilkS))
  (gr_text P0.6 (at 133.35 96.52 90) (layer F.SilkS))
  (gr_text KnightTech (at 135.382 96.266 90) (layer F.SilkS))
  (gr_text P0.5 (at 133.35 99.06 90) (layer F.SilkS))
  (gr_text P0.2 (at 133.35 106.68 90) (layer F.SilkS))
  (gr_text P0.1 (at 133.35 109.22 90) (layer F.SilkS))
  (gr_text P0.0 (at 133.35 111.506 90) (layer F.SilkS))
  (gr_text GND (at 138.43 111.76 90) (layer F.SilkS))
  (gr_line (start 133.096 91.44) (end 132.08 92.456) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 138.684 91.44) (end 133.096 91.44) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 139.7 92.456) (end 138.684 91.44) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 139.7 113.284) (end 139.7 92.456) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 138.684 114.3) (end 139.7 113.284) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 133.096 114.3) (end 138.684 114.3) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 132.08 113.284) (end 133.096 114.3) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 132.08 92.456) (end 132.08 113.284) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_text EFM8SB2-24 (at 136.906 96.012 90) (layer F.SilkS))
  (zone (net 1) (net_name "Net-(uC1-Pad25)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.4516 92.8878) (xy 138.3792 92.8878) (xy 138.3792 105.537) (xy 133.4262 105.5116) (xy 133.4262 92.8878)
      )
    )
  )
  (zone (net 2) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.604 106.172) (xy 138.684 106.172) (xy 138.684 110.236) (xy 139.192 110.236) (xy 139.192 112.776)
        (xy 133.604 112.776)
      )
    )
  )
  (zone (net 3) (net_name /+3.3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.684 108.204) (xy 139.192 108.204) (xy 139.192 110.236) (xy 138.684 110.236) (xy 138.684 112.776)
        (xy 133.604 112.776) (xy 133.604 106.172) (xy 138.684 106.172)
      )
    )
  )
)
