(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 20)
    (no_connects 0)
    (area 78.663676 58.170559 178.510001 123.265001)
    (thickness 1.6)
    (drawings 46)
    (tracks 147)
    (zones 0)
    (modules 11)
    (nets 34)
  )
  (page A4)
  (title_block
    (company "This design uses a KiCad DIP template created by Jenner at Wickerbox Electronics")
    (comment 1 "Released under the CERN Open Hardware License v1.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 0.762 0.762)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.1524)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory test-board-gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /D15)
  (net 3 /D0)
  (net 4 /D1)
  (net 5 /D2)
  (net 6 /D3)
  (net 7 /D4)
  (net 8 /D5)
  (net 9 /D6)
  (net 10 /D7)
  (net 11 /D8)
  (net 12 OLED_DATA)
  (net 13 OLED_CLK)
  (net 14 OLED_DC)
  (net 15 OLED_CS)
  (net 16 "/D17(VIN)")
  (net 17 VIN)
  (net 18 /PROG)
  (net 19 /DAC)
  (net 20 OLED_RST)
  (net 21 /D16)
  (net 22 BMP280_SDI)
  (net 23 /D17)
  (net 24 /D22)
  (net 25 /D21)
  (net 26 /D20)
  (net 27 BMP280_SCK)
  (net 28 /D23)
  (net 29 "Net-(J1-Pad14)")
  (net 30 "Net-(J6-Pad2)")
  (net 31 "Net-(J6-Pad5)")
  (net 32 "Net-(J6-Pad7)")
  (net 33 "Net-(J7-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /D0)
    (add_net /D1)
    (add_net /D15)
    (add_net /D16)
    (add_net /D17)
    (add_net "/D17(VIN)")
    (add_net /D2)
    (add_net /D20)
    (add_net /D21)
    (add_net /D22)
    (add_net /D23)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /DAC)
    (add_net /PROG)
    (add_net BMP280_SCK)
    (add_net BMP280_SDI)
    (add_net GND)
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J6-Pad7)")
    (add_net "Net-(J7-Pad3)")
    (add_net OLED_CLK)
    (add_net OLED_CS)
    (add_net OLED_DATA)
    (add_net OLED_DC)
    (add_net OLED_RST)
    (add_net VIN)
  )
  (module TEENSY-LC (layer F.Cu) (tedit 578EAE47)
    (at 105.41 82.804)
    (fp_text reference J1 (at -7.62 20.066 270) (layer F.SilkS))
    (fp_text value TEENSY-LC (at -2.54 20.32 180) (layer F.Fab))
    (fp_text user "TEENSY LC" (at -2.54 -6.604 180) (layer B.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /D0))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D1))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D2))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D3))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D4))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D5))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D6))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D7))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D8))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 OLED_DATA))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 OLED_CLK))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 OLED_DC))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 OLED_CS))
    (pad 17A thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "/D17(VIN)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 VIN))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /PROG))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /DAC))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 OLED_RST))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D16))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 VIN))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 BMP280_SDI))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /D17))
    (pad G3 thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /D22))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 VIN))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D21))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /D20))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 BMP280_SCK))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D23))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /D15))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578EA6B6)
    (at 86.487 71.882)
    (fp_text reference CAP15 (at 0 -0.508) (layer F.SilkS))
    (fp_text value CAP15 (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 2 /D15) (clearance 0.508))
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EAD86)
    (at 122.174 70.358)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CAP23 (at 5.461 -0.254 90) (layer F.SilkS))
    (fp_text value CAP23 (at 0 -3.1) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 9 5) (layers F.Cu F.Paste F.Mask)
      (net 28 /D23))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EA7DD)
    (at 110.617 63.881)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CAP22 (at -0.127 -2.286) (layer F.SilkS))
    (fp_text value CAP22 (at 0 -3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 8 6) (layers F.Cu)
      (net 24 /D22))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EAD76)
    (at 122.301 98.933 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CAP17 (at 0 5.461 270) (layer F.SilkS))
    (fp_text value CAP17 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 5 9) (layers F.Cu F.Paste F.Mask)
      (net 23 /D17))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EA91A)
    (at 97.663 63.881 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CAP16 (at -2.286 0.254 360) (layer F.SilkS))
    (fp_text value CAP16 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 smd trapezoid (at 0 0 270) (size 6 5) (rect_delta 4 0 ) (layers F.Cu)
      (net 21 /D16))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 578EA606)
    (at 86.995 80.01)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference BMP280 (at -2.794 7.239 270) (layer F.SilkS))
    (fp_text value I2C_BMP280 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 BMP280_SCK))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 BMP280_SDI))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J6-Pad7)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 578EA602)
    (at 123.698 75.946)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "SPI OLED" (at 2.921 9.398 90) (layer F.SilkS))
    (fp_text value SPI_OLED_128x64 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 VIN))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 OLED_CS))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 OLED_RST))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 OLED_DC))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 OLED_CLK))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 OLED_DATA))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 115.316 103.378 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module teensy-big-oled:oshpark-silk-25dpi (layer B.Cu) (tedit 0)
    (at 96.774 107.315)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module teensy-big-oled:osh-park-logo-300dpi-normal-silk (layer F.Cu) (tedit 0)
    (at 84.074 104.648 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text "DREW\nFUSTINI" (at 115.824 83.185 270) (layer B.Mask))
  (gr_text "DREW\nFUSTINI" (at 115.824 83.185 270) (layer B.Cu))
  (gr_text drew@oshpark.com (at 105.156 59.563) (layer F.Cu))
  (gr_text drew@oshpark.com (at 105.156 59.563) (layer F.Mask))
  (gr_text "DREW\nFUSTINI" (at 115.824 84.709 270) (layer F.Mask))
  (gr_text "DREW\nFUSTINI" (at 115.824 84.709 270) (layer F.Cu))
  (gr_text "DREW FUSTINI" (at 102.743 108.458 180) (layer F.Mask))
  (gr_text "DREW FUSTINI" (at 102.743 108.458 180) (layer F.Cu))
  (gr_circle (center 122.555 105.156) (end 124.333 107.188) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 123.19 63.246) (end 124.968 65.278) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 83.439 63.373) (end 85.217 65.405) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 83.947 104.521) (end 85.725 106.553) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.778 101.219) (end 128.778 101.854) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.778 64.897) (end 128.778 65.659) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 101.092) (end 78.74 104.013) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.328 109.982) (end 85.471 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.364 109.982) (end 120.65 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.507 109.982) (end 84.836 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 84.836 103.886) (end 84.709 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 120.142 101.346) (end 128.778 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 101.219) (end 78.74 100.457) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 63.627) (end 78.74 101.219) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.778 65.405) (end 128.778 101.473) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.598 58.293) (end 120.523 58.293) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.158 65.913) (end 120.396 58.293) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 84.836 64.389) (end 78.74 63.627) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "VIN\n\nGND\n\n3.3V\n\n23\n\n22\n\n21\n\n20\n\n19\n\n18\n\n17\n\n16\n\n15\n\n14\n\n13\n" (at 112.268 89.154) (layer F.Fab))
  (gr_text "GND\n\n0\n\n1\n\n2\n\n3\n\n4\n\n5\n\n6\n\n7\n\n8\n\n9\n\n10\n\n11\n\n12" (at 93.218 89.154) (layer F.Fab))
  (gr_text "17(VIN)\n\n3.3V\n\nGND\n\nPROG\n\nDAC" (at 102.87 107.95 90) (layer F.Fab))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.968 60.198) (xy 127.381 62.992) (xy 127.889 67.056) (xy 127.635 102.997) (xy 125.857 106.68)
        (xy 123.698 108.585) (xy 121.158 108.966) (xy 118.618 108.966) (xy 84.328 108.966) (xy 81.788 108.077)
        (xy 80.899 106.68) (xy 79.883 105.41) (xy 79.502 62.484) (xy 81.026 60.579) (xy 84.328 59.055)
        (xy 121.92 58.928) (xy 124.968 60.198)
      )
    )
  )
)
