(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 185)
    (zones 0)
    (modules 29)
    (nets 33)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 INT)
  (net 4 MOSI)
  (net 5 CS)
  (net 6 SCK)
  (net 7 RESET)
  (net 8 RTS)
  (net 9 LOUT)
  (net 10 GBUF)
  (net 11 ROUT)
  (net 12 CANH)
  (net 13 CANL)
  (net 14 TOSC2)
  (net 15 TOSC1)
  (net 16 OSC1)
  (net 17 OSC2)
  (net 18 RX0BF)
  (net 19 RX1BF)
  (net 20 N$35)
  (net 21 TX)
  (net 22 RX)
  (net 23 TXCAN)
  (net 24 RXCAN)
  (net 25 MISO)
  (net 26 STDBY)
  (net 27 +12)
  (net 28 N$13)
  (net 29 XRESET)
  (net 30 N$15)
  (net 31 N$17)
  (net 32 N$18)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12)
    (add_net +5V)
    (add_net CANH)
    (add_net CANL)
    (add_net CS)
    (add_net GBUF)
    (add_net GND)
    (add_net INT)
    (add_net LOUT)
    (add_net MISO)
    (add_net MOSI)
    (add_net N$13)
    (add_net N$15)
    (add_net N$17)
    (add_net N$18)
    (add_net N$35)
    (add_net OSC1)
    (add_net OSC2)
    (add_net RESET)
    (add_net ROUT)
    (add_net RTS)
    (add_net RX)
    (add_net RX0BF)
    (add_net RX1BF)
    (add_net RXCAN)
    (add_net SCK)
    (add_net STDBY)
    (add_net TOSC1)
    (add_net TOSC2)
    (add_net TX)
    (add_net TXCAN)
    (add_net XRESET)
  )
  (module LED_THT:LED_D5.0mm (layer Top) (tedit 5DDA27A0)
    (at 137.668 101.6)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference AUDIO (at 4.064 5.08) (layer F.SilkS))
    (fp_text value 5V (at 3.2004 1.8034) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 XRESET))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 N$15))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DDBFB7C)
    (at 137.668 94.3 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at -0.696 1.524) (layer F.SilkS))
    (fp_text value 1K (at 3.876 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 N$15))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 164.2 110.082173 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 2.91 1.878173) (layer F.SilkS))
    (fp_text value 470nF (at 5.196 3.402173) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 +12))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 166.37 124.42 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 1.23 -3.81) (layer F.SilkS))
    (fp_text value 0.1uF (at -2.58 -4.826) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 158.75 134.62)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.27 2.794) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 RTS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 RESET))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer Top) (tedit 5DDA272A)
    (at 169.3 102.87)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at -4.2 0.715827) (layer F.SilkS))
    (fp_text value 1uF (at -5.216 -0.808173) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 +12))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp (layer Top) (tedit 5DDA26F2)
    (at 164.188512 115.182173 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 3.660512 -3.689827) (layer F.SilkS))
    (fp_text value 1N4007-01 (at -3.959488 -4.197827 180) (layer F.Fab) hide)
    (fp_text user K (at -2.1 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer Top) (tedit 5AE5139B)
    (at 154.94 124.46 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 6.35 -0.604488 90) (layer F.SilkS))
    (fp_text value 10K (at 2.54 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 RESET))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 136.078112 119.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -0.508 1.589888) (layer F.SilkS))
    (fp_text value 1K (at 4.064 -0.950112) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 RX0BF))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 N$13))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 134.112 101.6 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -3.048 -1.034712) (layer F.SilkS))
    (fp_text value 10K (at 3.556 -1.524) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 N$35))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 131 131.5 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -3.12 -0.952) (layer F.SilkS))
    (fp_text value 10K (at -4.644 -1.46) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 RX1BF))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 STDBY))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 148.8 85.344)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at -1.48 -1.524) (layer F.SilkS))
    (fp_text value 1K (at -4.02 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 N$17))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 LOUT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 165.4 85.344 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -1.224 1.524) (layer F.SilkS))
    (fp_text value 1K (at -4.272 -0.508) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 N$18))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ROUT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer Top) (tedit 5DDA27A0)
    (at 136 124.46)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference CAN (at 3.192 5.08) (layer F.SilkS))
    (fp_text value 5V (at 3.2004 1.8034) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 N$13))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Resonator-3Pin_W10.0mm_H5.0mm (layer Top) (tedit 5A0FD1B2)
    (at 155.463512 115.2 90)
    (descr "Ceramic Resomator/Filter 10.0x5.0mm^2 RedFrequency MG/MT/MX series, http://www.red-frequency.com/download/datenblatt/redfrequency-datenblatt-ir-zta.pdf, length*width=10.0x5.0mm^2 package, package length=10.0mm, package width=5.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (fp_text reference Y1 (at 2.17 2.016488 90) (layer F.SilkS))
    (fp_text value 16MHz (at 2.17 -1.793512 90) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 5 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 TOSC2))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 TOSC1))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Resonator-3Pin_W10.0mm_H5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Resonator-3Pin_W10.0mm_H5.0mm (layer Top) (tedit 5A0FD1B2)
    (at 128.113312 122.5 270)
    (descr "Ceramic Resomator/Filter 10.0x5.0mm^2 RedFrequency MG/MT/MX series, http://www.red-frequency.com/download/datenblatt/redfrequency-datenblatt-ir-zta.pdf, length*width=10.0x5.0mm^2 package, package length=10.0mm, package width=5.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (fp_text reference Y2 (at 1.452 -1.426688 270) (layer F.SilkS))
    (fp_text value 16MHz (at -0.58 2.129312 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 OSC2))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 OSC1))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Resonator-3Pin_W10.0mm_H5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer Top) (tedit 5DDA2619)
    (at 168.91 110 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference IC4 (at 4.391 -1.76 270) (layer F.SilkS) hide)
    (fp_text value 7805 (at 4.3 -5.08 90) (layer F.SilkS))
    (fp_text user - (at -0.635 3.81 270) (layer F.Fab))
    (fp_text user I (at -3.175 3.81 270) (layer F.Fab))
    (fp_text user O (at 1.905 3.81 270) (layer F.Fab))
    (fp_text user %R (at -0.78 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 +12))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_LongPads (layer Top) (tedit 5DD8C639)
    (at 123.19 95.25 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference IC2 (at 1.778 1.778) (layer F.SilkS) hide)
    (fp_text value HVD251 (at 3.302 0.762) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 TXCAN))
    (pad "" np_thru_hole circle (at 7.62 7.62 90) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 CANL))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 CANH))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 RXCAN))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 STDBY))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-18_W7.62mm_LongPads (layer Top) (tedit 5DD8C5A8)
    (at 123.19 99.06)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference IC1 (at 1.778 0.508 -180) (layer F.SilkS) hide)
    (fp_text value MCP2515 (at 4.318 3.048 90) (layer F.SilkS))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 N$35))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 OSC1))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 CS))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 OSC2))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 MISO))
    (pad "" np_thru_hole circle (at 0 12.7) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 MOSI))
    (pad "" np_thru_hole circle (at 0 10.16) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 SCK))
    (pad "" np_thru_hole circle (at 0 7.62) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 INT))
    (pad "" np_thru_hole circle (at 0 5.08) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 RX0BF))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 RXCAN))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 RX1BF))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 TXCAN))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer Top) (tedit 5DDDA5D6)
    (at 170.088512 121.92)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference JP1 (at 1.432512 3.110173) (layer F.SilkS) hide)
    (fp_text value FTDI (at -1.940512 9.144 90) (layer F.SilkS) hide)
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 RTS))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 TX))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W7.62mm_LongPads (layer Top) (tedit 5DDB46CF)
    (at 151.13 134.62 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference IC3 (at -19.2024 2.54 90) (layer F.SilkS) hide)
    (fp_text value MEGA328 (at 3.302 14.224 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 RESET))
    (pad 15 thru_hole oval (at 7.62 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 XRESET))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 TX))
    (pad 16 thru_hole oval (at 7.62 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 CS))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 RX))
    (pad 17 thru_hole oval (at 7.62 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 MOSI))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 INT))
    (pad 18 thru_hole oval (at 7.62 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 MISO))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 7.62 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 SCK))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 7.62 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad "" np_thru_hole circle (at 7.62 17.78 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole oval (at 7.62 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 TOSC1))
    (pad "" np_thru_hole circle (at 7.62 12.7 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 TOSC2))
    (pad "" np_thru_hole circle (at 7.62 10.16 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 25.4 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 7.62 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 0 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 5.08 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 2.54 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 33.02 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 0 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer Top) (tedit 5DD849CC)
    (at 154.6 85.344 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference "Audio In" (at 2.54 2.372) (layer F.Fab))
    (fp_text value "L C R" (at -2.54 2.54 180) (layer F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 N$18))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GBUF))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 N$17))
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer Top) (tedit 5DD848DF)
    (at 148.8 93.472 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 2.54 0.044 90) (layer F.SilkS))
    (fp_text value 4.7nF (at 2.5 2.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 LOUT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer Top) (tedit 5DD848D8)
    (at 165.5 93.472 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.5 0.108 90) (layer F.SilkS))
    (fp_text value 4.7nF (at 2.5 2.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ROUT))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "" (layer Top) (tedit 0)
    (at 121.541712 76.934773)
    (fp_text reference @HOLE0 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 175.516712 76.934773)
    (fp_text reference @HOLE1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 175.516712 130.909773)
    (fp_text reference @HOLE2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 121.541712 130.909773)
    (fp_text reference @HOLE3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module iSaab:827229-1 (layer Top) (tedit 5DD8490B)
    (at 147.542712 77.405573 90)
    (fp_text reference U$5 (at 2.221573 -13.430712 90) (layer F.SilkS) hide)
    (fp_text value 827229-1 (at 0.189573 -1.238712 180) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 2.96 -0.505 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.04 1.995 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.96 14.495 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.04 -3.005 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -2.04 11.995 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 ROUT) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.96 9.495 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 GBUF) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at -2.04 6.995 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 LOUT) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.96 4.495 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 GBUF) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 2.96 -5.505 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 CANL) (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at -2.04 -8.005 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 CANH) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 2.96 -10.505 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 +12) (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at -2.04 -13.005 90) (size 2.54 2.54) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad "" np_thru_hole circle (at 0.46 19.86 90) (size 3.1 3.1) (drill 3.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.46 -17.84 90) (size 3.1 3.1) (drill 3.1) (layers *.Cu *.Mask))
  )
  (gr_text RTS (at 173.228 134.62) (layer F.SilkS))
  (gr_text RX (at 172.72 132.08) (layer F.SilkS))
  (gr_text TX (at 172.72 129.54) (layer F.SilkS))
  (gr_text VCC (at 173.228 127) (layer F.SilkS))
  (gr_text GND (at 173.228 121.92) (layer F.SilkS))
  (gr_text 1 (at 145.288 114.3) (layer B.SilkS))
  (gr_text 10 (at 148.844 124.46) (layer B.SilkS))
  (gr_text 9 (at 149.352 106.68) (layer B.SilkS))
  (gr_text 8 (at 145.288 101.6) (layer B.SilkS))
  (gr_text 7 (at 149.352 104.14) (layer B.SilkS))
  (gr_text 6 (at 145.288 111.76) (layer B.SilkS))
  (gr_text 5 (at 145.288 106.68) (layer B.SilkS))
  (gr_text 4 (at 145.288 109.22) (layer B.SilkS))
  (gr_text 3 (at 149.352 121.92) (layer B.SilkS))
  (gr_text 2 (at 145.288 119.38) (layer B.SilkS))
  (gr_line (start 119.237055 75.677723) (end 119.237055 133.968142) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.833651 133.968143) (end 119.237055 133.968142) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.833652 137.564739) (end 174.480374 137.564739) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 174.480374 134.279967) (end 174.480374 137.564739) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.765146 134.279967) (end 177.765146 75.650095) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 174.557512 75.650095) (end 177.765146 75.650095) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.557512 72.442461) (end 122.472318 72.442461) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 122.472317 75.677724) (end 122.472318 72.442461) (angle -90) (layer Edge.Cuts) (width 0.05))
)
