(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 65)
    (zones 0)
    (modules 6)
    (nets 32)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.8448 1.4224)
    (pad_drill 0.9144)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(MS1-Pad1)")
  (net 2 3V)
  (net 3 "Net-(MS1-Pad3)")
  (net 4 /GND)
  (net 5 "Net-(MS1-Pad16)")
  (net 6 "Net-(MS1-Pad15)")
  (net 7 "Net-(MS1-Pad14)")
  (net 8 "Net-(MS1-Pad13)")
  (net 9 "Net-(MS1-Pad12)")
  (net 10 "Net-(MS1-Pad11)")
  (net 11 "Net-(MS1-Pad10)")
  (net 12 "Net-(MS1-Pad9)")
  (net 13 "Net-(MS1-Pad8)")
  (net 14 "Net-(MS1-Pad7)")
  (net 15 "Net-(MS1-Pad6)")
  (net 16 "Net-(MS1-Pad5)")
  (net 17 "Net-(MS1-Pad17)")
  (net 18 "Net-(MS1-Pad18)")
  (net 19 "Net-(MS1-Pad19)")
  (net 20 "Net-(MS1-Pad20)")
  (net 21 "Net-(MS1-Pad21)")
  (net 22 "Net-(MS1-Pad22)")
  (net 23 "Net-(MS1-Pad23)")
  (net 24 "Net-(MS1-Pad24)")
  (net 25 "Net-(MS1-Pad25)")
  (net 26 /USB)
  (net 27 "Net-(MS1-Pad27)")
  (net 28 VBAT)
  (net 29 /RX)
  (net 30 /N$1)
  (net 31 /12V)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /12V)
    (add_net /GND)
    (add_net /N$1)
    (add_net /RX)
    (add_net /USB)
    (add_net 3V)
    (add_net "Net-(MS1-Pad1)")
    (add_net "Net-(MS1-Pad10)")
    (add_net "Net-(MS1-Pad11)")
    (add_net "Net-(MS1-Pad12)")
    (add_net "Net-(MS1-Pad13)")
    (add_net "Net-(MS1-Pad14)")
    (add_net "Net-(MS1-Pad15)")
    (add_net "Net-(MS1-Pad16)")
    (add_net "Net-(MS1-Pad17)")
    (add_net "Net-(MS1-Pad18)")
    (add_net "Net-(MS1-Pad19)")
    (add_net "Net-(MS1-Pad20)")
    (add_net "Net-(MS1-Pad21)")
    (add_net "Net-(MS1-Pad22)")
    (add_net "Net-(MS1-Pad23)")
    (add_net "Net-(MS1-Pad24)")
    (add_net "Net-(MS1-Pad25)")
    (add_net "Net-(MS1-Pad27)")
    (add_net "Net-(MS1-Pad3)")
    (add_net "Net-(MS1-Pad5)")
    (add_net "Net-(MS1-Pad6)")
    (add_net "Net-(MS1-Pad7)")
    (add_net "Net-(MS1-Pad8)")
    (add_net "Net-(MS1-Pad9)")
    (add_net VBAT)
  )
  (module shield2:FEATHERWING (layer Top) (tedit 0)
    (at 148.5011 105.0036)
    (fp_text reference MS1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FEATHERWING (at 0 0) (layer F.SilkS) hide)
    (fp_arc (start 2.54 -2.54) (end 0 -2.54) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 0 -20.32) (end 0 -2.54) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 2.54 -20.32) (end 2.54 -22.86) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 48.26 -22.86) (end 2.54 -22.86) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 48.26 -20.32) (end 50.8 -20.32) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 50.8 -2.54) (end 50.8 -20.32) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 48.26 -2.54) (end 48.26 0) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.54 0) (end 48.26 0) (layer Edge.Cuts) (width 0.1))
    (pad 1 thru_hole circle (at 6.35 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(MS1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 8.89 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 2 3V) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 11.43 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(MS1-Pad3)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 13.97 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 4 /GND) (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 44.45 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(MS1-Pad16)") (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 41.91 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(MS1-Pad15)") (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 39.37 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(MS1-Pad14)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 36.83 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(MS1-Pad13)") (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 34.29 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(MS1-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 31.75 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(MS1-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 29.21 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(MS1-Pad10)") (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 26.67 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(MS1-Pad9)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 24.13 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(MS1-Pad8)") (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 21.59 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(MS1-Pad7)") (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 19.05 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(MS1-Pad6)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 16.51 -1.27) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(MS1-Pad5)") (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 44.45 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(MS1-Pad17)") (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 41.91 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(MS1-Pad18)") (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 39.37 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(MS1-Pad19)") (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 36.83 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(MS1-Pad20)") (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 34.29 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(MS1-Pad21)") (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 31.75 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(MS1-Pad22)") (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 29.21 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(MS1-Pad23)") (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 26.67 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(MS1-Pad24)") (solder_mask_margin 0.1016))
    (pad 25 thru_hole circle (at 24.13 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(MS1-Pad25)") (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at 21.59 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 26 /USB) (solder_mask_margin 0.1016))
    (pad 27 thru_hole circle (at 19.05 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(MS1-Pad27)") (solder_mask_margin 0.1016))
    (pad 28 thru_hole circle (at 16.51 -21.59) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 28 VBAT) (solder_mask_margin 0.1016))
    (pad P$2 thru_hole circle (at 2.54 -2.54) (size 3.81 3.81) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1 thru_hole circle (at 2.54 -20.32) (size 3.81 3.81) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad "" np_thru_hole circle (at 48.26 -2.54) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 48.26 -20.32) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module shield2:JST-5-PTH (layer Bottom) (tedit 5CCF39C3)
    (at 189.9011 93.5536 90)
    (descr "<h3>JST 5 Pin Right Angle Plated Through Hole</h3>\n<p>Specifications:\n<ul><li>Pin count: 5</li>\n<li>Pin pitch: 2mm</li>\n</ul></p>\n<p><a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”>Datasheet referenced for footprint</a></p>\n<p>Example device(s):\n<ul><li>CONN_05</li>\n</ul></p>")
    (fp_text reference AIRCON (at 6.3046 1.6149 180) (layer B.SilkS))
    (fp_text value CONN_05JST (at -1.651 2.413 90) (layer B.Fab))
    (pad TX thru_hole circle (at 4 0 90) (size 1.6 1.6) (drill 0.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad RX thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.7) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 /USB) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -2 0 90) (size 1.6 1.6) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 /GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -4 0 90) (size 1.6 1.6) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 /12V) (solder_mask_margin 0.1016))
  )
  (module shield2:JP2 (layer Bottom) (tedit 5CCF3A20)
    (at 163.5011 91.0036 180)
    (descr <b>JUMPER</b>)
    (fp_text reference TXSEL (at -2.4879 1.9766) (layer B.SilkS))
    (fp_text value JP2E (at -3.556 -4.318) (layer B.Fab))
    (fp_text user SW (at 0.5601 -3.4844 180) (layer B.SilkS))
    (fp_text user "" (at 0 -2.667 180) (layer B.SilkS))
    (fp_text user HW (at -2.2339 -3.4844 180) (layer B.SilkS))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 25 "Net-(MS1-Pad25)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 /RX) (solder_mask_margin 0.1016))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 6 "Net-(MS1-Pad15)") (solder_mask_margin 0.1016))
  )
  (module shield2:JP2 (layer Bottom) (tedit 5CCF2DB1)
    (at 163.5011 97.0036 180)
    (descr <b>JUMPER</b>)
    (fp_text reference RXSEL (at -2.6149 -3.0724) (layer B.SilkS))
    (fp_text value JP2E (at -3.556 -4.318) (layer B.Fab))
    (fp_text user "" (at 2.54 -2.667 180) (layer B.SilkS))
    (fp_text user "" (at 0 -2.667 180) (layer B.SilkS))
    (fp_text user "" (at -2.54 -2.667 180) (layer B.SilkS))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 24 "Net-(MS1-Pad24)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 30 /N$1) (solder_mask_margin 0.1016))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.8448 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 7 "Net-(MS1-Pad14)") (solder_mask_margin 0.1016))
  )
  (module shield2:AXIAL-0.3 (layer Bottom) (tedit 5CCF4521)
    (at 178.435 91.567 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference RXPULLUP1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 0) (layer B.SilkS) hide)
    (fp_text user 10k (at 0 -1.016 180) (layer B.SilkS))
    (fp_text user RXPULLUP (at 0 1.016 180) (layer B.SilkS))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 /USB) (solder_mask_margin 0.1016))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 /N$1) (solder_mask_margin 0.1016))
  )
  (module shield2:AXIAL-0.3 (layer Bottom) (tedit 5CCF4526)
    (at 178.435 96.139 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference TXPULLUP1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 0) (layer B.SilkS) hide)
    (fp_text user 10k (at 0 -1.016 180) (layer B.SilkS))
    (fp_text user TXPULLUP (at 0 1.016 180) (layer B.SilkS))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 /USB) (solder_mask_margin 0.1016))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 /RX) (solder_mask_margin 0.1016))
  )
  (gr_text GND (at 186.817 95.631) (layer B.SilkS))
  (gr_text 5V (at 186.817 93.472) (layer B.SilkS))
  (gr_text RX (at 186.817 91.567) (layer B.SilkS))
  (gr_text TX (at 186.944 89.535) (layer B.SilkS))
  (gr_text "RX\nGPIO12" (at 175.641 86.868 270) (layer B.SilkS))
  (gr_text "TX\nGPIO14" (at 172.72 86.868 270) (layer B.SilkS))
  (gr_text GND (at 162.433 101.854) (layer B.SilkS))
  (gr_text 5V (at 169.926 85.598 270) (layer B.SilkS))
  (gr_text "RX\n(HW)" (at 187.833 101.346) (layer B.SilkS))
  (gr_text "TX\n(HW)" (at 190.627 101.346) (layer B.SilkS))
  (gr_text "Mitsubishi Electric A/C Controller\nv0.5\ngithub.com/endeavour" (at 159.004 82.677 -90) (layer B.SilkS))
)
