(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "STM32MP135 Dev Boart")
    (rev "A")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(AE1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(U8-XTAL_I)")
  (net 4 "Net-(U8-XTAL_O)")
  (net 5 "+3V3")
  (net 6 "+1V8")
  (net 7 "+5V")
  (net 8 "Net-(J1-VBUS)")
  (net 9 "Net-(J2-VBUS)")
  (net 10 "Vdrive")
  (net 11 "Net-(U8-RF_1)")
  (net 12 "Earth")
  (net 13 "Net-(D2-A1)")
  (net 14 "Net-(U8-RF_2)")
  (net 15 "unconnected-(U8-GPIO{slash}FEM_1-Pad1)")
  (net 16 "unconnected-(U8-GPIO{slash}FEM_2-Pad2)")
  (net 17 "unconnected-(U8-GPIO{slash}FEM_3-Pad3)")
  (net 18 "unconnected-(U8-GPIO{slash}FEM_4-Pad4)")
  (net 19 "unconnected-(U8-GPIO{slash}FEM_PDET-Pad5)")
  (net 20 "unconnected-(U8-RESERVE_2-Pad6)")
  (net 21 "WIFI_RST")
  (net 22 "WIFI_UP")
  (net 23 "unconnected-(U8-GPIO{slash}FEM_5-Pad17)")
  (net 24 "unconnected-(U8-GPIO{slash}FEM_6-Pad18)")
  (net 25 "unconnected-(U8-GPIO{slash}PTA_TX_CONF-Pad19)")
  (net 26 "unconnected-(U8-GPIO{slash}PTA_RF_ACT-Pad20)")
  (net 27 "unconnected-(U8-GPIO{slash}PTA_STATUS-Pad21)")
  (net 28 "unconnected-(U8-GPIO{slash}PTA_FREQ-Pad22)")
  (net 29 "LP_CLK")
  (net 30 "unconnected-(U8-GPIO{slash}WIRQ-Pad24)")
  (net 31 "SPI5_MOSI")
  (net 32 "SPI5_MISO")
  (net 33 "WIFI_IRQ")
  (net 34 "WIFI_CS")
  (net 35 "USB1_N")
  (net 36 "USB1_P")
  (net 37 "USB2_N")
  (net 38 "USB2_P")
  (net 39 "MMC1_D2")
  (net 40 "MMC1_D3")
  (net 41 "MMC1_CMD")
  (net 42 "MMC1_CK")
  (net 43 "MMC1_D0")
  (net 44 "MMC1_D1")
  (net 45 "unconnected-(J3-SHIELD-PadP1)")
  (net 46 "MMC1_DETECT")
  (net 47 "Net-(J4-CC1)")
  (net 48 "/Debug/USB_P")
  (net 49 "/Debug/USB_N")
  (net 50 "unconnected-(J4-SBU1-PadA8)")
  (net 51 "Net-(J4-CC2)")
  (net 52 "unconnected-(J4-SBU2-PadB8)")
  (net 53 "UART4_RX")
  (net 54 "UART4_TX")
  (net 55 "CTP_RESET")
  (net 56 "CTP_INT")
  (net 57 "I2C1_SCL")
  (net 58 "I2C1_SDA")
  (net 59 "LCD_R0")
  (net 60 "LCD_R1")
  (net 61 "LCD_R2")
  (net 62 "LCD_R3")
  (net 63 "LCD_R4")
  (net 64 "LCD_R5")
  (net 65 "LCD_R6")
  (net 66 "LCD_R7")
  (net 67 "LCD_G0")
  (net 68 "LCD_G1")
  (net 69 "LCD_G2")
  (net 70 "LCD_G3")
  (net 71 "LCD_G4")
  (net 72 "LCD_G5")
  (net 73 "LCD_G6")
  (net 74 "LCD_G7")
  (net 75 "LCD_B0")
  (net 76 "LCD_B1")
  (net 77 "LCD_B2")
  (net 78 "LCD_B3")
  (net 79 "LCD_B4")
  (net 80 "LCD_B5")
  (net 81 "LCD_B6")
  (net 82 "LCD_B7")
  (net 83 "LCD_CLK")
  (net 84 "LCD_H_SYNC")
  (net 85 "LCD_V_SYNC")
  (net 86 "LCD_DATA_EN")
  (net 87 "Net-(U7-VOUTR+)")
  (net 88 "Net-(U7-VOUTL+)")
  (net 89 "/Audio/VCOM")
  (net 90 "Net-(U6-Pin_4)")
  (net 91 "Net-(U5-USBDM)")
  (net 92 "Net-(U5-USBDP)")
  (net 93 "NRST")
  (net 94 "BOOT0")
  (net 95 "BOOT1")
  (net 96 "BOOT2")
  (net 97 "SPI5_SCK")
  (net 98 "UART5_RX")
  (net 99 "UART5_TX")
  (net 100 "SAI1_MCLK_B")
  (net 101 "SAI1_SD_B")
  (net 102 "SAI1_SCK_B")
  (net 103 "SAI1_FS_B")
  (net 104 "SWCLK")
  (net 105 "SWDIO")
  (net 106 "unconnected-(U3-~{OC2}-Pad5)")
  (net 107 "unconnected-(U3-~{OC1}-Pad8)")
  (net 108 "unconnected-(U5-~{DTR}-Pad1)")
  (net 109 "unconnected-(U5-~{RTS}-Pad2)")
  (net 110 "unconnected-(U5-~{RI}-Pad5)")
  (net 111 "unconnected-(U5-~{DSR}-Pad7)")
  (net 112 "unconnected-(U5-~{DCD}-Pad8)")
  (net 113 "unconnected-(U5-~{CTS}-Pad9)")
  (net 114 "unconnected-(U5-CBUS2-Pad10)")
  (net 115 "unconnected-(U5-3V3OUT-Pad13)")
  (net 116 "unconnected-(U5-CBUS1-Pad17)")
  (net 117 "unconnected-(U5-CBUS0-Pad18)")
  (net 118 "unconnected-(U5-CBUS3-Pad19)")
  (net 119 "unconnected-(U7-DOUT-Pad3)")
  (net 120 "unconnected-(U7-LRCK1-Pad4)")
  (net 121 "unconnected-(U7-BCK1-Pad5)")
  (net 122 "unconnected-(U7-SCKI1-Pad6)")
  (net 123 "unconnected-(U7-ZEROR-Pad13)")
  (net 124 "unconnected-(U7-ZEROL-Pad14)")
  (net 125 "unconnected-(U7-VOUTR--Pad17)")
  (net 126 "unconnected-(U7-VOUTL--Pad19)")
  (net 127 "unconnected-(U7-VINL-Pad25)")
  (net 128 "unconnected-(U7-VINR-Pad26)")
  (net 129 "Net-(J7-Pin_1)")
  (net 130 "unconnected-(J7-Pin_35-Pad35)")
  (net 131 "unconnected-(J7-Pin_36-Pad36)")
  (net 132 "unconnected-(J7-Pin_37-Pad37)")
  (net 133 "unconnected-(J7-Pin_38-Pad38)")
  (net 134 "unconnected-(J7-Pin_39-Pad39)")
  (net 135 "unconnected-(J7-Pin_40-Pad40)")
  (net 136 "Net-(U1-USB_D2_P)")
  (net 137 "Net-(U1-USB_D2_N)")
  (net 138 "Net-(U1-USB_D1_P)")
  (net 139 "Net-(U1-USB_D1_N)")
  (net 140 "unconnected-(U1-NC-Pad111)")
  (net 141 "unconnected-(U1-PI2-Pad103)")
  (net 142 "unconnected-(U1-PI3-Pad102)")
  (net 143 "unconnected-(U1-PH5-Pad99)")
  (net 144 "unconnected-(U1-PH4-Pad98)")
  (net 145 "unconnected-(U1-PI7-Pad97)")
  (net 146 "unconnected-(U1-FDCAN2_RX-Pad96)")
  (net 147 "unconnected-(U1-FDCAN2_TX-Pad95)")
  (net 148 "unconnected-(U1-ADC1_INP2-Pad92)")
  (net 149 "unconnected-(U1-ADC1_INP8-Pad91)")
  (net 150 "unconnected-(U1-PWM1-Pad90)")
  (net 151 "unconnected-(U1-PWM2-Pad89)")
  (net 152 "unconnected-(U1-PI1-Pad87)")
  (net 153 "unconnected-(U1-I2S1_SDI-Pad77)")
  (net 154 "unconnected-(U1-NC-Pad62)")
  (net 155 "unconnected-(U1-ETH1_TXD3-Pad61)")
  (net 156 "unconnected-(U1-ETH1_TXCTL-Pad60)")
  (net 157 "unconnected-(U1-ETH1_TXD0-Pad59)")
  (net 158 "unconnected-(U1-ETH1_TXD2-Pad58)")
  (net 159 "unconnected-(U1-ETH1_TXD1-Pad57)")
  (net 160 "unconnected-(U1-ETH1_TXC-Pad55)")
  (net 161 "unconnected-(U1-ETH1_RXD0-Pad53)")
  (net 162 "unconnected-(U1-ETH1_RXCTL-Pad52)")
  (net 163 "unconnected-(U1-ETH1_RXD3-Pad51)")
  (net 164 "unconnected-(U1-ETH1_RXD1-Pad50)")
  (net 165 "unconnected-(U1-ETH1_RXD2-Pad49)")
  (net 166 "unconnected-(U1-ETH1_RXC-Pad48)")
  (net 167 "unconnected-(U1-ETH1_MDIO-Pad47)")
  (net 168 "unconnected-(U1-ETH1_MDC-Pad46)")
  (net 169 "unconnected-(U1-ETH1_CLK125-Pad44)")
  (net 170 "unconnected-(U1-ETH2_CLK125-Pad37)")
  (net 171 "unconnected-(U1-ETH2_RXD1-Pad35)")
  (net 172 "unconnected-(U1-ETH2_RXD0-Pad34)")
  (net 173 "unconnected-(U1-ETH2_RXD3-Pad33)")
  (net 174 "unconnected-(U1-ETH2_RXD2-Pad32)")
  (net 175 "unconnected-(U1-ETH2_RXC-Pad31)")
  (net 176 "unconnected-(U1-ETH2_RXCTL-Pad30)")
  (net 177 "unconnected-(U1-ETH2_TXC-Pad28)")
  (net 178 "unconnected-(U1-ETH2_TXD0-Pad26)")
  (net 179 "unconnected-(U1-ETH2_TXD1-Pad25)")
  (net 180 "unconnected-(U1-ETH2_TXD2-Pad24)")
  (net 181 "unconnected-(U1-ETH2_TXD3-Pad23)")
  (net 182 "unconnected-(U1-ETH2_TXCTL-Pad22)")
  (net 183 "unconnected-(U1-ETH2_MDC-Pad21)")
  (net 184 "unconnected-(U1-ETH2_MDIO-Pad20)")
  (net 185 "unconnected-(U1-VBAT-Pad17)")
  (net 186 "unconnected-(U1-DCMIPP_HS-Pad12)")
  (net 187 "unconnected-(U1-DCMIPP_VS-Pad11)")
  (net 188 "unconnected-(U1-DCMIPP_PIXCLK-Pad10)")
  (net 189 "unconnected-(U1-DCMIPP_D3-Pad9)")
  (net 190 "unconnected-(U1-DCMIPP_D6-Pad8)")
  (net 191 "unconnected-(U1-DCMIPP_D2-Pad7)")
  (net 192 "unconnected-(U1-DCMIPP_D7-Pad6)")
  (net 193 "unconnected-(U1-DCMIPP_D5-Pad5)")
  (net 194 "unconnected-(U1-DCMIPP_D1-Pad4)")
  (net 195 "unconnected-(U1-DCMIPP_D4-Pad3)")
  (net 196 "unconnected-(U1-DCMIPP_D0-Pad2)")
  (net 197 "unconnected-(U2-NC-Pad4)")
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 25 85)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 121 85)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal" (layer "F.Cu")
    (at 72.5 50.35)
    (descr "Hirose FH12, FFC/FPC connector, FH12-40S-0.5SH, 40 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Generic connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J7" (at 0 -5.15) (layer "F.SilkS"))
    (fp_text value "AFY480272A0" (at -0.5 -3.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.7) (layer "F.Fab"))
    (pad "1" smd rect (at -9.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(J7-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -9.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Vdrive") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -8.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at -8.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -7.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "LCD_R0") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at -7.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "LCD_R1") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at -6.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "LCD_R2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at -6.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "LCD_R3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at -5.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "LCD_R4") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at -5.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "LCD_R5") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at -4.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "LCD_R6") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at -4.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "LCD_R7") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at -3.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "LCD_G0") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at -3.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "LCD_G1") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at -2.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "LCD_G2") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at -2.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "LCD_G3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at -1.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "LCD_G4") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at -1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "LCD_G5") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at -0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "LCD_G6") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at -0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "LCD_G7") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "LCD_B0") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "LCD_B1") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "LCD_B2") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 1.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "LCD_B3") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 2.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "LCD_B4") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 2.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "LCD_B5") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 3.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "LCD_B6") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 3.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "LCD_B7") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 4.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 4.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "LCD_CLK") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 5.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3V3") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 5.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "LCD_H_SYNC") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 6.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "LCD_V_SYNC") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 6.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "LCD_DATA_EN") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 7.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "unconnected-(J7-Pin_35-Pad35)") (pinfunction "Pin_35") (pintype "passive+no_connect"))
    (pad "36" smd rect (at 7.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "unconnected-(J7-Pin_36-Pad36)") (pinfunction "Pin_36") (pintype "passive+no_connect"))
    (pad "37" smd rect (at 8.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "unconnected-(J7-Pin_37-Pad37)") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "38" smd rect (at 8.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "unconnected-(J7-Pin_38-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" smd rect (at 9.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "unconnected-(J7-Pin_39-Pad39)") (pinfunction "Pin_39") (pintype "passive+no_connect"))
    (pad "40" smd rect (at 9.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "unconnected-(J7-Pin_40-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (pad "MP" smd rect (at -11.65 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP" smd rect (at 11.65 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 25 25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal" (layer "F.Cu")
    (at 114 55.3)
    (descr "Hirose FH12, FFC/FPC connector, FH12-6S-0.5SH, 6 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J6" (at -0.8 -4.9) (layer "F.SilkS"))
    (fp_text value "CTP" (at -0.4 -3.5 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.7) (layer "F.Fab"))
    (pad "1" smd rect (at -1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "CTP_RESET") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "CTP_INT") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "I2C1_SCL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "I2C1_SDA") (pinfunction "Pin_6") (pintype "passive"))
    (pad "MP" smd rect (at -3.15 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP" smd rect (at 3.15 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV" (layer "B.Cu")
    (at 123.205 69.21 -90)
    (descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2204071530_G-Switch-GT-USB-7010ASV_C2988369.pdf")
    (tags "USB C Type-C Receptacle SMD")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "USB 2.0-only Type-C Receptacle connector")
    (property "ki_keywords" "usb universal serial bus type-C USB2.0")
    (clearance 0.17)
    (attr smd)
    (fp_text reference "J4" (at 0 5.5 90) (layer "B.SilkS"))
    (fp_text value "USB_DEBUG" (at -6.41 1.805) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at -2.89 2.605 270) (size 0.65 0.65) (drill 0.65) (layers "F&B.Cu" "*.Mask")
      (clearance 0.17))
    (pad "" np_thru_hole circle (at 2.89 2.605 270) (size 0.65 0.65) (drill 0.65) (layers "*.Cu" "*.Mask"))
    (pad "A1" smd rect (at -3.2 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.4 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(D2-A1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "Net-(J4-CC1)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "/Debug/USB_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "/Debug/USB_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "unconnected-(J4-SBU1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "A9" smd rect (at 2.4 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(D2-A1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.2 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.2 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.4 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(D2-A1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "Net-(J4-CC2)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "/Debug/USB_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "/Debug/USB_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 3.725 270) (size 0.3 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "unconnected-(J4-SBU2-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "B9" smd rect (at -2.4 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(D2-A1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.2 3.725 270) (size 0.6 1.24) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 -1.075 270) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 3.125 270) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 -1.075 270) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 3.125 270) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7010ASV.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 108.5875 63.96 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0.36 -3.1875 270) (layer "B.SilkS"))
    (fp_text value "27R" (at 0.56 -4.3875 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 49 "/Debug/USB_N") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 91 "Net-(U5-USBDM)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 102.95 87.9 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 3.25) (layer "B.SilkS"))
    (fp_text value "GND" (at -0.1 1.75) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.252) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_USB:USB_A_Molex_67643_Horizontal" (layer "B.Cu")
    (at 85.5 78.64 180)
    (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "USB Type A connector")
    (property "ki_keywords" "connector USB")
    (attr through_hole)
    (fp_text reference "J2" (at 3.75 5.14) (layer "B.SilkS"))
    (fp_text value "USB_2" (at 3.5 3.24) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 3.5 -3.7) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.5) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-VBUS)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 37 "USB2_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 4.5 0 180) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 38 "USB2_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 7 0 180) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle (at -3.07 -2.71 180) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.07 -2.71 180) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 101.03 57.46 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -3.25 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "B.Cu")
    (at 114.11 28.4825)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 7.19 0.855) (layer "B.SilkS"))
    (fp_text value "0.8pF" (at 3.25 0.855) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(AE1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 43.25 42.75 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 26.8 15.2 -270) (layer "B.SilkS"))
    (fp_text value "47K" (at 37.25 -8.65 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 41 "MMC1_CMD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 94 83.75 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0.25 5.25 90) (layer "B.SilkS"))
    (fp_text value "10uF" (at 0 3.75 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0 90) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 9 "Net-(J2-VBUS)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0 90) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 24.6 73.2 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 3.8 0 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 2.5 -0.5 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0402_1005Metric_Pad0.77x0.64mm_HandSolder" (layer "B.Cu")
    (at 113.61 30.2325 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 0.005 -2.75 90) (layer "B.SilkS"))
    (fp_text value "2.7nH" (at 0 -1.25 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.5725 0 90) (size 0.765 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U8-RF_1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5725 0 90) (size 0.765 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(AE1-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 106.2 87.9 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 0 3.25) (layer "B.SilkS"))
    (fp_text value "3V3" (at 0 1.75) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.252) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 5 "+3V3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 109.45 87.9 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 3.25) (layer "B.SilkS"))
    (fp_text value "5V" (at -0.05 1.7) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.252) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 7 "+5V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 47 41.5 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at -13.45 25.55) (layer "B.SilkS"))
    (fp_text value "47K" (at 8.65 36.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 39 "MMC1_D2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile" (layer "B.Cu")
    (at 26.695 39.96 180)
    (descr "SMD 3x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile")
    (tags "SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
    (property "ki_keywords" "dip switch")
    (attr smd)
    (fp_text reference "SW2" (at -6.705 -2.64 270) (layer "B.SilkS"))
    (fp_text value "BOOT" (at -0.005 5.71) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 2.58 0 90) (layer "B.Fab"))
    (fp_text user "on" (at 0.4275 3.8825) (layer "B.Fab"))
    (pad "1" smd rect (at -4.305 2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "BOOT0") (pintype "passive"))
    (pad "2" smd rect (at -4.305 0 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "BOOT1") (pintype "passive"))
    (pad "3" smd rect (at -4.305 -2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "BOOT2") (pintype "passive"))
    (pad "4" smd rect (at 4.305 -2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "+5V") (pintype "passive"))
    (pad "5" smd rect (at 4.305 0 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "+5V") (pintype "passive"))
    (pad "6" smd rect (at 4.305 2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 60.25 66.25 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP135_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 3.75 0 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 137 "Net-(U1-USB_D2_N)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 37 "USB2_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 104.85 37.8)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 3.2) (layer "B.SilkS"))
    (fp_text value "10pF" (at 0 1.75) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U8-XTAL_O)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_A_Molex_67643_Horizontal" (layer "B.Cu")
    (at 67.5 78.64 180)
    (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "USB Type A connector")
    (property "ki_keywords" "connector USB")
    (attr through_hole)
    (fp_text reference "J1" (at 3.5 5.39) (layer "B.SilkS"))
    (fp_text value "USB_1" (at 3.6 3.24) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 3.5 -3.7) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.5) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-VBUS)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 35 "USB1_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 4.5 0 180) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 36 "USB1_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 7 0 180) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle (at -3.07 -2.71 180) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.07 -2.71 180) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 40.7125 39.25 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at -16.7375 25.05) (layer "B.SilkS"))
    (fp_text value "47K" (at 8.6125 35.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 43 "MMC1_D0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 46 57.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 4.4 0 90) (layer "B.SilkS"))
    (fp_text value "0.22uF" (at 3.2 -0.5 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Vdrive") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "STM32MP135_Dev_Board:HRS_DM3AT-SF-PEJM5" (layer "B.Cu")
    (at 42.3125 36.5875)
    (descr "Micro SD card holder with push-to-eject feature.")
    (property "AVAILABILITY" "Unavailable")
    (property "DESCRIPTION" "DM3 RA SMT microSD memory card push/push")
    (property "MANUFACTURER" "Hirose")
    (property "MF" "Hirose")
    (property "MP" "DM3AT-SF-PEJM5")
    (property "PACKAGE" "None")
    (property "PARTREV" "n/a")
    (property "PRICE" "None")
    (property "STANDARED" "manufacturer recommendation")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (attr smd)
    (fp_text reference "J3" (at -8.0125 -3.0875 -90) (layer "B.SilkS"))
    (fp_text value "BOOT_SD" (at 5.55359 -22.58781 -180) (layer "B.Fab"))
    (fp_text user "PCB Edge" (at -4.75766 -15.525 -180) (layer "B.Fab"))
    (pad "1" smd rect (at 3.2 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "MMC1_D2") (pinfunction "DAT2") (pintype "bidirectional"))
    (pad "2" smd rect (at 2.1 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "MMC1_D3") (pinfunction "CD/DAT3") (pintype "bidirectional"))
    (pad "3" smd rect (at 1 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "MMC1_CMD") (pinfunction "CMD") (pintype "bidirectional"))
    (pad "4" smd rect (at -0.1 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd rect (at -1.2 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "MMC1_CK") (pinfunction "CLK") (pintype "bidirectional"))
    (pad "6" smd rect (at -2.3 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "7" smd rect (at -3.4 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "MMC1_D0") (pinfunction "DAT0") (pintype "bidirectional"))
    (pad "8" smd rect (at -4.5 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "MMC1_D1") (pinfunction "DAT1") (pintype "bidirectional"))
    (pad "P1" smd rect (at -6.4 -4.3) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "unconnected-(J3-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "P2" smd rect (at -6.4 -14.65) (size 1 2.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "unconnected-(J3-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "P3" smd rect (at 7.1 -15.1) (size 1.3 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "unconnected-(J3-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "P4" smd rect (at 4.75 0) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "unconnected-(J3-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "SWA" smd rect (at -6.4 -10.5) (size 1 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "+3V3") (pintype "bidirectional"))
    (pad "SWB" smd rect (at -5.45 0) (size 0.7 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "MMC1_DETECT") (pintype "bidirectional"))
    (zone (net 0) (net_name "") (layer "B.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 35.49944 36.1375)
          (xy 36.2625 36.1375)
          (xy 36.2625 32.88039)
          (xy 35.49944 32.88039)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "B.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 35.50856 31.6875)
          (xy 36.2625 31.6875)
          (xy 36.2625 28.08258)
          (xy 35.50856 28.08258)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "B.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 36.60645 30.2875)
          (xy 37.3125 30.2875)
          (xy 37.3125 22.6727)
          (xy 36.60645 22.6727)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "B.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 45.664 21.8875)
          (xy 48.2125 21.8875)
          (xy 48.2125 20.5303)
          (xy 45.664 20.5303)
        )
      )
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 113.9 48.5 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "10K" (at -0.1 3.2) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 55 "CTP_RESET") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 106.73 74.46 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at -0.25 -3 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.68 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 116.93 65.91 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 8.61 0 90) (layer "B.SilkS"))
    (fp_text value "5K1" (at 5.51 0.07 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 47 "Net-(J4-CC1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 109.2 41.7 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -3.3) (layer "B.SilkS"))
    (fp_text value "10pF" (at 0 -1.68) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U8-XTAL_I)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 47.25 75.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 2.5 0) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0.25 -2 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric" (layer "B.Cu")
    (at 111.23 69.21 180)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F1" (at 0.23 -3.29 90) (layer "B.SilkS"))
    (fp_text value "2A" (at 0.25 -2 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 13 "Net-(D2-A1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 7 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 24.5 62.8 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 3.8 0 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 2.5 0.5 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 45.15 52.85 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 3) (layer "B.SilkS"))
    (fp_text value "LED+" (at 0.25 1.7) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 10 "Vdrive") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 45.75 39.25 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -13.95 25.05) (layer "B.SilkS"))
    (fp_text value "47K" (at 8.65 35.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 40 "MMC1_D3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_6.3x6.3_H3" (layer "B.Cu")
    (at 42 62.6 180)
    (descr "Choke, SMD, 6.3x6.3mm 3mm height")
    (tags "Choke SMD")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L2" (at 0.1 -5.5) (layer "B.SilkS"))
    (fp_text value "20uH" (at 0 -4.2) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -2.75 0 180) (size 1.5 2.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0 180) (size 1.5 2.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "Net-(U6-Pin_4)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_6.3x6.3_H3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 115.35 33.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 6.25 -1.5) (layer "B.SilkS"))
    (fp_text value "50R" (at 3.25 -1.25) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(U8-RF_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 30 75.75)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 1.75 5) (layer "B.SilkS"))
    (fp_text value "10uF" (at 1.25 3.75) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "B.Cu")
    (at 114.11 31.9825)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 7.19 -1.125) (layer "B.SilkS"))
    (fp_text value "1.8pF" (at 3.19 -1.145) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U8-RF_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SSOP-20_3.9x8.7mm_P0.635mm" (layer "B.Cu")
    (at 106.9225 57.36 -90)
    (descr "SSOP20: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf)")
    (tags "SSOP 0.635")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Full Speed USB to Full Handshake UART, SSOP-20")
    (property "ki_keywords" "FTDI USB UART interface converter")
    (attr smd)
    (fp_text reference "U5" (at -0.65 -6.8925 90) (layer "B.SilkS"))
    (fp_text value "FT231XS" (at 0.1 -5.3925 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -2.6 2.8575 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "unconnected-(U5-~{DTR}-Pad1)") (pinfunction "~{DTR}") (pintype "output+no_connect"))
    (pad "2" smd rect (at -2.6 2.2225 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "unconnected-(U5-~{RTS}-Pad2)") (pinfunction "~{RTS}") (pintype "output+no_connect"))
    (pad "3" smd rect (at -2.6 1.5875 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "+3V3") (pinfunction "VCCIO") (pintype "power_in"))
    (pad "4" smd rect (at -2.6 0.9525 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "UART4_TX") (pinfunction "RXD") (pintype "input"))
    (pad "5" smd rect (at -2.6 0.3175 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "unconnected-(U5-~{RI}-Pad5)") (pinfunction "~{RI}") (pintype "input+no_connect"))
    (pad "6" smd rect (at -2.6 -0.3175 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd rect (at -2.6 -0.9525 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "unconnected-(U5-~{DSR}-Pad7)") (pinfunction "~{DSR}") (pintype "input+no_connect"))
    (pad "8" smd rect (at -2.6 -1.5875 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "unconnected-(U5-~{DCD}-Pad8)") (pinfunction "~{DCD}") (pintype "input+no_connect"))
    (pad "9" smd rect (at -2.6 -2.2225 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 113 "unconnected-(U5-~{CTS}-Pad9)") (pinfunction "~{CTS}") (pintype "input+no_connect"))
    (pad "10" smd rect (at -2.6 -2.8575 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "unconnected-(U5-CBUS2-Pad10)") (pinfunction "CBUS2") (pintype "bidirectional+no_connect"))
    (pad "11" smd rect (at 2.6 -2.8575 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(U5-USBDP)") (pinfunction "USBDP") (pintype "bidirectional"))
    (pad "12" smd rect (at 2.6 -2.2225 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "Net-(U5-USBDM)") (pinfunction "USBDM") (pintype "bidirectional"))
    (pad "13" smd rect (at 2.6 -1.5875 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "unconnected-(U5-3V3OUT-Pad13)") (pinfunction "3V3OUT") (pintype "power_out+no_connect"))
    (pad "14" smd rect (at 2.6 -0.9525 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "+3V3") (pinfunction "~{RESET}") (pintype "input"))
    (pad "15" smd rect (at 2.6 -0.3175 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "16" smd rect (at 2.6 0.3175 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "17" smd rect (at 2.6 0.9525 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 116 "unconnected-(U5-CBUS1-Pad17)") (pinfunction "CBUS1") (pintype "bidirectional+no_connect"))
    (pad "18" smd rect (at 2.6 1.5875 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "unconnected-(U5-CBUS0-Pad18)") (pinfunction "CBUS0") (pintype "bidirectional+no_connect"))
    (pad "19" smd rect (at 2.6 2.2225 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "unconnected-(U5-CBUS3-Pad19)") (pinfunction "CBUS3") (pintype "bidirectional+no_connect"))
    (pad "20" smd rect (at 2.6 2.8575 270) (size 1.2 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "UART4_RX") (pinfunction "TXD") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-20_3.9x8.7mm_P0.635mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 35.9625 39.25)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 19.2375 -25.05 -360) (layer "B.SilkS"))
    (fp_text value "47K" (at -7.8625 -35.75 -360) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -360) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 44 "MMC1_D1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Audio:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal" (layer "B.Cu")
    (at 39.75 83.75)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS)")
    (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector")
    (attr smd)
    (fp_text reference "J8" (at 0 9.9) (layer "B.SilkS"))
    (fp_text value "AudioJack3" (at 0.05 -9.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at 0 -4.5) (size 1.7 1.7) (drill 1.7) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 2.5) (size 1.7 1.7) (drill 1.7) (layers "*.Cu" "*.Mask"))
    (pad "R" smd rect (at 3.7 1.6) (size 2.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "Net-(U7-VOUTR+)") (pintype "passive"))
    (pad "S" smd rect (at -3.7 3.6) (size 2.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "Net-(U7-VOUTL+)") (pintype "passive"))
    (pad "T" smd rect (at -3.7 -5.8) (size 2.8 2.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "/Audio/VCOM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RF_Antenna:Texas_SWRA117D_2.4GHz_Left" (layer "B.Cu")
    (at 113.56 25.7575 180)
    (descr "http://www.ti.com/lit/an/swra117d/swra117d.pdf")
    (tags "PCB antenna")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Dipole antenna")
    (property "ki_keywords" "dipole antenna")
    (zone_connect 2)
    (attr smd exclude_from_pos_files)
    (fp_text reference "AE1" (at 4.56 1.7575 90) (layer "B.SilkS"))
    (fp_text value "Antenna" (at -4.35 1) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -4.55 6.4) (layer "B.Fab"))
    (pad "1" smd rect (at 0 0.3 180) (size 0.5 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Net-(AE1-Pad1)") (pintype "input") (zone_connect 0))
    (pad "2" thru_hole rect (at 2.1 0 180) (size 0.9 2) (drill 0.3) (layers "*.Cu")
      (net 2 "GND") (pintype "input") (zone_connect 2))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 46.9 59.9 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at -0.6 1.7 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at -3.1 0.1 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm" (layer "B.Cu")
    (at 26.75 50.25 90)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr smd)
    (fp_text reference "SW1" (at -0.05 -3.95 270) (layer "B.SilkS"))
    (fp_text value "RESET" (at -5.85 0.05) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at -5.75 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -3.975 2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "NRST") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 3.975 2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "NRST") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -3.975 -2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 3.975 -2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_PUSH_6mm_H9.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "B.Cu")
    (at 119.6 37.8375 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "150mA low quiescent current low noise voltage regulator, Fixed Output 1.8V, SOT-23-5")
    (property "ki_keywords" "150mA LDO Regulator Fixed Positive")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.55 -270) (layer "B.SilkS"))
    (fp_text value "LD39015M18R" (at 2.98 -3.74 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+3V3") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+3V3") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 197 "unconnected-(U2-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+1V8") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (at 114.53 73.01 -90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Bidirectional transient-voltage-suppression diode")
    (property "ki_keywords" "diode TVS thyrector")
    (attr smd)
    (fp_text reference "D1" (at 4.75 0) (layer "B.SilkS"))
    (fp_text value "TVS" (at 3.25 0 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 12 "Earth") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 2 "GND") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (at 52.25 75.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Dual power-distribution switcher")
    (property "ki_keywords" "2-chanel power-distribution USB")
    (attr smd)
    (fp_text reference "U3" (at -0.061906 -5) (layer "B.SilkS"))
    (fp_text value "TPS2042D" (at -0.061906 -3.5) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pinfunction "IN1") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "~{EN1}") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "~{EN2}") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 106 "unconnected-(U3-~{OC2}-Pad5)") (pinfunction "~{OC2}") (pintype "open_collector+no_connect"))
    (pad "6" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J2-VBUS)") (pinfunction "OUT2") (pintype "power_out"))
    (pad "7" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J1-VBUS)") (pinfunction "OUT1") (pintype "power_out"))
    (pad "8" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 107 "unconnected-(U3-~{OC1}-Pad8)") (pinfunction "~{OC1}") (pintype "open_collector+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 110.8375 65.71 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0.91 -4.2375 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0.11 1.7625 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 48 "/Debug/USB_P") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 92 "Net-(U5-USBDP)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 31.75 50.25 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0.25 3.5 90) (layer "B.SilkS"))
    (fp_text value "10K" (at 0.05 2.05 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 93 "NRST") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 7 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 58 69.3 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP135_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 4 0 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 138 "Net-(U1-USB_D1_P)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 36 "USB1_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "B.Cu")
    (at 42 57.1 180)
    (descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Generic connector, double row, 02x03, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "U6" (at -5.5 4) (layer "B.SilkS"))
    (fp_text value "R1218NO41" (at -2 2.5) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.1375 0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -1.1375 0 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Vdrive") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -1.1375 -0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.1375 -0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(U6-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at 1.1375 0 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at 1.1375 0.95 180) (size 1.325 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(J7-Pin_1)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 106.3 52.71)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at -0.1 -2.91) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at -0.1 -1.71) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 100.28 75.46)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 3.7) (layer "B.SilkS"))
    (fp_text value "10uF" (at 4.7 0 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (at 114.53 62.96 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Bidirectional transient-voltage-suppression diode")
    (property "ki_keywords" "diode TVS thyrector")
    (attr smd)
    (fp_text reference "D2" (at 4.25 0 180) (layer "B.SilkS"))
    (fp_text value "TVS" (at 3 0 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 13 "Net-(D2-A1)") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 12 "Earth") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 123.8 59.14)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -10.24 180) (layer "B.SilkS"))
    (fp_text value "UART4" (at -2.5 -3.79 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "UART4_RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "UART4_TX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 119.35 34.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -3.74 0.52 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at -2.49 0.27 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 39.75 41.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 16.7 -25.55) (layer "B.SilkS"))
    (fp_text value "10K" (at -8.65 -36.5 -360) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -360) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 42 "MMC1_CK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 30.25 60.25)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 1.5 -5.25) (layer "B.SilkS"))
    (fp_text value "10uF" (at 0.75 -3.75) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 7 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 62.5 69.3 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP135_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 3.75 0 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 136 "Net-(U1-USB_D2_P)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 38 "USB2_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "STM32MP135_Dev_Board:SOP65P640X120-28N" (layer "B.Cu")
    (at 28 68 90)
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (attr smd)
    (fp_text reference "U7" (at 0.12 7.275 90) (layer "B.SilkS"))
    (fp_text value "PCM3060PWR" (at -0.2 5.8 90) (layer "B.SilkS"))
    (pad "1" smd roundrect (at -2.87 4.225 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 57 "I2C1_SCL") (pinfunction "MC/SCL/FMT") (pintype "input"))
    (pad "2" smd roundrect (at -2.87 3.575 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 58 "I2C1_SDA") (pinfunction "MD/SDA/DEMP") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.87 2.925 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 119 "unconnected-(U7-DOUT-Pad3)") (pinfunction "DOUT") (pintype "output"))
    (pad "4" smd roundrect (at -2.87 2.275 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 120 "unconnected-(U7-LRCK1-Pad4)") (pinfunction "LRCK1") (pintype "bidirectional+no_connect"))
    (pad "5" smd roundrect (at -2.87 1.625 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 121 "unconnected-(U7-BCK1-Pad5)") (pinfunction "BCK1") (pintype "bidirectional+no_connect"))
    (pad "6" smd roundrect (at -2.87 0.975 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 122 "unconnected-(U7-SCKI1-Pad6)") (pinfunction "SCKI1") (pintype "input+no_connect"))
    (pad "7" smd roundrect (at -2.87 0.325 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 5 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "8" smd roundrect (at -2.87 -0.325 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 2 "GND") (pinfunction "DGND") (pintype "power_in"))
    (pad "9" smd roundrect (at -2.87 -0.975 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 100 "SAI1_MCLK_B") (pinfunction "SCKI2") (pintype "input"))
    (pad "10" smd roundrect (at -2.87 -1.625 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 102 "SAI1_SCK_B") (pinfunction "BCK2") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -2.87 -2.275 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 103 "SAI1_FS_B") (pinfunction "LRCK2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.87 -2.925 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 101 "SAI1_SD_B") (pinfunction "DIN") (pintype "input"))
    (pad "13" smd roundrect (at -2.87 -3.575 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 123 "unconnected-(U7-ZEROR-Pad13)") (pinfunction "ZEROR") (pintype "output+no_connect"))
    (pad "14" smd roundrect (at -2.87 -4.225 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 124 "unconnected-(U7-ZEROL-Pad14)") (pinfunction "ZEROL") (pintype "output+no_connect"))
    (pad "15" smd roundrect (at 2.87 -4.225 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 93 "NRST") (pinfunction "~{RST}") (pintype "input"))
    (pad "16" smd roundrect (at 2.87 -3.575 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 2 "GND") (pinfunction "SGND") (pintype "power_in"))
    (pad "17" smd roundrect (at 2.87 -2.925 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 125 "unconnected-(U7-VOUTR--Pad17)") (pinfunction "VOUTR-") (pintype "output+no_connect"))
    (pad "18" smd roundrect (at 2.87 -2.275 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 87 "Net-(U7-VOUTR+)") (pinfunction "VOUTR+") (pintype "output"))
    (pad "19" smd roundrect (at 2.87 -1.625 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 126 "unconnected-(U7-VOUTL--Pad19)") (pinfunction "VOUTL-") (pintype "output+no_connect"))
    (pad "20" smd roundrect (at 2.87 -0.975 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 88 "Net-(U7-VOUTL+)") (pinfunction "VOUTL+") (pintype "output"))
    (pad "21" smd roundrect (at 2.87 -0.325 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 89 "/Audio/VCOM") (pinfunction "VCOM") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.87 0.325 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 2 "GND") (pinfunction "AGND2") (pintype "power_in"))
    (pad "23" smd roundrect (at 2.87 0.975 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 2 "GND") (pinfunction "AGND1") (pintype "power_in"))
    (pad "24" smd roundrect (at 2.87 1.625 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 7 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "25" smd roundrect (at 2.87 2.275 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 127 "unconnected-(U7-VINL-Pad25)") (pinfunction "VINL") (pintype "input+no_connect"))
    (pad "26" smd roundrect (at 2.87 2.925 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 128 "unconnected-(U7-VINR-Pad26)") (pinfunction "VINR") (pintype "input+no_connect"))
    (pad "27" smd roundrect (at 2.87 3.575 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 2 "GND") (pinfunction "~{MS/ADR/IFMD}") (pintype "input"))
    (pad "28" smd roundrect (at 2.87 4.225 90) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 2 "GND") (pinfunction "MODE") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 38.5 56.6 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 -3.25 90) (layer "B.SilkS"))
    (fp_text value "10R" (at 0 -1.82 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 129 "Net-(J7-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 52 84 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 -3.6 90) (layer "B.SilkS"))
    (fp_text value "10uF" (at 4.6 -0.2 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0 90) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 8 "Net-(J1-VBUS)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0 90) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 118.6 41.8375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at -0.0375 -3.05 -270) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0.1625 -1.65 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "+1V8") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "STM32MP135_Dev_Board:MYCYA151C256N256D65CT" (layer "B.Cu")
    (at 73 42.5 180)
    (descr "MYC-YA151C-256N256D-65-C-T-5")
    (tags "Undefined or Miscellaneous")
    (property "Height" "3.5")
    (property "Manufacturer_Name" "MYIR")
    (property "Manufacturer_Part_Number" "MYC-YA151C-256N256D-65-C-T")
    (property "Mouser Part Number" "885-MCA151CN256D65CT")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/MYIR/MYC-YA151C-256N256D-65-C-T?qs=e8oIoAS2J1SxKfhSw3h3gA%3D%3D")
    (property "Sheetfile" "STM32MP135_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Embedded Module ARM Cortex-A7, ARM Cortex-M4 650MHz 256MB 256MB")
    (attr smd)
    (fp_text reference "U1" (at 0.25 -22.75) (layer "B.SilkS"))
    (fp_text value "MYC-YF135" (at 0 0) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0.25 -22.75) (layer "B.Fab"))
    (pad "1" smd oval (at -18.5 18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "2" smd oval (at -18.5 17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 196 "unconnected-(U1-DCMIPP_D0-Pad2)") (pinfunction "DCMIPP_D0") (pintype "passive"))
    (pad "3" smd oval (at -18.5 16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 195 "unconnected-(U1-DCMIPP_D4-Pad3)") (pinfunction "DCMIPP_D4") (pintype "passive"))
    (pad "4" smd oval (at -18.5 15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 194 "unconnected-(U1-DCMIPP_D1-Pad4)") (pinfunction "DCMIPP_D1") (pintype "passive"))
    (pad "5" smd oval (at -18.5 14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 193 "unconnected-(U1-DCMIPP_D5-Pad5)") (pinfunction "DCMIPP_D5") (pintype "passive"))
    (pad "6" smd oval (at -18.5 13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 192 "unconnected-(U1-DCMIPP_D7-Pad6)") (pinfunction "DCMIPP_D7") (pintype "passive"))
    (pad "7" smd oval (at -18.5 12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 191 "unconnected-(U1-DCMIPP_D2-Pad7)") (pinfunction "DCMIPP_D2") (pintype "passive"))
    (pad "8" smd oval (at -18.5 11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 190 "unconnected-(U1-DCMIPP_D6-Pad8)") (pinfunction "DCMIPP_D6") (pintype "passive"))
    (pad "9" smd oval (at -18.5 10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 189 "unconnected-(U1-DCMIPP_D3-Pad9)") (pinfunction "DCMIPP_D3") (pintype "passive"))
    (pad "10" smd oval (at -18.5 9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 188 "unconnected-(U1-DCMIPP_PIXCLK-Pad10)") (pinfunction "DCMIPP_PIXCLK") (pintype "passive"))
    (pad "11" smd oval (at -18.5 8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 187 "unconnected-(U1-DCMIPP_VS-Pad11)") (pinfunction "DCMIPP_VS") (pintype "passive"))
    (pad "12" smd oval (at -18.5 7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 186 "unconnected-(U1-DCMIPP_HS-Pad12)") (pinfunction "DCMIPP_HS") (pintype "passive"))
    (pad "13" smd oval (at -18.5 6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "14" smd oval (at -18.5 5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "+5V") (pinfunction "VSOM_5V") (pintype "passive"))
    (pad "15" smd oval (at -18.5 4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "+5V") (pinfunction "VSOM_5V") (pintype "passive"))
    (pad "16" smd oval (at -18.5 3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "+3V3") (pinfunction "VDD_3V3") (pintype "passive"))
    (pad "17" smd oval (at -18.5 2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 185 "unconnected-(U1-VBAT-Pad17)") (pinfunction "VBAT") (pintype "passive"))
    (pad "18" smd oval (at -18.5 1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "19" smd oval (at -18.5 0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "20" smd oval (at -18.5 -0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 184 "unconnected-(U1-ETH2_MDIO-Pad20)") (pinfunction "ETH2_MDIO") (pintype "passive"))
    (pad "21" smd oval (at -18.5 -1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 183 "unconnected-(U1-ETH2_MDC-Pad21)") (pinfunction "ETH2_MDC") (pintype "passive"))
    (pad "22" smd oval (at -18.5 -2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 182 "unconnected-(U1-ETH2_TXCTL-Pad22)") (pinfunction "ETH2_TXCTL") (pintype "passive"))
    (pad "23" smd oval (at -18.5 -3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 181 "unconnected-(U1-ETH2_TXD3-Pad23)") (pinfunction "ETH2_TXD3") (pintype "passive"))
    (pad "24" smd oval (at -18.5 -4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 180 "unconnected-(U1-ETH2_TXD2-Pad24)") (pinfunction "ETH2_TXD2") (pintype "passive"))
    (pad "25" smd oval (at -18.5 -5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 179 "unconnected-(U1-ETH2_TXD1-Pad25)") (pinfunction "ETH2_TXD1") (pintype "passive"))
    (pad "26" smd oval (at -18.5 -6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 178 "unconnected-(U1-ETH2_TXD0-Pad26)") (pinfunction "ETH2_TXD0") (pintype "passive"))
    (pad "27" smd oval (at -18.5 -7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "28" smd oval (at -18.5 -8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 177 "unconnected-(U1-ETH2_TXC-Pad28)") (pinfunction "ETH2_TXC") (pintype "passive"))
    (pad "29" smd oval (at -18.5 -9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "30" smd oval (at -18.5 -10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 176 "unconnected-(U1-ETH2_RXCTL-Pad30)") (pinfunction "ETH2_RXCTL") (pintype "passive"))
    (pad "31" smd oval (at -18.5 -11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 175 "unconnected-(U1-ETH2_RXC-Pad31)") (pinfunction "ETH2_RXC") (pintype "passive"))
    (pad "32" smd oval (at -18.5 -12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 174 "unconnected-(U1-ETH2_RXD2-Pad32)") (pinfunction "ETH2_RXD2") (pintype "passive"))
    (pad "33" smd oval (at -18.5 -13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 173 "unconnected-(U1-ETH2_RXD3-Pad33)") (pinfunction "ETH2_RXD3") (pintype "passive"))
    (pad "34" smd oval (at -18.5 -14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "unconnected-(U1-ETH2_RXD0-Pad34)") (pinfunction "ETH2_RXD0") (pintype "passive"))
    (pad "35" smd oval (at -18.5 -15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 171 "unconnected-(U1-ETH2_RXD1-Pad35)") (pinfunction "ETH2_RXD1") (pintype "passive"))
    (pad "36" smd oval (at -18.5 -16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "37" smd oval (at -18.5 -17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 170 "unconnected-(U1-ETH2_CLK125-Pad37)") (pinfunction "ETH2_CLK125") (pintype "passive"))
    (pad "38" smd oval (at -18.5 -18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "39" smd oval (at -17.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "40" smd oval (at -16.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "SPI5_SCK") (pinfunction "SPI5_SCK") (pintype "passive"))
    (pad "41" smd oval (at -15.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "SPI5_MOSI") (pinfunction "SPI5_MOSI") (pintype "passive"))
    (pad "42" smd oval (at -14.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "SPI5_MISO") (pinfunction "SPI5_MISO") (pintype "passive"))
    (pad "43" smd oval (at -13.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "44" smd oval (at -12.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 169 "unconnected-(U1-ETH1_CLK125-Pad44)") (pinfunction "ETH1_CLK125") (pintype "passive"))
    (pad "45" smd oval (at -11.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "46" smd oval (at -10.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 168 "unconnected-(U1-ETH1_MDC-Pad46)") (pinfunction "ETH1_MDC") (pintype "passive"))
    (pad "47" smd oval (at -9.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 167 "unconnected-(U1-ETH1_MDIO-Pad47)") (pinfunction "ETH1_MDIO") (pintype "passive"))
    (pad "48" smd oval (at -8.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 166 "unconnected-(U1-ETH1_RXC-Pad48)") (pinfunction "ETH1_RXC") (pintype "passive"))
    (pad "49" smd oval (at -7.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 165 "unconnected-(U1-ETH1_RXD2-Pad49)") (pinfunction "ETH1_RXD2") (pintype "passive"))
    (pad "50" smd oval (at -6.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 164 "unconnected-(U1-ETH1_RXD1-Pad50)") (pinfunction "ETH1_RXD1") (pintype "passive"))
    (pad "51" smd oval (at -5.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 163 "unconnected-(U1-ETH1_RXD3-Pad51)") (pinfunction "ETH1_RXD3") (pintype "passive"))
    (pad "52" smd oval (at -4.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 162 "unconnected-(U1-ETH1_RXCTL-Pad52)") (pinfunction "ETH1_RXCTL") (pintype "passive"))
    (pad "53" smd oval (at -3.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "unconnected-(U1-ETH1_RXD0-Pad53)") (pinfunction "ETH1_RXD0") (pintype "passive"))
    (pad "54" smd oval (at -2.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "55" smd oval (at -1.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 160 "unconnected-(U1-ETH1_TXC-Pad55)") (pinfunction "ETH1_TXC") (pintype "passive"))
    (pad "56" smd oval (at -0.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "57" smd oval (at 0.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "unconnected-(U1-ETH1_TXD1-Pad57)") (pinfunction "ETH1_TXD1") (pintype "passive"))
    (pad "58" smd oval (at 1.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "unconnected-(U1-ETH1_TXD2-Pad58)") (pinfunction "ETH1_TXD2") (pintype "passive"))
    (pad "59" smd oval (at 2.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "unconnected-(U1-ETH1_TXD0-Pad59)") (pinfunction "ETH1_TXD0") (pintype "passive"))
    (pad "60" smd oval (at 3.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "unconnected-(U1-ETH1_TXCTL-Pad60)") (pinfunction "ETH1_TXCTL") (pintype "passive"))
    (pad "61" smd oval (at 4.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "unconnected-(U1-ETH1_TXD3-Pad61)") (pinfunction "ETH1_TXD3") (pintype "passive"))
    (pad "62" smd oval (at 5.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "unconnected-(U1-NC-Pad62)") (pinfunction "NC") (pintype "passive"))
    (pad "63" smd oval (at 6.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "64" smd oval (at 7.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "UART4_RX") (pinfunction "UART4_RX") (pintype "passive"))
    (pad "65" smd oval (at 8.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "UART4_TX") (pinfunction "UART4_TX") (pintype "passive"))
    (pad "66" smd oval (at 9.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "UART5_RX") (pinfunction "UART5_RX") (pintype "passive"))
    (pad "67" smd oval (at 10.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "UART5_TX") (pinfunction "UART5_TX") (pintype "passive"))
    (pad "68" smd oval (at 11.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "69" smd oval (at 12.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "Net-(U1-USB_D2_P)") (pinfunction "USB_D2_P") (pintype "passive"))
    (pad "70" smd oval (at 13.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "Net-(U1-USB_D2_N)") (pinfunction "USB_D2_N") (pintype "passive"))
    (pad "71" smd oval (at 14.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "72" smd oval (at 15.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "Net-(U1-USB_D1_P)") (pinfunction "USB_D1_P") (pintype "passive"))
    (pad "73" smd oval (at 16.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "Net-(U1-USB_D1_N)") (pinfunction "USB_D1_N") (pintype "passive"))
    (pad "74" smd oval (at 17.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "75" smd oval (at 18.5 -18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "76" smd oval (at 18.5 -17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "SAI1_MCLK_B") (pinfunction "I2S1_MCLK") (pintype "passive"))
    (pad "77" smd oval (at 18.5 -16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 153 "unconnected-(U1-I2S1_SDI-Pad77)") (pinfunction "I2S1_SDI") (pintype "passive"))
    (pad "78" smd oval (at 18.5 -15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "SAI1_SD_B") (pinfunction "I2S1_SDO") (pintype "passive"))
    (pad "79" smd oval (at 18.5 -14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "SAI1_SCK_B") (pinfunction "I2S1_CK") (pintype "passive"))
    (pad "80" smd oval (at 18.5 -13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "SAI1_FS_B") (pinfunction "I2S1_WS") (pintype "passive"))
    (pad "81" smd oval (at 18.5 -12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "SWCLK") (pinfunction "SWCLK") (pintype "passive"))
    (pad "82" smd oval (at 18.5 -11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "SWDIO") (pinfunction "SWDIO") (pintype "passive"))
    (pad "83" smd oval (at 18.5 -10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "BOOT2") (pinfunction "BOOT2") (pintype "passive"))
    (pad "84" smd oval (at 18.5 -9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "BOOT1") (pinfunction "BOOT1") (pintype "passive"))
    (pad "85" smd oval (at 18.5 -8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "BOOT0") (pinfunction "BOOT0") (pintype "passive"))
    (pad "86" smd oval (at 18.5 -7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "87" smd oval (at 18.5 -6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "unconnected-(U1-PI1-Pad87)") (pinfunction "PI1") (pintype "passive"))
    (pad "88" smd oval (at 18.5 -5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "NRST") (pinfunction "NRST") (pintype "passive"))
    (pad "89" smd oval (at 18.5 -4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 151 "unconnected-(U1-PWM2-Pad89)") (pinfunction "PWM2") (pintype "passive"))
    (pad "90" smd oval (at 18.5 -3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 150 "unconnected-(U1-PWM1-Pad90)") (pinfunction "PWM1") (pintype "passive"))
    (pad "91" smd oval (at 18.5 -2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "unconnected-(U1-ADC1_INP8-Pad91)") (pinfunction "ADC1_INP8") (pintype "passive"))
    (pad "92" smd oval (at 18.5 -1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "unconnected-(U1-ADC1_INP2-Pad92)") (pinfunction "ADC1_INP2") (pintype "passive"))
    (pad "93" smd oval (at 18.5 -0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "I2C1_SCL") (pinfunction "I2C3_SCL") (pintype "passive"))
    (pad "94" smd oval (at 18.5 0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "I2C1_SDA") (pinfunction "I2C3_SDA") (pintype "passive"))
    (pad "95" smd oval (at 18.5 1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "unconnected-(U1-FDCAN2_TX-Pad95)") (pinfunction "FDCAN2_TX") (pintype "passive"))
    (pad "96" smd oval (at 18.5 2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "unconnected-(U1-FDCAN2_RX-Pad96)") (pinfunction "FDCAN2_RX") (pintype "passive"))
    (pad "97" smd oval (at 18.5 3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 145 "unconnected-(U1-PI7-Pad97)") (pinfunction "PI7") (pintype "passive"))
    (pad "98" smd oval (at 18.5 4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 144 "unconnected-(U1-PH4-Pad98)") (pinfunction "PH4") (pintype "passive"))
    (pad "99" smd oval (at 18.5 5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "unconnected-(U1-PH5-Pad99)") (pinfunction "PH5") (pintype "passive"))
    (pad "100" smd oval (at 18.5 6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "101" smd oval (at 18.5 7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "LP_CLK") (pinfunction "PB10") (pintype "passive"))
    (pad "102" smd oval (at 18.5 8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "unconnected-(U1-PI3-Pad102)") (pinfunction "PI3") (pintype "passive"))
    (pad "103" smd oval (at 18.5 9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "unconnected-(U1-PI2-Pad103)") (pinfunction "PI2") (pintype "passive"))
    (pad "104" smd oval (at 18.5 10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "WIFI_RST") (pinfunction "PC13") (pintype "passive"))
    (pad "105" smd oval (at 18.5 11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "WIFI_UP") (pinfunction "PE10") (pintype "passive"))
    (pad "106" smd oval (at 18.5 12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "WIFI_CS") (pinfunction "PE8") (pintype "passive"))
    (pad "107" smd oval (at 18.5 13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "WIFI_IRQ") (pinfunction "PI0") (pintype "passive"))
    (pad "108" smd oval (at 18.5 14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "CTP_INT") (pinfunction "PA13") (pintype "passive"))
    (pad "109" smd oval (at 18.5 15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "CTP_RESET") (pinfunction "PG12") (pintype "passive"))
    (pad "110" smd oval (at 18.5 16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "MMC1_DETECT") (pinfunction "PD12") (pintype "passive"))
    (pad "111" smd oval (at 18.5 17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "unconnected-(U1-NC-Pad111)") (pinfunction "NC") (pintype "passive"))
    (pad "112" smd oval (at 18.5 18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "113" smd oval (at 17.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "MMC1_D0") (pinfunction "SDMMC1_D0") (pintype "passive"))
    (pad "114" smd oval (at 16.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "MMC1_CMD") (pinfunction "SDMMC1_CMD") (pintype "passive"))
    (pad "115" smd oval (at 15.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "MMC1_D1") (pinfunction "SDMMC1_D1") (pintype "passive"))
    (pad "116" smd oval (at 14.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "MMC1_D3") (pinfunction "SDMMC1_D3") (pintype "passive"))
    (pad "117" smd oval (at 13.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "MMC1_D2") (pinfunction "SDMMC1_D2") (pintype "passive"))
    (pad "118" smd oval (at 12.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "MMC1_CK") (pinfunction "SDMMC1_CK") (pintype "passive"))
    (pad "119" smd oval (at 11.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "120" smd oval (at 10.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "LCD_CLK") (pinfunction "LTDC_CLK") (pintype "passive"))
    (pad "121" smd oval (at 9.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "LCD_DATA_EN") (pinfunction "LTDC_DE") (pintype "passive"))
    (pad "122" smd oval (at 8.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "LCD_H_SYNC") (pinfunction "LTDC_HS") (pintype "passive"))
    (pad "123" smd oval (at 7.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "LCD_V_SYNC") (pinfunction "LTDC_VS") (pintype "passive"))
    (pad "124" smd oval (at 6.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "LCD_R2") (pinfunction "LTDC_R2") (pintype "passive"))
    (pad "125" smd oval (at 5.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "LCD_R3") (pinfunction "LTDC_R3") (pintype "passive"))
    (pad "126" smd oval (at 4.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "LCD_R7") (pinfunction "LTDC_R7") (pintype "passive"))
    (pad "127" smd oval (at 3.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "LCD_R0") (pinfunction "LTDC_R0") (pintype "passive"))
    (pad "128" smd oval (at 2.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 60 "LCD_R1") (pinfunction "LTDC_R1") (pintype "passive"))
    (pad "129" smd oval (at 1.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "LCD_R6") (pinfunction "LTDC_R6") (pintype "passive"))
    (pad "130" smd oval (at 0.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "LCD_R4") (pinfunction "LTDC_R4") (pintype "passive"))
    (pad "131" smd oval (at -0.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "LCD_R5") (pinfunction "LTDC_R5") (pintype "passive"))
    (pad "132" smd oval (at -1.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "LCD_G3") (pinfunction "LTDC_G3") (pintype "passive"))
    (pad "133" smd oval (at -2.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "LCD_G2") (pinfunction "LTDC_G2") (pintype "passive"))
    (pad "134" smd oval (at -3.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "LCD_G4") (pinfunction "LTDC_G4") (pintype "passive"))
    (pad "135" smd oval (at -4.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "LCD_G1") (pinfunction "LTDC_G1") (pintype "passive"))
    (pad "136" smd oval (at -5.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "LCD_G5") (pinfunction "LTDC_G5") (pintype "passive"))
    (pad "137" smd oval (at -6.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "LCD_G7") (pinfunction "LTDC_G7") (pintype "passive"))
    (pad "138" smd oval (at -7.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "LCD_G6") (pinfunction "LTDC_G6") (pintype "passive"))
    (pad "139" smd oval (at -8.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "LCD_G0") (pinfunction "LTDC_G0") (pintype "passive"))
    (pad "140" smd oval (at -9.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "LCD_B0") (pinfunction "LTDC_B0") (pintype "passive"))
    (pad "141" smd oval (at -10.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "LCD_B7") (pinfunction "LTDC_B7") (pintype "passive"))
    (pad "142" smd oval (at -11.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "LCD_B3") (pinfunction "LTDC_B3") (pintype "passive"))
    (pad "143" smd oval (at -12.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "LCD_B2") (pinfunction "LTDC_B2") (pintype "passive"))
    (pad "144" smd oval (at -13.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "LCD_B5") (pinfunction "LTDC_B5") (pintype "passive"))
    (pad "145" smd oval (at -14.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "LCD_B4") (pinfunction "LTDC_B4") (pintype "passive"))
    (pad "146" smd oval (at -15.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "LCD_B1") (pinfunction "LTDC_B1") (pintype "passive"))
    (pad "147" smd oval (at -16.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "LCD_B6") (pinfunction "LTDC_B6") (pintype "passive"))
    (pad "148" smd oval (at -17.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (model "MYC-YA151C-256N256D-65-C-T.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 104.48 69.21 180)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 6.25 0.5 90) (layer "B.SilkS") hide)
    (fp_text value "100uF" (at 4.75 0.75 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0 180) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 7 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0 180) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "STM32MP135_Dev_Board:QFN40P400X400X90-33N-D" (layer "B.Cu")
    (at 114.2 37.5875)
    (descr "WF200")
    (tags "Integrated Circuit")
    (property "Height" "0.9")
    (property "Manufacturer_Name" "Silicon Labs")
    (property "Manufacturer_Part_Number" "WF200DR")
    (property "Mouser Part Number" "634-WF200DR")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Silicon-Labs/WF200DR?qs=vEM7xhTegWiKlOdS7zwpkg%3D%3D")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "WF200 802.11bgn NCP, 4x4 QFN32")
    (clearance 0.17)
    (attr smd)
    (fp_text reference "U8" (at 0.1 3.6125 180) (layer "B.SilkS"))
    (fp_text value "WF200DR" (at 0 0 180) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -2 1.4 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "unconnected-(U8-GPIO{slash}FEM_1-Pad1)") (pinfunction "GPIO/FEM_1") (pintype "passive+no_connect"))
    (pad "2" smd rect (at -2 1 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "unconnected-(U8-GPIO{slash}FEM_2-Pad2)") (pinfunction "GPIO/FEM_2") (pintype "passive+no_connect"))
    (pad "3" smd rect (at -2 0.6 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "unconnected-(U8-GPIO{slash}FEM_3-Pad3)") (pinfunction "GPIO/FEM_3") (pintype "passive+no_connect"))
    (pad "4" smd rect (at -2 0.2 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "unconnected-(U8-GPIO{slash}FEM_4-Pad4)") (pinfunction "GPIO/FEM_4") (pintype "passive+no_connect"))
    (pad "5" smd rect (at -2 -0.2 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "unconnected-(U8-GPIO{slash}FEM_PDET-Pad5)") (pinfunction "GPIO/FEM_PDET") (pintype "passive+no_connect"))
    (pad "6" smd rect (at -2 -0.6 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "unconnected-(U8-RESERVE_2-Pad6)") (pinfunction "RESERVE_2") (pintype "passive+no_connect"))
    (pad "7" smd rect (at -2 -1 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(U8-XTAL_I)") (pinfunction "XTAL_I") (pintype "passive"))
    (pad "8" smd rect (at -2 -1.4 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(U8-XTAL_O)") (pinfunction "XTAL_O") (pintype "passive"))
    (pad "9" smd rect (at -1.4 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "+1V8") (pinfunction "VDD_RF") (pintype "passive"))
    (pad "10" smd rect (at -1 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "11" smd rect (at -0.6 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(U8-RF_1)") (pinfunction "RF_1") (pintype "passive"))
    (pad "12" smd rect (at -0.2 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "Net-(U8-RF_2)") (pinfunction "RF_2") (pintype "passive"))
    (pad "13" smd rect (at 0.2 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "+3V3") (pinfunction "VDD_PA") (pintype "passive"))
    (pad "14" smd rect (at 0.6 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "RESERVE_1") (pintype "passive"))
    (pad "15" smd rect (at 1 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "WIFI_RST") (pinfunction "RESETN") (pintype "passive"))
    (pad "16" smd rect (at 1.4 -2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "WIFI_UP") (pinfunction "GPIO/WUP") (pintype "passive"))
    (pad "17" smd rect (at 2 -1.4 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "unconnected-(U8-GPIO{slash}FEM_5-Pad17)") (pinfunction "GPIO/FEM_5") (pintype "passive+no_connect"))
    (pad "18" smd rect (at 2 -1 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "unconnected-(U8-GPIO{slash}FEM_6-Pad18)") (pinfunction "GPIO/FEM_6") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2 -0.6 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "unconnected-(U8-GPIO{slash}PTA_TX_CONF-Pad19)") (pinfunction "GPIO/PTA_TX_CONF") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2 -0.2 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "unconnected-(U8-GPIO{slash}PTA_RF_ACT-Pad20)") (pinfunction "GPIO/PTA_RF_ACT") (pintype "passive+no_connect"))
    (pad "21" smd rect (at 2 0.2 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "unconnected-(U8-GPIO{slash}PTA_STATUS-Pad21)") (pinfunction "GPIO/PTA_STATUS") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2 0.6 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "unconnected-(U8-GPIO{slash}PTA_FREQ-Pad22)") (pinfunction "GPIO/PTA_FREQ") (pintype "passive+no_connect"))
    (pad "23" smd rect (at 2 1 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "LP_CLK") (pinfunction "GPIO/LP_CLK") (pintype "passive"))
    (pad "24" smd rect (at 2 1.4 270) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "unconnected-(U8-GPIO{slash}WIRQ-Pad24)") (pinfunction "GPIO/WIRQ") (pintype "passive+no_connect"))
    (pad "25" smd rect (at 1.4 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "+1V8") (pinfunction "VDD_DIG") (pintype "passive"))
    (pad "26" smd rect (at 1 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "SPI5_SCK") (pinfunction "SDIO_CLK/_SPI_CLK") (pintype "passive"))
    (pad "27" smd rect (at 0.6 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "SPI5_MOSI") (pinfunction "SDIO_CMD/_SPI_MOSI") (pintype "passive"))
    (pad "28" smd rect (at 0.2 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "SPI5_MISO") (pinfunction "SDIO_DAT0/_SPI_MISO") (pintype "passive"))
    (pad "29" smd rect (at -0.2 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "WIFI_IRQ") (pinfunction "SDIO_DAT1_/_SPI_WIRQ") (pintype "passive"))
    (pad "30" smd rect (at -0.6 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "SDIO_DAT2/_HIF_SEL") (pintype "passive"))
    (pad "31" smd rect (at -1 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "WIFI_CS") (pinfunction "SDIO_DAT3/_SPI_CSN") (pintype "passive"))
    (pad "32" smd rect (at -1.4 2) (size 0.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "+1V8") (pinfunction "VDD_IO") (pintype "passive"))
    (pad "33" smd rect (at 0 0) (size 2.8 2.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (model "WF200DR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 40.9 52.85 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 0 3) (layer "B.SilkS"))
    (fp_text value "LED-" (at 0.25 1.75) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 129 "Net-(J7-Pin_1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 117.03 72.51 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 7.09 0 90) (layer "B.SilkS"))
    (fp_text value "5K1" (at 3.75 0 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 51 "Net-(J4-CC2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (layer "B.Cu")
    (at 108.9 38.75 180)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "Four pin crystal, GND on pins 2 and 4")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr smd)
    (fp_text reference "Y1" (at 0.1 3.65) (layer "B.SilkS"))
    (fp_text value "38.4MHz" (at 0.6 2.35) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -1.1 -0.85 180) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(U8-XTAL_I)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 -0.85 180) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 0.85 180) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(U8-XTAL_O)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 0.85 180) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 37.25 43.75 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdmmc.kicad_sch")
    (property "Sheetname" "SDMMC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at -19.2 26.3 -360) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 7.4 37.25 -360) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -360) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 55.75 66.25 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP135_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 3.75 0 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 1.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 139 "Net-(U1-USB_D1_N)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 35 "USB1_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:Texas_DRT-3" (layer "B.Cu")
    (at 115.075 68.9 90)
    (descr "Texas Instrument DRT-3 1x0.8mm Pitch 0.7mm http://www.ti.com/lit/ds/symlink/tpd2eusb30.pdf")
    (tags "DRT-3 1x0.8mm Pitch 0.7mm")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Debug")
    (property "ki_description" "2-Channel ESD Protection for Super-Speed USB 3.0 Interface, DRT-3")
    (property "ki_keywords" "ESD protection USB 3.0")
    (attr smd)
    (fp_text reference "U4" (at 1.5 -0.375 180) (layer "B.SilkS"))
    (fp_text value "TPD2EUSB30" (at -0.1 -1.675 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "B.Fab"))
    (pad "1" smd rect (at -0.35 -0.425 90) (size 0.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "/Debug/USB_P") (pinfunction "D+") (pintype "passive"))
    (pad "2" smd rect (at 0.35 -0.425 90) (size 0.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "/Debug/USB_N") (pinfunction "D-") (pintype "passive"))
    (pad "3" smd rect (at 0 0.425 90) (size 0.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "Earth") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Texas_DRT-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 108.7 29.3 -90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 3 90) (layer "B.SilkS"))
    (fp_text value "GND" (at -0.25 1.75 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 270) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 108.7 32.3 -90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "WiFi.kicad_sch")
    (property "Sheetname" "WiFi")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 2.998 90) (layer "B.SilkS"))
    (fp_text value "1V8" (at 0 1.75 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 270) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 6 "+1V8") (pinfunction "1") (pintype "passive"))
  )
  (gr_line (start 126 90) (end 20 90)
    (layer "Edge.Cuts"))
  (gr_line (start 20 90) (end 20 20)
    (layer "Edge.Cuts"))
  (gr_line (start 20 20) (end 126 20)
    (layer "Edge.Cuts"))
  (gr_line (start 126 20) (end 126 90)
    (layer "Edge.Cuts"))
  (gr_text "https://github.com/BasicCode" (at 91.45 68.4) (layer "B.SilkS" knockout))
  (gr_text "REV A" (at 91.4 71.1) (layer "B.SilkS"))
  (gr_text "STM32MP135 Dev Board" (at 91.35 70.1) (layer "B.SilkS"))
  (gr_text "SD CARD" (at 50.8 30.6 270) (layer "B.SilkS" knockout))
  (gr_text "AUDIO" (at 45.4 89.4 -90) (layer "B.SilkS" knockout))
  (gr_text "LCD FPC" (at 69 52) (layer "User.3"))
  (gr_text "CTP FPC" (at 118 58 90) (layer "User.3"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 20 90) (xy 73 90))
    (height 11)
    (gr_text "53.0000 mm" (at 46.5 99.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 126 20) (xy 126 90))
    (height -17)
    (gr_text "70.0000 mm" (at 145 55 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 126 20) (xy 126 55))
    (height -14)
    (gr_text "35.0000 mm" (at 138.85 37.5 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 20 90) (xy 126 90))
    (height 14)
    (gr_text "106.0000 mm" (at 73 106) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 20 20)
        (xy 126 20)
        (xy 126 90)
        (xy 20 90)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu") (name "wifi Antenna") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 126 20)
        (xy 110.4 20)
        (xy 110.4 26.1)
        (xy 126 26.1)
      )
    )
  )
)
