(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 36)
    (no_connects 0)
    (area 109.195 90.094999 156.774763 111.835001)
    (thickness 1.6)
    (drawings 9)
    (tracks 31)
    (zones 0)
    (modules 13)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57ECB639)
    (at 120.65 100.965 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value C_Small (at 8.255 3.175 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57ECB62E)
    (at 127 102.87 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value C_Small (at -2.54 -12.7 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57ECB62B)
    (at 139.065 102.87 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 4.445 0 360) (layer F.SilkS))
    (fp_text value C_Small (at 0 -12.065 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57ECB637)
    (at 145.415 100.965 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value C_Small (at -7.62 2.54 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57ECB615)
    (at 121.92 100.965 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 9.525 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57ECB625)
    (at 127 104.14 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at -0.635 -12.065 90) (layer F.SilkS))
    (fp_text value C_Small (at -0.635 -12.065 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57ECB630)
    (at 139.065 101.6 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 1.905 -12.7 270) (layer F.SilkS))
    (fp_text value C_Small (at 0.635 -12.065 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57ECB63E)
    (at 146.685 100.965 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -5.715 -3.175 180) (layer F.SilkS))
    (fp_text value C_Small (at -6.35 1.905 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_6,5x13mm_Vertical (layer F.Cu) (tedit 57ECB5ED)
    (at 118.11 97.79)
    (descr "Toroid, Coil, Choke,  6,5mm x 13mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke,  6,5mm x 13mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L1 (at 1.905 -3.175) (layer F.SilkS))
    (fp_text value L_Small (at -5.715 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.604 -0.508) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 6.604 -6.096) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_6,5x13mm_Vertical (layer F.Cu) (tedit 57ECB5F4)
    (at 129.54 98.425 270)
    (descr "Toroid, Coil, Choke,  6,5mm x 13mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke,  6,5mm x 13mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L2 (at 11.43 -3.175 360) (layer F.SilkS))
    (fp_text value L_Small (at 8.255 16.51 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.604 -0.508 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 6.604 -6.096 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_6,5x13mm_Vertical (layer F.Cu) (tedit 57ECB60A)
    (at 134.62 97.79)
    (descr "Toroid, Coil, Choke,  6,5mm x 13mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke,  6,5mm x 13mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L3 (at 11.43 -3.175) (layer F.SilkS))
    (fp_text value L_Small (at 19.05 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.604 -0.508) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 6.604 -6.096) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 57ECB7F9)
    (at 120.65 107.315)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P1 (at -7.62 -1.905) (layer F.SilkS))
    (fp_text value BNC (at -6.985 -4.445) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 smd rect (at 2.54 1.778) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at 0 1.524) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -2.54 1.778) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 2.54 1.778) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -2.54 1.778) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 57ECB7F7)
    (at 145.415 107.315)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P2 (at 6.35 -1.905) (layer F.SilkS))
    (fp_text value BNC (at 6.35 -3.175) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 smd rect (at 2.54 1.778) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at 0 1.524) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -2.54 1.778) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 2.54 1.778) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -2.54 1.778) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text @SmittyHalibut (at 132.715 95.885) (layer B.SilkS))
  (gr_text "HPF v1.0a" (at 132.715 92.075) (layer B.SilkS))
  (gr_text "BY-NC-SA 2016 Mark Smith" (at 132.715 93.98) (layer B.SilkS))
  (gr_line (start 149.225 111.76) (end 149.86 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.225 90.17) (end 149.86 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 90.17) (end 149.86 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.205 90.17) (end 149.225 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.205 111.76) (end 116.205 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.225 111.76) (end 116.205 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.205 90.17) (xy 149.86 90.17) (xy 149.86 111.76) (xy 116.205 111.76)
      )
    )
  )
)
