(kicad_pcb (version 3) (host pcbnew "(22-Jun-2014 BZR 4027)-stable")
  (general
    (links 239)
    (no_connects 0)
    (area 6.990999 16.706999 89.458001 81.708)
    (thickness 1.6)
    (drawings 4)
    (tracks 754)
    (zones 0)
    (modules 70)
    (nets 73)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.22)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.16)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.51)
    (via_drill 0.33)
    (via_min_size 0.51)
    (via_min_drill 0.33)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 0.9)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 284196865)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /A33VDD)
  (net 2 /AVDD)
  (net 3 /B_0)
  (net 4 /B_1)
  (net 5 /B_2)
  (net 6 /B_3)
  (net 7 /B_4)
  (net 8 /B_5)
  (net 9 /B_6)
  (net 10 /B_7)
  (net 11 /CLK27)
  (net 12 /DVDD)
  (net 13 /FIDOUT)
  (net 14 /G_0)
  (net 15 /G_1)
  (net 16 /G_2)
  (net 17 /G_3)
  (net 18 /G_4)
  (net 19 /G_5)
  (net 20 /G_6)
  (net 21 /G_7)
  (net 22 /HSOUT)
  (net 23 /IOVDD)
  (net 24 /PCLK)
  (net 25 /PLL_VDD)
  (net 26 /RESET)
  (net 27 /RGB1_B)
  (net 28 /RGB1_G)
  (net 29 /RGB1_R)
  (net 30 /RGB1_S)
  (net 31 /RGB2_B)
  (net 32 /RGB2_G)
  (net 33 /RGB2_HS)
  (net 34 /RGB2_HS_B)
  (net 35 /RGB2_R)
  (net 36 /RGB2_VS)
  (net 37 /RGB2_VS_B)
  (net 38 /RGB3_B)
  (net 39 /RGB3_G)
  (net 40 /RGB3_R)
  (net 41 /R_0)
  (net 42 /R_1)
  (net 43 /R_2)
  (net 44 /R_3)
  (net 45 /R_4)
  (net 46 /R_5)
  (net 47 /R_6)
  (net 48 /R_7)
  (net 49 /SCL)
  (net 50 /SDA)
  (net 51 /VSOUT)
  (net 52 GND)
  (net 53 N-0000036)
  (net 54 N-0000044)
  (net 55 N-0000045)
  (net 56 N-0000046)
  (net 57 N-0000047)
  (net 58 N-0000054)
  (net 59 N-0000055)
  (net 60 N-0000057)
  (net 61 N-0000058)
  (net 62 N-0000060)
  (net 63 N-0000061)
  (net 64 N-0000062)
  (net 65 N-0000071)
  (net 66 N-0000072)
  (net 67 N-0000073)
  (net 68 N-0000088)
  (net 69 N-0000089)
  (net 70 N-0000090)
  (net 71 N-0000095)
  (net 72 N-0000096)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.22)
    (via_dia 0.51)
    (via_drill 0.33)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net /HSOUT)
    (add_net /RGB2_HS)
    (add_net /RGB2_HS_B)
    (add_net /RGB2_VS)
    (add_net /RGB2_VS_B)
    (add_net N-0000036)
    (add_net N-0000044)
    (add_net N-0000045)
    (add_net N-0000046)
    (add_net N-0000047)
    (add_net N-0000054)
    (add_net N-0000055)
    (add_net N-0000057)
    (add_net N-0000058)
    (add_net N-0000060)
    (add_net N-0000061)
    (add_net N-0000062)
    (add_net N-0000071)
    (add_net N-0000072)
    (add_net N-0000073)
    (add_net N-0000089)
    (add_net N-0000090)
    (add_net N-0000095)
    (add_net N-0000096)
  )
  (net_class 75ohm_vid ""
    (clearance 0.3)
    (trace_width 0.64)
    (via_dia 0.6)
    (via_drill 0.35)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /RGB1_B)
    (add_net /RGB1_G)
    (add_net /RGB1_R)
    (add_net /RGB1_S)
    (add_net /RGB2_B)
    (add_net /RGB2_G)
    (add_net /RGB2_R)
    (add_net /RGB3_B)
    (add_net /RGB3_G)
    (add_net /RGB3_R)
  )
  (net_class FAT_power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 0.33)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net N-0000088)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.55)
    (via_drill 0.35)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /A33VDD)
    (add_net /AVDD)
    (add_net /DVDD)
    (add_net /IOVDD)
    (add_net /PLL_VDD)
    (add_net GND)
  )
  (net_class digi_hs ""
    (clearance 0.18)
    (trace_width 0.18)
    (via_dia 0.51)
    (via_drill 0.33)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /B_0)
    (add_net /B_1)
    (add_net /B_2)
    (add_net /B_3)
    (add_net /B_4)
    (add_net /B_5)
    (add_net /B_6)
    (add_net /B_7)
    (add_net /CLK27)
    (add_net /FIDOUT)
    (add_net /G_0)
    (add_net /G_1)
    (add_net /G_2)
    (add_net /G_3)
    (add_net /G_4)
    (add_net /G_5)
    (add_net /G_6)
    (add_net /G_7)
    (add_net /PCLK)
    (add_net /RESET)
    (add_net /R_0)
    (add_net /R_1)
    (add_net /R_2)
    (add_net /R_3)
    (add_net /R_4)
    (add_net /R_5)
    (add_net /R_6)
    (add_net /R_7)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VSOUT)
  )
  (module SCART_CONN (layer F.Cu) (tedit 54120F1E)
    (at 64.77 76.708)
    (fp_text reference P1 (at -24.84 -8.61) (layer F.SilkS))
    (fp_text value SCART-F (at -11.87 -8.61) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 3 thru_hole circle (at -1.905 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 4 thru_hole circle (at -3.81 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 5 thru_hole circle (at -5.715 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 6 thru_hole circle (at -7.62 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 7 thru_hole circle (at -9.525 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 27 /RGB1_B)
    )
    (pad 8 thru_hole circle (at -11.43 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 9 thru_hole circle (at -13.335 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 10 thru_hole circle (at -15.24 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 11 thru_hole circle (at -17.145 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 28 /RGB1_G)
    )
    (pad 12 thru_hole circle (at -19.05 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 13 thru_hole circle (at -20.955 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 20 thru_hole circle (at -34.29 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 30 /RGB1_S)
    )
    (pad 15 thru_hole circle (at -24.765 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 29 /RGB1_R)
    )
    (pad 14 thru_hole circle (at -22.86 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 17 thru_hole circle (at -28.575 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 16 thru_hole circle (at -26.67 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 19 thru_hole circle (at -32.385 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 18 thru_hole circle (at -30.48 0) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 21 thru_hole circle (at -36.195 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 1 thru_hole circle (at 1.905 -5.08) (size 2.2 2.2) (drill 1.3)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" thru_hole circle (at -43.54 2.2) (size 5 5) (drill 5)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" thru_hole circle (at 9.25 2.2) (size 5 5) (drill 5)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module 1pin (layer F.Cu) (tedit 5411F6E9)
    (at 15.748 76.708)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS))
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 4)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module 1pin (layer F.Cu) (tedit 5411F6E3)
    (at 15.748 21.082)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS))
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 4)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module 1pin (layer F.Cu) (tedit 5411F6DD)
    (at 73.406 21.844)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS))
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 4)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 43.434 38.862 90)
    (attr smd)
    (fp_text reference C37 (at 0 0 360) (layer B.SilkS))
    (fp_text value 1u (at -1.651 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /DVDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 37.338 38.608 270)
    (attr smd)
    (fp_text reference C34 (at 0 0 540) (layer B.SilkS))
    (fp_text value 1u (at -1.651 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer B.Cu) (tedit 4ECF78EF)
    (at 40.386 38.862 90)
    (attr smd)
    (fp_text reference U8 (at 2.19964 0.29972 360) (layer B.SilkS))
    (fp_text value TLV71209DBV (at 0 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 -1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 3 smd rect (at 0.9525 -1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 5 smd rect (at -0.9525 1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /DVDD)
    )
    (pad 2 smd rect (at 0 -1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (pad 4 smd rect (at 0.9525 1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VGA_CONN (layer F.Cu) (tedit 540F4180)
    (at 18.796 56.646 270)
    (fp_text reference J1 (at 13.458 -5.08 270) (layer F.SilkS))
    (fp_text value VGA (at 10.918 -5.08 270) (layer F.SilkS))
    (pad 8 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 9 thru_hole circle (at -2.29 0 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 10 thru_hole circle (at -4.58 0 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 1 thru_hole circle (at 3.44 -2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 35 /RGB2_R)
    )
    (pad 2 thru_hole circle (at 1.15 -2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 32 /RGB2_G)
    )
    (pad 3 thru_hole circle (at -1.14 -2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 31 /RGB2_B)
    )
    (pad 4 thru_hole circle (at -3.43 -2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 5 thru_hole circle (at -5.72 -2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 6 thru_hole circle (at 4.58 0 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 7 thru_hole circle (at 2.29 0 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 11 thru_hole circle (at 3.44 2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 12 thru_hole circle (at 1.15 2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 13 thru_hole circle (at -1.14 2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 33 /RGB2_HS)
    )
    (pad 14 thru_hole circle (at -3.43 2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 36 /RGB2_VS)
    )
    (pad 15 thru_hole circle (at -5.72 2.54 270) (size 1.6 1.6) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" thru_hole circle (at 11.62 0 270) (size 3.2 3.2) (drill 3.2)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" thru_hole circle (at -13.38 0 270) (size 3.2 3.2) (drill 3.2)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module SOT23-5 (layer B.Cu) (tedit 4ECF78EF)
    (at 32.766 47.498 90)
    (attr smd)
    (fp_text reference U7 (at 2.19964 0.29972 360) (layer B.SilkS))
    (fp_text value TLV71209DBV (at 0 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 -1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 3 smd rect (at 0.9525 -1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 5 smd rect (at -0.9525 1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 25 /PLL_VDD)
    )
    (pad 2 smd rect (at 0 -1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (pad 4 smd rect (at 0.9525 1.27 90) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT23-5 (layer B.Cu) (tedit 4ECF78EF)
    (at 23.622 67.564 180)
    (attr smd)
    (fp_text reference U6 (at 2.19964 0.29972 450) (layer B.SilkS))
    (fp_text value TLV71209DBV (at 0 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 -1.27 180) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 3 smd rect (at 0.9525 -1.27 180) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 5 smd rect (at -0.9525 1.27 180) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD)
    )
    (pad 2 smd rect (at 0 -1.27 180) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (pad 4 smd rect (at 0.9525 1.27 180) (size 0.508 0.762)
      (layers B.Cu B.Paste B.Mask)
    )
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMA_CONN (layer F.Cu) (tedit 5404DBE5)
    (at 69.596 60.198)
    (tags "SMA Connector")
    (fp_text reference P3 (at 0 5.08) (layer F.SilkS))
    (fp_text value SMA_PCLK (at 1.27 7.62) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 1.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 24 /PCLK)
    )
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.7 2.7) (drill 1.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.7 2.7) (drill 1.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.7 2.7) (drill 1.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.7 2.7) (drill 1.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (model connectors/sma.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 -90))
    )
  )
  (module SM1206POL (layer B.Cu) (tedit 42806E4C)
    (at 60.706 52.832)
    (attr smd)
    (fp_text reference C29 (at 0 0) (layer B.SilkS))
    (fp_text value 2.2u (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers B.Cu B.Paste B.Mask)
      (net 1 /A33VDD)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd/chip_cms_pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206POL (layer B.Cu) (tedit 42806E4C)
    (at 58.166 47.752 90)
    (attr smd)
    (fp_text reference C30 (at 0 0 90) (layer B.SilkS))
    (fp_text value 2.2u (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /IOVDD)
    )
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd/chip_cms_pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 45.72 42.926 180)
    (attr smd)
    (fp_text reference C28 (at 0 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /IOVDD)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 41.148 61.468 90)
    (attr smd)
    (fp_text reference C5 (at 0 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 28 /RGB1_G)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 59 N-0000055)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 43.688 55.372)
    (attr smd)
    (fp_text reference C8 (at 0 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 35.814 57.404)
    (attr smd)
    (fp_text reference C12 (at 0 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 32 /RGB2_G)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 67 N-0000073)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 29.21 55.626)
    (attr smd)
    (fp_text reference C13 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1n (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 70 N-0000090)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 34.036 55.626)
    (attr smd)
    (fp_text reference C15 (at 0 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 39 /RGB3_G)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 66 N-0000072)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 34.036 54.102)
    (attr smd)
    (fp_text reference C16 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1n (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 39 /RGB3_G)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 69 N-0000089)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 29.21 53.594)
    (attr smd)
    (fp_text reference C17 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10n (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 65 N-0000071)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 50.292 55.372)
    (attr smd)
    (fp_text reference C9 (at 0 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 39.116 52.324 270)
    (attr smd)
    (fp_text reference C18 (at 0 0 540) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 1 /A33VDD)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 35.814 47.498 90)
    (attr smd)
    (fp_text reference C23 (at 0 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 25 /PLL_VDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 44.196 41.402)
    (attr smd)
    (fp_text reference C27 (at 0 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /DVDD)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 23.622 64.516 180)
    (attr smd)
    (fp_text reference C35 (at 0 0 450) (layer B.SilkS))
    (fp_text value 1u (at -1.651 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 2 /AVDD)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 51.308 42.926 180)
    (attr smd)
    (fp_text reference C26 (at 0 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /IOVDD)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 54.102 55.372 90)
    (attr smd)
    (fp_text reference C14 (at 0 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /IOVDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 54.61 50.292 90)
    (attr smd)
    (fp_text reference C21 (at 0 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 12 /DVDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 54.61 47.498 90)
    (attr smd)
    (fp_text reference C22 (at 0 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /IOVDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 33.528 49.53)
    (attr smd)
    (fp_text reference C20 (at 0 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-0000045)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 56 N-0000046)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 35.052 51.054 180)
    (attr smd)
    (fp_text reference C19 (at 0 0 270) (layer F.SilkS))
    (fp_text value 4.7n (at -1.651 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 57 N-0000047)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-0000045)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 28.956 49.276 270)
    (attr smd)
    (fp_text reference C24 (at 0 0 360) (layer F.SilkS))
    (fp_text value 1n (at -1.651 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 53 N-0000036)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 30.226 41.148 180)
    (attr smd)
    (fp_text reference C25 (at 0 0 450) (layer B.SilkS))
    (fp_text value 10n (at -1.651 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /IOVDD)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 38.862 61.468 90)
    (attr smd)
    (fp_text reference C11 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1n (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 30 /RGB1_S)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 71 N-0000095)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 67.056 49.53 270)
    (attr smd)
    (fp_text reference C38 (at 0 0 540) (layer B.SilkS))
    (fp_text value 1u (at -1.651 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 61.722 46.736)
    (attr smd)
    (fp_text reference C31 (at 0 0 270) (layer B.SilkS))
    (fp_text value 470p (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 72 N-0000096)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 46.482 61.468 90)
    (attr smd)
    (fp_text reference C6 (at 0 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 29 /RGB1_R)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 64 N-0000062)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 44.196 61.468 90)
    (attr smd)
    (fp_text reference C3 (at 0 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 35 /RGB2_R)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 63 N-0000061)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 42.672 60.198)
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 40 /RGB3_R)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 62 N-0000060)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 29.718 47.244 270)
    (attr smd)
    (fp_text reference C33 (at 0 0 540) (layer B.SilkS))
    (fp_text value 1u (at -1.651 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 51.562 63.246 90)
    (attr smd)
    (fp_text reference C7 (at 0 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 27 /RGB1_B)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 61 N-0000058)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer F.Cu) (tedit 5051B1EC)
    (at 48.768 61.468 90)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at -1.651 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 31 /RGB2_B)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 58 N-0000054)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 48.768 60.96 180)
    (attr smd)
    (fp_text reference C2 (at 0 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 38 /RGB3_B)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 60 N-0000057)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 35.814 47.498 90)
    (attr smd)
    (fp_text reference C36 (at 0 0 360) (layer B.SilkS))
    (fp_text value 1u (at -1.651 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 25 /PLL_VDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 23.368 70.612)
    (attr smd)
    (fp_text reference C32 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1u (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603_Capa (layer B.Cu) (tedit 5051B1EC)
    (at 46.99 55.372)
    (attr smd)
    (fp_text reference C10 (at 0 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at -1.651 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 1 /A33VDD)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 26.67 48.514 180)
    (attr smd)
    (fp_text reference R12 (at 0 0 180) (layer F.SilkS))
    (fp_text value 330 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 53 N-0000036)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 36 /RGB2_VS)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 45.212 36.83 90)
    (attr smd)
    (fp_text reference R14 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 49 /SCL)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 39.37 41.656 270)
    (attr smd)
    (fp_text reference R13 (at 0 0 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 50 /SDA)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 48.26 36.322 180)
    (attr smd)
    (fp_text reference R15 (at 0 0 180) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 26 /RESET)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 40.132 64.008 180)
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 28 /RGB1_G)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 36.068 49.53)
    (attr smd)
    (fp_text reference R11 (at 0 0) (layer F.SilkS))
    (fp_text value 1.5k (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 56 N-0000046)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 54 N-0000044)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 46.228 64.262)
    (attr smd)
    (fp_text reference R7 (at 0 0) (layer F.SilkS))
    (fp_text value 75 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 29 /RGB1_R)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 42.926 63.5 180)
    (attr smd)
    (fp_text reference R4 (at 0 0 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 35 /RGB2_R)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 4E43A3D1)
    (at 41.148 58.42 180)
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer B.SilkS))
    (fp_text value 75 (at 0 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 40 /RGB3_R)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 36.576 62.484 180)
    (attr smd)
    (fp_text reference R3 (at 0 0 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 30 /RGB1_S)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 4E43A3D1)
    (at 31.242 55.626)
    (attr smd)
    (fp_text reference R10 (at 0 0) (layer B.SilkS))
    (fp_text value 75 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 39 /RGB3_G)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 54.102 64.262)
    (attr smd)
    (fp_text reference R8 (at 0 0) (layer F.SilkS))
    (fp_text value 75 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 27 /RGB1_B)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 48.768 64.262 180)
    (attr smd)
    (fp_text reference R5 (at 0 0 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 31 /RGB2_B)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 4E43A3D1)
    (at 33.528 58.674 270)
    (attr smd)
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS))
    (fp_text value 75 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 32 /RGB2_G)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer B.Cu) (tedit 4E43A3D1)
    (at 51.054 60.452 90)
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer B.SilkS))
    (fp_text value 75 (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 38 /RGB3_B)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module sc70-6 (layer F.Cu) (tedit 490474FF)
    (at 30.226 46.736 270)
    (descr SC70-6)
    (attr smd)
    (fp_text reference U4 (at 0 -0.2794 270) (layer F.SilkS))
    (fp_text value SN74LVC2G17 (at 0 0.3556 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604)
      (layers F.Cu F.Paste F.Mask)
      (net 33 /RGB2_HS)
    )
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604)
      (layers F.Cu F.Paste F.Mask)
      (net 53 N-0000036)
    )
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604)
      (layers F.Cu F.Paste F.Mask)
      (net 37 /RGB2_VS_B)
    )
    (pad 6 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604)
      (layers F.Cu F.Paste F.Mask)
      (net 34 /RGB2_HS_B)
    )
    (pad 5 smd rect (at 0 -1.016 270) (size 0.4064 0.6604)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (model smd/smd_transistors/sc70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSOP_8 (layer B.Cu) (tedit 48A96A8A)
    (at 62.992 49.53 90)
    (fp_text reference U5 (at 0 -0.635 90) (layer B.SilkS))
    (fp_text value MIC5210 (at 0 0.762 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.97536 -2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 1 /A33VDD)
    )
    (pad 2 smd rect (at -0.32512 -2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 52 GND)
    )
    (pad 3 smd rect (at 0.32512 -2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 23 /IOVDD)
    )
    (pad 4 smd rect (at 0.97536 -2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 72 N-0000096)
    )
    (pad 5 smd rect (at 0.97536 2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 6 smd rect (at 0.32512 2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 7 smd rect (at -0.32512 2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (pad 8 smd rect (at -0.97536 2.159 90) (size 0.381 1.27)
      (layers B.Cu B.Paste B.Mask)
      (net 68 N-0000088)
    )
    (model smd/MSOP_8.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_20X2 (layer F.Cu) (tedit 5031D84E)
    (at 83.312 48.26 270)
    (descr "Double rangee de contacts 2 x 12 pins")
    (tags CONN)
    (fp_text reference P2 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value CONN_20X2 (at 0 3.81 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 41 /R_0)
    )
    (pad 2 thru_hole circle (at -24.13 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 42 /R_1)
    )
    (pad 11 thru_hole circle (at -11.43 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 4 thru_hole circle (at -21.59 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 44 /R_3)
    )
    (pad 13 thru_hole circle (at -8.89 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 /G_2)
    )
    (pad 6 thru_hole circle (at -19.05 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 46 /R_5)
    )
    (pad 15 thru_hole circle (at -6.35 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 18 /G_4)
    )
    (pad 8 thru_hole circle (at -16.51 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 48 /R_7)
    )
    (pad 17 thru_hole circle (at -3.81 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 20 /G_6)
    )
    (pad 10 thru_hole circle (at -13.97 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 /G_1)
    )
    (pad 19 thru_hole circle (at -1.27 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 /B_0)
    )
    (pad 12 thru_hole circle (at -11.43 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 21 thru_hole circle (at 1.27 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 5 /B_2)
    )
    (pad 14 thru_hole circle (at -8.89 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 17 /G_3)
    )
    (pad 23 thru_hole circle (at 3.81 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /B_4)
    )
    (pad 16 thru_hole circle (at -6.35 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 19 /G_5)
    )
    (pad 25 thru_hole circle (at 6.35 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 9 /B_6)
    )
    (pad 18 thru_hole circle (at -3.81 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 21 /G_7)
    )
    (pad 27 thru_hole circle (at 8.89 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 20 thru_hole circle (at -1.27 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 /B_1)
    )
    (pad 29 thru_hole circle (at 11.43 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 22 thru_hole circle (at 1.27 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /B_3)
    )
    (pad 31 thru_hole circle (at 13.97 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 50 /SDA)
    )
    (pad 24 thru_hole circle (at 3.81 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 8 /B_5)
    )
    (pad 26 thru_hole circle (at 6.35 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 /B_7)
    )
    (pad 33 thru_hole circle (at 16.51 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 49 /SCL)
    )
    (pad 28 thru_hole circle (at 8.89 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 26 /RESET)
    )
    (pad 32 thru_hole circle (at 13.97 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 34 thru_hole circle (at 16.51 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 36 thru_hole circle (at 19.05 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 38 thru_hole circle (at 21.59 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 35 thru_hole circle (at 19.05 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 22 /HSOUT)
    )
    (pad 37 thru_hole circle (at 21.59 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 51 /VSOUT)
    )
    (pad 3 thru_hole circle (at -21.59 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 43 /R_2)
    )
    (pad 5 thru_hole circle (at -19.05 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 45 /R_4)
    )
    (pad 7 thru_hole circle (at -16.51 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 47 /R_6)
    )
    (pad 9 thru_hole circle (at -13.97 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 /G_0)
    )
    (pad 39 thru_hole circle (at 24.13 1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 /FIDOUT)
    )
    (pad 40 thru_hole circle (at 24.13 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 30 thru_hole circle (at 11.43 -1.27 270) (size 1.524 1.524) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (model pin_array/pins_array_20x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1pin (layer F.Cu) (tedit 5411F6D3)
    (at 74.168 72.136)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS))
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 4 4) (drill 4)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module TQFP_100-thermal (layer F.Cu) (tedit 5411F948)
    (at 46.736 50.292 180)
    (descr "Module SMD TQFP 100 Pins")
    (tags "CMS TQFP")
    (attr smd)
    (fp_text reference U1 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value TVP7002PZP (at 0 2.54 180) (layer F.SilkS))
    (pad 100 smd rect (at 7.747 -5.9944 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 67 N-0000073)
    )
    (pad 76 smd rect (at 7.747 5.9944 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 77 smd rect (at 7.747 5.4864 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 78 smd rect (at 7.747 5.0038 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 37 /RGB2_VS_B)
    )
    (pad 79 smd rect (at 7.747 4.4958 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 80 smd rect (at 7.747 3.9878 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /CLK27)
    )
    (pad 81 smd rect (at 7.747 3.5052 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 34 /RGB2_HS_B)
    )
    (pad 82 smd rect (at 7.747 2.9972 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 83 smd rect (at 7.747 2.4892 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 84 smd rect (at 7.747 2.0066 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 25 /PLL_VDD)
    )
    (pad 85 smd rect (at 7.747 1.4986 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 25 /PLL_VDD)
    )
    (pad 86 smd rect (at 7.747 0.9906 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 87 smd rect (at 7.747 0.4826 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 54 N-0000044)
    )
    (pad 88 smd rect (at 7.747 0 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 57 N-0000047)
    )
    (pad 89 smd rect (at 7.747 -0.508 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 55 N-0000045)
    )
    (pad 90 smd rect (at 7.747 -1.016 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 91 smd rect (at 7.747 -1.4986 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 92 smd rect (at 7.747 -2.0066 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 93 smd rect (at 7.747 -2.5146 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /A33VDD)
    )
    (pad 94 smd rect (at 7.747 -2.9972 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /A33VDD)
    )
    (pad 95 smd rect (at 7.747 -3.5052 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 96 smd rect (at 7.747 -4.0132 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 65 N-0000071)
    )
    (pad 97 smd rect (at 7.747 -4.4958 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 69 N-0000089)
    )
    (pad 98 smd rect (at 7.747 -5.0038 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 66 N-0000072)
    )
    (pad 99 smd rect (at 7.747 -5.5118 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 70 N-0000090)
    )
    (pad 75 smd rect (at 5.9944 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 50 /SDA)
    )
    (pad 51 smd rect (at -5.9944 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 52 smd rect (at -5.4864 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 53 smd rect (at -5.0038 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (pad 54 smd rect (at -4.4958 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 55 smd rect (at -3.9878 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 48 /R_7)
    )
    (pad 56 smd rect (at -3.5052 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 47 /R_6)
    )
    (pad 57 smd rect (at -2.9972 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 46 /R_5)
    )
    (pad 58 smd rect (at -2.4892 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 45 /R_4)
    )
    (pad 59 smd rect (at -2.0066 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 44 /R_3)
    )
    (pad 60 smd rect (at -1.4986 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 61 smd rect (at -0.9906 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 43 /R_2)
    )
    (pad 62 smd rect (at -0.4826 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 42 /R_1)
    )
    (pad 63 smd rect (at 0 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 41 /R_0)
    )
    (pad 64 smd rect (at 0.508 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 65 smd rect (at 1.016 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 66 smd rect (at 1.4986 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (pad 67 smd rect (at 2.0066 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 68 smd rect (at 2.5146 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 69 smd rect (at 2.9972 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /DVDD)
    )
    (pad 70 smd rect (at 3.5052 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 71 smd rect (at 4.0132 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 26 /RESET)
    )
    (pad 72 smd rect (at 4.4958 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 73 smd rect (at 5.0038 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 74 smd rect (at 5.5118 7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 49 /SCL)
    )
    (pad 1 smd rect (at 5.9944 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 71 N-0000095)
    )
    (pad 2 smd rect (at 5.4864 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 59 N-0000055)
    )
    (pad 3 smd rect (at 5.0038 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 4 smd rect (at 4.4958 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /AVDD)
    )
    (pad 5 smd rect (at 3.9878 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 6 smd rect (at 3.5052 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /AVDD)
    )
    (pad 7 smd rect (at 2.9972 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /AVDD)
    )
    (pad 8 smd rect (at 2.4892 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 9 smd rect (at 2.0066 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 62 N-0000060)
    )
    (pad 10 smd rect (at 1.4986 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 63 N-0000061)
    )
    (pad 11 smd rect (at 0.9906 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 64 N-0000062)
    )
    (pad 12 smd rect (at 0.4826 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 13 smd rect (at 0 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /A33VDD)
    )
    (pad 14 smd rect (at -0.508 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 1 /A33VDD)
    )
    (pad 15 smd rect (at -1.016 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 16 smd rect (at -1.4986 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 60 N-0000057)
    )
    (pad 17 smd rect (at -2.0066 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 58 N-0000054)
    )
    (pad 18 smd rect (at -2.5146 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 61 N-0000058)
    )
    (pad 19 smd rect (at -2.9972 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /AVDD)
    )
    (pad 20 smd rect (at -3.5052 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 21 smd rect (at -4.0132 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 22 smd rect (at -4.4958 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /FIDOUT)
    )
    (pad 23 smd rect (at -5.0038 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 51 /VSOUT)
    )
    (pad 24 smd rect (at -5.5118 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
      (net 22 /HSOUT)
    )
    (pad 25 smd rect (at -5.9944 -7.747 180) (size 0.254 2.016)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 26 smd rect (at -7.747 -5.9944 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (pad 27 smd rect (at -7.747 -5.4864 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 28 smd rect (at -7.747 -5.0038 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 24 /PCLK)
    )
    (pad 29 smd rect (at -7.747 -4.4958 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /B_7)
    )
    (pad 30 smd rect (at -7.747 -3.9878 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 9 /B_6)
    )
    (pad 31 smd rect (at -7.747 -3.5052 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /B_5)
    )
    (pad 32 smd rect (at -7.747 -2.9972 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /B_4)
    )
    (pad 33 smd rect (at -7.747 -2.4892 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /B_3)
    )
    (pad 34 smd rect (at -7.747 -2.0066 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /B_2)
    )
    (pad 35 smd rect (at -7.747 -1.4986 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /B_1)
    )
    (pad 36 smd rect (at -7.747 -0.9906 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /B_0)
    )
    (pad 37 smd rect (at -7.747 -0.4826 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 38 smd rect (at -7.747 0 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
    )
    (pad 39 smd rect (at -7.747 0.508 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /DVDD)
    )
    (pad 40 smd rect (at -7.747 1.016 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 41 smd rect (at -7.747 1.4986 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /IOVDD)
    )
    (pad 42 smd rect (at -7.747 2.0066 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 43 smd rect (at -7.747 2.5146 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 21 /G_7)
    )
    (pad 44 smd rect (at -7.747 2.9972 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /G_6)
    )
    (pad 45 smd rect (at -7.747 3.5052 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /G_5)
    )
    (pad 46 smd rect (at -7.747 4.0132 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 18 /G_4)
    )
    (pad 47 smd rect (at -7.747 4.4958 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 17 /G_3)
    )
    (pad 48 smd rect (at -7.747 5.0038 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 16 /G_2)
    )
    (pad 49 smd rect (at -7.747 5.5118 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /G_1)
    )
    (pad 50 smd rect (at -7.747 5.9944 180) (size 2.016 0.254)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /G_0)
    )
    (pad 40 smd rect (at 0 0 180) (size 6.2 6.2)
      (layers F.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 40 smd rect (at 0 0 180) (size 6.2 6.2)
      (layers B.Cu F.Paste F.Mask)
      (net 52 GND)
    )
    (pad 40 thru_hole circle (at -1.56 1.56 180) (size 2.5 2.5) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 40 thru_hole circle (at 1.56 1.56 180) (size 2.5 2.5) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 40 thru_hole circle (at -1.56 -1.56 180) (size 2.5 2.5) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 40 thru_hole circle (at 1.56 -1.56 180) (size 2.5 2.5) (drill 1)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (model smd/TQFP_100.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module BARREL_JACK_roundconn (layer F.Cu) (tedit 54120F78)
    (at 14.986 29.972)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at 10.09904 0 90) (layer F.SilkS))
    (fp_text value 5VDC_IN (at 0 -5.99948) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 6.20014 0) (size 4 4) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
      (net 68 N-0000088)
    )
    (pad 2 thru_hole rect (at 0.20066 0) (size 4 4) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 3 thru_hole rect (at 3.2004 4.699) (size 4 4) (drill 3)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
  )
  (module 3xRCA_CONN (layer F.Cu) (tedit 54DA6FD5)
    (at 47.752 21.082 180)
    (fp_text reference U2 (at -3.54 -7.21 180) (layer F.SilkS))
    (fp_text value 3XRCA_CONN (at 7.99 -7.09 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 11.25 -3.7 180) (size 4 4) (drill 2.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 40 /RGB3_R)
    )
    (pad 3 thru_hole circle (at 18.75 -3.7 180) (size 4 4) (drill 2.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 40 /RGB3_R)
    )
    (pad 1 thru_hole circle (at -18.75 -3.7 180) (size 4 4) (drill 2.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 39 /RGB3_G)
    )
    (pad 1 thru_hole circle (at -11.25 -3.7 180) (size 4 4) (drill 2.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 39 /RGB3_G)
    )
    (pad 4 thru_hole circle (at -15 0 180) (size 4 4) (drill 2.82)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 4 thru_hole circle (at 0 0 180) (size 4 4) (drill 2.82)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad 4 thru_hole circle (at 15 0 180) (size 4 4) (drill 2.82)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (pad "" thru_hole oval (at 19.8 0 180) (size 2.5 2.5) (drill 2.5)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad "" thru_hole oval (at -19.8 0 180) (size 2.5 2.5) (drill 2.5)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 2 thru_hole circle (at 3.75 -3.7 180) (size 4 4) (drill 2.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 38 /RGB3_B)
    )
    (pad 2 thru_hole circle (at -3.75 -3.7 180) (size 4 4) (drill 2.7)
      (layers *.Cu *.Mask F.SilkS)
      (net 38 /RGB3_B)
    )
  )
  (module ACHL-24 (layer F.Cu) (tedit 54DA78D3)
    (at 30.734 38.354 270)
    (tags "SMA Connector")
    (fp_text reference U3 (at 0 -7.62 270) (layer F.SilkS))
    (fp_text value ACHL-27MHZ-EK (at 0.254 0 270) (layer F.SilkS))
    (pad 5 thru_hole circle (at 3.81 -3.81 270) (size 0.9 0.9) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 11 /CLK27)
    )
    (pad 8 thru_hole circle (at -3.81 -3.81 270) (size 0.9 0.9) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 23 /IOVDD)
    )
    (pad 1 thru_hole circle (at -3.81 3.81 270) (size 0.9 0.9) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 4 thru_hole circle (at 3.81 3.81 270) (size 0.9 0.9) (drill 0.6)
      (layers *.Cu *.Mask F.SilkS)
      (net 52 GND)
    )
    (model connectors/sma.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_line (start 11.938 80.264) (end 11.938 17.018) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.408 80.264) (end 11.938 80.264) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.408 17.018) (end 89.408 80.264) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 11.938 17.018) (end 89.408 17.018) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 52) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.408 80.264) (xy 11.938 80.264) (xy 11.938 17.018) (xy 89.408 17.018)
      )
    )
  )
  (zone (net 52) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.408 80.264) (xy 11.938 80.264) (xy 11.938 17.018) (xy 89.408 17.018)
      )
    )
  )
)
