<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="35.56" y1="10.795" x2="84.76" y2="10.795" width="0" layer="20"/>
<wire x1="84.76" y1="10.795" x2="84.76" y2="51.425" width="0" layer="20"/>
<wire x1="84.76" y1="51.425" x2="35.56" y2="51.425" width="0" layer="20"/>
<wire x1="35.56" y1="51.425" x2="35.56" y2="10.795" width="0" layer="20"/>
<text>680pf</text>
<text>1M</text>
<text>3.3K</text>
<text>12K</text>
<text>4.7K</text>
<text>33K</text>
<text>1M</text>
<text>10u 1/2</text>
<text>2.2K</text>
<text>180</text>
<text>2uF</text>
<text>5uF</text>
<text>2uF</text>
<text>5.6k</text>
<text>12K</text>
<text>330</text>
<text>680</text>
<text>2.2K</text>
<text>39</text>
<text>39</text>
<text>47K</text>
<text>47K</text>
<text>2uF</text>
<text>100uF</text>
<text>2uF</text>
<text>10uF</text>
<text>330K</text>
<text>33K</text>
<text>3.3K</text>
<text>22K</text>
<text>2uF</text>
<text>2uF</text>
<text>4.7K</text>
<text>.001uF</text>
<text>120K</text>
<text>10K</text>
<text>10K</text>
<text>470K</text>
<text>10K</text>
<text>2uF</text>
<text>580K</text>
<text>22K</text>
<text>250uF</text>
<text>2uF</text>
<text>470K</text>
<text>220K</text>
<text>1M</text>
<text>150K</text>
<text>2.7M</text>
<text>100K</text>
<text>.1uF</text>
<text>.01uF</text>
<text>G</text>
<text>G</text>
<hole x="40.005" y="14.605" drill="2"/>
<hole x="79.375" y="14.605" drill="2"/>
<hole x="79.375" y="48.26" drill="2"/>
<hole x="38.735" y="49.53" drill="2"/>
<text>2.2K</text>
<text>120K</text>
<text>'62 Crushasaurus</text>
<text>F</text>
<text>F</text>
<text>F</text>
</plain>
<libraries>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="ROUND">
<description>&lt;b&gt;Round Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
<package name="0703">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 7.5mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/2 watt metal film.</description>
</package>
<package name="R0207/1V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
vertical position&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 1 hole

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
</packages>
</library>
<library name="gm-trans">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-caps-film-chicklet">
<description>&lt;b&gt;Capacitors, Film, Chicklet&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;100pF - 0.1uF (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors
&lt;li&gt;available from smallbearelec.com as Panasonic ECQ-B capacitors
&lt;li&gt;these become quite large for values near 1uF
&lt;/ul&gt;</description>
<packages>
<package name="070X030_3">
<description>&lt;b&gt;7mm x 3mm, 0.3" pad spacing&lt;/b&gt;
&lt;p&gt;Panasonic ECQ-B</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P2" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="R1" library="gm-resistors" package="R0207/3" value="33k"/>
<element name=".1UF" library="gm-caps-film-box" package="072X025" value="">
<attribute name="VALUE"/>
</element>
<element name="Q9" library="gm-trans" package="TO92-" value="2N5458">
<attribute name="NAME"/>
</element>
<element name="R2" library="gm-resistors" package="R0207/3" value="330k"/>
<element name=".01" library="gm-caps-film-box" package="072X025" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="gm-caps-electro-pol" package="050_020" value="10uf"/>
<element name="R3" library="gm-resistors" package="R0207/3" value="120k"/>
<element name="R4" library="gm-resistors" package="R0207/3" value="33k"/>
<element name="R5" library="gm-resistors" package="0703" value="10  1/2w"/>
<element name="R6" library="gm-resistors" package="R0207/3" value="4.7k"/>
<element name="Q1" library="gm-trans" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="Q2" library="gm-trans" package="TO92-" value="2N5088"/>
<element name="R9" library="gm-resistors" package="R0207/3" value="1m"/>
<element name="C2" library="gm-caps-film-chicklet" package="070X030_3" value="680pf"/>
<element name="R10" library="gm-resistors" package="R0207/3" value="3.3k"/>
<element name="C3" library="gm-caps-electro-pol" package="050_020" value="100u"/>
<element name="R12" library="gm-resistors" package="R0207/3" value="1m"/>
<element name="C5" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="18''" library="gm-supply" package="ROUND" value="18">
<attribute name="NAME"/>
</element>
<element name="12''" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="6''" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="S4" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="C6" library="gm-caps-electro-pol" package="050_020" value="250uf"/>
<element name="-E" library="gm-supply" package="ROUND" value="|_|_|"/>
<element name="IN-P1" library="gm-supply" package="ROUND" value="18">
<attribute name="NAME"/>
</element>
<element name="R17" library="gm-resistors" package="R0207/3" value="10k"/>
<element name="C4" library="gm-caps-electro-pol" package="050_020" value="5uf"/>
<element name="Q8" library="gm-trans" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="AUXOUT" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="R19" library="gm-resistors" package="R0207/3" value="2.2k"/>
<element name="C7" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="C8" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="Q3" library="gm-trans" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="R27" library="gm-resistors" package="R0207/3" value="22k"/>
<element name=".001UF" library="gm-caps-film-box" package="072X025" value="">
<attribute name="VALUE"/>
</element>
<element name="C9" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="Q4" library="gm-trans" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="R31" library="gm-resistors" package="R0207/3" value="680"/>
<element name="C10" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="R33" library="gm-resistors" package="R0207/3" value="470k"/>
<element name="Q5" library="gm-trans" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="R34" library="gm-resistors" package="R0207/3" value="180"/>
<element name="C11" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="C12" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="R37" library="gm-resistors" package="R0207/3" value="47k"/>
<element name="Q6" library="gm-trans" package="TO92-" value="TIS93">
<attribute name="NAME"/>
</element>
<element name="Q7" library="gm-trans" package="TO92-" value="TIS93">
<attribute name="NAME"/>
</element>
<element name="R38" library="gm-resistors" package="R0207/3" value="39"/>
<element name="R39" library="gm-resistors" package="R0207/3" value="47k"/>
<element name="R40" library="gm-resistors" package="R0207/3" value="39"/>
<element name="R41" library="gm-resistors" package="R0207/3" value="2.2k"/>
<element name="C13" library="gm-caps-electro-pol" package="050_020" value="2uf"/>
<element name="6''D" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="B+" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="GND" library="gm-supply" package="ROUND" value=""/>
<element name="R21" library="gm-resistors" package="R0207/1V" value="220k"/>
<element name="R22" library="gm-resistors" package="R0207/1V" value="150k"/>
<element name="R20" library="gm-resistors" package="R0207/1V" value="1m"/>
<element name="R23" library="gm-resistors" package="R0207/1V" value="22k"/>
<element name="R29" library="gm-resistors" package="R0207/1V" value="10k"/>
<element name="R25" library="gm-resistors" package="R0207/1V" value="470k"/>
<element name="R18" library="gm-resistors" package="R0207/1V" value="580k"/>
<element name="R26" library="gm-resistors" package="R0207/1V" value="120k"/>
<element name="R11" library="gm-resistors" package="R0207/3" value="2.2k"/>
<element name="R30" library="gm-resistors" package="R0207/1V" value="2.7m"/>
<element name="R7" library="gm-resistors" package="R0207/1V" value="100k"/>
<element name="R8" library="gm-resistors" package="R0207/1V" value="10k"/>
<element name="R14" library="gm-resistors" package="R0207/1V" value="3.3k"/>
<element name="R13" library="gm-resistors" package="R0207/1V" value="12k"/>
<element name="R15" library="gm-resistors" package="R0207/1V" value="12k"/>
<element name="R16" library="gm-resistors" package="R0207/1V" value="5.6k"/>
<element name="R24" library="gm-resistors" package="R0207/1V" value="4.7k"/>
<element name="R28" library="gm-resistors" package="R0207/1V" value="330"/>
<element name="GND1" library="gm-supply" package="ROUND" value=""/>
<element name="GND2" library="gm-supply" package="ROUND" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="P2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element=".1UF" pad="1"/>
</signal>
<signal name="N$3">
<contactref element=".1UF" pad="2"/>
<contactref element="Q9" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element=".01" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="Q9" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element=".01" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="-"/>
<contactref element="R3" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C3" pad="-"/>
<contactref element="C6" pad="-"/>
<contactref element="R19" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="C13" pad="-"/>
<contactref element="GND" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="GND1" pad="1"/>
<contactref element="GND2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="Q2" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="+"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="Q9" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="C5" pad="-"/>
<contactref element="18''" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="6''" pad="1"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="1"/>
<contactref element="-E" pad="1"/>
</signal>
<signal name="VA">
<contactref element="C6" pad="+"/>
<contactref element="R17" pad="2"/>
<contactref element="R33" pad="1"/>
<contactref element="R37" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="R39" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="B+" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R17" pad="1"/>
<contactref element="C4" pad="+"/>
<contactref element="Q8" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="C4" pad="-"/>
<contactref element="AUXOUT" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="Q8" pad="3"/>
<contactref element="R19" pad="1"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="C8" pad="+"/>
<contactref element="Q3" pad="2"/>
<contactref element=".001UF" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="Q3" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="C9" pad="+"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$21">
<contactref element=".001UF" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="R26" pad="1"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="Q4" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="C9" pad="-"/>
<contactref element="R21" pad="2"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="Q4" pad="3"/>
<contactref element="R31" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="C10" pad="+"/>
<contactref element="C7" pad="+"/>
<contactref element="Q4" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="C10" pad="-"/>
<contactref element="R33" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="Q5" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="Q5" pad="3"/>
<contactref element="C12" pad="-"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="Q5" pad="1"/>
<contactref element="C11" pad="-"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="C11" pad="+"/>
<contactref element="R37" pad="2"/>
<contactref element="Q6" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="R38" pad="2"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="N$36">
<contactref element="R40" pad="2"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="N$37">
<contactref element="R39" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="C12" pad="+"/>
</signal>
<signal name="N$38">
<contactref element="Q6" pad="1"/>
<contactref element="Q7" pad="1"/>
<contactref element="C13" pad="+"/>
<contactref element="R41" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="Q8" pad="2"/>
<contactref element="C7" pad="-"/>
<contactref element="R22" pad="2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R10" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C3" pad="+"/>
<contactref element="R27" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IN-P1" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="12''" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="S4" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="C8" pad="-"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="6''D" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$26">
</signal>
<signal name="N$28">
</signal>
<signal name="N$39">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
</signals>
</board>
</drawing>
</eagle>
