<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="48.26" y1="0" x2="50.8" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="50.8" y1="2.54" x2="50.8" y2="20.32" width="0" layer="20"/>
<wire x1="50.8" y1="20.32" x2="48.26" y2="22.86" width="0" layer="20" curve="90"/>
<wire x1="48.26" y1="22.86" x2="2.54" y2="22.86" width="0" layer="20"/>
<wire x1="2.54" y1="22.86" x2="0" y2="20.32" width="0" layer="20" curve="90"/>
<wire x1="0" y1="20.32" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<hole x="48.26" y="20.32" drill="2.54"/>
<hole x="48.26" y="2.54" drill="2.54"/>
<text>USB</text>
<text>SCL</text>
<text>SDA</text>
<text>BAT</text>
<text>En</text>
<text>RST</text>
<text>MD</text>
<text>3V3</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>SCK</text>
<text>MOSI</text>
<text>MISO</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>NC</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>D8</text>
<text>BRD-0014-01</text>
<text>Sara R410</text>
<text>&gt;LAST_DATE_TIME</text>
</plain>
<libraries>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="MOUNTINGHOLE_2.5_PLATED">
</package>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="wolff-den">
<description>&lt;b&gt;Library for all Circuit Dojo Designs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by jared@circuitdojo.org&lt;/author&gt;</description>
<packages>
<package name="PLACEHOLDER">
</package>
<package name="LOGO-CIRCUITDOJO-BULB">
</package>
<package name="LOGO-CIRCUITDOJO">
</package>
<package name="CON-HEADER-1X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="CON-HEADER-1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="XCVR_SARA-R410M-02B">
</package>
<package name="R0402-M">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CAPC1005X55N">
</package>
<package name="IND0402_22N_TAI">
</package>
<package name="XCVR_SN74AXCH8T245RHLR">
</package>
<package name="DIO_RB558WMF-L">
</package>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SOD123">
</package>
<package name="TE_1909763-1">
</package>
<package name="DSK0010A">
</package>
<package name="IND-2P0X2P0X1P2">
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT353-L">
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="F93-C-L">
</package>
</packages>
</library>
<library name="78646-3001">
<packages>
<package name="MOLEX_78646-3001">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REV" value="C"/>
</attributes>
<variantdefs>
<variantdef name="Production"/>
</variantdefs>
<elements>
<element name="U$34" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL&quot;&quot;">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$35" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL&quot;&quot;">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$31" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$32" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="PCB1" library="wolff-den" package="PLACEHOLDER" value="PCB-PS-CCS811-SI7021">
<attribute name="MPN" value="BRD-0010"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="wolff-den" package="LOGO-CIRCUITDOJO-BULB" value=""/>
<element name="U$2" library="wolff-den" package="LOGO-CIRCUITDOJO" value=""/>
<element name="J2" library="wolff-den" package="CON-HEADER-1X12" value="HEADER-12">
<attribute name="DESC" value="CONN HDR 12POS 0.1 GOLD PCB"/>
<attribute name="DIGIKEYPN" value="S7045-ND"/>
<attribute name="MF" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PPPC121LFBN-RC"/>
<attribute name="NAME"/>
</element>
<element name="J3" library="wolff-den" package="CON-HEADER-1X16" value="HEADER-16">
<attribute name="DESC" value="CONN HDR 16POS 0.1 GOLD PCB"/>
<attribute name="DIGIKEYPN" value="S7049-ND"/>
<attribute name="MF" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PPPC161LFBN-RC"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="wolff-den" package="XCVR_SARA-R410M-02B" value="SARA-R410M-02B">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Cellular 4G LTE CAT M1/NB-IoT Transceiver Module 700MHz, 850MHz, 1.7GHz, 1.9GHz Antenna Not Included, Castellation Surface Mount "/>
<attribute name="MF" value="U-Blox America"/>
<attribute name="MP" value="SARA-R410M-02B"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SMD-96 u-blox"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="78646-3001" package="MOLEX_78646-3001" value="78646-3001">
<attribute name="DESCRIPTION" value=" 6 Position Card Connector Micro SIM Surface Mount, Right Angle Gold "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="WM9364CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/molex/0786463001/WM9364CT-ND/3770350?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="786463001"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R4" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R5" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="C1" library="wolff-den" package="CAPC1005X55N" value="12p">
<attribute name="DESC" value="CAP CER 12PF 50V C0G/NP0 0402"/>
<attribute name="DIGIKEYPN" value="490-6196-1-ND"/>
<attribute name="MPN" value="GRM1555C1H120FA01D"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Murata"/>
<attribute name="VOLTHIGH" value="50V"/>
</element>
<element name="L1" library="wolff-den" package="IND0402_22N_TAI" value="3.9n">
<attribute name="CURRENT" value="170mA"/>
<attribute name="DESC" value="FIXED IND 3.9NH 170MA 500 MOHM "/>
<attribute name="DIGIKEYPN" value="490-1131-1-ND"/>
<attribute name="MPN" value="LQP15MN3N9B02D"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="wolff-den" package="CAPC1005X55N" value="0.1u">
<attribute name="DESC" value="CAP CER 0.1UF 50V X5R 0402"/>
<attribute name="DIGIKEYPN" value="587-3499-1-ND"/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="UMK105BJ104KV-F"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VOLTHIGH" value="50V"/>
</element>
<element name="R2" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R3" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="U2" library="wolff-den" package="XCVR_SN74AXCH8T245RHLR" value="SN74AXCH8T245RHLR">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Voltage Level Translator Bidirectional 1 Circuit 8 Channel 380Mbps 24-VQFN _5.5x3.5_ "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="SN74AXCH8T245RHLR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="VFQFN-24 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R7" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R8" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R9" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R10" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="Q1" library="wolff-den" package="DIO_RB558WMF-L" value="RE1C002UNTCLDIO_RB558WMF-L">
<attribute name="BUILT_BY" value="EMA_Matt"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RE1C002UNTCL"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="ROHM Semiconductor"/>
</element>
<element name="Q2" library="wolff-den" package="DIO_RB558WMF-L" value="RE1C002UNTCLDIO_RB558WMF-L">
<attribute name="BUILT_BY" value="EMA_Matt"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RE1C002UNTCL"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="ROHM Semiconductor"/>
</element>
<element name="Q3" library="wolff-den" package="SOT23" value="MOSFET-P-SOT23">
<attribute name="DESC" value="MOSFET P-CH 20V 4.2A SOT23"/>
<attribute name="DIGIKEYPN" value="DMG2305UX-13DICT-ND"/>
<attribute name="MPN" value="DMG2305UX-13"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="R11" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="D1" library="wolff-den" package="SOD123" value="DIO-SCHOTTKY-3A">
<attribute name="DIGIKEYPN" value="DB2W40300LCT-ND"/>
<attribute name="MPN" value="DB2W40300L"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Panasonic Electronic Components"/>
</element>
<element name="C3" library="wolff-den" package="CAPC1005X55N" value="0.1u">
<attribute name="DESC" value="CAP CER 0.1UF 50V X5R 0402"/>
<attribute name="DIGIKEYPN" value="587-3499-1-ND"/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="UMK105BJ104KV-F"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VOLTHIGH" value="50V"/>
</element>
<element name="J4" library="wolff-den" package="TE_1909763-1" value="1909763-1">
<attribute name="COMMENT" value="1909763-1"/>
<attribute name="DESCRIPTION" value=" Conn Coaxial PL 50Ohm Solder ST SMD Gold Over Nickel T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="A118077CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/te-connectivity-amp-connectors/1909763-1/A118077CT-ND/4729711?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="1909763-1"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_POSITIONS" value="1"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="TE_PURCHASE_URL" value="https://www.te.com/usa-en/product-1909763-1.html?te_bu=Cor&amp;te_type=disp&amp;te_campaign=seda_glo_cor-seda-global-disp-prtnr-fy19-seda-model-bom-cta_sma-317_1&amp;elqCampaignId=32493"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="wolff-den" package="DSK0010A" value="Value">
<attribute name="COMPTYPE" value="IC"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MOUNTTYPE" value="SMT"/>
<attribute name="NAME"/>
<attribute name="PACKAGEREFERENCE" value="DSK0010A"/>
<attribute name="PARTNUMBER" value="TPS63030DSK"/>
<attribute name="PIN_COUNT" value="11"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="ROHS" value="Y"/>
<attribute name="TYPE" value="TYPE"/>
</element>
<element name="L2" library="wolff-den" package="IND-2P0X2P0X1P2" value="1.5u">
<attribute name="CURRENT" value="1.4A"/>
<attribute name="DIGIKEYPN" value="587-4702-1-ND"/>
<attribute name="MPN" value="NRV2012T1R5NGF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="wolff-den" package="C0603" value="10u">
<attribute name="DESC" value="CAP CER 10UF 6.3V X5R 0603"/>
<attribute name="DIGIKEYPN" value="587-5869-1-ND"/>
<attribute name="MPN" value="JMK107ABJ106MA-T"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VOLTHIGH" value="6.3"/>
</element>
<element name="C5" library="wolff-den" package="C0603" value="10u">
<attribute name="DESC" value="CAP CER 10UF 6.3V X5R 0603"/>
<attribute name="DIGIKEYPN" value="587-5869-1-ND"/>
<attribute name="MPN" value="JMK107ABJ106MA-T"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VOLTHIGH" value="6.3"/>
</element>
<element name="C7" library="wolff-den" package="C0603" value="10u">
<attribute name="DESC" value="CAP CER 10UF 6.3V X5R 0603"/>
<attribute name="DIGIKEYPN" value="587-5869-1-ND"/>
<attribute name="MPN" value="JMK107ABJ106MA-T"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VOLTHIGH" value="6.3"/>
</element>
<element name="R12" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="C6" library="wolff-den" package="CAPC1005X55N" value="0.1u">
<attribute name="DESC" value="CAP CER 0.1UF 50V X5R 0402"/>
<attribute name="DIGIKEYPN" value="587-3499-1-ND"/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MPN" value="UMK105BJ104KV-F"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VOLTHIGH" value="50V"/>
</element>
<element name="R13" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="R14" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="U4" library="wolff-den" package="SOT353-L" value="74LVC1G08GW,125SOT353-L">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="74LVC1G08GW,125"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Nexperia"/>
</element>
<element name="R15" library="wolff-den" package="R0402-M" value="100k">
<attribute name="DESC" value="RES SMD 100K OHM 1% 1/16W 0402"/>
<attribute name="DIGIKEYPN" value="311-100KLRCT-ND"/>
<attribute name="MPN" value="RC0402FR07100KL"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="POWER" value="1/16W"/>
<attribute name="TOLERANCE" value="1%"/>
</element>
<element name="L3" library="wolff-den" package="R0603" value="FERRITE-0603">
<attribute name="DIGIKEYPN" value="490-3992-1-ND"/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value="BLM18EG221SN1D"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="wolff-den" package="F93-C-L" value="F930J227KBAF93-C-L">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="F930J227KBA"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="AVX Corporation"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J3" pad="4"/>
<contactref element="U1" pad="73"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="89"/>
<contactref element="U1" pad="77"/>
<contactref element="U1" pad="86"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="80"/>
<contactref element="U1" pad="91"/>
<contactref element="U1" pad="69"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="95"/>
<contactref element="U1" pad="82"/>
<contactref element="U1" pad="60"/>
<contactref element="U1" pad="71"/>
<contactref element="U1" pad="87"/>
<contactref element="U1" pad="65"/>
<contactref element="U1" pad="74"/>
<contactref element="U1" pad="43"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="78"/>
<contactref element="U1" pad="67"/>
<contactref element="U1" pad="57"/>
<contactref element="U1" pad="54"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="83"/>
<contactref element="U1" pad="92"/>
<contactref element="U1" pad="61"/>
<contactref element="U1" pad="70"/>
<contactref element="U1" pad="58"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="96"/>
<contactref element="U1" pad="75"/>
<contactref element="U1" pad="85"/>
<contactref element="U1" pad="72"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="50"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="79"/>
<contactref element="U1" pad="88"/>
<contactref element="U1" pad="76"/>
<contactref element="U1" pad="66"/>
<contactref element="U1" pad="55"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="93"/>
<contactref element="U1" pad="81"/>
<contactref element="U1" pad="90"/>
<contactref element="U1" pad="59"/>
<contactref element="U1" pad="68"/>
<contactref element="U1" pad="84"/>
<contactref element="U1" pad="94"/>
<contactref element="J1" pad="G6"/>
<contactref element="J1" pad="G2"/>
<contactref element="J1" pad="G4"/>
<contactref element="J1" pad="G5"/>
<contactref element="J1" pad="G1"/>
<contactref element="J1" pad="G3"/>
<contactref element="J1" pad="C5"/>
<contactref element="R1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="12"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="30"/>
<contactref element="U2" pad="32"/>
<contactref element="U2" pad="27"/>
<contactref element="U2" pad="29"/>
<contactref element="U2" pad="28"/>
<contactref element="U2" pad="25"/>
<contactref element="U2" pad="33"/>
<contactref element="U2" pad="31"/>
<contactref element="U2" pad="26"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="3"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="11"/>
<contactref element="U3" pad="9"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="U4" pad="3"/>
<contactref element="R15" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="J3" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="J2" pad="3"/>
<contactref element="Q3" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="PB22/I6/SERCOM5.2">
</signal>
<signal name="PB23/I7/SERCOM5.3">
</signal>
<signal name="PB03/I3/AIN11/SERCOM5.1">
</signal>
<signal name="SCL">
<contactref element="J2" pad="11"/>
</signal>
<signal name="SDA">
<contactref element="J2" pad="12"/>
</signal>
<signal name="D6">
<contactref element="J2" pad="6"/>
</signal>
<signal name="D5">
<contactref element="J2" pad="7"/>
</signal>
<signal name="VBAT">
<contactref element="J2" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="D4">
<contactref element="J2" pad="8"/>
</signal>
<signal name="EN">
<contactref element="J2" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="CELL_VCC_EN">
<contactref element="J3" pad="10"/>
<contactref element="R12" pad="1"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="A4">
<contactref element="J3" pad="9"/>
</signal>
<signal name="A3">
<contactref element="J3" pad="8"/>
</signal>
<signal name="A2">
<contactref element="J3" pad="7"/>
</signal>
<signal name="A1">
<contactref element="J3" pad="6"/>
</signal>
<signal name="MD">
<contactref element="J3" pad="3"/>
</signal>
<signal name="A0">
<contactref element="J3" pad="5"/>
</signal>
<signal name="!RESET">
<contactref element="J3" pad="1"/>
</signal>
<signal name="NC">
<contactref element="J3" pad="16"/>
</signal>
<signal name="VPP">
<contactref element="J1" pad="C6"/>
</signal>
<signal name="SIM_CLK">
<contactref element="J1" pad="C3"/>
<contactref element="U1" pad="38"/>
</signal>
<signal name="SIM_RST">
<contactref element="J1" pad="C2"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="UB_PWR_ON">
<contactref element="U1" pad="15"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="UB_RST_N">
<contactref element="U1" pad="18"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="SIM_IO">
<contactref element="U1" pad="39"/>
<contactref element="J1" pad="C7"/>
</signal>
<signal name="SIM_VCC">
<contactref element="U1" pad="41"/>
<contactref element="J1" pad="C1"/>
</signal>
<signal name="UB_VCC">
<contactref element="U1" pad="52"/>
<contactref element="U1" pad="51"/>
<contactref element="U1" pad="53"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="UB_VINT">
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="23"/>
<contactref element="U2" pad="24"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="UB_TXD">
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="UB_RXD">
<contactref element="U1" pad="13"/>
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="UB_RTS">
<contactref element="U1" pad="10"/>
<contactref element="U2" pad="21"/>
</signal>
<signal name="UB_CTS">
<contactref element="U1" pad="11"/>
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="UB_DSR">
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="ANT">
<contactref element="U1" pad="56"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="ANT_FILT">
<contactref element="C1" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="UB_GPIO1">
<contactref element="U1" pad="16"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="CELL_PWR_ON">
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="CELL_RST">
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="DIR1">
<contactref element="U2" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="CELL_BUF_EN_N">
<contactref element="U2" pad="22"/>
<contactref element="R7" pad="1"/>
<contactref element="J3" pad="11"/>
</signal>
<signal name="DIR2">
<contactref element="U2" pad="11"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="CELL_RTS">
<contactref element="U2" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="CELL_RXD">
<contactref element="J3" pad="14"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="CELL_TXD">
<contactref element="U2" pad="4"/>
<contactref element="J3" pad="15"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="CELL_CTS">
<contactref element="J2" pad="9"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="CELL_VINT">
<contactref element="J3" pad="13"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="CELL_GPIO1">
<contactref element="J3" pad="12"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="VSYS">
<contactref element="Q3" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="7"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U3" pad="4"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="L2" pad="P$2"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="CELL_VCC">
<contactref element="U3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="L3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="FB">
<contactref element="R14" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="CELL_VCC_EN_AND">
<contactref element="U4" pad="4"/>
<contactref element="U3" pad="6"/>
<contactref element="R15" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
