(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 15)
    (zones 0)
    (modules 5)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.4)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(X1-Pad7)")
  (net 2 "Net-(X1-Pad8)")
  (net 3 "Net-(X1-Pad14)")
  (net 4 "Net-(X1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(X1-Pad1)")
    (add_net "Net-(X1-Pad14)")
    (add_net "Net-(X1-Pad7)")
    (add_net "Net-(X1-Pad8)")
  )
  (module novosc:Oscillator_SMD_4Pin_7.0x5.0mm_HandSoldering (layer F.Cu) (tedit 5F3C6D8E)
    (at 35.700001 31.925)
    (descr "Miniature Crystal Clock Oscillator EuroQuartz XO91 series, http://cdn-reichelt.de/documents/datenblatt/B400/XO91.pdf, hand-soldering, 7.0x5.0mm^2 package")
    (tags "SMD SMT crystal oscillator hand-soldering")
    (attr smd)
    (fp_text reference X2 (at 0 -4.1) (layer F.SilkS) hide)
    (fp_text value Oscillator_SMD_4Pin_7.0x5.0mm (at 0 4.1) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 4 smd rect (at -3.25 -2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(X1-Pad14)"))
    (pad 3 smd rect (at 3.25 -2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(X1-Pad8)"))
    (pad 2 smd rect (at 3.25 2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(X1-Pad7)"))
    (pad 1 smd rect (at -3.25 2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(X1-Pad1)"))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_EuroQuartz_XO91-4Pin_7.0x5.0mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module novosc:Oscillator_DIP-14 (layer F.Cu) (tedit 5F3C4589)
    (at 28.080001 35.535001)
    (descr "Oscillator, DIP14, Large Pads, http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference X1 (at 7.62 -11.26) (layer F.SilkS) hide)
    (fp_text value Oscillator-DIP14 (at 7.62 3.74) (layer F.Fab) hide)
    (fp_text user %R (at 7.62 -3.81) (layer F.Fab) hide)
    (pad 7 thru_hole circle (at 15.24 0) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(X1-Pad7)"))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(X1-Pad8)"))
    (pad 14 thru_hole circle (at 0 -7.62) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(X1-Pad14)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(X1-Pad1)"))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_DIP-14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_DIP-8_LargePads (layer F.Cu) (tedit 5F3C6A6D)
    (at 28.075 35.545)
    (descr "Oscillator, DIP8, Large Pads, http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference REF** (at 3.81 -11.26) (layer F.SilkS) hide)
    (fp_text value Oscillator_DIP-8_LargePads (at 3.81 3.74) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 -7.62) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 7.62 0) (size 2.5 2.5) (drill 1.4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_DIP-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module novosc:Oscillator_SMD_4Pin_5.0x3.2mm_HandSoldering (layer F.Cu) (tedit 5F3C52BD)
    (at 35.685 31.775)
    (descr "Miniature Crystal Clock Oscillator EuroQuartz XO53 series, http://cdn-reichelt.de/documents/datenblatt/B400/XO53.pdf, hand-soldering, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal oscillator hand-soldering")
    (attr smd)
    (fp_text reference REF** (at 0 -3.3) (layer F.SilkS) hide)
    (fp_text value 5.0x3.2mm (at 0 3.3) (layer F.Fab) hide)
    (pad 4 smd rect (at -1.34 -1.4) (size 1.54 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.34 -1.4) (size 1.54 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.34 1.4) (size 1.54 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.34 1.4) (size 1.54 1.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_EuroQuartz_XO53-4Pin_5.0x3.2mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module novosc:Oscillator_SMD_4Pin_3.2x2.5mm_HandSoldering (layer F.Cu) (tedit 5F3C5295)
    (at 35.7 31.95)
    (descr "Miniature Crystal Clock Oscillator EuroQuartz XO32 series, http://cdn-reichelt.de/documents/datenblatt/B400/XO32.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal oscillator hand-soldering")
    (attr smd)
    (fp_text reference REF** (at 0 -2.45) (layer F.SilkS) hide)
    (fp_text value Oscillator_SMD_4Pin_3.2x2.5mm_HandSoldering (at 0 2.45) (layer F.Fab) hide)
    (pad 4 smd rect (at -1.45 -0.775) (size 1.75 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.45 -0.775) (size 1.75 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.45 0.775) (size 1.75 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.45 0.775) (size 1.75 0.9) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_EuroQuartz_XO32-4Pin_3.2x2.5mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 25.1 38.325) (end 25.1 25.95) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 45.475 38.325) (end 25.1 38.325) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25.925 25.125) (end 45.55 25.125) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 46.3 25.95) (end 46.3 37.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 45.475 37.5) (end 46.3 37.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 45.475 25.95) (end 45.475 25.125) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 25.925 25.95) (end 25.1 25.95) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_text "amiga.technology\noscillator adapter" (at 35.700001 31.725) (layer B.SilkS))
  (gr_text "amiga.technology\n" (at 35.9 25.9) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.3 25.2) (xy 46.3 38.275) (xy 25.075 38.3) (xy 25.075 25.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.275 38.3) (xy 25.1 38.275) (xy 25.075 25.125) (xy 46.3 25.125)
      )
    )
  )
)
