(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 283)
    (zones 0)
    (modules 15)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.635)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4064)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.27)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(N1-PadLHDP)")
  (net 4 "Net-(N1-PadRHDP)")
  (net 5 "Net-(N2-PadRHDP)")
  (net 6 "Net-(N2-PadLHDP)")
  (net 7 "Net-(N3-PadRHDP)")
  (net 8 "Net-(N3-PadLHDP)")
  (net 9 "Net-(J2-Pad1)")
  (net 10 "Net-(N4-PadLHDP)")
  (net 11 "Net-(N4-PadRHDP)")
  (net 12 "Net-(N5-PadRHDP)")
  (net 13 "Net-(N5-PadLHDP)")
  (net 14 "Net-(J4-Pad1)")
  (net 15 "Net-(J4-Pad2)")
  (net 16 "Net-(N6-PadLHDP)")
  (net 17 "Net-(N6-PadRHDP)")
  (net 18 "Net-(J2-Pad2)")
  (net 19 "Net-(J3-Pad1)")
  (net 20 "Net-(J3-Pad2)")
  (net 21 "Net-(J3-Pad3)")
  (net 22 "Net-(J3-Pad4)")
  (net 23 "Net-(J3-Pad5)")
  (net 24 "Net-(J3-Pad6)")
  (net 25 "Net-(J3-Pad7)")
  (net 26 "Net-(J3-Pad8)")
  (net 27 "Net-(J3-Pad9)")
  (net 28 "Net-(J3-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.635)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 1.524)
    (diff_pair_width 0.254)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(N1-PadLHDP)")
    (add_net "Net-(N1-PadRHDP)")
    (add_net "Net-(N2-PadLHDP)")
    (add_net "Net-(N2-PadRHDP)")
    (add_net "Net-(N3-PadLHDP)")
    (add_net "Net-(N3-PadRHDP)")
    (add_net "Net-(N4-PadLHDP)")
    (add_net "Net-(N4-PadRHDP)")
    (add_net "Net-(N5-PadLHDP)")
    (add_net "Net-(N5-PadRHDP)")
    (add_net "Net-(N6-PadLHDP)")
    (add_net "Net-(N6-PadRHDP)")
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5D2A5B39)
    (at 78.74 105.41)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5D2A5B3E)
    (at 78.74 82.55)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5D2A5B43)
    (at 204.47 82.55)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module library:chris_ss_n (layer B.Cu) (tedit 0)
    (at 99.06 95.25 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module nixies-us:nixies-us-IN-14 (layer F.Cu) (tedit 5D2944B9)
    (at 173.99 93.98)
    (attr virtual)
    (fp_text reference N5 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value IN-14 (at 0 0) (layer F.SilkS))
    (pad RHDP thru_hole circle (at -2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(N5-PadRHDP)"))
    (pad LHDP thru_hole circle (at 2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(N5-PadLHDP)"))
    (pad A thru_hole circle (at 0 6.18744) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(J4-Pad1)"))
    (pad 9 thru_hole circle (at 6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 28 "Net-(J3-Pad10)"))
    (pad 8 thru_hole circle (at 5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 23 "Net-(J3-Pad5)"))
    (pad 7 thru_hole circle (at 4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 19 "Net-(J3-Pad1)"))
    (pad 6 thru_hole circle (at 1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 5 thru_hole circle (at -1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at -4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at -5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 2 thru_hole circle (at -6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 1 thru_hole circle (at -5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 26 "Net-(J3-Pad8)"))
    (pad 0 thru_hole circle (at 5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 27 "Net-(J3-Pad9)"))
  )
  (module nixies-us:nixies-us-IN-14 (layer F.Cu) (tedit 5D2944BF)
    (at 195.58 93.98)
    (attr virtual)
    (fp_text reference N6 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value IN-14 (at 0 0) (layer F.SilkS))
    (pad 0 thru_hole circle (at 5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 27 "Net-(J3-Pad9)"))
    (pad 1 thru_hole circle (at -5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 26 "Net-(J3-Pad8)"))
    (pad 2 thru_hole circle (at -6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 3 thru_hole circle (at -5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 4 thru_hole circle (at -4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 6 thru_hole circle (at 1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 7 thru_hole circle (at 4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 19 "Net-(J3-Pad1)"))
    (pad 8 thru_hole circle (at 5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 23 "Net-(J3-Pad5)"))
    (pad 9 thru_hole circle (at 6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 28 "Net-(J3-Pad10)"))
    (pad A thru_hole circle (at 0 6.18744) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(J4-Pad2)"))
    (pad LHDP thru_hole circle (at 2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 16 "Net-(N6-PadLHDP)"))
    (pad RHDP thru_hole circle (at -2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(N6-PadRHDP)"))
  )
  (module nixies-us:nixies-us-IN-14 (layer F.Cu) (tedit 5D2944AE)
    (at 130.81 93.98)
    (attr virtual)
    (fp_text reference N3 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value IN-14 (at 0 0) (layer F.SilkS))
    (pad RHDP thru_hole circle (at -2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(N3-PadRHDP)"))
    (pad LHDP thru_hole circle (at 2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(N3-PadLHDP)"))
    (pad A thru_hole circle (at 0 6.18744) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 9 thru_hole circle (at 6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 28 "Net-(J3-Pad10)"))
    (pad 8 thru_hole circle (at 5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 23 "Net-(J3-Pad5)"))
    (pad 7 thru_hole circle (at 4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 19 "Net-(J3-Pad1)"))
    (pad 6 thru_hole circle (at 1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 5 thru_hole circle (at -1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at -4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at -5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 2 thru_hole circle (at -6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 1 thru_hole circle (at -5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 26 "Net-(J3-Pad8)"))
    (pad 0 thru_hole circle (at 5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 27 "Net-(J3-Pad9)"))
  )
  (module nixies-us:nixies-us-IN-14 (layer F.Cu) (tedit 5D2944B4)
    (at 152.4 93.98)
    (attr virtual)
    (fp_text reference N4 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value IN-14 (at 0 0) (layer F.SilkS))
    (pad 0 thru_hole circle (at 5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 27 "Net-(J3-Pad9)"))
    (pad 1 thru_hole circle (at -5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 26 "Net-(J3-Pad8)"))
    (pad 2 thru_hole circle (at -6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 3 thru_hole circle (at -5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 4 thru_hole circle (at -4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 6 thru_hole circle (at 1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 7 thru_hole circle (at 4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 19 "Net-(J3-Pad1)"))
    (pad 8 thru_hole circle (at 5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 23 "Net-(J3-Pad5)"))
    (pad 9 thru_hole circle (at 6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 28 "Net-(J3-Pad10)"))
    (pad A thru_hole circle (at 0 6.18744) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 18 "Net-(J2-Pad2)"))
    (pad LHDP thru_hole circle (at 2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(N4-PadLHDP)"))
    (pad RHDP thru_hole circle (at -2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(N4-PadRHDP)"))
  )
  (module nixies-us:nixies-us-IN-14 (layer F.Cu) (tedit 5D294436)
    (at 109.22 93.98)
    (attr virtual)
    (fp_text reference N2 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value IN-14 (at 0 0) (layer F.SilkS))
    (pad RHDP thru_hole circle (at -2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(N2-PadRHDP)"))
    (pad LHDP thru_hole circle (at 2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(N2-PadLHDP)"))
    (pad A thru_hole circle (at 0 6.18744) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 9 thru_hole circle (at 6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 28 "Net-(J3-Pad10)"))
    (pad 8 thru_hole circle (at 5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 23 "Net-(J3-Pad5)"))
    (pad 7 thru_hole circle (at 4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 19 "Net-(J3-Pad1)"))
    (pad 6 thru_hole circle (at 1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 5 thru_hole circle (at -1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at -4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at -5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 2 thru_hole circle (at -6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 1 thru_hole circle (at -5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 26 "Net-(J3-Pad8)"))
    (pad 0 thru_hole circle (at 5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 27 "Net-(J3-Pad9)"))
  )
  (module nixies-us:nixies-us-IN-14 (layer F.Cu) (tedit 200000)
    (at 87.63 93.98)
    (attr virtual)
    (fp_text reference N1 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value IN-14 (at 0 0) (layer F.SilkS))
    (pad 0 thru_hole circle (at 5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 27 "Net-(J3-Pad9)"))
    (pad 1 thru_hole circle (at -5.0927 3.51536) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 26 "Net-(J3-Pad8)"))
    (pad 2 thru_hole circle (at -6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 3 thru_hole circle (at -5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 4 thru_hole circle (at -4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 6 thru_hole circle (at 1.48082 -6.00964) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 7 thru_hole circle (at 4.10464 -4.63296) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 19 "Net-(J3-Pad1)"))
    (pad 8 thru_hole circle (at 5.78612 -2.19456) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 23 "Net-(J3-Pad5)"))
    (pad 9 thru_hole circle (at 6.14426 0.74422) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 28 "Net-(J3-Pad10)"))
    (pad A thru_hole circle (at 0 6.18744) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad LHDP thru_hole circle (at 2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(N1-PadLHDP)"))
    (pad RHDP thru_hole circle (at -2.87528 5.47878) (size 1.3462 1.3462) (drill 0.8382) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(N1-PadRHDP)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5D29FA7F)
    (at 97.155 100.965 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5D29FA83)
    (at 140.335 100.965 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad2)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 5D29FA79)
    (at 71.755 82.55)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Female (at 0 25.19) (layer F.Fab) hide)
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 3.302 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5D29FA89)
    (at 183.515 100.965 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.27) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5D2A5B47)
    (at 204.47 105.41)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "IN-14 Nixie Tube Board v1.0" (at 184.15 81.28 180) (layer F.SilkS))
  (gr_text 9 (at 74.93 105.41 270) (layer F.SilkS))
  (gr_text 7 (at 74.803 82.55 270) (layer F.SilkS))
  (gr_text 6 (at 74.803 85.09 270) (layer F.SilkS))
  (gr_text 5 (at 74.803 87.63 270) (layer F.SilkS))
  (gr_text 4 (at 74.803 90.17 270) (layer F.SilkS))
  (gr_text 8 (at 74.803 92.71 270) (layer F.SilkS))
  (gr_text 3 (at 74.803 95.25 270) (layer F.SilkS))
  (gr_text 2 (at 74.803 97.79 270) (layer F.SilkS))
  (gr_text 1 (at 74.803 100.33 270) (layer F.SilkS))
  (gr_text 0 (at 74.803 102.87 270) (layer F.SilkS))
  (gr_line (start 68.58 78.74) (end 68.58 109.22) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 208.28 78.74) (end 208.28 109.22) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 208.28 109.22) (end 68.58 109.22) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 68.58 78.74) (end 208.28 78.74) (layer Edge.Cuts) (width 0.2))
)
