(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 84)
    (zones 0)
    (modules 9)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.475)
    (user_trace_width 0.475)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 /CN4_12)
  (net 3 /CN3_15)
  (net 4 "Net-(D2-Pad1)")
  (net 5 /CN3_1)
  (net 6 /CN3_2)
  (net 7 GND)
  (net 8 /CN3_14)
  (net 9 /CN3_13)
  (net 10 /CN3_12)
  (net 11 /CN3_11)
  (net 12 /CN3_10)
  (net 13 /CN3_9)
  (net 14 /CN3_8)
  (net 15 /CN3_7)
  (net 16 /CIPO)
  (net 17 /CN3_5)
  (net 18 /CN3_3)
  (net 19 /CN4_15)
  (net 20 +3V3)
  (net 21 /CN4_13)
  (net 22 /CN4_11)
  (net 23 /CN4_10)
  (net 24 /CN4_9)
  (net 25 /CN4_8)
  (net 26 /CN4_7)
  (net 27 /CN4_6)
  (net 28 /CN4_5)
  (net 29 /CN4_4)
  (net 30 /CN4_3)
  (net 31 /CN4_1)
  (net 32 "Net-(U2-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /CIPO)
    (add_net /CN3_1)
    (add_net /CN3_10)
    (add_net /CN3_11)
    (add_net /CN3_12)
    (add_net /CN3_13)
    (add_net /CN3_14)
    (add_net /CN3_15)
    (add_net /CN3_2)
    (add_net /CN3_3)
    (add_net /CN3_5)
    (add_net /CN3_7)
    (add_net /CN3_8)
    (add_net /CN3_9)
    (add_net /CN4_1)
    (add_net /CN4_10)
    (add_net /CN4_11)
    (add_net /CN4_12)
    (add_net /CN4_13)
    (add_net /CN4_15)
    (add_net /CN4_3)
    (add_net /CN4_4)
    (add_net /CN4_5)
    (add_net /CN4_6)
    (add_net /CN4_7)
    (add_net /CN4_8)
    (add_net /CN4_9)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(U2-Pad10)")
  )
  (module JohnAdriaan:Mandel_half (layer B.Cu) (tedit 0)
    (at 98.5 111)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module WIZnet:WIZ850io locked (layer B.Cu) (tedit 5F349824)
    (at 110.16 83.49 180)
    (descr <b>WIZ850io-7</b><br>)
    (fp_text reference U2 (at 10.16 -6.1) (layer B.SilkS) hide)
    (fp_text value WIZ850io (at 10.16 -6.1) (layer B.Fab))
    (pad 12 thru_hole circle (at 20.32 -12.7 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 16 /CIPO))
    (pad 11 thru_hole circle (at 20.32 -10.16 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 18 /CN3_3))
    (pad 10 thru_hole circle (at 20.32 -7.62 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad10)"))
    (pad 9 thru_hole circle (at 20.32 -5.08 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad 8 thru_hole circle (at 20.32 -2.54 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad 7 thru_hole rect (at 20.32 0 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 6 thru_hole circle (at 0 -12.7 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 2 /CN4_12))
    (pad 5 thru_hole circle (at 0 -10.16 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 28 /CN4_5))
    (pad 4 thru_hole circle (at 0 -7.62 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 23 /CN4_10))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 13 /CN3_9))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.665 1.665) (drill 1.11) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (module Nucleo32:Nucleo32 locked (layer F.Cu) (tedit 5F349646)
    (at 100 98.435)
    (fp_text reference U1 (at -5.715 -26.035) (layer F.SilkS) hide)
    (fp_text value Nucleo32 (at 3.81 26.035) (layer F.Fab) hide)
    (pad CN4_1 thru_hole rect (at 7.62 -16.215) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 /CN4_1))
    (pad CN4_2 thru_hole circle (at 7.62 -13.675) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad CN4_3 thru_hole circle (at 7.62 -11.135) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 /CN4_3))
    (pad CN4_4 thru_hole circle (at 7.62 -8.595) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 /CN4_4))
    (pad CN4_5 thru_hole circle (at 7.62 -6.055) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 /CN4_5))
    (pad CN4_6 thru_hole circle (at 7.62 -3.515) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 /CN4_6))
    (pad CN4_7 thru_hole circle (at 7.62 -0.975) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 /CN4_7))
    (pad CN4_8 thru_hole circle (at 7.62 1.565) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 25 /CN4_8))
    (pad CN4_9 thru_hole circle (at 7.62 4.105) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 24 /CN4_9))
    (pad CN4_10 thru_hole circle (at 7.62 6.645) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 /CN4_10))
    (pad CN4_11 thru_hole circle (at 7.62 9.185) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 /CN4_11))
    (pad CN4_12 thru_hole circle (at 7.62 11.725) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 /CN4_12))
    (pad CN4_13 thru_hole circle (at 7.62 14.265) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 /CN4_13))
    (pad CN4_14 thru_hole circle (at 7.62 16.805) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad CN4_15 thru_hole circle (at 7.62 19.345) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 /CN4_15))
    (pad CN3_1 thru_hole rect (at -7.62 -16.215) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 /CN3_1))
    (pad CN3_2 thru_hole circle (at -7.62 -13.675) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 /CN3_2))
    (pad CN3_3 thru_hole circle (at -7.62 -11.135) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 /CN3_3))
    (pad CN3_4 thru_hole circle (at -7.62 -8.595) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad CN3_5 thru_hole circle (at -7.62 -6.055) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 /CN3_5))
    (pad CN3_6 thru_hole circle (at -7.62 -3.515) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 /CIPO))
    (pad CN3_7 thru_hole circle (at -7.62 -0.975) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 /CN3_7))
    (pad CN3_8 thru_hole circle (at -7.62 1.565) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 /CN3_8))
    (pad CN3_9 thru_hole circle (at -7.62 4.105) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 /CN3_9))
    (pad CN3_10 thru_hole circle (at -7.62 6.645) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 /CN3_10))
    (pad CN3_11 thru_hole circle (at -7.62 9.185) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 /CN3_11))
    (pad CN3_12 thru_hole circle (at -7.62 11.725) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 /CN3_12))
    (pad CN3_13 thru_hole circle (at -7.62 14.265) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 /CN3_13))
    (pad CN3_14 thru_hole circle (at -7.62 16.805) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 /CN3_14))
    (pad CN3_15 thru_hole circle (at -7.62 19.345) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 /CN3_15))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 88.8 121.2 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value R_US (at 1.27 2.37) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 111.2 121.2)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.27 -2.37) (layer F.SilkS) hide)
    (fp_text value 100R (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x15_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 112.7 82.22)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J4 (at 0 -2.545) (layer F.SilkS) hide)
    (fp_text value Conn_01x15 (at 0 37.89) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /CN4_15))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /CN4_13))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /CN4_12))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /CN4_11))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /CN4_10))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /CN4_9))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /CN4_8))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /CN4_7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /CN4_6))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /CN4_5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /CN4_4))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /CN4_3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /CN4_1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x15_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 87.3 82.22)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x15 (at 0 37.89) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /CN3_15))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /CN3_14))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /CN3_13))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /CN3_12))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /CN3_11))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CN3_10))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /CN3_9))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /CN3_8))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CN3_7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /CIPO))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /CN3_5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /CN3_3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CN3_2))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /CN3_1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 87.3 124 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value Debug (at 1.3 -4.5 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /CN3_15))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 112.7 124 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS) hide)
    (fp_text value IRQ (at 1.3 3.8 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 /CN4_12))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text STM5500 (at 100 121) (layer B.SilkS))
  (gr_line (start 93.5 128) (end 98 123.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.5 128) (end 102 123.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102 123.5) (end 98 123.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.5 128) (end 86 128) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 114 127) (end 114 128) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 86 127) (end 85 127) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 86 81) (end 86 80) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 114 81) (end 115 81) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 85 127) (end 85 81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114 128) (end 106.5 128) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115 81) (end 115 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86 80) (end 114 80) (layer Edge.Cuts) (width 0.05))
  (zone (net 20) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 128) (xy 85 128) (xy 85 80) (xy 86.5 80) (xy 115 80)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 128) (xy 85 128) (xy 85 80) (xy 115 80)
      )
    )
  )
)
