(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 10)
    (no_connects 2)
    (area 151.054999 86.284999 168.985001 99.135001)
    (thickness 1.6)
    (drawings 8)
    (tracks 36)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.381)
    (trace_clearance 0.2)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 ~IRQ)
  (net 4 MOSI)
  (net 5 CE)
  (net 6 MISO)
  (net 7 ~CSN)
  (net 8 SCK)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CE)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net SCK)
    (add_net VDD)
    (add_net ~CSN)
    (add_net ~IRQ)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 153.289 95.25 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.921 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nRF24L01p_adapter:Socket_Strip_Straight_2x04_mirrored (layer F.Cu) (tedit 5918BB9C)
    (at 156.21 96.52 90)
    (descr "Through hole socket strip, mirrored")
    (tags "socket strip mirrored")
    (fp_text reference P2 (at -1.016 5.207 360) (layer F.SilkS))
    (fp_text value 2x4 (at 0 -3.1 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 ~CSN))
    (pad 3 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 CE))
    (pad 6 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 MOSI))
    (pad 5 thru_hole oval (at 5.08 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 SCK))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 ~IRQ))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MISO))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz 0.15 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x04 (layer B.Cu) (tedit 5918F609)
    (at 163.83 88.9 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 2.667 360) (layer B.SilkS))
    (fp_text value 2x4 (at 0 3.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 ~IRQ))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 MOSI))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 MISO))
    (pad 6 thru_hole oval (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 CE))
    (pad 7 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 SCK))
    (pad 8 thru_hole oval (at 7.62 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 ~CSN))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz 0.15 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_arc (start 152.4 87.63) (end 151.13 87.63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 97.79) (end 152.4 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 97.79) (end 168.91 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.64 87.63) (end 167.64 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 97.79) (end 168.91 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 99.06) (end 167.64 99.06) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.13 87.63) (end 151.13 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 86.36) (end 152.4 86.36) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.13 86.36) (xy 168.91 86.36) (xy 168.91 99.06) (xy 151.13 99.06)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.13 86.36) (xy 168.91 86.36) (xy 168.91 99.06) (xy 151.13 99.06)
      )
    )
  )
)
