<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="11.43" y2="0" width="0" layer="20"/>
<text>8086.net</text>
<text>AVRFT234</text>
<wire x1="12.7" y1="3.81" x2="12.7" y2="7.62" width="0" layer="20"/>
<wire x1="10.16" y1="13.462" x2="2.54" y2="13.462" width="0" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="2.54" y1="13.462" x2="0" y2="7.62" width="0" layer="20" curve="20"/>
<wire x1="10.16" y1="13.462" x2="12.7" y2="7.62" width="0" layer="20" curve="-20"/>
<wire x1="1.27" y1="0" x2="0" y2="3.81" width="0" layer="20" curve="-20"/>
<wire x1="11.43" y1="0" x2="12.7" y2="3.81" width="0" layer="20" curve="20"/>
<text>GND</text>
<text>MOSI</text>
<text>!RST</text>
<text>SCK</text>
<text>MISO</text>
<text>VTG</text>
<text>3</text>
<text>5</text>
<text>VTG</text>
</plain>
<libraries>
<library name="8086NET">
<description>8086.net Part Library</description>
<packages>
<package name="0805">
</package>
<package name="YV/TC164">
</package>
<package name="2X3_EDGE">
<description>4UCON 15881&lt;br&gt;
Male .1" spaced SMT&lt;br&gt;
Keying posts into board</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="11-egna-ic">
<description>Library for Eagle</description>
<packages>
<package name="DFN-12-(3X3)">
</package>
</packages>
</library>
<library name="Molex-47346-0001">
<packages>
<package name="MOLEX_47346-0001">
<description>MICRO USB R/A-473460001</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="8086NET" package="0805" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="8086NET" package="0805" value="4.7uF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="8086NET" package="0805" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="11-egna-ic" package="DFN-12-(3X3)" value="USB-UART-FT234XD"/>
<element name="R2" library="8086NET" package="0805" value="22R">
<attribute name="VALUE"/>
</element>
<element name="R3" library="8086NET" package="0805" value="22R">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="8086NET" package="YV/TC164" value="YC/TC164"/>
<element name="J1" library="Molex-47346-0001" package="MOLEX_47346-0001" value="">
<attribute name="OC_FARNELL" value="1568026"/>
<attribute name="PACKAGE" value="5 POS MICRO USB R/A"/>
<attribute name="OC_NEWARK" value="47M0505"/>
<attribute name="SUPPLIER" value="MOLEX"/>
<attribute name="MPN" value="47346-0001"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="8086NET" package="2X3_EDGE" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="8086NET" package="SJ_2" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="IC1" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="SJ2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="THERMAL-PAD"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="12"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="!CTS">
<contactref element="IC1" pad="11"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="!RST">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="V">
<contactref element="JP1" pad="2"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="10"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="8"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="7"/>
<contactref element="U$1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
