(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu14.04.1)
  (general
    (links 23)
    (no_connects 1)
    (area 122.118837 92.2116 157.281163 115.475733)
    (thickness 1.6)
    (drawings 22)
    (tracks 98)
    (zones 0)
    (modules 14)
    (nets 4)
  )
  (page A4 portrait)
  (title_block
    (title HaveSomePCB)
    (date 2017-01-18)
    (rev 1.1)
    (company DeuxVis)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2286)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 0.9144)
    (user_trace_width 1.2192)
    (trace_clearance 0.1524)
    (zone_clearance 0.1)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.8382 0.4826)
    (user_via 0.9906 0.635)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.0762)
    (uvia_min_drill 0.0508)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.6576 2.032)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 135.89 93.98)
    (visible_elements 7FFCFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 "Net-(PINS1-Pad2)")
  (net 2 "Net-(PINS1-Pad1)")
  (net 3 "Net-(PINS1-Pad3)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(PINS1-Pad1)")
    (add_net "Net-(PINS1-Pad2)")
    (add_net "Net-(PINS1-Pad3)")
  )
  (net_class Beefier ""
    (clearance 0.1524)
    (trace_width 0.2286)
    (via_dia 0.8382)
    (via_drill 0.4826)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class Gross ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.9906)
    (via_drill 0.635)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 587F627E)
    (at 139.7 96.139)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference REF**22 (at 0 3) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Big (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 587F6295)
    (at 141.224 99.187)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference REF**22 (at 0 3) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Big (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 587F6288)
    (at 138.176 99.187)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference REF**12 (at 0 3) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Big (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 "Net-(PINS1-Pad2)") (zone_connect 2))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 587F62A9)
    (at 141.224 102.235)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference REF**23 (at 0 3) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Big (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 587F629E)
    (at 138.176 102.235)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference REF**13 (at 0 3) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Big (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 "Net-(PINS1-Pad2)") (zone_connect 2))
  )
  (module SOT-23 (layer F.Cu) (tedit 57516026)
    (at 137.795 99.06)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference SOT23 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value APE8865NL-33-HF-3 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(PINS1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(PINS1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT-223 (layer F.Cu) (tedit 587F62F4)
    (at 139.7 99.06)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference SOT223 (at 0 -0.762) (layer F.SilkS) hide)
    (fp_text value LD1117S33CTR (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(PINS1-Pad3)"))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(PINS1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT-323 (layer F.Cu) (tedit 5751601E)
    (at 141.605 99.06 90)
    (tags "SMD SOT")
    (attr smd)
    (fp_text reference SOT323 (at 0.127 -2.032 90) (layer F.SilkS) hide)
    (fp_text value BFR92 (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.65024 -0.94996 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (pad 1 smd rect (at 0.65024 -0.94996 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(PINS1-Pad1)"))
    (pad 3 smd rect (at 0 0.94996 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(PINS1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-323.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module R_0402 (layer F.Cu) (tedit 5751600D)
    (at 141.732 106.045 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference SMD402 (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text value R0402 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(PINS1-Pad3)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module R_0603 (layer F.Cu) (tedit 57516003)
    (at 138.303 106.045 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference SMD603 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value R0603 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(PINS1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module R_0805 (layer F.Cu) (tedit 57516015)
    (at 141.732 106.045 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference SMD805 (at 0 -2.1 180) (layer F.SilkS) hide)
    (fp_text value R0805 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(PINS1-Pad3)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module R_1206 (layer F.Cu) (tedit 57515FF6)
    (at 138.303 106.045 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference SMD1206 (at 0 -2.3 180) (layer F.SilkS) hide)
    (fp_text value R1206 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(PINS1-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(PINS1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57515FB6)
    (at 137.16 110.49 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference PINS1 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(PINS1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(PINS1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(PINS1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module HaveSomeLib:NoteZone (layer B.Cu) (tedit 0)
    (at 139.7 108.204)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text 2 (at 137.541 96.52) (layer F.SilkS))
  (gr_text 3 (at 141.732 99.06) (layer F.SilkS))
  (gr_text 2 (at 141.478 99.949) (layer F.SilkS))
  (gr_text 1 (at 141.478 98.171) (layer F.SilkS))
  (gr_text 3 (at 137.033 98.298) (layer F.SilkS))
  (gr_text 2 (at 138.049 99.822) (layer F.SilkS))
  (gr_text 1 (at 137.668 100.711) (layer F.SilkS))
  (gr_text 3 (at 141.097 103.251) (layer F.SilkS))
  (gr_text 2 (at 138.811 103.251) (layer F.SilkS))
  (gr_text 1 (at 136.525 103.251) (layer F.SilkS))
  (gr_text "by DeuxVis" (at 143.129 94.234 90) (layer F.SilkS))
  (gr_text "HaveSome PCB V1.1" (at 136.271 94.234 90) (layer F.SilkS))
  (gr_line (start 135.89 112.395) (end 143.51 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 93.98) (end 135.89 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 93.98) (end 135.89 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 112.395) (end 143.51 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 3 (at 142.24 108.204) (layer B.SilkS))
  (gr_text 2 (at 139.7 108.204) (layer B.SilkS))
  (gr_text 1 (at 137.16 108.204) (layer B.SilkS))
  (gr_text 3 (at 142.24 108.204) (layer F.SilkS))
  (gr_text 2 (at 139.7 108.204) (layer F.SilkS))
  (gr_text 1 (at 137.16 108.204) (layer F.SilkS))
  (zone (net 1) (net_name "Net-(PINS1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 2))
    (polygon
      (pts
        (xy 143.51 97.028) (xy 135.89 97.028) (xy 135.89 93.98) (xy 143.51 93.98)
      )
    )
  )
  (zone (net 1) (net_name "Net-(PINS1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 107.95) (xy 135.89 107.95) (xy 135.89 93.98) (xy 143.51 93.98)
      )
    )
  )
)
