(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 4540)
    (zones 0)
    (modules 65)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.38)
    (user_trace_width 0.44)
    (user_trace_width 2.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1.4)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 154.05 179.45)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D4-Pad2)")
  (net 3 "Net-(F1-Pad2)")
  (net 4 Pout)
  (net 5 "Net-(F2-Pad2)")
  (net 6 "Net-(F3-Pad2)")
  (net 7 "Net-(F4-Pad2)")
  (net 8 "Net-(F5-Pad2)")
  (net 9 "Net-(F6-Pad2)")
  (net 10 L-6_Enet_Rx+)
  (net 11 L-6_Enet_Tx+)
  (net 12 L-6_Enet_Rx-)
  (net 13 L-6_Enet_Tx-)
  (net 14 GPS_Pulse)
  (net 15 L-1_Enet_Tx+)
  (net 16 L-1_Enet_Rx-)
  (net 17 L-1_Enet_Rx+)
  (net 18 L-2_Enet_Tx+)
  (net 19 L-2_Enet_Tx-)
  (net 20 L-2_Enet_Rx-)
  (net 21 L-2_Enet_Rx+)
  (net 22 L-3_Enet_Tx+)
  (net 23 L-3_Enet_Tx-)
  (net 24 L-3_Enet_Rx-)
  (net 25 L-3_Enet_Rx+)
  (net 26 L-4_Enet_Tx+)
  (net 27 L-4_Enet_Tx-)
  (net 28 L-4_Enet_Rx-)
  (net 29 L-4_Enet_Rx+)
  (net 30 L-5_Enet_Tx+)
  (net 31 L-5_Enet_Tx-)
  (net 32 L-5_Enet_Rx-)
  (net 33 L-5_Enet_Rx+)
  (net 34 "Net-(J7-Pad2)")
  (net 35 "Net-(R7-Pad2)")
  (net 36 "Net-(D1-Pad2)")
  (net 37 "Net-(D2-Pad2)")
  (net 38 "Net-(D3-Pad2)")
  (net 39 "Net-(D5-Pad2)")
  (net 40 "Net-(D6-Pad2)")
  (net 41 L-1_Enet_Tx-)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.25)
    (add_net GND)
    (add_net GPS_Pulse)
    (add_net L-1_Enet_Rx+)
    (add_net L-1_Enet_Rx-)
    (add_net L-1_Enet_Tx+)
    (add_net L-1_Enet_Tx-)
    (add_net L-2_Enet_Rx+)
    (add_net L-2_Enet_Rx-)
    (add_net L-2_Enet_Tx+)
    (add_net L-2_Enet_Tx-)
    (add_net L-3_Enet_Rx+)
    (add_net L-3_Enet_Rx-)
    (add_net L-3_Enet_Tx+)
    (add_net L-3_Enet_Tx-)
    (add_net L-4_Enet_Rx+)
    (add_net L-4_Enet_Rx-)
    (add_net L-4_Enet_Tx+)
    (add_net L-4_Enet_Tx-)
    (add_net L-5_Enet_Rx+)
    (add_net L-5_Enet_Rx-)
    (add_net L-5_Enet_Tx+)
    (add_net L-5_Enet_Tx-)
    (add_net L-6_Enet_Rx+)
    (add_net L-6_Enet_Rx-)
    (add_net L-6_Enet_Tx+)
    (add_net L-6_Enet_Tx-)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad2)")
    (add_net "Net-(F3-Pad2)")
    (add_net "Net-(F4-Pad2)")
    (add_net "Net-(F5-Pad2)")
    (add_net "Net-(F6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net Pout)
  )
  (module "480 Component Footprints:SMA" (layer F.Cu) (tedit 5DD72261)
    (at 126.22 21.55)
    (fp_text reference SMA (at 0 -1.9) (layer F.SilkS))
    (fp_text value SMA (at 0.15 -4.45) (layer F.Fab))
    (pad 5 thru_hole circle (at 0 0) (size 2 2) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 GPS_Pulse))
    (pad 4 thru_hole circle (at -2.65 -2.65) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.65 -2.65) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.65 2.65) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.65 2.65) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 32.6 -58.93)
    (fp_text reference "" (at 124.45 100.75) (layer F.SilkS))
    (fp_text value "" (at 124.45 100.75) (layer F.SilkS))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.45 100.75 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F3 (at 11.25 3.975) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Pout))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(F3-Pad2)"))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.45 49.65 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F6 (at 11.375 -3.775) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Pout))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(F6-Pad2)"))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 198.85 154.6 90)
    (fp_text reference "" (at 110.25 27.175 90) (layer F.SilkS))
    (fp_text value "" (at 110.25 27.175 90) (layer F.SilkS))
    (fp_text user GPS_Pulse (at 132.86 -67.22 270) (layer F.SilkS))
  )
  (module "480 Component Footprints:T3507900U" (layer F.Cu) (tedit 5DC07BBC)
    (at 83.52 113.49 270)
    (fp_text reference J3 (at 0.6858 0.9144 90) (layer F.SilkS))
    (fp_text value T3507900U (at 1.143 -0.7874 90) (layer F.Fab))
    (fp_text user SHIELD (at -7.493 -8.1534 90) (layer F.SilkS))
    (fp_text user SHIELD (at 7.6708 -8.255 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at 7.675 -16.15 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at 2.6 -16.125 90) (layer F.SilkS))
    (fp_text user "ENET TX-" (at 0 -18.7 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at -2.475 -16.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 0.025 -13.675 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -4.9276 -13.7414 90) (layer F.SilkS))
    (fp_text user 12V+ (at -7.425 -16.225 90) (layer F.SilkS))
    (fp_text user GND (at 5.08 -13.6906 90) (layer F.SilkS))
    (pad GND thru_hole circle (at -7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at 7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 -20.0914 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 27 L-4_Enet_Tx-))
    (pad 7 thru_hole circle (at -7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 6 "Net-(F3-Pad2)"))
    (pad 6 thru_hole circle (at 7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 28 L-4_Enet_Rx-))
    (pad 5 thru_hole circle (at -2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 26 L-4_Enet_Tx+))
    (pad 4 thru_hole circle (at 2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 29 L-4_Enet_Rx+))
    (pad 3 thru_hole circle (at -4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 14 GPS_Pulse))
    (pad 2 thru_hole circle (at 0 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "480 Component Footprints:T3507900U" (layer F.Cu) (tedit 5DC07BBC)
    (at 83.52 62.37 270)
    (fp_text reference J6 (at 0.6858 0.9144 90) (layer F.SilkS))
    (fp_text value T3507900U (at 1.143 -0.7874 90) (layer F.Fab))
    (fp_text user SHIELD (at -7.493 -8.1534 90) (layer F.SilkS))
    (fp_text user SHIELD (at 7.6708 -8.255 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at 7.675 -16.15 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at 2.6 -16.125 90) (layer F.SilkS))
    (fp_text user "ENET TX-" (at 0 -18.7 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at -2.475 -16.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 0.025 -13.675 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -4.9276 -13.7414 90) (layer F.SilkS))
    (fp_text user 12V+ (at -7.425 -16.225 90) (layer F.SilkS))
    (fp_text user GND (at 5.08 -13.6906 90) (layer F.SilkS))
    (pad GND thru_hole circle (at -7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at 7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 -20.0914 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 19 L-2_Enet_Tx-))
    (pad 7 thru_hole circle (at -7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 9 "Net-(F6-Pad2)"))
    (pad 6 thru_hole circle (at 7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 20 L-2_Enet_Rx-))
    (pad 5 thru_hole circle (at -2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 18 L-2_Enet_Tx+))
    (pad 4 thru_hole circle (at 2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 21 L-2_Enet_Rx+))
    (pad 3 thru_hole circle (at -4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 14 GPS_Pulse))
    (pad 2 thru_hole circle (at 0 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "480 Component Footprints:T3507900U" (layer F.Cu) (tedit 5DC07BBC)
    (at 83.53 36.82 270)
    (fp_text reference J5 (at 0.6858 0.9144 90) (layer F.SilkS))
    (fp_text value T3507900U (at 1.143 -0.7874 90) (layer F.Fab))
    (fp_text user SHIELD (at -7.493 -8.1534 90) (layer F.SilkS))
    (fp_text user SHIELD (at 7.6708 -8.255 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at 7.675 -16.15 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at 2.6 -16.125 90) (layer F.SilkS))
    (fp_text user "ENET TX-" (at 0 -18.7 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at -2.475 -16.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 0.025 -13.675 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -4.9276 -13.7414 90) (layer F.SilkS))
    (fp_text user 12V+ (at -7.425 -16.225 90) (layer F.SilkS))
    (fp_text user GND (at 5.08 -13.6906 90) (layer F.SilkS))
    (pad GND thru_hole circle (at -7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at 7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 -20.0914 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 41 L-1_Enet_Tx-))
    (pad 7 thru_hole circle (at -7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 8 "Net-(F5-Pad2)"))
    (pad 6 thru_hole circle (at 7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 16 L-1_Enet_Rx-))
    (pad 5 thru_hole circle (at -2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 15 L-1_Enet_Tx+))
    (pad 4 thru_hole circle (at 2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 17 L-1_Enet_Rx+))
    (pad 3 thru_hole circle (at -4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 14 GPS_Pulse))
    (pad 2 thru_hole circle (at 0 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "480 Component Footprints:T3507900U" (layer F.Cu) (tedit 5DC07BBC)
    (at 83.51 164.76 270)
    (fp_text reference J4 (at 0.6858 0.9144 90) (layer F.SilkS))
    (fp_text value T3507900U (at 1.143 -0.7874 90) (layer F.Fab))
    (fp_text user SHIELD (at -7.493 -8.1534 90) (layer F.SilkS))
    (fp_text user SHIELD (at 7.6708 -8.255 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at 7.675 -16.15 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at 2.6 -16.125 90) (layer F.SilkS))
    (fp_text user "ENET TX-" (at 0 -18.7 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at -2.475 -16.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 0.025 -13.675 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -4.9276 -13.7414 90) (layer F.SilkS))
    (fp_text user 12V+ (at -7.425 -16.225 90) (layer F.SilkS))
    (fp_text user GND (at 5.08 -13.6906 90) (layer F.SilkS))
    (pad GND thru_hole circle (at -7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at 7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 -20.0914 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 13 L-6_Enet_Tx-))
    (pad 7 thru_hole circle (at -7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad2)"))
    (pad 6 thru_hole circle (at 7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 12 L-6_Enet_Rx-))
    (pad 5 thru_hole circle (at -2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 11 L-6_Enet_Tx+))
    (pad 4 thru_hole circle (at 2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 10 L-6_Enet_Rx+))
    (pad 3 thru_hole circle (at -4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 14 GPS_Pulse))
    (pad 2 thru_hole circle (at 0 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "480 Component Footprints:T3507900U" (layer F.Cu) (tedit 5DC07BBC)
    (at 83.51 139.11 270)
    (fp_text reference J2 (at 0.6858 0.9144 90) (layer F.SilkS))
    (fp_text value T3507900U (at 1.143 -0.7874 90) (layer F.Fab))
    (fp_text user SHIELD (at -7.493 -8.1534 90) (layer F.SilkS))
    (fp_text user SHIELD (at 7.6708 -8.255 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at 7.675 -16.15 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at 2.6 -16.125 90) (layer F.SilkS))
    (fp_text user "ENET TX-" (at 0 -18.7 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at -2.475 -16.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 0.025 -13.675 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -4.9276 -13.7414 90) (layer F.SilkS))
    (fp_text user 12V+ (at -7.425 -16.225 90) (layer F.SilkS))
    (fp_text user GND (at 5.08 -13.6906 90) (layer F.SilkS))
    (pad GND thru_hole circle (at -7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at 7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 -20.0914 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 31 L-5_Enet_Tx-))
    (pad 7 thru_hole circle (at -7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 5 "Net-(F2-Pad2)"))
    (pad 6 thru_hole circle (at 7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 32 L-5_Enet_Rx-))
    (pad 5 thru_hole circle (at -2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 30 L-5_Enet_Tx+))
    (pad 4 thru_hole circle (at 2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 33 L-5_Enet_Rx+))
    (pad 3 thru_hole circle (at -4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 14 GPS_Pulse))
    (pad 2 thru_hole circle (at 0 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "480 Component Footprints:T3507900U" (layer F.Cu) (tedit 5DC07BBC)
    (at 83.47 87.92 270)
    (fp_text reference J1 (at 0.6858 0.9144 90) (layer F.SilkS))
    (fp_text value T3507900U (at 1.143 -0.7874 90) (layer F.Fab))
    (fp_text user SHIELD (at -7.493 -8.1534 90) (layer F.SilkS))
    (fp_text user SHIELD (at 7.6708 -8.255 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at 7.675 -16.15 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at 2.6 -16.125 90) (layer F.SilkS))
    (fp_text user "ENET TX-" (at 0 -18.7 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at -2.475 -16.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 0.025 -13.675 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -4.9276 -13.7414 90) (layer F.SilkS))
    (fp_text user 12V+ (at -7.425 -16.225 90) (layer F.SilkS))
    (fp_text user GND (at 5.08 -13.6906 90) (layer F.SilkS))
    (pad GND thru_hole circle (at -7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at 7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 -20.0914 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 23 L-3_Enet_Tx-))
    (pad 7 thru_hole circle (at -7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 3 "Net-(F1-Pad2)"))
    (pad 6 thru_hole circle (at 7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 24 L-3_Enet_Rx-))
    (pad 5 thru_hole circle (at -2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 22 L-3_Enet_Tx+))
    (pad 4 thru_hole circle (at 2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 25 L-3_Enet_Rx+))
    (pad 3 thru_hole circle (at -4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 14 GPS_Pulse))
    (pad 2 thru_hole circle (at 0 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 117.05 36.2 90)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F5 (at 11.225 4.025 90) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6 90) (layer F.Fab))
    (fp_text user %R (at 11.25 4 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Pout))
    (pad 2 thru_hole circle (at 15 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(F5-Pad2)"))
    (pad "" np_thru_hole circle (at 7.5 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.45 126.35 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F2 (at 11.275 3.975) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Pout))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(F2-Pad2)"))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.35 75.15 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F1 (at 11.25 3.925) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Pout))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(F1-Pad2)"))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 96.05 49.65)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 40 "Net-(D6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 100.35 23.25)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 96.15 100.75)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 96.15 126.35)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at -2.43 0.01) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 95.45 75.15)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 102.3 49.65)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(F6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 106.25 23.25)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(F5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 102.2 100.75)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(F3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 102.2 126.35)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 4.6 0.01) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(F2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 101.6 75.15)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09DAC)
    (at 127.35 135.45)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L5_Enet_TX-1 (at -0.7 1.4) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L5_Enet_TX- (at -2.975 1.925) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 31 L-5_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09D8C)
    (at 126.05 133.05)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L5_Enet_TX+1 (at 0.2 -1.2) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L5_Enet_TX+ (at -4.6 1.375) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 30 L-5_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09D5E)
    (at 128.45 152.75 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L5_Enet_Rx-1 (at -3.1 -1.2 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55 90) (layer F.Fab))
    (fp_text user L5_Enet_Rx- (at -3.85 -1.475 90) (layer F.SilkS))
    (pad 1 smd circle (at 0 0 90) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 32 L-5_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09D46)
    (at 128.05 147.35)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L5_Enet_Rx+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L5_Enet_Rx+ (at -3.65 -1.45) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 33 L-5_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC094EC)
    (at 126.35 115.55)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L4_Enet_TX-1 (at 0.1 1.4) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L4_Enet_TX- (at -2.4 1.75) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 27 L-4_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC0950D)
    (at 127.25 113.05)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L4_Enet_TX+1 (at -3.7 -0.1) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L4_Enet_TX+ (at -5.525 -0.225) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 26 L-4_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09583)
    (at 127.85 125.35)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L4_Enet_Rx-1 (at -0.3 -1.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L4_Enet_Rx- (at 0.875 4.2 90) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 28 L-4_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC0953A)
    (at 127.25 121.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L4_Enet_Rx+1 (at -1 -1.3) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L4_Enet_Rx+ (at -3.3 -1.575) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 29 L-4_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08C07)
    (at 126.25 92.75)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L3_Enet_TX-1 (at -0.1 1.4) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L3_Enet_TX- (at -1.95 1.5) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 23 L-3_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08A9C)
    (at 125.35 90.85)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L3_Enet_TX+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L3_Enet_TX+ (at -5.475 -0.7) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 22 L-3_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08B76)
    (at 125.05 110.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L3_Enet_Rx-1 (at 0.2 1.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L3_Enet_Rx- (at -1.25 1.05) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 24 L-3_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08B62)
    (at 122.55 109.35)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L3_Enet_Rx+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L3_Enet_Rx+ (at 0 -1.45) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 25 L-3_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08868)
    (at 122.65 67.85)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L2_Enet_TX-1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L2_Enet_TX- (at -4.125 -1.375) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 19 L-2_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08878)
    (at 124.55 68.65)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L2_Enet_TX+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L2_Enet_TX+ (at -5.65 0.55) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 18 L-2_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08B41)
    (at 123.75 86.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L2_Enet_Rx-1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L2_Enet_Rx- (at 0 -1.45) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 20 L-2_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08B13)
    (at 125.35 82.75)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L2_Enet_Rx+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L2_Enet_Rx+ (at -1.15 -1.425) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 21 L-2_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC08508)
    (at 126.15 54.55)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L1_Enet_TX-1 (at 0 -1.448 180) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L1_Enet_TX- (at -1.75 1.5) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 41 L-1_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC0840E)
    (at 127.95 53.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L1_Enet_TX+1 (at -0.5 -1.1) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L1_Enet_TX+ (at -0.1 -4.7 90) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 15 L-1_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC0846B)
    (at 127.65 64.55)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L1_Enet_Rx-1 (at -1.5 1.4) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L1_Enet_Rx- (at -5.65 -0.15) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 16 L-1_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC0838F)
    (at 126.35 61.35 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L1_Enet_Rx+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L1_Enet_Rx+ (at 6.125 -0.1) (layer F.SilkS))
    (pad 1 smd circle (at 0 0 180) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 17 L-1_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09E09)
    (at 121.95 168.35)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L6_Enet_TX-1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L6_Enet_TX- (at 0 -1.45) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 13 L-6_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09DE6)
    (at 126.65 163.45)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L6_Enet_TX+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L6_Enet_TX+ (at -5.825 0.025) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 11 L-6_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09DFE)
    (at 126.45 172.25)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L6_Enet_Rx-1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L6_Enet_Rx- (at -1.725 1.6) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 12 L-6_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DC09E3C)
    (at 122.45 171.45)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference L6_Enet_Rx+1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user L6_Enet_Rx+ (at 0 -1.45) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 10 L-6_Enet_Rx+))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 137.55 21.45)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 137.55 179.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 94.59 21.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 95.7 179.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Diode_SMD:MMSZ5242B-TP (layer F.Cu) (tedit 5DAFB067)
    (at 124.9 37.75)
    (fp_text reference U2 (at 1.625 1.05) (layer F.SilkS))
    (fp_text value MMSZ5242B-TP (at 1.55 -1.075) (layer F.Fab))
    (fp_text user Cathode (at 5.825 0.025 180) (layer F.SilkS))
    (fp_text user Anode (at -2.175 0 180) (layer F.SilkS))
    (pad 2 smd rect (at 3.2766 0 90) (size 1.2192 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.2192 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 4 Pout))
  )
  (module Package_TO_SOT_THT:FQP47P06 (layer F.Cu) (tedit 5DB39E0F)
    (at 127.55 41.5 180)
    (fp_text reference U1 (at -6.175 -0.05) (layer F.SilkS))
    (fp_text value FQP47P06 (at 0 1.725) (layer F.Fab))
    (fp_text user Drain (at 0 -1.55) (layer F.SilkS))
    (fp_text user Source (at 2.675 -1.55) (layer F.SilkS))
    (fp_text user Gate (at -2.7 -1.575) (layer F.SilkS))
    (pad 3 thru_hole rect (at 2.67 0 270) (size 2 2.125) (drill 1.62) (layers *.Cu *.Mask)
      (net 4 Pout))
    (pad 2 thru_hole rect (at 0 0 180) (size 2.125 2.125) (drill 1.62) (layers *.Cu *.Mask)
      (net 34 "Net-(J7-Pad2)"))
    (pad 1 thru_hole rect (at -2.67 0 180) (size 2.125 2.125) (drill 1.62) (layers *.Cu *.Mask)
      (net 35 "Net-(R7-Pad2)"))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 102.2 152.05)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 4.58 -0.05) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 132.75 45.85 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -2.725 -0.075) (layer F.SilkS))
    (fp_text value 120K (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at -2.725 -0.075) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 170.6104 90)
    (fp_text reference J13 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 12 L-6_Enet_Rx-))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 10 L-6_Enet_Rx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 13 L-6_Enet_Tx-))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 11 L-6_Enet_Tx+))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 149.308944 90)
    (fp_text reference J12 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 32 L-5_Enet_Rx-))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 33 L-5_Enet_Rx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 31 L-5_Enet_Tx-))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 30 L-5_Enet_Tx+))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 128.007488 90)
    (fp_text reference J11 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 28 L-4_Enet_Rx-))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 29 L-4_Enet_Rx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 27 L-4_Enet_Tx-))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 26 L-4_Enet_Tx+))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 106.706032 90)
    (fp_text reference J10 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 24 L-3_Enet_Rx-))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 25 L-3_Enet_Rx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 23 L-3_Enet_Tx-))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 22 L-3_Enet_Tx+))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 85.404576 90)
    (fp_text reference J9 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 20 L-2_Enet_Rx-))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 21 L-2_Enet_Rx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 19 L-2_Enet_Tx-))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 18 L-2_Enet_Tx+))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 64.10312 90)
    (fp_text reference J8 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 16 L-1_Enet_Rx-))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 17 L-1_Enet_Rx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 41 L-1_Enet_Tx-))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 15 L-1_Enet_Tx+))
  )
  (module Connector:0768250002 (layer F.Cu) (tedit 5DB3ADC9)
    (at 139.05 30.35 270)
    (fp_text reference J7 (at -0.525 15.75 90) (layer F.SilkS))
    (fp_text value 76825-0002 (at 0 -4.95 90) (layer F.Fab))
    (fp_text user foot (at 0 3.55 90) (layer F.SilkS))
    (fp_text user GND (at 0.025 4.85 90) (layer F.SilkS))
    (fp_text user +12V (at -0.1 10.425 90) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 6.2 6.2) (drill 3.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 7.3 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 12.8 270) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 34 "Net-(J7-Pad2)"))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.45 152.05 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F4 (at 11.25 3.925) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 Pout))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(F4-Pad2)"))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 96.15 152.05)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at -2.46 -0.05) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Power (at 135.65 36.39) (layer F.SilkS))
  (gr_text "Lidar 1" (at 140.6 57.9 90) (layer F.SilkS))
  (gr_text "Lidar 2" (at 140.6 79.33 90) (layer F.SilkS))
  (gr_text "Lidar 3" (at 140.6 100.76 90) (layer F.SilkS))
  (gr_text "Lidar 4" (at 140.6 122.19 90) (layer F.SilkS))
  (gr_text "Lidar 5" (at 140.6 143.62 90) (layer F.SilkS))
  (gr_text "Lidar 6" (at 140.6 165.05 90) (layer F.SilkS))
  (gr_text "Lidar 6" (at 110.35 164.75 90) (layer F.SilkS))
  (gr_text "Lidar 5" (at 110.35 139.025 90) (layer F.SilkS))
  (gr_text "Lidar 4" (at 110.35 113.15 90) (layer F.SilkS))
  (gr_text "Lidar 3" (at 110.35 87.025 90) (layer F.SilkS))
  (gr_text "Lidar 2\n" (at 110.35 61.475 90) (layer F.SilkS))
  (gr_text "Lidar 1\n" (at 110.45 37.925 90) (layer F.SilkS))
  (gr_line (start 89 184.95) (end 89 16.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.45 16.225) (end 143.45 184.95) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89 16.25) (end 143.45 16.225) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.45 184.95) (end 89 184.95) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 140.25 176.25) (xy 90.055 176.04) (xy 90.05 17.45) (xy 140.2475 17.65)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 140.225 17.65) (xy 129.2 17.6) (xy 140.25 27.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 90.03 17.42) (xy 90.05 27.61) (xy 102.99 17.45)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 140.2525 176.245) (xy 90.055 176.04) (xy 90.05 17.45) (xy 140.2475 17.655)
      )
    )
  )
)
