(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 641)
    (zones 0)
    (modules 73)
    (nets 88)
  )
  (page A4)
  (title_block
    (title "RGBA - Reasonably Good Bluetooth Audio")
    (date 2021-03-06)
    (rev 1.1)
    (company "Fusha LLC")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.199)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.19)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.2)
    (user_via 0.4 0.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.65 1.14)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(C23-Pad1)")
  (net 4 "Net-(C24-Pad2)")
  (net 5 "Net-(C24-Pad1)")
  (net 6 "Net-(C25-Pad2)")
  (net 7 "Net-(C26-Pad2)")
  (net 8 +3.3VA)
  (net 9 "Net-(C30-Pad1)")
  (net 10 "Net-(C41-Pad1)")
  (net 11 +5VA)
  (net 12 -5VA)
  (net 13 "Net-(C610-Pad1)")
  (net 14 "Net-(C610-Pad2)")
  (net 15 "Net-(C611-Pad1)")
  (net 16 OUT_R)
  (net 17 "Net-(C612-Pad1)")
  (net 18 "Net-(C620-Pad1)")
  (net 19 "Net-(C620-Pad2)")
  (net 20 "Net-(C621-Pad1)")
  (net 21 OUT_L)
  (net 22 "Net-(C625-Pad1)")
  (net 23 "Net-(D1-Pad1)")
  (net 24 VBAT)
  (net 25 VBUS)
  (net 26 "Net-(J1-PadA5)")
  (net 27 "Net-(J1-PadB5)")
  (net 28 UART_TX)
  (net 29 UART_RX)
  (net 30 "Net-(L30-Pad1)")
  (net 31 "Net-(L50-Pad2)")
  (net 32 "Net-(L51-Pad1)")
  (net 33 LED_CHG)
  (net 34 LED_CONN)
  (net 35 LED_PWR)
  (net 36 "Net-(R10-Pad2)")
  (net 37 VREG_IN)
  (net 38 +1V8)
  (net 39 DAC_R-)
  (net 40 DAC_R+)
  (net 41 DAC_L-)
  (net 42 DAC_L+)
  (net 43 "Net-(U1-Pad2)")
  (net 44 "Net-(U1-Pad3)")
  (net 45 I2S_CLK)
  (net 46 "Net-(U1-Pad5)")
  (net 47 I2S_DATA)
  (net 48 I2S_LRCK)
  (net 49 "Net-(U1-Pad9)")
  (net 50 "Net-(U1-Pad10)")
  (net 51 "Net-(U1-Pad11)")
  (net 52 "Net-(U1-Pad12)")
  (net 53 "Net-(U1-Pad20)")
  (net 54 "Net-(U1-Pad21)")
  (net 55 "Net-(U1-Pad37)")
  (net 56 "Net-(U1-Pad38)")
  (net 57 "Net-(U1-Pad40)")
  (net 58 "Net-(U1-Pad41)")
  (net 59 "Net-(U1-Pad42)")
  (net 60 "Net-(U1-Pad43)")
  (net 61 "Net-(U1-Pad44)")
  (net 62 "Net-(U1-Pad45)")
  (net 63 "Net-(U1-Pad46)")
  (net 64 "Net-(U1-Pad47)")
  (net 65 "Net-(U1-Pad48)")
  (net 66 "Net-(U1-Pad49)")
  (net 67 "Net-(U1-Pad51)")
  (net 68 "Net-(U1-Pad23)")
  (net 69 "Net-(U1-Pad24)")
  (net 70 "Net-(U1-Pad25)")
  (net 71 "Net-(U1-Pad26)")
  (net 72 "Net-(U1-Pad29)")
  (net 73 "Net-(U1-Pad30)")
  (net 74 "Net-(U1-Pad31)")
  (net 75 "Net-(U2-Pad22)")
  (net 76 "Net-(U2-Pad26)")
  (net 77 "Net-(U2-Pad29)")
  (net 78 "Net-(U2-Pad30)")
  (net 79 "Net-(J4-Pad3)")
  (net 80 "Net-(J5-Pad3)")
  (net 81 "Net-(LED1-Pad1)")
  (net 82 "Net-(LED2-Pad1)")
  (net 83 "Net-(LED3-Pad1)")
  (net 84 VOL+_NEXT)
  (net 85 VOL-_PREV)
  (net 86 "Net-(U1-Pad16)")
  (net 87 "Net-(U1-Pad15)")
  (net_class Default "This is the default net class."
    (clearance 0.199)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +3.3VA)
    (add_net +3V3)
    (add_net +5VA)
    (add_net -5VA)
    (add_net DAC_L+)
    (add_net DAC_L-)
    (add_net DAC_R+)
    (add_net DAC_R-)
    (add_net GND)
    (add_net I2S_CLK)
    (add_net I2S_DATA)
    (add_net I2S_LRCK)
    (add_net LED_CHG)
    (add_net LED_CONN)
    (add_net LED_PWR)
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C610-Pad1)")
    (add_net "Net-(C610-Pad2)")
    (add_net "Net-(C611-Pad1)")
    (add_net "Net-(C612-Pad1)")
    (add_net "Net-(C620-Pad1)")
    (add_net "Net-(C620-Pad2)")
    (add_net "Net-(C621-Pad1)")
    (add_net "Net-(C625-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-PadA5)")
    (add_net "Net-(J1-PadB5)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(L30-Pad1)")
    (add_net "Net-(L50-Pad2)")
    (add_net "Net-(L51-Pad1)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net OUT_L)
    (add_net OUT_R)
    (add_net UART_RX)
    (add_net UART_TX)
    (add_net VBAT)
    (add_net VBUS)
    (add_net VOL+_NEXT)
    (add_net VOL-_PREV)
    (add_net VREG_IN)
  )
  (module rgba:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 60691E28)
    (at 84.5 109.25 90)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J8 (at 0 -1.648 90) (layer F.SilkS) hide)
    (fp_text value UART_RX (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 UART_RX))
  )
  (module rgba:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 60691E28)
    (at 85.75 110.7 90)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J7 (at 0 -1.648 90) (layer F.SilkS) hide)
    (fp_text value UART_VBUS (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +3V3))
  )
  (module rgba:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 60691E28)
    (at 83.25 107.75)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J6 (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value UART_TX (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 UART_TX))
  )
  (module rgba:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer F.Cu) (tedit 60691E28)
    (at 82 106.25 90)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J3 (at 0 -1.648 90) (layer F.SilkS) hide)
    (fp_text value UART_GND (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module rgba:SolderWire_AudioOut_1x03_P2.0mm (layer F.Cu) (tedit 60662331)
    (at 117.45 100.65 270)
    (attr virtual)
    (fp_text reference J4 (at 3.6 -2 90) (layer F.SilkS) hide)
    (fp_text value "R SPK OUT" (at 3.75 -2.868 90) (layer F.Fab))
    (fp_text user %R (at 3.6 0) (layer F.Fab))
    (pad 3 smd rect (at 5.6 0 270) (size 1.6 2.8) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(J4-Pad3)"))
    (pad 2 smd rect (at 2.8 0 270) (size 1.6 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd oval (at 0 0 270) (size 1.6 2.8) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT_R))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x03_P3.6mm_D0.4mm_OD1mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:SolderWire_AudioOut_1x03_P2.0mm (layer F.Cu) (tedit 60662331)
    (at 117.45 114.1 90)
    (attr virtual)
    (fp_text reference J5 (at 3.6 -2 90) (layer F.SilkS) hide)
    (fp_text value "L SPK OUT" (at 3.6 2.87 90) (layer F.Fab))
    (fp_text user %R (at 3.6 0) (layer F.Fab))
    (pad 3 smd rect (at 5.6 0 90) (size 1.6 2.8) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(J5-Pad3)"))
    (pad 2 smd rect (at 2.8 0 90) (size 1.6 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd oval (at 0 0 90) (size 1.6 2.8) (layers F.Cu F.Paste F.Mask)
      (net 21 OUT_L))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x03_P3.6mm_D0.4mm_OD1mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Castellated (layer B.Cu) (tedit 5F68FEF1)
    (at 95.5 94.75 180)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (attr smd)
    (fp_text reference LED1 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value ORNG (at 0 -1.17) (layer B.Fab) hide)
    (fp_text user %R (at 0.381 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1008_2520Metric_Pad1.43x2.20mm_HandSolder (layer F.Cu) (tedit 5F68FEF0)
    (at 93.8 100.1)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L30 (at 0 -2.05) (layer F.SilkS) hide)
    (fp_text value 4.7uH (at 0 2.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.1625 0) (size 1.425 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.1625 0) (size 1.425 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 30 "Net-(L30-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 99.1 97.1 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 1.43 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.43 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 LED_CONN))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(LED2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 102.6 96.35 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 LED_PWR))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(LED3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 97.4 97.15 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.43 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.43 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 LED_CHG))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:FSC-BT806 locked (layer B.Cu) (tedit 6065E0C1)
    (at 88.9 106.68 270)
    (descr "Feasycom BT806 Bluetooth Low Energy audio module featuring Qualcomm CSR8670/8675")
    (tags "audio bluetooth aptx feasycom")
    (attr smd)
    (fp_text reference U1 (at 0 -1.5 270) (layer B.SilkS) hide)
    (fp_text value FSC-BT806 (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -6.5 8.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -6.5 7.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -6.5 6.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -6.5 5.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 I2S_CLK))
    (pad 5 smd rect (at -6.5 4.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -6.5 3.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 47 I2S_DATA))
    (pad 7 smd rect (at -6.5 2.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 48 I2S_LRCK))
    (pad 8 smd rect (at -6.5 1.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(R10-Pad2)"))
    (pad 9 smd rect (at -6.5 0.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -6.5 -0.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -6.5 -1.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -6.5 -2.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -6.5 -3.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 UART_TX))
    (pad 14 smd rect (at -6.5 -4.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 29 UART_RX))
    (pad 15 smd rect (at -6.5 -5.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -6.5 -6.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at -6.5 -7.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 33 LED_CHG))
    (pad 18 smd rect (at -6.5 -8.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 34 LED_CONN))
    (pad 19 smd rect (at -6.5 -9.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 35 LED_PWR))
    (pad 20 smd rect (at -6.5 -10.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at -6.5 -11.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(U1-Pad21)"))
    (pad 32 smd rect (at 6.5 -11.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 33 smd rect (at 6.5 -10.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 24 VBAT))
    (pad 34 smd rect (at 6.5 -9.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 37 VREG_IN))
    (pad 35 smd rect (at 6.5 -8.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 38 +1V8))
    (pad 36 smd rect (at 6.5 -7.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 37 smd rect (at 6.5 -6.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 6.5 -5.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 6.5 -4.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 25 VBUS))
    (pad 40 smd rect (at 6.5 -3.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(U1-Pad40)"))
    (pad 41 smd rect (at 6.5 -2.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at 6.5 -1.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at 6.5 -0.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(U1-Pad43)"))
    (pad 44 smd rect (at 6.5 0.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(U1-Pad44)"))
    (pad 45 smd rect (at 6.5 1.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(U1-Pad45)"))
    (pad 46 smd rect (at 6.5 2.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(U1-Pad46)"))
    (pad 47 smd rect (at 6.5 3.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(U1-Pad47)"))
    (pad 48 smd rect (at 6.5 4.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(U1-Pad48)"))
    (pad 49 smd rect (at 6.5 5.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U1-Pad49)"))
    (pad 50 smd rect (at 6.5 6.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 51 smd rect (at 6.5 7.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(U1-Pad51)"))
    (pad 52 smd rect (at 6.5 8.5 270) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd rect (at -4.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -3.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at -2.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at -1.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at -0.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 0.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 VOL+_NEXT))
    (pad 28 smd rect (at 1.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 85 VOL-_PREV))
    (pad 29 smd rect (at 2.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 3.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 4.5 -13 180) (size 1.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(U1-Pad31)"))
  )
  (module LED_SMD:LED_0603_1608Metric_Castellated (layer B.Cu) (tedit 5F68FEF1)
    (at 99.1 94.75 180)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (attr smd)
    (fp_text reference LED2 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value BLUE (at 0 -1.17) (layer B.Fab) hide)
    (fp_text user %R (at -1.524 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(LED2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Castellated (layer B.Cu) (tedit 5F68FEF1)
    (at 102.7 94.75 180)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (attr smd)
    (fp_text reference LED3 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value WHITE (at 0 -1.17) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(LED3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:WSON-12-1EP_3x3mm_P0.45mm_EP1.2x2mm (layer B.Cu) (tedit 60646083)
    (at 111.17 105.96 90)
    (descr "WSON-12 http://www.ti.com/lit/ds/symlink/lm27762.pdf")
    (tags WSON-12)
    (attr smd)
    (fp_text reference U5 (at 0.385 2.617 90) (layer B.SilkS) hide)
    (fp_text value TPS65133DPD (at 0 -2.921 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.25) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 1.125 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 31 "Net-(L50-Pad2)"))
    (pad 13 smd rect (at 0 0 90) (size 1.2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd roundrect (at -1.4 0.675 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 2 GND))
    (pad 3 smd roundrect (at -1.4 0.225 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 11 +5VA))
    (pad 4 smd roundrect (at -1.4 -0.225 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 2 GND))
    (pad 5 smd roundrect (at -1.4 -0.675 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 2 GND))
    (pad 6 smd roundrect (at -1.4 -1.125 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 2 GND))
    (pad 7 smd roundrect (at 1.4 -1.125 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 8 +3.3VA))
    (pad 8 smd roundrect (at 1.4 -0.675 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 2 GND))
    (pad 9 smd roundrect (at 1.4 -0.225 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 12 -5VA))
    (pad 10 smd roundrect (at 1.4 0.225 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 32 "Net-(L51-Pad1)"))
    (pad 11 smd roundrect (at 1.4 0.675 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 8 +3.3VA))
    (pad 12 smd roundrect (at 1.4 1.125 90) (size 0.6 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 8 +3.3VA))
    (pad 13 thru_hole circle (at 0 0.5 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole circle (at 0 -0.5 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-12-1EP_3x2mm_P0.5mm_EP1x2.65.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:MountingHole_1.2mm_M1_Pad (layer F.Cu) (tedit 6064577C)
    (at 104.84 111.55)
    (attr virtual)
    (fp_text reference J12 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Screw 1" (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module rgba:TL4110AF160Q (layer B.Cu) (tedit 60642D64)
    (at 109.975 115.45 180)
    (descr TL4110AF160Q-3)
    (tags Switch)
    (attr smd)
    (fp_text reference SW1 (at 0 1.297) (layer B.SilkS) hide)
    (fp_text value Switch_RA (at 0 1.297) (layer B.SilkS) hide)
    (fp_text user %R (at 0 1.297) (layer B.Fab))
    (pad 2 smd rect (at 1.27 1.27 90) (size 2.032 1.14) (layers B.Cu B.Paste B.Mask)
      (net 24 VBAT))
    (pad 1 smd rect (at -1.27 1.27 90) (size 2.032 1.14) (layers B.Cu B.Paste B.Mask)
      (net 37 VREG_IN))
    (model G:\KiCad\ext_libs\libraryloader\SamacSys_Parts.3dshapes\TL4110AF160Q.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:TL4110AF160Q (layer B.Cu) (tedit 60642D64)
    (at 104.15 115.5 180)
    (descr TL4110AF160Q-3)
    (tags Switch)
    (attr smd)
    (fp_text reference SW3 (at 0 1.297) (layer B.SilkS) hide)
    (fp_text value Switch_RA (at 0 1.297) (layer B.SilkS) hide)
    (fp_text user %R (at 0 1.297) (layer B.Fab))
    (pad 2 smd rect (at 1.27 1.27 90) (size 2.032 1.14) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -1.27 1.27 90) (size 2.032 1.14) (layers B.Cu B.Paste B.Mask)
      (net 85 VOL-_PREV))
    (model G:\KiCad\ext_libs\libraryloader\SamacSys_Parts.3dshapes\TL4110AF160Q.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:TL4110AF160Q (layer B.Cu) (tedit 60642D64)
    (at 115.8 115.45 180)
    (descr TL4110AF160Q-3)
    (tags Switch)
    (attr smd)
    (fp_text reference SW2 (at 0 1.297) (layer B.SilkS) hide)
    (fp_text value Switch_RA (at 0 1.297) (layer B.SilkS) hide)
    (fp_text user %R (at 0 1.297) (layer B.Fab))
    (pad 2 smd rect (at 1.27 1.27 90) (size 2.032 1.14) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -1.27 1.27 90) (size 2.032 1.14) (layers B.Cu B.Paste B.Mask)
      (net 84 VOL+_NEXT))
    (model G:\KiCad\ext_libs\libraryloader\SamacSys_Parts.3dshapes\TL4110AF160Q.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:VSSOP-8_3.0x3.0mm_P0.65mm (layer F.Cu) (tedit 60645F01)
    (at 111.309 105.776 270)
    (descr "VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf")
    (tags "VSSOP-8 3.0 x 3.0")
    (attr smd)
    (fp_text reference U6 (at 0 -2.5 90) (layer F.SilkS) hide)
    (fp_text value OPA1662 (at 0.02 2.73 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT_R))
    (pad 2 smd rect (at -2.2 -0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C612-Pad1)"))
    (pad 3 smd rect (at -2.2 0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C611-Pad1)"))
    (pad 4 smd rect (at -2.2 0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 12 -5VA))
    (pad 5 smd rect (at 2.2 0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C621-Pad1)"))
    (pad 6 smd rect (at 2.2 0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C625-Pad1)"))
    (pad 7 smd rect (at 2.2 -0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 21 OUT_L))
    (pad 8 smd rect (at 2.2 -0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 11 +5VA))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-8_3.0x3.0mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm_ThermalVias (layer F.Cu) (tedit 60645FBD)
    (at 102.362 98.608 270)
    (descr "WSON, 6 Pin (http://www.ti.com/lit/ds/symlink/tps61040.pdf#page=35), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "WSON NoLead")
    (attr smd)
    (fp_text reference U4 (at 0 -1.95 90) (layer F.SilkS) hide)
    (fp_text value TPS7A3501 (at 0 1.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1 -0.65 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at -1 0 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 3 smd roundrect (at -1 0.65 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at 1 0.65 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C41-Pad1)"))
    (pad 5 smd roundrect (at 1 0 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3VA))
    (pad 6 smd roundrect (at 1 -0.65 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3VA))
    (pad 7 smd rect (at 0 0 270) (size 1 1.6) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 -0.55 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 0.55 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 2 GND))
    (pad 7 smd rect (at 0 0 270) (size 0.5 1.6) (layers B.Cu)
      (net 2 GND))
    (pad "" smd roundrect (at 0 -0.4 270) (size 0.87 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0.4 270) (size 0.87 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm (layer F.Cu) (tedit 60645F76)
    (at 94.418 105.657 90)
    (descr "QFN, 32 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_32_05-08-1693.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U2 (at 0 -3.82 90) (layer F.SilkS) hide)
    (fp_text value PCM5242 (at 0 3.82 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.4375 -1.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at -2.4375 -1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C23-Pad1)"))
    (pad 3 smd roundrect (at -2.4375 -0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -2.4375 -0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 5 smd roundrect (at -2.4375 0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 6 smd roundrect (at -2.4375 0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C24-Pad2)"))
    (pad 7 smd roundrect (at -2.4375 1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at -2.4375 1.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C24-Pad1)"))
    (pad 9 smd roundrect (at -1.75 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C25-Pad2)"))
    (pad 10 smd roundrect (at -1.25 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 DAC_L+))
    (pad 11 smd roundrect (at -0.75 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 DAC_L-))
    (pad 12 smd roundrect (at -0.25 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 DAC_R-))
    (pad 13 smd roundrect (at 0.25 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 DAC_R+))
    (pad 14 smd roundrect (at 0.75 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3VA))
    (pad 15 smd roundrect (at 1.25 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 16 smd roundrect (at 1.75 2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C26-Pad2)"))
    (pad 17 smd roundrect (at 2.4375 1.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 18 smd roundrect (at 2.4375 1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 19 smd roundrect (at 2.4375 0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 20 smd roundrect (at 2.4375 0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 21 smd roundrect (at 2.4375 -0.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 22 smd roundrect (at 2.4375 -0.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(U2-Pad22)"))
    (pad 23 smd roundrect (at 2.4375 -1.25 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 24 smd roundrect (at 2.4375 -1.75 90) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 25 smd roundrect (at 1.75 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 26 smd roundrect (at 1.25 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U2-Pad26)"))
    (pad 27 smd roundrect (at 0.75 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 I2S_CLK))
    (pad 28 smd roundrect (at 0.25 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 I2S_DATA))
    (pad 29 smd roundrect (at -0.25 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U2-Pad29)"))
    (pad 30 smd roundrect (at -0.75 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U2-Pad30)"))
    (pad 31 smd roundrect (at -1.25 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 I2S_LRCK))
    (pad 32 smd roundrect (at -1.75 -2.4375 90) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 33 smd rect (at 0 0 90) (size 3.45 3.45) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad "" smd roundrect (at -1.15 -1.15 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.15 0 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.15 1.15 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.15 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 1.15 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.15 -1.15 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.15 0 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.15 1.15 90) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:VSON-8_1.5x2mm_P0.5mm (layer F.Cu) (tedit 60645EAB)
    (at 93.3 97.35 270)
    (descr "Texas Instruments DLC0008B package")
    (fp_text reference U3 (at 1.515 -2.017 90) (layer F.SilkS) hide)
    (fp_text value TPS62849DLCR (at 0 2.54 90) (layer F.Fab))
    (pad 1 smd rect (at -0.685 -0.75 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.685 -0.25 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C30-Pad1)"))
    (pad 3 smd rect (at -0.685 0.25 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.685 0.75 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 38 +1V8))
    (pad 5 smd rect (at 0.685 0.75 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.685 0.25 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.685 -0.25 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(L30-Pad1)"))
    (pad 8 smd rect (at 0.685 -0.75 270) (size 0.86 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module rgba:MountingHole_1.2mm_M1_Pad (layer F.Cu) (tedit 6064577C)
    (at 105.85 95.9)
    (attr virtual)
    (fp_text reference J11 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Screw 1" (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEF0)
    (at 87.15 94.35 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D2 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value D_Small (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 VBUS))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEF0)
    (at 87.15 95.95 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value D_Small (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 VBAT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_ACH_BM02B-ACHSS-GAN-ETF_1x02-1MP_P1.20mm_Vertical (layer F.Cu) (tedit 5C2814B0)
    (at 83.85 97.35 90)
    (descr "JST ACH series connector, BM02B-ACHSS-GAN-ETF (http://www.jst-mfg.com/product/pdf/eng/eACH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST ACH vertical")
    (attr smd)
    (fp_text reference J2 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value "BATT CONN" (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.5 90) (layer F.Fab))
    (pad MP smd roundrect (at 1.75 1.9 90) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad MP smd roundrect (at -1.75 1.9 90) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.6 -1.875 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.6 -1.875 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 VBAT))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_ACH_BM02B-ACHSS-GAN-ETF_1x02-1MP_P1.20mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rgba:USB_C_Receptacle_UJC-HP-3-SMT-TR (layer B.Cu) (tedit 6063F4C9)
    (at 112.7 94.55)
    (descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
    (tags "usb usb-c 2.0 pd")
    (attr smd)
    (fp_text reference J1 (at 0 6.745) (layer B.SilkS) hide)
    (fp_text value "CHARGE CONN" (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 1.1) (layer B.Fab))
    (pad S1 thru_hole oval (at 4.32 0) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad S1 thru_hole oval (at -4.32 0) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad S1 thru_hole oval (at -4.32 3.8) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad S1 thru_hole oval (at 4.32 3.8) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad B1 smd rect (at -2.75 4.1625) (size 0.7 1.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad A1 smd rect (at 2.75 4.1625) (size 0.7 1.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad B9 smd rect (at -1.5 4.1625) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 25 VBUS))
    (pad A9 smd rect (at 1.5 4.1625) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 25 VBUS))
    (pad A5 smd rect (at 0.5 4.1625) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J1-PadA5)"))
    (pad B5 smd rect (at -0.5 4.1625) (size 0.6 1.45) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J1-PadB5)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_HRO_TYPE-C-31-M-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 95.3 97.6 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C31 (at 0 -1.16 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 94.35 95.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C30 (at 0 -1.16) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.16) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C30-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 108.1715 110.094)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R624 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 68R (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C621-Pad1)"))
    (pad 1 smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 108.134 108.697)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R623 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C621-Pad1)"))
    (pad 1 smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C620-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 108.134 107.3 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R622 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C620-Pad2)"))
    (pad 1 smd roundrect (at -0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C625-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 103.308 109.332)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R621 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C620-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 DAC_L+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 103.308 107.554 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R620 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 DAC_L-))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C620-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 112.15 101.65 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R615 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 68R (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C612-Pad1)"))
    (pad 1 smd roundrect (at -0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 OUT_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 108.134 102.982)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R614 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 68R (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C611-Pad1)"))
    (pad 1 smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 108.134 104.379)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R613 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C611-Pad1)"))
    (pad 1 smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C610-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 108.134 105.776 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R612 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C610-Pad2)"))
    (pad 1 smd roundrect (at -0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C612-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 103.308 103.744)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R611 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C610-Pad1)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 DAC_R+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 103.308 105.522 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R610 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 DAC_R-))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C610-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BB9E0)
    (at 111.563 109.967 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 68R (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C625-Pad1)"))
    (pad 1 smd roundrect (at -0.5975 0 180) (size 0.715 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 OUT_L))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1008_2520Metric_Pad1.43x2.20mm_HandSolder (layer B.Cu) (tedit 5F68FEF0)
    (at 112.22 101.46)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L51 (at 0 2.05 180) (layer B.SilkS) hide)
    (fp_text value 4.7uH (at 0 -2.05 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.1625 0) (size 1.425 2.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1754385964912281)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.1625 0) (size 1.425 2.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1754385964912281)
      (net 32 "Net-(L51-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1008_2520Metric_Pad1.43x2.20mm_HandSolder (layer B.Cu) (tedit 5F68FEF0)
    (at 115.5 106.6 270)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L50 (at 0 2.05 270) (layer B.SilkS) hide)
    (fp_text value 4.7uH (at 0 -2.05 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.1625 0 270) (size 1.425 2.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1754385964912281)
      (net 8 +3.3VA))
    (pad 2 smd roundrect (at 1.1625 0 270) (size 1.425 2.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1754385964912281)
      (net 31 "Net-(L50-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 111.817 111.491)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C625 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 33pF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 OUT_L))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C625-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 108.3 111.55 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C621 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 33pF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C621-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 105.848 108.443 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C620 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 4.3nF (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C620-Pad2)"))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C620-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 112.66 100.33)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C612 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 33pF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 OUT_R))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C612-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 106.61 101.331 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C611 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 33pF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C611-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 105.848 104.633 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C610 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 4.3nF (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C610-Pad2)"))
    (pad 1 smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C610-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 113.722 108.57 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C602 (at 0 -1.16 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.16 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +5VA))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 114.865 108.57 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C600 (at 0 -1.16 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.16 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +5VA))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 109.4565 103.343)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C53 (at 0 1.16 180) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 -1.16 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 -5VA))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 110.54 108.4 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C52 (at 0 1.16) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 -1.16) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 +5VA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 113.55 105.23 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C50 (at 0 1.16 90) (layer B.SilkS) hide)
    (fp_text value 10uF (at 0 -1.16 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3VA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 101.981 101.021 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C42 (at 0 -1.16) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.16) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3VA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 100.575 99 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C41 (at 0 -1.16 90) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.16 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C41-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 104.15 97.75 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C40 (at 0 -1.16 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.16 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 98.57 104.13 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C27 (at 0 -1.16 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.16 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3VA))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 99.244 110.102 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C25 (at 0 -1.68 90) (layer F.SilkS) hide)
    (fp_text value 2.2uF (at 0 1.68 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 6 "Net-(C25-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 97.085 110.8855 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C24 (at 0 -1.68 90) (layer F.SilkS) hide)
    (fp_text value 2.2uF (at 0 1.68 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 "Net-(C24-Pad2)"))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 5 "Net-(C24-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 91.624 110.483 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C23 (at 0 -1.16 90) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.16 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 94.164 110.991 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C22 (at 0 -1.16) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.16) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 93.402 109.848 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C21 (at 0 -1.16) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.16) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 88.77 109.2875 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C20 (at 0 -1.68 90) (layer F.SilkS) hide)
    (fp_text value 2.2uF (at 0 1.68 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 109.75 101.65)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C603 (at 0 -1.16) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.16) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 -5VA))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 109.75 100.55)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C601 (at 0 -1.16) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.16) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 -5VA))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEF0)
    (at 89.1 95.9 270)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D30 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value D_Small (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 VBAT))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C30-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer B.Cu) (tedit 5F6BB9E0)
    (at 86.8 98.3)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 VBAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 94.8 114.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 1.16) (layer B.SilkS) hide)
    (fp_text value 1uF (at 0 -1.16) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder (layer B.Cu) (tedit 5F6BB9E0)
    (at 97.6 114.7)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 VREG_IN))
    (pad 1 smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 112.72 103.56)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C51 (at 0 1.16) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -1.16) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 +3.3VA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 99.2 102.4 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C26 (at 0 -1.16) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.16) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C26-Pad2)"))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "gray olson" (at 87.14 113.685) (layer F.SilkS))
  (gr_text "designed by" (at 87.14 112.435) (layer F.SilkS))
  (gr_text "rev 1.1" (at 83.475 113.625) (layer F.SilkS))
  (gr_text "bluetooth audio" (at 87 105.3) (layer F.SilkS))
  (gr_text "reasonably good" (at 86.8 104.3) (layer F.SilkS))
  (gr_text rgba (at 86.5 101.1) (layer F.SilkS))
  (gr_text R (at 115 102.1 90) (layer F.SilkS))
  (gr_text L (at 114.4 112.7 90) (layer F.SilkS))
  (gr_text S (at 114.7 107.2 90) (layer F.SilkS))
  (gr_text - (at 115.1 103.6 90) (layer F.SilkS))
  (gr_text + (at 115.1 100.6 90) (layer F.SilkS))
  (gr_text - (at 115.1 111.3 90) (layer F.SilkS))
  (gr_text + (at 115.1 114.1 90) (layer F.SilkS))
  (gr_text rx (at 83 110.5) (layer F.SilkS))
  (gr_text tx (at 81.8 109) (layer F.SilkS))
  (gr_text "+\n" (at 84.4 111.9) (layer F.SilkS))
  (gr_text "-\n" (at 80.6 107.4) (layer F.SilkS))
  (gr_arc (start 81 114) (end 79.5 114) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 118 114) (end 118 115.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 118 95) (end 119.5 95) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 81.5 95.5) (end 81.5 93.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.5 95) (end 119.5 114) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 81 115.5) (end 118 115.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 81.5 93.5) (end 118 93.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 79.5 114) (end 79.5 95.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.8 118.2) (xy 69.9 118.2) (xy 69.9 95.1) (xy 79.8 95.1)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.5 115.5) (xy 79.5 115.5) (xy 79.5 93.5) (xy 119.5 93.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.5 115.5) (xy 79.5 115.5) (xy 79.5 93.5) (xy 119.5 93.5)
      )
    )
  )
)
