(kicad_pcb (version 20171130) (host pcbnew 5.1.0-060a0da~80~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 117)
    (zones 0)
    (modules 23)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 /CLK-P)
  (net 4 /CLK-N)
  (net 5 /DAT-N)
  (net 6 /DAT-P)
  (net 7 /CLK)
  (net 8 /DAT)
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(JP2-Pad1)")
  (net 11 "Net-(JP1-Pad1)")
  (net 12 /DIR)
  (net 13 /LED)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /CLK)
    (add_net /CLK-N)
    (add_net /CLK-P)
    (add_net /DAT)
    (add_net /DAT-N)
    (add_net /DAT-P)
    (add_net /DIR)
    (add_net /LED)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C7457A0)
    (at 123.19 88.265)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP8 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value GND (at -2.54 -0.635) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C745795)
    (at 111.125 88.265)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP9 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value GND (at 2.54 -0.635) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C738DA1)
    (at 107.315 102.235 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C738A01)
    (at 104.14 90.17)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference PMOD1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value PMOD-Device-x1-Type-1-GPIO (at 0 15.03) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /CLK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /DIR))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DAT))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /LED))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C744E12)
    (at 107.315 90.805)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value CLK (at 0 -1.905) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /CLK))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C744E24)
    (at 107.315 93.98)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value DIR (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 /DIR))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C744E39)
    (at 107.315 98.425)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP3 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value DAT (at 0 1.905) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DAT))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C744DDC)
    (at 120.015 92.075)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value CLK-P (at 0 -1.905) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /CLK-P))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C745A4B)
    (at 120.015 94.615)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP5 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value N (at 0 2.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /CLK-N))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C745A3B)
    (at 120.015 98.425)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value N (at 0 2.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /DAT-N))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5C745A1F)
    (at 120.015 100.965)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP7 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value DAT-P (at 0 1.905) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /DAT-P))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer F.Cu) (tedit 5C658233)
    (at 117.475 94.6 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd custom (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 11 "Net-(JP1-Pad1)")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.4 -0.3) (xy 0.9 -0.3) (xy 0.9 0.3) (xy 0.4 0.3)) (width 0))
      ))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 4 /CLK-N))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer F.Cu) (tedit 5C658224)
    (at 117.475 98.425 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.905 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 5 /DAT-N))
    (pad 1 smd custom (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 10 "Net-(JP2-Pad1)")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.4 -0.3) (xy 0.9 -0.3) (xy 0.9 0.3) (xy 0.4 0.3)) (width 0))
      ))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5C644E91)
    (at 115.824 104.14 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /LED))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C632CA0)
    (at 115.7225 88.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.3875 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C632D9A)
    (at 115.57 96.52 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C632C88)
    (at 111.2775 96.52 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5C632D25)
    (at 118.999 104.14 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5C632CEE)
    (at 117.475 100.965)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(JP2-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /DAT-P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5C632D13)
    (at 117.475 92.075 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(JP1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /CLK-P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SN65MLVD206DR (layer F.Cu) (tedit 5C644F03)
    (at 112.395 100.33)
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value SN65MLVD206DR (at -0.635 -5.08) (layer F.SilkS) hide)
    (fp_text user * (at -1.6129 -2.54) (layer F.Fab))
    (fp_text user * (at -2.7178 -2.54) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 8 smd rect (at 2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at 2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 5 /DAT-N))
    (pad 6 smd rect (at 2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 /DAT-P))
    (pad 5 smd rect (at 2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 /DAT))
    (pad 3 smd rect (at -2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 /DIR))
    (pad 2 smd rect (at -2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 /DIR))
    (pad 1 smd rect (at -2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 /DAT))
  )
  (module footprints:SN65MLVD206DR (layer F.Cu) (tedit 5C632D76)
    (at 112.395 92.71)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value SN65MLVD206DR (at 0 11.43) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -2.7178 -2.54) (layer F.SilkS))
    (fp_text user * (at -1.6129 -2.4257) (layer F.Fab))
    (pad 1 smd rect (at -2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 7 /CLK))
    (pad 2 smd rect (at -2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 /DIR))
    (pad 3 smd rect (at -2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 /DIR))
    (pad 4 smd rect (at -2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 7 /CLK))
    (pad 5 smd rect (at 2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 /CLK-P))
    (pad 7 smd rect (at 2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 /CLK-N))
    (pad 8 smd rect (at 2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module SamacSys_Parts:615004143821 (layer F.Cu) (tedit 5C632D60)
    (at 122.555 96.52 90)
    (descr 615004143821)
    (tags Connector)
    (fp_text reference J1 (at -0.165 5.704 90) (layer F.SilkS))
    (fp_text value 4P4C (at -0.165 5.704 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 1.53 3.4 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 /DAT-P))
    (pad 2 thru_hole circle (at 0.51 0.86 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /CLK-N))
    (pad 3 thru_hole circle (at -0.51 3.4 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /CLK-P))
    (pad 4 thru_hole circle (at -1.53 0.86 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /DAT-N))
    (pad 5 thru_hole circle (at -5 5.7 180) (size 2.36 2.36) (drill 2.36) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 5 5.7 180) (size 2.36 2.36) (drill 2.36) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text + (at 113.03 97.155) (layer F.SilkS))
  (gr_text + (at 108.585 103.505) (layer F.SilkS))
  (gr_text "SPOKE PMOD\nM-LVDS \nV0.4" (at 113.792 96.52) (layer B.SilkS))
  (gr_line (start 101.6 106.68) (end 101.6 86.36) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 106.68) (end 101.6 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 86.36) (end 130.81 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 86.36) (end 130.81 86.36) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.981 86.6775) (xy 130.429 86.868) (xy 130.429 106.299) (xy 101.981 106.1085)
      )
    )
  )
)
