(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 35)
    (no_connects 0)
    (area 124.814286 77.999999 160.485715 110.275001)
    (thickness 1.6)
    (drawings 6)
    (tracks 248)
    (zones 0)
    (modules 15)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.14)
    (user_trace_width 0.14)
    (trace_clearance 0.2)
    (zone_clearance 0.18)
    (zone_45_only no)
    (trace_min 0.14)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 /AVDD)
  (net 5 /VDD)
  (net 6 +2V8)
  (net 7 "Net-(P1-Pad3)")
  (net 8 /CA_D1)
  (net 9 /CA_D3)
  (net 10 /CA_D5)
  (net 11 /CA_D7)
  (net 12 "Net-(P1-Pad8)")
  (net 13 /CA_D0)
  (net 14 /CA_D2)
  (net 15 /CA_D4)
  (net 16 /CA_D6)
  (net 17 /CAB_SDA)
  (net 18 /CA_HREF)
  (net 19 /CAB_XCLK)
  (net 20 /CA_PWDN)
  (net 21 /CAB_SCL)
  (net 22 /CA_VSYNC)
  (net 23 /CA_PCLK)
  (net 24 "Net-(P1-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class BGA ""
    (clearance 0.03)
    (trace_width 0.14)
    (via_dia 0.4)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net /AVDD)
    (add_net /CAB_SCL)
    (add_net /CAB_SDA)
    (add_net /CAB_XCLK)
    (add_net /CA_D0)
    (add_net /CA_D1)
    (add_net /CA_D2)
    (add_net /CA_D3)
    (add_net /CA_D4)
    (add_net /CA_D5)
    (add_net /CA_D6)
    (add_net /CA_D7)
    (add_net /CA_HREF)
    (add_net /CA_PCLK)
    (add_net /CA_PWDN)
    (add_net /CA_VSYNC)
    (add_net /VDD)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad8)")
  )
  (module BGA_20_x500_y500 placed (layer F.Cu) (tedit 58943A70)
    (at 144.05 99 180)
    (descr "OVM7690 CameraCube")
    (tags "Omnivision CameraCube 7690")
    (clearance 0.1)
    (fp_text reference U1 (at 3.12 1.03 180) (layer F.SilkS))
    (fp_text value OVM7690 (at -0.2 3.75 180) (layer F.Fab) hide)
    (pad A1 smd circle (at -0.75 -1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /CA_PWDN) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad A3 smd circle (at 0.25 -1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)") (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad A4 smd circle (at 0.75 -1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)") (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B1 smd circle (at -0.75 -0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAB_SDA) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B2 smd circle (at -0.25 -0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /CAB_SCL) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B3 smd circle (at 0.25 -0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /CA_D0) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B4 smd circle (at 0.75 -0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /CA_D1) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C1 smd circle (at -0.75 0 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /CA_HREF) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C2 smd circle (at -0.25 0 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /CA_VSYNC) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C3 smd circle (at 0.25 0 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C4 smd circle (at 0.75 0 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /CA_D2) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D1 smd circle (at -0.75 0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /CA_PCLK) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D2 smd circle (at -0.25 0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /CAB_XCLK) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D3 smd circle (at 0.25 0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /CA_D5) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D4 smd circle (at 0.75 0.5 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /CA_D3) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E1 smd circle (at -0.75 1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /CA_D7) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E2 smd circle (at -0.25 1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /CA_D6) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E3 smd circle (at 0.25 1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CA_D4) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E4 smd circle (at 0.75 1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDD) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
    (pad A2 smd circle (at -0.25 -1 180) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /AVDD) (solder_mask_margin 0.0375) (clearance 0.03) (thermal_width 0.15) (thermal_gap 0.4))
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 541A9B4D)
    (at 134 99.9 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.75 -0.1 180) (layer B.SilkS))
    (fp_text value "0.1 uF" (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 541A9B8D)
    (at 134 101.9 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.43 -0.02 180) (layer B.SilkS))
    (fp_text value "10 uF" (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gj_feet:HOLE-2.5 (layer F.Cu) (tedit 5893E5EF)
    (at 130.3 102.7)
    (descr "Hole 2.5 mm")
    (tags hole)
    (fp_text reference REF** (at 0.3 -2.8) (layer F.SilkS) hide)
    (fp_text value Dummy_Empty (at 0 3.1) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.6) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 541A9B4D)
    (at 139.2 106.8)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.04 1.48) (layer B.SilkS))
    (fp_text value "0.1 uF" (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 541A9B4D)
    (at 142.8 106.8 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.44 180) (layer B.SilkS))
    (fp_text value "0.1 uF" (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 541A9B8D)
    (at 150.6 102)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.06 0.12) (layer B.SilkS))
    (fp_text value "10 uF" (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /AVDD))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer B.Cu) (tedit 541A9B4D)
    (at 150.2 100.5)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.71 -0.03) (layer B.SilkS))
    (fp_text value "0.1 uF" (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 /AVDD))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_1008 placed (layer B.Cu) (tedit 589440D0)
    (at 150.3 104.4 180)
    (descr "Inductor SMD, 1008")
    (fp_text reference L1 (at 3.01 -0.03 180) (layer B.SilkS))
    (fp_text value 3.3uH (at 0 -2.49936 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.143 0 180) (size 1.016 2.54) (layers B.Cu B.Paste B.Mask)
      (net 6 +2V8))
    (pad 2 smd rect (at 1.143 0 180) (size 1.016 2.54) (layers B.Cu B.Paste B.Mask)
      (net 4 /AVDD))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_1008 placed (layer F.Cu) (tedit 58944073)
    (at 134 100.8)
    (descr "Inductor SMD, 1008")
    (fp_text reference L2 (at 0 -2.30124) (layer F.SilkS))
    (fp_text value 3.3uH (at 0.1 2.3) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.143 0) (size 1.016 2.54) (layers F.Cu F.Paste F.Mask)
      (net 6 +2V8))
    (pad 2 smd rect (at 1.143 0) (size 1.016 2.54) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDD))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:WurthFFC_1mm_20 placed (layer F.Cu) (tedit 0)
    (at 142.75 105)
    (fp_text reference P1 (at 0.05 3.4) (layer F.SilkS))
    (fp_text value CONN_01X20 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -9.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -8.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 6 +2V8))
    (pad 3 smd rect (at -7.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at -6.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 8 /CA_D1))
    (pad 5 smd rect (at -5.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /CA_D3))
    (pad 6 smd rect (at -4.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /CA_D5))
    (pad 7 smd rect (at -3.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /CA_D7))
    (pad 8 smd rect (at -2.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P1-Pad8)"))
    (pad 9 smd rect (at -1.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 13 /CA_D0))
    (pad 10 smd rect (at -0.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 14 /CA_D2))
    (pad 11 smd rect (at 0.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 15 /CA_D4))
    (pad 12 smd rect (at 1.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 16 /CA_D6))
    (pad 13 smd rect (at 2.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAB_SDA))
    (pad 14 smd rect (at 3.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 18 /CA_HREF))
    (pad 15 smd rect (at 4.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 19 /CAB_XCLK))
    (pad 16 smd rect (at 5.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 20 /CA_PWDN))
    (pad 17 smd rect (at 6.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /CAB_SCL))
    (pad 18 smd rect (at 7.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 22 /CA_VSYNC))
    (pad 19 smd rect (at 8.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 23 /CA_PCLK))
    (pad 20 smd rect (at 9.5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P1-Pad20)"))
    (pad 0 smd rect (at -12.5 2.9) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 12.5 2.9) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
  )
  (module visionFeet:PAD-2x3.5mm placed (layer F.Cu) (tedit 588AEA6C)
    (at 130.5 98.1 90)
    (fp_text reference W1 (at 1.87 -0.69 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad3)"))
  )
  (module visionFeet:PAD-2x3.5mm placed (layer F.Cu) (tedit 588AEA6C)
    (at 154.7 98.4)
    (fp_text reference W2 (at 0.08 -2.99 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P1-Pad8)"))
  )
  (module visionFeet:PAD-2x3.5mm placed (layer F.Cu) (tedit 588AEA6C)
    (at 151.4 99.4)
    (fp_text reference W3 (at -0.03 -3.04 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P1-Pad20)"))
  )
  (module gj_feet:HOLE-2.5 (layer F.Cu) (tedit 5893E5EF)
    (at 155 102.7)
    (descr "Hole 2.5 mm")
    (tags hole)
    (fp_text reference REF** (at 0.3 -2.8) (layer F.SilkS) hide)
    (fp_text value Dummy_Empty (at 0 3.1) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.6) (layers *.Cu *.Mask))
  )
  (gr_text v1.0 (at 144.3 95.34) (layer F.SilkS))
  (gr_text OVM7690 (at 136.24 95.39) (layer F.SilkS))
  (gr_line (start 157.4 93.9) (end 128.1 93.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.4 110.2) (end 157.4 93.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.1 110.2) (end 157.4 110.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.1 93.9) (end 128.1 110.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.18))
    (min_thickness 0.18)
    (fill yes (arc_segments 32) (thermal_gap 0.18) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 128.1 93.9) (xy 157.35 93.9) (xy 157.35 110.15) (xy 128.1 110.15)
      )
    )
  )
)
