<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="78.74" y1="64.4525" x2="78.74" y2="1.5875" width="0" layer="20"/>
<wire x1="78.74" y1="1.5875" x2="77.1525" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="77.1525" y1="0" x2="1.5875" y2="0" width="0" layer="20"/>
<wire x1="1.5875" y1="0" x2="0" y2="1.5875" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="1.5875" x2="0" y2="64.4525" width="0" layer="20"/>
<wire x1="0" y1="64.4525" x2="1.5875" y2="66.04" width="0" layer="20" curve="-90"/>
<wire x1="1.5875" y1="66.04" x2="77.1525" y2="66.04" width="0" layer="20"/>
<wire x1="77.1525" y1="66.04" x2="78.74" y2="64.4525" width="0" layer="20" curve="-90"/>
<text>RPUno</text>
<text>EPCCS.ORG</text>
<text>IOREF</text>
<text>MOSI</text>
<text>0V</text>
<text>!RESET</text>
<text>SCK</text>
<text>MISO</text>
<text>SPI</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>SDA</text>
<text>SCL</text>
<text>13</text>
<text>0V</text>
<text>NC</text>
<text>D0 RX</text>
<text>D1 TX</text>
<text>+5V (*E1)</text>
<text>0V (*E0)</text>
<text>D2   INT0</text>
<text>D3   INT1/OC2B</text>
<text>D4 T0</text>
<text>D5 OC0B/T1</text>
<text>D6 OC0A</text>
<text>D7</text>
<text>B0 ICP1</text>
<text>B1 OC1A</text>
<text>B2 !SS!/OC1B</text>
<text>B3 MOSI/OC2A</text>
<text>B4 MISO</text>
<text>B5 SCK</text>
<text>0V</text>
<text>NC</text>
<text>C4 SDA</text>
<text>C5 SCL</text>
<text>SHIELD VIN IS 
CNTRLD BY D2 (IO2)</text>
<text>0V</text>
<text>0V</text>
<text>VIN</text>
<text>5V</text>
<text>NC</text>
<text>!RESET</text>
<text>IOREF 5V</text>
<text>NC</text>
<text>ADC0 C0</text>
<text>ADC1 C1</text>
<text>ADC2 C2</text>
<text>ADC3 C3</text>
<text>FT/PULSE</text>
<text>12V
17mA</text>
<text>+PV</text>
<text>-PV</text>
<text>B=4250
  100K</text>
<text>MPP IDEAL:ACTUAL
13.8:14.5V-15.2k at 70ºC
15.8:15.7V-50.7k at 40ºC
17:16.8V-100k at 25ºC
19:18.7V-357k at 0ºC</text>
<text>+BAT</text>
<text>-BAT</text>
<text>B=4250
  100K</text>
<text>13.278V:50.7k at 40ºC 
13.63V:100k at 25ºC
14.068V:357k at 0ºC</text>
<text>CHARGE RATE IS FUNCTION 
OF PV POWER UP TO MAX, 
ABOUT 0.11A PER WATT.</text>
<text>S2: CONNECT
BAT TO CC</text>
<text>S1: VIN
CONNECT</text>
<text>POWER MCU AT 13.1V 
DISCONNECT AT 11.58V.</text>
<text>RPUno</text>
<text>EPCCS.ORG</text>
<text>14140^5</text>
<text>ADC6 E2</text>
<text>ADC7 E3</text>
<text>12V 
SLA</text>
<text>36 CELL
STRING</text>
<text>PWR</text>
<text>10k B=3380 NTC
CHRG IF &gt; 0ºC  
CHRG IF &lt; 40ºC</text>
<text>0V</text>
<text>NC</text>
<text>NC</text>
<text>NC</text>
<text>ANALOG LOOP</text>
<text>12V
22mA</text>
<text>12V
22mA</text>
<text>ADC1</text>
<text>ADC0</text>
<text>0V</text>
<text>0V</text>
<text>0V</text>
<text>DIGITAL IO</text>
<text>3</text>
<text>4</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>12V
22mA</text>
<text>10mA 
TO PL</text>
<text>PL</text>
<text>0V</text>
<text>5V</text>
<text>5V</text>
<text>0V</text>
</plain>
<libraries>
<library name="J-BoardHDR">
<description>&lt;pre&gt;Arduino Footprint
Standard Interface
USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="ARDUINO_UNO">
<description>&lt;pre&gt;UNO R3 board footprint</description>
</package>
</packages>
</library>
<library name="H-Fiducial">
<description>&lt;pre&gt;Fiducianl Mark
USE AT YOUR OWN RISK...
Copyright (C) 2013 Ronald Steven Sutherland
Permission is granted to copy, distribute and/or modify this document 
under the terms of the GNU Free Documentation License, Version 1.2 or 
any later version published by the Free Software Foundation; with no 
Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A 
copy of the license is included in the section entitled "GNU Free 
Documentation License".</description>
<packages>
<package name="FIDUCIAL-1.27">
<description>&lt;pre&gt;Fiducian R=1.27mm 
STOP=2.54mm
It is up to designer to not put traces under Fiducial (i.e. Void or sold plane only)
Autorouter restricted areas are defined as RECTangles, POLYGONs, or CIRCLEs on the 
tRestrict, bRestrict, or vRestrict layers.</description>
</package>
</packages>
</library>
<library name="HW-DINMnt">
<description>&lt;pre&gt;DIN Rail Adapters

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="USA10">
<description>&lt;pre&gt;USA10-4.6 [PhxCont,1202713] DINRAIL ADAPTER UNIVERSAL 10MM 4.6MM
with #6 screw size mounting holes</description>
</package>
</packages>
</library>
<library name="R-C">
<description>&lt;pre&gt;CHIP RESISTOR
NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest highly rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805).

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C1210(3225)">
<description>&lt;pre&gt;EIA 1210 (Metric Code Size 3225) Ceramic Chip
rounded pads are added in IPC 782 rev A.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip
rounded pads are added in IPC 782 rev A
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="C-C">
<description>&lt;pre&gt; MULTILAYER CERAMIC CHIP CAPACITORS

Type: C1005 [EIA CC0402], C1608 [EIA CC0603], C2012 [EIA CC0805],
C3216 [EIA CC1206], C3225 [EIA CC1210], C4532 [EIA CC1812], C5750 [EIA CC2220]

CH 0±60 ppm/°C -25 to +85°C
C0G 0±30 ppm/°C -55 to +125°C
JB ±10% -25 to +85°C
X5R ±15% -55 to +85°C
X6S ±22% -55 to +105°C
X7R ±15% -55 to +125°C
X7S ±22% -55 to +125°C
X7T +22/-33% -55 to +125°C

TDK voltage cods
0G 4V
0J 6.3V
1A 10V
1C 16V
1E 25V
1V 35V
1H 50V
2A 100V
2E 250V
2V 350V
2W 450V
2J 630V

NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest highly rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805).

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C1206(3216)">
<description>&lt;pre&gt;EIA 1206 (Metric Code Size 3216) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A, this pad was on Arduino and may have originated from Sparkfun.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="C0603(1608)">
<description>&lt;pre&gt;EIA 0603 (Metric Code Size 1608) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A, this pad was on Arduino Due and may have originated from Sparkfun.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="U-BUCK">
<description>&lt;pre&gt;BUCK Control and ilk

USE AT YOUR OWN RISK...

Copyright (C) 2015 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="12MSOP-EDP-HAND">
<description>&lt;pre&gt;12 Micro-SMALL OUTLINE PACKAGE (MSOP) with Exposed Die Pad
Warning: This Exposed Die Pad is setup for hand solder, not PnP.</description>
</package>
</packages>
</library>
<library name="L-PSMD">
<description>&lt;pre&gt;Inductor Power SMD

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="L3939">
<description>&lt;pre&gt;Dimension (mm): 0.39 x 0.39 (10.1 x 10.1)
15UH2A2 [TDK,SLF10145T-150M2R2-PF] INDUCTOR POWER SHIELDED 15UH 2A2 SMD</description>
</package>
</packages>
</library>
<library name="D-GP">
<description>&lt;pre&gt;GEN PURPOSE DIODE
USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOD123">
<description>&lt;pre&gt;SOD123
http://www.diodes.com/datasheets/ap02001.pdf</description>
</package>
</packages>
</library>
<library name="Q-NPN">
<description>&lt;pre&gt;NPN Bipolar junction transistor

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 1 is alone (Cathode)
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="Q-NCH">
<description>&lt;pre&gt;N-CHANNEL MOSFET
ENHANCEMENT MODE is shown with a open/broken channel
DEPLETION MODE is shown with a closed/complete channel thus the idea of being on with zero gate voltage.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 3 is alone
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="S-Tactile">
<description>&lt;pre&gt;Switch Tactile/Snap-acting

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip
rounded pads are added in IPC 782 rev A</description>
</package>
</packages>
</library>
<library name="U-Linear">
<description>&lt;pre&gt;Linear Amplifiers, Sensor Interfaces

USE AT YOUR OWN RISK...

Copyright (C) 2014 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23-6">
<description>&lt;pre&gt; Based on TI drawing 4204403-3/E which falls within JEDEC MO-193 variation AA (6p in)</description>
</package>
<package name="SOT23-5">
<description>&lt;pre&gt;Small Outline SOT23-5
Diodes calls it a SOT25</description>
</package>
</packages>
</library>
<library name="Q-PCH">
<description>&lt;pre&gt;N-CHANNEL MOSFET
ENHANCEMENT MODE is shown with a open/broken channel
DEPLETION MODE is shown with a closed/complete channel thus the idea of being on with zero gate voltage.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 3 is alone
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="D-SBR">
<description>&lt;pre&gt;Super Barrier Rectifier
Super barrier diodes are rectifier diodes that incorporate the low forward voltage
drop of the Schottky diode with the surge-handling capability and low reverse 
leakage current of a normal p–n junction diode.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SMA">
<description>&lt;pre&gt;SMB 
http://www.diodes.com/datasheets/ap02001.pdf
center to center 4 mm
pad 2.5X x 1.7Y mm</description>
</package>
</packages>
</library>
<library name="J-HDR3.5mm">
<description>&lt;pre&gt;HEADER 3.5MM center to center
USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="MCV4">
<description>&lt;pre&gt;MCV 1,5/4-G-3,5-RN [PHOENIX CONTACT,1843622] CONN HEADER SHROUDED 4POS 3.5MM
PST 1,0/4-3,5 [PHOENIX CONTACT,1945119] CONN HEADER STRIP PIN 4POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV5">
<description>&lt;pre&gt;MCV 1,5/5-G-3,5-RN [PHOENIX CONTACT,1843635] CONN HEADER SHROUDED 5POS 3.5MM
MCVR 1,5/5-ST-3,5 [PHOENIX CONTACT,1863181] CONN PLUG 5POS SCREW 3.5MM
PST 1,0/5-3,5 [PHOENIX CONTACT,1945122] CONN HEADER STRIP PIN 5POS 3.5MM
PT 1,5/5-PVH-3,5 [PHOENIX CONTACT,1984044] CONN PLUG STRIP 5POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV3">
<description>&lt;pre&gt;MCV 1,5/ 3-G-3,5-RN [PHOENIX CONTACT,1731484] CONN HEADER SHROUDED 3POS 3.5MM
PST 1,0/3-3,5 [PHOENIX CONTACT,1945106] CONN HEADER STRIP PIN 3POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV8">
<description>&lt;pre&gt;PHOENIX CONTACT 1843664
MCV 1,5/ 8-G-3,5
Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV6">
<description>&lt;pre&gt;MCV 1,5/6-G-3,5 [PHOENIX CONTACT,1843648] CONN HEADER SHROUDED 6POS 3.5MM
MCVR 1,5/6-ST-3,5 [PHOENIX CONTACT,1863194] CONN PLUG 6POS SCREW 3.5MM
PST 1,0/6-3,5 [PHOENIX CONTACT,1945135] CONN HEADER STRIP PIN 6POS 3.5MM
PT 1,5/6-PVH-3,5 [PHOENIX CONTACT,1984057] CONN PLUG STRIP 6POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
</packages>
</library>
<library name="U-AVR">
<description>&lt;pre&gt;MCU's 8bit AVR 

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="ISP">
</package>
</packages>
</library>
<library name="L-FB">
<description>&lt;pre&gt;CHIP FERRITE BEADS
NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805) and similar devices.

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ferrite Chip
rounded pads are added in IPC 782 rev A
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="Y-XTL">
<description>&lt;pre&gt;CRYSTAL
i.e. NDK NX3225SA-12.000000MHZ-STD-CSR-1

USE AT YOUR OWN RISK...

Copyright (C) 2014 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="CSM-3X">
<description>&lt;pre&gt;SMD CRYSTAL
16MHZ20  [ECS,ECS-160-20-3X-TR] CRYSTAL 16MHZ 20PF 30PPM  CSM-3X
Source: www.ecsxtal.com .. Crystal 16MHz CSM-3X.PDF</description>
</package>
</packages>
</library>
<library name="J-HDR2.54mm">
<description>&lt;pre&gt;HEADER 2.54MM center to center

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="F1X10">
<description>&lt;pre&gt;FEMALE HEADER 10POS</description>
</package>
<package name="F1X8">
<description>&lt;pre&gt;FEMALE HEADER 8POS</description>
</package>
<package name="1X2">
</package>
</packages>
</library>
<library name="C-T">
<description>&lt;pre&gt;Tantalum Electrolytic Capacitors
EIA Code 	Case Code 	L 	W 	H 	W1 	A
Tolerance 	±0.2 	+0.2/–0.1 	+0.2/–0.1 	+0.2 	+0.3/–0.2
3216-10 	I, K 	3.2 	1.6 	1.0 (max) 	1.2 	0.8
3216-12 	S 	3.2 	1.6 	1.2 (max) 	1.2 	0.8
3216-18 	A 	3.2 	1.6 	1.6 	1.2 	0.8
3528-12 	T 	3.5 	2.8 	1.2 (max) 	2.2 	0.8
3528-15 	M, H 	3.5 	2.8 	1.5 (max) 	2.2 	0.8
3528-21 	B 	3.5 	2.8 	1.9 	2.2 	0.8
6032-15 	U, W 	6.0 	3.2 	1.5 (max) 	2.2 	1.3
6032-28 	C 	6.0 	3.2 	2.6 	2.2 	1.3
7343-20 	V, Y 	7.3 	4.3 	2.0 (max) 	2.4 	1.3
7343-31 	D 	7.3 	4.3 	2.9 	2.4 	1.3
7343-43 	X, E 	7.3 	4.3 	4.1 	2.4 	1.3

Metric	[inch]
2013 	[0805]
3216 	[1206]
3528 	[1411]
6032 	[2413]
7343 	[2917]

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="3216">
<description>&lt;pre&gt;3.2mm x 1.6mm
Surface mount dimensions (EIA standard package sizes)
EIA Code 	Case Code 	L 	W 	H 	W1 	A
Tolerance 	±0.2 	+0.2/–0.1 	+0.2/–0.1 	+0.2 	+0.3/–0.2
3216-10 	I, K 	3.2 	1.6 	1.0 (max) 	1.2 	0.8
3216-12 	S, P 	3.2 	1.6 	1.2 (max) 	1.2 	0.8
3216-18 	A 	3.2 	1.6 	1.6 	1.2 	0.8

Note 3.2mm x 1.6mm is about 1206 (or .012 x .006 in)</description>
</package>
</packages>
</library>
<library name="P-DCDC">
<description>&lt;pre&gt;POWER SUPPLIE DC 2 DC
some units are for schmatics only

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="OKI-78SR-H">
<description>&lt;pre&gt;OKI-78SR Horizontal Mount
OKI-78SR-5/1.5-W36H-C
Murata Power Solutions
Ultra wide 7 to 36 VDC input range
this pinout is odd so check it</description>
</package>
</packages>
</library>
<library name="J-TP">
<description>&lt;pre&gt;Test Pins/Pads

Cream on SMD OFF
Attribute TP_SIGNAL_NAME

USE AT YOUR OWN RISK...

    Copyright (C) 2015 Ronald Sutherland
    Released under the Creative Commons 
    Attribution-ShareAlike 4.0 International
    http://creativecommons.org/licenses/by-sa/4.0</description>
<packages>
<package name="P1-08">
<description>&lt;pre&gt;TEST PAD 20AWG</description>
</package>
</packages>
</library>
<library name="Q-PNP">
<description>&lt;pre&gt;PNP Bipolar junction transistor

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 1 is alone (Cathode)
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="J-BoardHDR" package="ARDUINO_UNO" value="ARDUINO-UNO"/>
<element name="U$2" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="U$3" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="U$4" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="HW1" library="HW-DINMnt" package="USA10" value="USA10-4,6">
<attribute name="NAME"/>
</element>
<element name="HW2" library="HW-DINMnt" package="USA10" value="USA10-4,6">
<attribute name="NAME"/>
</element>
<element name="R11" library="R-C" package="C1210(3225)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="R-C" package="C0805(2012)" value="200k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="R-C" package="C0805(2012)" value="68.1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="R-C" package="C0805(2012)" value="182k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="U-BUCK" package="12MSOP-EDP-HAND" value="LT3652">
<attribute name="NAME"/>
</element>
<element name="R26" library="R-C" package="C0805(2012)" value="45.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="R-C" package="C1210(3225)" value="0R068">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="L-PSMD" package="L3939" value="15uH 2A2">
<attribute name="NAME"/>
</element>
<element name="D2" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="C1" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="R-C" package="C0805(2012)" value="121k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="R-C" package="C0805(2012)" value="**10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="S-Tactile" package="C0805(2012)" value="PAD"/>
<element name="C9" library="C-C" package="C0805(2012)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="R2" library="R-C" package="C0805(2012)" value="205k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="R-C" package="C0805(2012)" value="316k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="R-C" package="C0805(2012)" value="280k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="U-Linear" package="SOT23-6" value="TPS3700">
<attribute name="NAME"/>
</element>
<element name="Q9" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="S2" library="S-Tactile" package="C0805(2012)" value="PAD"/>
<element name="C2" library="C-C" package="C0603(1608)" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="R-C" package="C0805(2012)" value="5.62k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="D1" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="R19" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="J-HDR3.5mm" package="MCV4" value="PST1,0/4-3,5">
<attribute name="NAME"/>
</element>
<element name="C18" library="C-C" package="C0603(1608)" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="R-C" package="C0805(2012)" value="432k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="R-C" package="C0805(2012)" value="200k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="C-C" package="C0603(1608)" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="C-C" package="C0603(1608)" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="C-C" package="C0603(1608)" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="L-FB" package="C0805(2012)" value="JMP">
<attribute name="NAME"/>
</element>
<element name="C21" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="J11" library="U-AVR" package="ISP" value="ICSP">
<attribute name="NAME"/>
</element>
<element name="J5" library="J-HDR2.54mm" package="F1X10" value="PPPC101LFBN">
<attribute name="NAME"/>
</element>
<element name="J10" library="J-HDR2.54mm" package="F1X10" value="PPPC101LFBN">
<attribute name="NAME"/>
</element>
<element name="J9" library="J-HDR2.54mm" package="F1X10" value="PPPC101LFBN"/>
<element name="J6" library="J-HDR2.54mm" package="F1X8" value="PPPC081LFBN">
<attribute name="NAME"/>
</element>
<element name="U6" library="U-AVR" package="TQFP32-08" value="ATMEGA328PB-AU">
<attribute name="NAME"/>
</element>
<element name="C3" library="C-T" package="3216" value="106A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="Y-XTL" package="CSM-3X" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="R13" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="J-TP" package="P1-08" value="TPPAD1-08">
<attribute name="NAME"/>
</element>
<element name="TP4" library="J-TP" package="P1-08" value="TPPAD1-08">
<attribute name="NAME"/>
</element>
<element name="TP1" library="J-TP" package="P1-08" value="TPPAD1-08">
<attribute name="NAME"/>
</element>
<element name="R10" library="R-C" package="C0805(2012)" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="J-TP" package="P1-08" value="TPPAD1-08"/>
<element name="R44" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="J-HDR2.54mm" package="1X2" value="">
<attribute name="NAME"/>
</element>
<element name="R12" library="R-C" package="C1210(3225)" value="0R068">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="U-Linear" package="SOT23-5" value="1087">
<attribute name="NAME"/>
</element>
<element name="U3" library="U-Linear" package="SOT23-5" value="1087">
<attribute name="NAME"/>
</element>
<element name="C6" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="C-C" package="C0603(1608)" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="C-C" package="C0603(1608)" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="J-HDR3.5mm" package="MCV5" value="PST1,0/5-3,5"/>
<element name="R16" library="R-C" package="C0805(2012)" value="27">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q8" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="R-C" package="C0805(2012)" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="C-C" package="C0603(1608)" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="R-C" package="C0805(2012)" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="C-C" package="C0603(1608)" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="R-C" package="C0805(2012)" value="27">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q12" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q11" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="R-C" package="C0805(2012)" value="32.4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q15" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q14" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="R-C" package="C0805(2012)" value="60.4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q17" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q16" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="R-C" package="C0805(2012)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q26" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="J-HDR3.5mm" package="MCV3" value="PST1,0/3-3,5"/>
<element name="Q10" library="Q-PCH" package="SOT23" value="K84">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q13" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q21" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q23" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q30" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q31" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="J-HDR3.5mm" package="MCV8" value="PST1,0&amp;8-3,5"/>
<element name="Q20" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q22" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q29" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q32" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q27" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q28" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="P-DCDC" package="OKI-78SR-H" value="I50115"/>
<element name="Q25" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="R-C" package="C0805(2012)" value="182">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q24" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="R-C" package="C0805(2012)" value="27">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q34" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q33" library="Q-PNP" package="SOT23" value="K3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R59" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q18" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q19" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="J-HDR2.54mm" package="1X2" value="">
<attribute name="NAME"/>
</element>
<element name="J7" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5"/>
<element name="R53" library="R-C" package="C0805(2012)" value="JMP"/>
<element name="R54" library="R-C" package="C0805(2012)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="0V">
<contactref element="R27" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="SNK6"/>
<contactref element="C10" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="U1" pad="SNK5"/>
<contactref element="U1" pad="SNK7"/>
<contactref element="U1" pad="SNK0"/>
<contactref element="U1" pad="SNK1"/>
<contactref element="U1" pad="SNK3"/>
<contactref element="U1" pad="SNK4"/>
<contactref element="C9" pad="2"/>
<contactref element="Q3" pad="E"/>
<contactref element="Q4" pad="E"/>
<contactref element="R33" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="S2" pad="2"/>
<contactref element="R35" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="C24" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="J11" pad="6"/>
<contactref element="J10" pad="4"/>
<contactref element="J6" pad="2"/>
<contactref element="J6" pad="3"/>
<contactref element="U6" pad="5"/>
<contactref element="U6" pad="21"/>
<contactref element="C3" pad="-"/>
<contactref element="Q6" pad="2(S)"/>
<contactref element="J5" pad="9"/>
<contactref element="U4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="J4" pad="3"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="R30" pad="1"/>
<contactref element="Q26" pad="E"/>
<contactref element="R51" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="R43" pad="1"/>
<contactref element="Q13" pad="2(S)"/>
<contactref element="J3" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="R59" pad="1"/>
<contactref element="Q19" pad="2(S)"/>
<contactref element="J12" pad="1"/>
<contactref element="J7" pad="5"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="Q2" pad="1(G)"/>
<contactref element="Q1" pad="3(D)"/>
<contactref element="Q8" pad="E"/>
<contactref element="R16" pad="2"/>
<contactref element="Q12" pad="E"/>
<contactref element="R29" pad="2"/>
<contactref element="Q10" pad="2(S)"/>
<contactref element="R38" pad="2"/>
<contactref element="Q20" pad="C"/>
<contactref element="Q22" pad="C"/>
<contactref element="Q27" pad="C"/>
<contactref element="Q29" pad="C"/>
<contactref element="Q32" pad="C"/>
<contactref element="U2" pad="1"/>
<contactref element="Q24" pad="C"/>
<contactref element="R58" pad="2"/>
<contactref element="Q34" pad="E"/>
<contactref element="Q18" pad="2(S)"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="SW">
<contactref element="U1" pad="12"/>
<contactref element="L1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="D4" pad="K"/>
</signal>
<signal name="PWR">
<contactref element="R4" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="C12" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="C11" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="C17" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="2(S)"/>
<contactref element="R36" pad="2"/>
<contactref element="TP4" pad="TP"/>
<contactref element="R12" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="PV_IN">
<contactref element="C8" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="D1" pad="K"/>
<contactref element="R34" pad="2"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="SENSE">
<contactref element="R11" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="R3" pad="2"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="TC+">
<contactref element="R26" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="TC-">
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="D2" pad="C"/>
<contactref element="U1" pad="11"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C10" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="Q3" pad="C"/>
</signal>
<signal name="NTC1">
<contactref element="U1" pad="8"/>
<contactref element="R23" pad="1"/>
<contactref element="J12" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$46">
<contactref element="Q3" pad="B"/>
<contactref element="R5" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="5V88PL-DWN">
<contactref element="R14" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="R22" pad="1"/>
<contactref element="Q5" pad="1(G)"/>
</signal>
<signal name="+BAT">
<contactref element="R14" pad="1"/>
<contactref element="Q5" pad="2(S)"/>
<contactref element="Q6" pad="1(G)"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="!FAULT">
<contactref element="U1" pad="5"/>
<contactref element="R19" pad="2"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="2"/>
<contactref element="Q4" pad="B"/>
</signal>
<signal name="N$7">
<contactref element="Q4" pad="C"/>
<contactref element="R33" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="Q2" pad="2(S)"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Q9" pad="2(S)"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U5" pad="3"/>
<contactref element="R32" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="Q9" pad="1(G)"/>
<contactref element="R21" pad="2"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="6V58PL-DWN">
<contactref element="Q2" pad="3(D)"/>
<contactref element="R4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="Q1" pad="1(G)"/>
</signal>
<signal name="N$17">
<contactref element="S2" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="D6" pad="C"/>
<contactref element="U5" pad="6"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="S1" pad="1"/>
<contactref element="Q9" pad="3(D)"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="PV_IN_ADC6">
<contactref element="J5" pad="7"/>
<contactref element="U6" pad="19"/>
<contactref element="C18" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="L2" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="D7" pad="C"/>
<contactref element="J11" pad="2"/>
<contactref element="U6" pad="4"/>
<contactref element="J6" pad="7"/>
<contactref element="J6" pad="4"/>
<contactref element="C3" pad="+"/>
<contactref element="R44" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="C6" pad="1"/>
<contactref element="Q21" pad="1(G)"/>
<contactref element="Q23" pad="1(G)"/>
<contactref element="Q30" pad="1(G)"/>
<contactref element="Q31" pad="1(G)"/>
<contactref element="Q28" pad="1(G)"/>
<contactref element="U2" pad="3"/>
<contactref element="Q25" pad="1(G)"/>
<contactref element="L2" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="U6" pad="18"/>
<contactref element="J7" pad="6"/>
<contactref element="R46" pad="2"/>
</signal>
<signal name="RX">
<contactref element="J9" pad="3"/>
<contactref element="U6" pad="30"/>
</signal>
<signal name="TX">
<contactref element="J9" pad="4"/>
<contactref element="U6" pad="31"/>
</signal>
<signal name="IO2">
<contactref element="J9" pad="5"/>
<contactref element="U6" pad="32"/>
<contactref element="R53" pad="1"/>
<contactref element="R53" pad="2"/>
<contactref element="Q19" pad="1(G)"/>
<contactref element="R54" pad="1"/>
<contactref element="R46" pad="1"/>
</signal>
<signal name="IO3">
<contactref element="J9" pad="6"/>
<contactref element="U6" pad="1"/>
<contactref element="R57" pad="2"/>
</signal>
<signal name="IO4">
<contactref element="J9" pad="7"/>
<contactref element="U6" pad="2"/>
<contactref element="R50" pad="2"/>
</signal>
<signal name="IO5">
<contactref element="J9" pad="8"/>
<contactref element="U6" pad="9"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="IO6">
<contactref element="J9" pad="9"/>
<contactref element="U6" pad="10"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="IO7">
<contactref element="J9" pad="10"/>
<contactref element="U6" pad="11"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="J11" pad="3"/>
<contactref element="J10" pad="5"/>
<contactref element="U6" pad="17"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="J11" pad="1"/>
<contactref element="J10" pad="6"/>
<contactref element="U6" pad="16"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="J11" pad="4"/>
<contactref element="J10" pad="7"/>
<contactref element="U6" pad="15"/>
<contactref element="R55" pad="2"/>
</signal>
<signal name="!SS">
<contactref element="J10" pad="8"/>
<contactref element="U6" pad="14"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="IO9">
<contactref element="J10" pad="9"/>
<contactref element="U6" pad="13"/>
<contactref element="Q13" pad="1(G)"/>
</signal>
<signal name="IO8">
<contactref element="J10" pad="10"/>
<contactref element="U6" pad="12"/>
<contactref element="R42" pad="2"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="C22" pad="1"/>
<contactref element="U6" pad="20"/>
</signal>
<signal name="!RESET!">
<contactref element="R31" pad="1"/>
<contactref element="D7" pad="A"/>
<contactref element="J11" pad="5"/>
<contactref element="U6" pad="29"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="ADC0">
<contactref element="J5" pad="1"/>
<contactref element="U6" pad="23"/>
<contactref element="R15" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="ADC1">
<contactref element="J5" pad="2"/>
<contactref element="U6" pad="24"/>
<contactref element="C14" pad="1"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$115">
<contactref element="C23" pad="2"/>
<contactref element="U6" pad="7"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$116">
<contactref element="C24" pad="2"/>
<contactref element="U6" pad="8"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="SDA1">
<contactref element="U6" pad="3"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="SCL1">
<contactref element="U6" pad="6"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U6" pad="27"/>
<contactref element="J10" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U6" pad="28"/>
<contactref element="J10" pad="1"/>
</signal>
<signal name="-BAT">
<contactref element="Q6" pad="3(D)"/>
<contactref element="D5" pad="A"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="D5" pad="C"/>
<contactref element="R13" pad="2"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="PL">
<contactref element="R51" pad="2"/>
<contactref element="R52" pad="1"/>
<contactref element="J8" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="BAT_I">
<contactref element="Q5" pad="3(D)"/>
<contactref element="R12" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="CHRG_ADC2">
<contactref element="U4" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="J5" pad="3"/>
<contactref element="U6" pad="25"/>
</signal>
<signal name="DISCHRG_ADC3">
<contactref element="U3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="U6" pad="26"/>
</signal>
<signal name="N$20">
<contactref element="R16" pad="1"/>
<contactref element="Q7" pad="E"/>
<contactref element="Q8" pad="B"/>
</signal>
<signal name="N$23">
<contactref element="Q7" pad="B"/>
<contactref element="Q8" pad="C"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="22MA_A0">
<contactref element="Q7" pad="C"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R15" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="R28" pad="2"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$28">
<contactref element="R29" pad="1"/>
<contactref element="Q11" pad="E"/>
<contactref element="Q12" pad="B"/>
</signal>
<signal name="N$29">
<contactref element="Q11" pad="B"/>
<contactref element="Q12" pad="C"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="22MA_A1">
<contactref element="Q11" pad="C"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="PWR_ADC7">
<contactref element="J5" pad="8"/>
<contactref element="U6" pad="22"/>
<contactref element="C19" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$114">
<contactref element="R39" pad="1"/>
<contactref element="Q14" pad="E"/>
<contactref element="Q15" pad="B"/>
</signal>
<signal name="N$119">
<contactref element="Q14" pad="B"/>
<contactref element="Q15" pad="C"/>
<contactref element="R40" pad="2"/>
</signal>
<signal name="N$122">
<contactref element="R41" pad="1"/>
<contactref element="Q16" pad="E"/>
<contactref element="Q17" pad="B"/>
</signal>
<signal name="N$123">
<contactref element="Q16" pad="B"/>
<contactref element="Q17" pad="C"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="PL17MA">
<contactref element="Q14" pad="C"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$107">
<contactref element="Q26" pad="B"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="N$108">
<contactref element="Q26" pad="C"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="Q16" pad="C"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="Q10" pad="3(D)"/>
<contactref element="R39" pad="2"/>
<contactref element="Q15" pad="E"/>
<contactref element="R41" pad="2"/>
<contactref element="Q17" pad="E"/>
</signal>
<signal name="N$25">
<contactref element="R38" pad="1"/>
<contactref element="Q13" pad="3(D)"/>
<contactref element="Q10" pad="1(G)"/>
</signal>
<signal name="IO13_">
<contactref element="Q21" pad="3(D)"/>
<contactref element="J2" pad="8"/>
<contactref element="Q20" pad="E"/>
<contactref element="Q20" pad="B"/>
</signal>
<signal name="IO12_">
<contactref element="Q23" pad="3(D)"/>
<contactref element="Q22" pad="E"/>
<contactref element="Q22" pad="B"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="IO10_">
<contactref element="Q30" pad="3(D)"/>
<contactref element="Q29" pad="B"/>
<contactref element="Q29" pad="E"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="IO3_">
<contactref element="J2" pad="3"/>
<contactref element="Q31" pad="3(D)"/>
<contactref element="Q32" pad="B"/>
<contactref element="Q32" pad="E"/>
</signal>
<signal name="IO11_">
<contactref element="Q28" pad="3(D)"/>
<contactref element="Q27" pad="B"/>
<contactref element="Q27" pad="E"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="Q23" pad="2(S)"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="Q28" pad="2(S)"/>
<contactref element="R55" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="Q30" pad="2(S)"/>
<contactref element="R56" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="Q31" pad="2(S)"/>
<contactref element="R57" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="Q21" pad="2(S)"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="Q25" pad="2(S)"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="IO4_">
<contactref element="Q24" pad="B"/>
<contactref element="Q24" pad="E"/>
<contactref element="Q25" pad="3(D)"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$30">
<contactref element="R58" pad="1"/>
<contactref element="Q33" pad="E"/>
<contactref element="Q34" pad="B"/>
</signal>
<signal name="N$33">
<contactref element="Q33" pad="B"/>
<contactref element="Q34" pad="C"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="22MA_DIO">
<contactref element="Q33" pad="C"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="R45" pad="2"/>
<contactref element="Q18" pad="1(G)"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="SHLD_VIN">
<contactref element="J6" pad="1"/>
<contactref element="Q18" pad="3(D)"/>
</signal>
<signal name="N$37">
<contactref element="Q19" pad="3(D)"/>
<contactref element="R47" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
