<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.7" y2="0" width="0" layer="20"/>
<wire x1="12.7" y1="0" x2="12.7" y2="33.02" width="0" layer="20"/>
<wire x1="12.7" y1="33.02" x2="0" y2="33.02" width="0" layer="20"/>
<wire x1="0" y1="33.02" x2="0" y2="0" width="0" layer="20"/>
<text>3.3V</text>
<text>AI</text>
<text>QUAD B</text>
<text>QUAD A</text>
<text>QUAD IDX</text>
<text>GND</text>
<text>R LIMIT</text>
<text>NC</text>
<text>F LIMIT</text>
<text>5V</text>
<text>GND</text>
<text>R LIMIT</text>
<text>NC</text>
<text>F LIMIT</text>
<text>5V</text>
<text>3.3V</text>
<text>AI</text>
<text>QUAD B</text>
<text>QUAD A</text>
<text>QUAD IDX</text>
<hole x="6.35" y="3.81" drill="4.9784"/>
<hole x="6.35" y="29.21" drill="4.9784"/>
<text>REV 2017A</text>
<text>TEAMARGOS.ORG</text>
</plain>
<libraries>
<library name="pel_misc">
<packages>
<package name="FTSH-105-D">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="pel_misc" package="FTSH-105-D" value="CONN_5-2"/>
<element name="X2" library="pel_misc" package="FTSH-105-D" value="CONN_5-2"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="X1" pad="3"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="X2" pad="5"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="7"/>
<contactref element="X2" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="X2" pad="9"/>
<contactref element="X1" pad="9"/>
</signal>
<signal name="N$6">
<contactref element="X1" pad="10"/>
<contactref element="X2" pad="10"/>
</signal>
<signal name="N$7">
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="X1" pad="4"/>
<contactref element="X2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="X1" pad="6"/>
<contactref element="X2" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="X1" pad="8"/>
<contactref element="X2" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
