(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/Pin3")
	(net 2 "/Pin4")
	(net 3 "Net-(D1001-Pad1)")
	(net 4 "Net-(D1002-Pad1)")
	(net 5 "/Pin1")
	(net 6 "/Pin21")
	(net 7 "/Pin24")
	(net 8 "/Pin15")
	(net 9 "/Pin17")
	(net 10 "/Pin19")
	(net 11 "/Pin22")
	(net 12 "/Pin18")
	(net 13 "/Pin20")
	(net 14 "/Pin13")
	(net 15 "/Pin23")
	(net 16 "/Pin14")
	(net 17 "/Pin16")
	(net 18 "/Pin6")
	(net 19 "/Pin10")
	(net 20 "/Pin5")
	(net 21 "/Pin8")
	(net 22 "/Pin11")
	(net 23 "/Pin2")
	(net 24 "/Pin7")
	(net 25 "/Pin12")
	(net 26 "/Pin9")
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 146.89 74.550001 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1001"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_US"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(D1001-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/Pin3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "JSK:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 143.64 74.550001 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1002"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "JSK:LED_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Common 5mm diameter LED"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED_D5.0mm_Clear LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm LED_D5.0mm_Horizontal_O6.35mm_Z3.0mm")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1002-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/Pin1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "JSK:8-pin-clip"
		(layer "F.Cu")
		(at 146.75 71.07 90)
		(descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "J1003"
			(at 0.89 -5.62 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at -0.1 5.48 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "JSK:8-pin-clip"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr smd)
		(pad "" np_thru_hole circle
			(at -1.17 -2.5675 90)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "F&B.Cu")
		)
		(pad "" np_thru_hole circle
			(at -1.17 -1.285 90)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "F&B.Cu")
		)
		(pad "" np_thru_hole circle
			(at -1.17 -0.0025 90)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "F&B.Cu")
		)
		(pad "" np_thru_hole circle
			(at -1.17 1.28 90)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "F&B.Cu")
		)
		(pad "" np_thru_hole circle
			(at -1.17 2.5625 90)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "F&B.Cu")
		)
		(pad "A1" connect roundrect
			(at 0 -1.904999 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/Pin4")
			(pintype "passive")
		)
		(pad "A2" connect roundrect
			(at 0 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/Pin14")
			(pintype "passive")
		)
		(pad "A3" connect roundrect
			(at 0 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/Pin23")
			(pintype "passive")
		)
		(pad "A4" connect roundrect
			(at 0 1.904999 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/Pin3")
			(pintype "passive")
		)
		(pad "B1" connect roundrect
			(at -0.01 1.91 90)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/Pin4")
			(pintype "passive")
		)
		(pad "B2" connect roundrect
			(at -0.01 0.64 90)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/Pin14")
			(pintype "passive")
		)
		(pad "B3" connect roundrect
			(at -0.01 -0.63 90)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/Pin23")
			(pintype "passive")
		)
		(pad "B4" connect roundrect
			(at -0.01 -1.9 90)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/Pin3")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 142.93 77.6 45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1001"
			(at 0 -1.16 45)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 1.16 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.48 0 45)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/Pin4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 45)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/Pin3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 144.288391 99.292925 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW1001"
			(at 3.25 -2.000001 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Push_Button"
			(at 3.75 6.7 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Common 6mmx6mm Push Button"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 2.25 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Pin3")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Pin3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 4.500001 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Pin15")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.500001 4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Pin15")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "JSK:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 145.87 74.550001 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1001"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "JSK:LED_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Common 5mm diameter LED"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED_D5.0mm_Clear LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm LED_D5.0mm_Horizontal_O6.35mm_Z3.0mm")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(D1001-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/Pin4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 144.63 74.550001 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1002"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_US"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1002-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/Pin3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
		(layer "F.Cu")
		(at 145.775 79.76 -45)
		(descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U1001"
			(at 0 -3.299999 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ATtiny417-M"
			(at 0 3.299999 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001901B.pdf"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, VQFN-24"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*4x4mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.65 -0.65 315)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at -0.65 0.65 315)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at 0.65 -0.65 315)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at 0.65 0.65 315)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "1" smd roundrect
			(at -1.9375 -1.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/Pin1")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -1.937499 -0.75 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/Pin2")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -1.9375 -0.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/Pin3")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -1.9375 0.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/Pin4")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -1.937499 0.75 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/Pin5")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -1.9375 1.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/Pin6")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -1.25 1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/Pin7")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -0.75 1.937499 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/Pin8")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -0.25 1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/Pin9")
			(pinfunction "PB7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 0.25 1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/Pin10")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 0.75 1.937499 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/Pin11")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 1.25 1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/Pin12")
			(pinfunction "PB4")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 1.9375 1.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/Pin13")
			(pinfunction "PB3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 1.937499 0.75 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/Pin14")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 1.9375 0.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/Pin15")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 1.9375 -0.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/Pin16")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 1.937499 -0.75 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/Pin17")
			(pinfunction "PC0")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 1.9375 -1.25 315)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/Pin18")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 1.25 -1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/Pin19")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 0.75 -1.937499 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/Pin20")
			(pinfunction "PC3")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 0.25 -1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/Pin21")
			(pinfunction "PC4")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at -0.25 -1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/Pin22")
			(pinfunction "PC5")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at -0.75 -1.937499 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/Pin23")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at -1.25 -1.9375 315)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/Pin24")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 0 0 315)
			(size 2.6 2.6)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "/Pin3")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 140.375 71.76 180)
		(descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x12 2.54mm single row")
		(property "Reference" "J1002"
			(at 0 2.33 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x12_Pin"
			(at 0 -30.27 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -13.97 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Pin1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/Pin2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Pin3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/Pin4")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Pin5")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Pin6")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/Pin7")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/Pin8")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/Pin9")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Pin10")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/Pin11")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/Pin12")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 153.075 71.76 180)
		(descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x12 2.54mm single row")
		(property "Reference" "J1001"
			(at 0 2.33 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x12_Pin"
			(at 0 -30.27 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "qfn24-4x4-p0.5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -13.97 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Pin24")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Pin23")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Pin22")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Pin21")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Pin20")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Pin19")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Pin18")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Pin17")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/Pin16")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Pin15")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Pin14")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Pin13")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 138.06 69.13)
		(end 155.43 101.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "3V"
		(at 148.18 75.14 0)
		(layer "F.SilkS")
	)
	(gr_text "24\n\n23U\n\n22\n\n21\n\n20\n\n19\n\n18\n\n17\n\n16\n\nB15\n\n14T\n\n13R"
		(at 151.02 70.65 0)
		(layer "F.SilkS")
	)
	(gr_text "1\n\n2\n\n3V\n\n4G\n\n5\n\n6\n\n7\n\n8\n\n9\n\n10\n\n11\n\n12"
		(at 142.41 71.09 0)
		(layer "F.SilkS")
	)
	(gr_text "23U 14S"
		(at 149.5 72.52 180)
		(layer "F.SilkS")
	)
	(gr_text "QFN-24\n4x4 P0.5\nBreakout\n(+ATtiny417)\nv0.1\n2025-02-21\nJSK"
		(at 146.41 88.03 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 144.23 75.73 0)
		(layer "F.SilkS")
	)
	(gr_text "3G       4V"
		(at 150.58 69.38 180)
		(layer "F.SilkS")
	)
)
