(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 50)
    (zones 0)
    (modules 6)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "Net-(J1-Pad17)")
  (net 18 "Net-(J1-Pad18)")
  (net 19 "Net-(J1-Pad19)")
  (net 20 "Net-(J1-Pad20)")
  (net 21 "Net-(J3-Pad5)")
  (net 22 "Net-(J3-Pad3)")
  (net 23 "Net-(J3-Pad4)")
  (net 24 "Net-(J3-Pad1)")
  (net 25 "Net-(J3-Pad2)")
  (net 26 "Net-(J5-Pad14)")
  (net 27 "Net-(J5-Pad13)")
  (net 28 "Net-(J5-Pad12)")
  (net 29 "Net-(J5-Pad11)")
  (net 30 "Net-(J5-Pad10)")
  (net 31 "Net-(J5-Pad9)")
  (net 32 "Net-(J5-Pad8)")
  (net 33 "Net-(J5-Pad7)")
  (net 34 "Net-(J5-Pad6)")
  (net 35 "Net-(J5-Pad5)")
  (net 36 "Net-(J5-Pad4)")
  (net 37 "Net-(J5-Pad3)")
  (net 38 "Net-(J5-Pad2)")
  (net 39 "Net-(J5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad11)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad13)")
    (add_net "Net-(J5-Pad14)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
  )
  (module .Connector:B2B_Flex_14_Dual_Row_38milx24mil_Hole_10milx20mil (layer F.Cu) (tedit 5C2C5B2C)
    (at 27.28038 28.193)
    (fp_text reference J6 (at -0.0254 -1.6002) (layer F.SilkS) hide)
    (fp_text value Conn_01x14 (at 0.3556 3.048) (layer F.Fab))
    (pad 14 thru_hole circle (at 6.273793 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad14)") (zone_connect 0))
    (pad 13 thru_hole circle (at 5.791194 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad13)") (zone_connect 0))
    (pad 12 thru_hole circle (at 5.308594 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 28 "Net-(J5-Pad12)") (zone_connect 0))
    (pad 11 thru_hole circle (at 4.825995 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-Pad11)") (zone_connect 0))
    (pad 10 thru_hole circle (at 4.343395 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad10)") (zone_connect 0))
    (pad 9 thru_hole circle (at 3.860796 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad9)") (zone_connect 0))
    (pad 8 thru_hole circle (at 3.378196 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad8)") (zone_connect 0))
    (pad 7 thru_hole circle (at 2.895597 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad7)") (zone_connect 0))
    (pad 6 thru_hole circle (at 2.412997 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad6)") (zone_connect 0))
    (pad 5 thru_hole circle (at 1.930398 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad5)") (zone_connect 0))
    (pad 4 thru_hole circle (at 1.447798 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad4)") (zone_connect 0))
    (pad 3 thru_hole circle (at 0.965199 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad3)") (zone_connect 0))
    (pad 2 thru_hole circle (at 0.482599 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)") (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad1)") (zone_connect 0))
  )
  (module .Connector:B2B_Flex_14_Dual_Row_38milx24mil_Hole_10milx20mil locked (layer F.Cu) (tedit 5C2C5B2C)
    (at 27.28038 20.193)
    (fp_text reference J5 (at -0.0254 -1.6002) (layer F.SilkS) hide)
    (fp_text value Conn_01x14 (at 0.3556 3.048) (layer F.Fab))
    (pad 14 thru_hole circle (at 6.273793 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad14)") (zone_connect 0))
    (pad 13 thru_hole circle (at 5.791194 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad13)") (zone_connect 0))
    (pad 12 thru_hole circle (at 5.308594 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 28 "Net-(J5-Pad12)") (zone_connect 0))
    (pad 11 thru_hole circle (at 4.825995 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-Pad11)") (zone_connect 0))
    (pad 10 thru_hole circle (at 4.343395 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad10)") (zone_connect 0))
    (pad 9 thru_hole circle (at 3.860796 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad9)") (zone_connect 0))
    (pad 8 thru_hole circle (at 3.378196 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad8)") (zone_connect 0))
    (pad 7 thru_hole circle (at 2.895597 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad7)") (zone_connect 0))
    (pad 6 thru_hole circle (at 2.412997 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad6)") (zone_connect 0))
    (pad 5 thru_hole circle (at 1.930398 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad5)") (zone_connect 0))
    (pad 4 thru_hole circle (at 1.447798 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad4)") (zone_connect 0))
    (pad 3 thru_hole circle (at 0.965199 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad3)") (zone_connect 0))
    (pad 2 thru_hole circle (at 0.482599 0.6096) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)") (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad1)") (zone_connect 0))
  )
  (module .Connector:B2B_Flex_05_Dual_Row_38milx24mil_Hole_20mil (layer F.Cu) (tedit 5CC220E5)
    (at 17.2118 17.3736 90)
    (fp_text reference J4 (at -0.0254 -1.6002 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0.3556 3.048 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 1.955398 -0.025 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad5)") (zone_connect 0))
    (pad 3 thru_hole circle (at 0.990199 -0.025 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad3)") (zone_connect 0))
    (pad 4 thru_hole circle (at 1.472798 0.5846 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad4)") (zone_connect 0))
    (pad 1 thru_hole circle (at 0.025 -0.025 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)") (zone_connect 0))
    (pad 2 thru_hole circle (at 0.507599 0.5846 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad2)") (zone_connect 0))
  )
  (module .Connector:B2B_Flex_05_Dual_Row_38milx24mil_Hole_20mil locked (layer F.Cu) (tedit 5CC220E5)
    (at 27.2118 17.3736 90)
    (fp_text reference J3 (at -0.0254 -1.6002 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0.3556 3.048 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 1.955398 -0.025 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad5)") (zone_connect 0))
    (pad 3 thru_hole circle (at 0.990199 -0.025 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad3)") (zone_connect 0))
    (pad 4 thru_hole circle (at 1.472798 0.5846 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad4)") (zone_connect 0))
    (pad 1 thru_hole circle (at 0.025 -0.025 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)") (zone_connect 0))
    (pad 2 thru_hole circle (at 0.507599 0.5846 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad2)") (zone_connect 0))
  )
  (module .Connector:B2B_Flex_20_Dual_Row_38milx24mil_Hole_10milx20mil (layer F.Cu) (tedit 5C2FE264)
    (at 35.27884 28.39366 270)
    (fp_text reference J2 (at -0.0254 -1.6002 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x20 (at 0.3556 3.048 270) (layer F.Fab))
    (pad 20 thru_hole circle (at 9.16939 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad20)") (zone_connect 0))
    (pad 19 thru_hole circle (at 8.686791 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad19)") (zone_connect 0))
    (pad 18 thru_hole circle (at 8.204191 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)") (zone_connect 0))
    (pad 17 thru_hole circle (at 7.721592 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad17)") (zone_connect 0))
    (pad 16 thru_hole circle (at 7.238992 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)") (zone_connect 0))
    (pad 15 thru_hole circle (at 6.756393 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)") (zone_connect 0))
    (pad 14 thru_hole circle (at 6.273793 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)") (zone_connect 0))
    (pad 13 thru_hole circle (at 5.791194 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)") (zone_connect 0))
    (pad 12 thru_hole circle (at 5.308594 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)") (zone_connect 0))
    (pad 11 thru_hole circle (at 4.825995 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)") (zone_connect 0))
    (pad 10 thru_hole circle (at 4.343395 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)") (zone_connect 0))
    (pad 9 thru_hole circle (at 3.860796 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)") (zone_connect 0))
    (pad 8 thru_hole circle (at 3.378196 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)") (zone_connect 0))
    (pad 7 thru_hole circle (at 2.895597 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)") (zone_connect 0))
    (pad 6 thru_hole circle (at 2.412997 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (zone_connect 0))
    (pad 5 thru_hole circle (at 1.930398 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)") (zone_connect 0))
    (pad 4 thru_hole circle (at 1.447798 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (zone_connect 0))
    (pad 3 thru_hole circle (at 0.965199 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (zone_connect 0))
    (pad 2 thru_hole circle (at 0.482599 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (zone_connect 0))
    (pad 1 thru_hole circle (at 0 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (zone_connect 0))
  )
  (module .Connector:B2B_Flex_20_Dual_Row_38milx24mil_Hole_10milx20mil (layer F.Cu) (tedit 5C2FE260)
    (at 41.27884 28.39366 270)
    (fp_text reference J1 (at -1.44281 -0.4312) (layer F.SilkS) hide)
    (fp_text value Conn_01x20 (at 0.3556 3.048 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (zone_connect 0))
    (pad 2 thru_hole circle (at 0.482599 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (zone_connect 0))
    (pad 3 thru_hole circle (at 0.965199 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (zone_connect 0))
    (pad 4 thru_hole circle (at 1.447798 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (zone_connect 0))
    (pad 5 thru_hole circle (at 1.930398 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)") (zone_connect 0))
    (pad 6 thru_hole circle (at 2.412997 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (zone_connect 0))
    (pad 7 thru_hole circle (at 2.895597 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)") (zone_connect 0))
    (pad 8 thru_hole circle (at 3.378196 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)") (zone_connect 0))
    (pad 9 thru_hole circle (at 3.860796 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)") (zone_connect 0))
    (pad 10 thru_hole circle (at 4.343395 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)") (zone_connect 0))
    (pad 11 thru_hole circle (at 4.825995 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)") (zone_connect 0))
    (pad 12 thru_hole circle (at 5.308594 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)") (zone_connect 0))
    (pad 13 thru_hole circle (at 5.791194 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)") (zone_connect 0))
    (pad 14 thru_hole circle (at 6.273793 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)") (zone_connect 0))
    (pad 15 thru_hole circle (at 6.756393 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)") (zone_connect 0))
    (pad 16 thru_hole circle (at 7.238992 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)") (zone_connect 0))
    (pad 17 thru_hole circle (at 7.721592 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad17)") (zone_connect 0))
    (pad 18 thru_hole circle (at 8.204191 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)") (zone_connect 0))
    (pad 19 thru_hole circle (at 8.686791 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad19)") (zone_connect 0))
    (pad 20 thru_hole circle (at 9.16939 0.6096 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad20)") (zone_connect 0))
  )
  (gr_line (start 16.75 14.75) (end 16.75 15) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 28.75 14.75) (end 16.75 14.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 28.75 16.25) (end 28.75 14.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 34.25 16.25) (end 28.75 16.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 34.25 27.75) (end 34.25 16.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 42 27.75) (end 34.25 27.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 42 38.25) (end 42 27.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 34 38.25) (end 42 38.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 34 29.5) (end 34 38.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 26.75 29.5) (end 34 29.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 26.75 18) (end 26.75 29.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 16.75 18) (end 26.75 18) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 16.75 15) (end 16.75 18) (layer Edge.Cuts) (width 0.15))
  (gr_text 6mm (at 38.0492 33.1724) (layer F.SilkS))
  (gr_text 8mm (at 30.353 24.5364) (layer F.SilkS))
  (gr_text 10mm (at 22.3774 16.3322) (layer F.SilkS))
)
