(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 133)
    (tracks 5359)
    (zones 0)
    (modules 362)
    (nets 218)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.1)
    (pad_size 0.508 0.508)
    (pad_drill 0.254)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 129.6035 54.3814)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "layout_pdfs/"))
  )
  (net 0 "")
  (net 1 /receiver_2/ANT_IN)
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C10-Pad1)")
  (net 7 "Net-(C13-Pad2)")
  (net 8 /RX2_Q)
  (net 9 "Net-(C14-Pad1)")
  (net 10 "Net-(C15-Pad1)")
  (net 11 "Net-(C16-Pad2)")
  (net 12 /RX2_I)
  (net 13 "Net-(C17-Pad1)")
  (net 14 "Net-(C18-Pad1)")
  (net 15 /receiver_3/ANT_IN)
  (net 16 "Net-(C19-Pad1)")
  (net 17 "Net-(C20-Pad1)")
  (net 18 "Net-(C21-Pad1)")
  (net 19 "Net-(C25-Pad1)")
  (net 20 "Net-(C31-Pad2)")
  (net 21 /RX3_Q)
  (net 22 "Net-(C32-Pad1)")
  (net 23 "Net-(C33-Pad1)")
  (net 24 "Net-(C34-Pad2)")
  (net 25 /RX3_I)
  (net 26 "Net-(C35-Pad1)")
  (net 27 "Net-(C36-Pad1)")
  (net 28 /receiver_4/ANT_IN)
  (net 29 "Net-(C37-Pad1)")
  (net 30 "Net-(C38-Pad1)")
  (net 31 "Net-(C39-Pad1)")
  (net 32 "Net-(C43-Pad1)")
  (net 33 "Net-(C49-Pad2)")
  (net 34 /RX4_Q)
  (net 35 "Net-(C50-Pad1)")
  (net 36 "Net-(C51-Pad1)")
  (net 37 "Net-(C52-Pad2)")
  (net 38 /RX4_I)
  (net 39 "Net-(C53-Pad1)")
  (net 40 "Net-(C54-Pad1)")
  (net 41 /receiver_1/ANT_IN)
  (net 42 "Net-(C55-Pad1)")
  (net 43 "Net-(C56-Pad1)")
  (net 44 "Net-(C57-Pad1)")
  (net 45 "Net-(C61-Pad1)")
  (net 46 "Net-(C67-Pad2)")
  (net 47 /RX1_Q)
  (net 48 "Net-(C68-Pad1)")
  (net 49 "Net-(C69-Pad1)")
  (net 50 "Net-(C70-Pad2)")
  (net 51 /RX1_I)
  (net 52 "Net-(C71-Pad1)")
  (net 53 "Net-(C72-Pad1)")
  (net 54 /transmitter/LMX_CPOUT)
  (net 55 "Net-(C74-Pad2)")
  (net 56 /transmitter/VCO_OUT)
  (net 57 "Net-(C75-Pad2)")
  (net 58 "Net-(C76-Pad2)")
  (net 59 "Net-(C77-Pad1)")
  (net 60 "Net-(C78-Pad1)")
  (net 61 +3V3)
  (net 62 /transmitter/ATTEN_OUT)
  (net 63 "Net-(C80-Pad1)")
  (net 64 "Net-(C81-Pad1)")
  (net 65 "Net-(C82-Pad1)")
  (net 66 "Net-(C83-Pad1)")
  (net 67 /transmitter/LMX_VCP)
  (net 68 "Net-(C85-Pad1)")
  (net 69 "Net-(C86-Pad1)")
  (net 70 VCC)
  (net 71 "Net-(C93-Pad2)")
  (net 72 "Net-(C93-Pad1)")
  (net 73 "Net-(C94-Pad2)")
  (net 74 "Net-(C94-Pad1)")
  (net 75 "Net-(C100-Pad1)")
  (net 76 "Net-(C98-Pad2)")
  (net 77 /transmitter/LMX_FIN)
  (net 78 "Net-(C99-Pad2)")
  (net 79 "Net-(C99-Pad1)")
  (net 80 +5V)
  (net 81 "Net-(C104-Pad1)")
  (net 82 "Net-(C105-Pad1)")
  (net 83 "Net-(C110-Pad2)")
  (net 84 +10V)
  (net 85 /power/5V5_OUT)
  (net 86 +3V0)
  (net 87 "Net-(C117-Pad1)")
  (net 88 "Net-(C118-Pad1)")
  (net 89 "Net-(C119-Pad2)")
  (net 90 +5V25)
  (net 91 "Net-(C120-Pad2)")
  (net 92 "Net-(D1-Pad2)")
  (net 93 "Net-(D2-Pad2)")
  (net 94 "Net-(D3-Pad2)")
  (net 95 "Net-(D4-Pad2)")
  (net 96 "Net-(D5-Pad2)")
  (net 97 "Net-(D6-Pad2)")
  (net 98 "Net-(D7-Pad2)")
  (net 99 /LMX_MOD)
  (net 100 /LMX_MUXOUT)
  (net 101 /LMX_TRIG2)
  (net 102 /LMX_TRIG1)
  (net 103 /transmitter/TX_OUT)
  (net 104 "Net-(J9-Pad10)")
  (net 105 "Net-(J9-Pad9)")
  (net 106 "Net-(J9-Pad8)")
  (net 107 "Net-(J9-Pad7)")
  (net 108 "Net-(J9-Pad5)")
  (net 109 "Net-(J9-Pad4)")
  (net 110 "Net-(J9-Pad3)")
  (net 111 "Net-(J9-Pad2)")
  (net 112 "Net-(J9-Pad1)")
  (net 113 /~ATTEN_1DB)
  (net 114 /~ATTEN_2DB)
  (net 115 /~ATTEN_4DB)
  (net 116 /~ATTEN_8DB)
  (net 117 "Net-(JP5-Pad2)")
  (net 118 /receiver_2/IF2_RAW)
  (net 119 "Net-(R8-Pad1)")
  (net 120 /receiver_2/IF1_RAW)
  (net 121 "Net-(R11-Pad1)")
  (net 122 /receiver_3/IF2_RAW)
  (net 123 "Net-(R15-Pad1)")
  (net 124 /receiver_3/IF1_RAW)
  (net 125 "Net-(R18-Pad1)")
  (net 126 /receiver_4/IF2_RAW)
  (net 127 "Net-(R22-Pad1)")
  (net 128 /receiver_4/IF1_RAW)
  (net 129 "Net-(R25-Pad1)")
  (net 130 /receiver_1/IF2_RAW)
  (net 131 "Net-(R29-Pad1)")
  (net 132 /receiver_1/IF1_RAW)
  (net 133 "Net-(R32-Pad1)")
  (net 134 /transmitter/LMX_CE)
  (net 135 "Net-(R44-Pad1)")
  (net 136 /transmitter/LMX_CLK)
  (net 137 /transmitter/LMX_DATA)
  (net 138 /transmitter/LMX_LE)
  (net 139 /transmitter/REF_OUT)
  (net 140 "Net-(R55-Pad1)")
  (net 141 "Net-(R60-Pad1)")
  (net 142 "Net-(R61-Pad2)")
  (net 143 /power/5V5_PGD)
  (net 144 "Net-(R64-Pad2)")
  (net 145 "Net-(R78-Pad2)")
  (net 146 /power/5V0_PGD)
  (net 147 /power/5V25_PGD)
  (net 148 "Net-(SW1-Pad2)")
  (net 149 /transmitter/PA_OUT)
  (net 150 "Net-(TL2-Pad3)")
  (net 151 "Net-(TL2-Pad2)")
  (net 152 /transmitter/LO_2)
  (net 153 /transmitter/LO_1)
  (net 154 /transmitter/LO_4)
  (net 155 /transmitter/LO_3)
  (net 156 /receiver_2/LNA_OUT)
  (net 157 /receiver_3/LNA_OUT)
  (net 158 /receiver_4/LNA_OUT)
  (net 159 /receiver_1/LNA_OUT)
  (net 160 "Net-(R81-Pad1)")
  (net 161 "Net-(TL1-Pad4)")
  (net 162 "Net-(TL3-Pad1)")
  (net 163 "Net-(TL4-Pad1)")
  (net 164 "Net-(TL6-Pad2)")
  (net 165 "Net-(TL7-Pad1)")
  (net 166 "Net-(TL13-Pad2)")
  (net 167 "Net-(TL10-Pad1)")
  (net 168 "Net-(TL11-Pad1)")
  (net 169 "Net-(TL12-Pad1)")
  (net 170 "Net-(TL13-Pad1)")
  (net 171 "Net-(TL14-Pad1)")
  (net 172 "Net-(TL15-Pad1)")
  (net 173 "Net-(TL16-Pad1)")
  (net 174 "Net-(TL17-Pad1)")
  (net 175 "Net-(TL17-Pad2)")
  (net 176 "Net-(TL18-Pad2)")
  (net 177 "Net-(TL20-Pad1)")
  (net 178 "Net-(TL20-Pad2)")
  (net 179 "Net-(TL22-Pad1)")
  (net 180 /power/+12V0_IN_CONN)
  (net 181 "Net-(TL25-Pad1)")
  (net 182 "Net-(TL26-Pad1)")
  (net 183 "Net-(TL27-Pad1)")
  (net 184 "Net-(TL28-Pad1)")
  (net 185 "Net-(TL29-Pad1)")
  (net 186 "Net-(TL30-Pad1)")
  (net 187 "Net-(TL31-Pad1)")
  (net 188 "Net-(TL32-Pad1)")
  (net 189 "Net-(TL33-Pad1)")
  (net 190 "Net-(TL34-Pad1)")
  (net 191 "Net-(TL35-Pad1)")
  (net 192 "Net-(TL36-Pad1)")
  (net 193 /power/POWER_SW)
  (net 194 "Net-(TL23-Pad1)")
  (net 195 "Net-(TL24-Pad1)")
  (net 196 "Net-(TL37-Pad1)")
  (net 197 "Net-(TL38-Pad1)")
  (net 198 "Net-(TL39-Pad1)")
  (net 199 "Net-(TL40-Pad1)")
  (net 200 "Net-(TL41-Pad1)")
  (net 201 "Net-(TL42-Pad1)")
  (net 202 "Net-(TL43-Pad1)")
  (net 203 "Net-(TL44-Pad1)")
  (net 204 "Net-(TL45-Pad1)")
  (net 205 "Net-(TL46-Pad1)")
  (net 206 "Net-(TL23-Pad2)")
  (net 207 "Net-(TL38-Pad2)")
  (net 208 "Net-(TL41-Pad2)")
  (net 209 "Net-(TL44-Pad2)")
  (net 210 "Net-(TL3-Pad3)")
  (net 211 "Net-(TL3-Pad2)")
  (net 212 "Net-(TL4-Pad3)")
  (net 213 "Net-(TL4-Pad2)")
  (net 214 "Net-(TL51-Pad2)")
  (net 215 "Net-(TL52-Pad2)")
  (net 216 "Net-(TL53-Pad1)")
  (net 217 "Net-(TL54-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LMX_MOD)
    (add_net /LMX_MUXOUT)
    (add_net /LMX_TRIG1)
    (add_net /LMX_TRIG2)
    (add_net /power/+12V0_IN_CONN)
    (add_net /power/5V0_PGD)
    (add_net /power/5V25_PGD)
    (add_net /power/5V5_OUT)
    (add_net /power/5V5_PGD)
    (add_net /power/POWER_SW)
    (add_net /transmitter/LMX_CE)
    (add_net /transmitter/LMX_CLK)
    (add_net /transmitter/LMX_CPOUT)
    (add_net /transmitter/LMX_DATA)
    (add_net /transmitter/LMX_FIN)
    (add_net /transmitter/LMX_LE)
    (add_net /transmitter/LMX_VCP)
    (add_net /~ATTEN_1DB)
    (add_net /~ATTEN_2DB)
    (add_net /~ATTEN_4DB)
    (add_net /~ATTEN_8DB)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C100-Pad1)")
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(C105-Pad1)")
    (add_net "Net-(C110-Pad2)")
    (add_net "Net-(C117-Pad1)")
    (add_net "Net-(C118-Pad1)")
    (add_net "Net-(C119-Pad2)")
    (add_net "Net-(C120-Pad2)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C31-Pad2)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C34-Pad2)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C37-Pad1)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(C43-Pad1)")
    (add_net "Net-(C49-Pad2)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(C51-Pad1)")
    (add_net "Net-(C52-Pad2)")
    (add_net "Net-(C53-Pad1)")
    (add_net "Net-(C54-Pad1)")
    (add_net "Net-(C55-Pad1)")
    (add_net "Net-(C56-Pad1)")
    (add_net "Net-(C57-Pad1)")
    (add_net "Net-(C61-Pad1)")
    (add_net "Net-(C67-Pad2)")
    (add_net "Net-(C68-Pad1)")
    (add_net "Net-(C69-Pad1)")
    (add_net "Net-(C70-Pad2)")
    (add_net "Net-(C71-Pad1)")
    (add_net "Net-(C72-Pad1)")
    (add_net "Net-(C74-Pad2)")
    (add_net "Net-(C75-Pad2)")
    (add_net "Net-(C76-Pad2)")
    (add_net "Net-(C77-Pad1)")
    (add_net "Net-(C78-Pad1)")
    (add_net "Net-(C80-Pad1)")
    (add_net "Net-(C81-Pad1)")
    (add_net "Net-(C82-Pad1)")
    (add_net "Net-(C83-Pad1)")
    (add_net "Net-(C85-Pad1)")
    (add_net "Net-(C86-Pad1)")
    (add_net "Net-(C93-Pad1)")
    (add_net "Net-(C93-Pad2)")
    (add_net "Net-(C94-Pad1)")
    (add_net "Net-(C94-Pad2)")
    (add_net "Net-(C98-Pad2)")
    (add_net "Net-(C99-Pad1)")
    (add_net "Net-(C99-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(J9-Pad10)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(J9-Pad3)")
    (add_net "Net-(J9-Pad4)")
    (add_net "Net-(J9-Pad5)")
    (add_net "Net-(J9-Pad7)")
    (add_net "Net-(J9-Pad8)")
    (add_net "Net-(J9-Pad9)")
    (add_net "Net-(JP5-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R32-Pad1)")
    (add_net "Net-(R44-Pad1)")
    (add_net "Net-(R55-Pad1)")
    (add_net "Net-(R60-Pad1)")
    (add_net "Net-(R61-Pad2)")
    (add_net "Net-(R64-Pad2)")
    (add_net "Net-(R78-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(SW1-Pad2)")
    (add_net VCC)
  )
  (net_class 50-ohm ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RX1_I)
    (add_net /RX1_Q)
    (add_net /RX2_I)
    (add_net /RX2_Q)
    (add_net /RX3_I)
    (add_net /RX3_Q)
    (add_net /RX4_I)
    (add_net /RX4_Q)
    (add_net /receiver_1/ANT_IN)
    (add_net /receiver_1/IF1_RAW)
    (add_net /receiver_1/IF2_RAW)
    (add_net /receiver_1/LNA_OUT)
    (add_net /receiver_2/ANT_IN)
    (add_net /receiver_2/IF1_RAW)
    (add_net /receiver_2/IF2_RAW)
    (add_net /receiver_2/LNA_OUT)
    (add_net /receiver_3/ANT_IN)
    (add_net /receiver_3/IF1_RAW)
    (add_net /receiver_3/IF2_RAW)
    (add_net /receiver_3/LNA_OUT)
    (add_net /receiver_4/ANT_IN)
    (add_net /receiver_4/IF1_RAW)
    (add_net /receiver_4/IF2_RAW)
    (add_net /receiver_4/LNA_OUT)
    (add_net /transmitter/ATTEN_OUT)
    (add_net /transmitter/LO_1)
    (add_net /transmitter/LO_2)
    (add_net /transmitter/LO_3)
    (add_net /transmitter/LO_4)
    (add_net /transmitter/PA_OUT)
    (add_net /transmitter/REF_OUT)
    (add_net /transmitter/TX_OUT)
    (add_net /transmitter/VCO_OUT)
    (add_net "Net-(R81-Pad1)")
    (add_net "Net-(TL1-Pad4)")
    (add_net "Net-(TL10-Pad1)")
    (add_net "Net-(TL11-Pad1)")
    (add_net "Net-(TL12-Pad1)")
    (add_net "Net-(TL13-Pad1)")
    (add_net "Net-(TL13-Pad2)")
    (add_net "Net-(TL14-Pad1)")
    (add_net "Net-(TL15-Pad1)")
    (add_net "Net-(TL16-Pad1)")
    (add_net "Net-(TL17-Pad1)")
    (add_net "Net-(TL17-Pad2)")
    (add_net "Net-(TL18-Pad2)")
    (add_net "Net-(TL2-Pad2)")
    (add_net "Net-(TL2-Pad3)")
    (add_net "Net-(TL20-Pad1)")
    (add_net "Net-(TL20-Pad2)")
    (add_net "Net-(TL22-Pad1)")
    (add_net "Net-(TL23-Pad1)")
    (add_net "Net-(TL23-Pad2)")
    (add_net "Net-(TL24-Pad1)")
    (add_net "Net-(TL25-Pad1)")
    (add_net "Net-(TL26-Pad1)")
    (add_net "Net-(TL27-Pad1)")
    (add_net "Net-(TL28-Pad1)")
    (add_net "Net-(TL29-Pad1)")
    (add_net "Net-(TL3-Pad1)")
    (add_net "Net-(TL3-Pad2)")
    (add_net "Net-(TL3-Pad3)")
    (add_net "Net-(TL30-Pad1)")
    (add_net "Net-(TL31-Pad1)")
    (add_net "Net-(TL32-Pad1)")
    (add_net "Net-(TL33-Pad1)")
    (add_net "Net-(TL34-Pad1)")
    (add_net "Net-(TL35-Pad1)")
    (add_net "Net-(TL36-Pad1)")
    (add_net "Net-(TL37-Pad1)")
    (add_net "Net-(TL38-Pad1)")
    (add_net "Net-(TL38-Pad2)")
    (add_net "Net-(TL39-Pad1)")
    (add_net "Net-(TL4-Pad1)")
    (add_net "Net-(TL4-Pad2)")
    (add_net "Net-(TL4-Pad3)")
    (add_net "Net-(TL40-Pad1)")
    (add_net "Net-(TL41-Pad1)")
    (add_net "Net-(TL41-Pad2)")
    (add_net "Net-(TL42-Pad1)")
    (add_net "Net-(TL43-Pad1)")
    (add_net "Net-(TL44-Pad1)")
    (add_net "Net-(TL44-Pad2)")
    (add_net "Net-(TL45-Pad1)")
    (add_net "Net-(TL46-Pad1)")
    (add_net "Net-(TL51-Pad2)")
    (add_net "Net-(TL52-Pad2)")
    (add_net "Net-(TL53-Pad1)")
    (add_net "Net-(TL54-Pad1)")
    (add_net "Net-(TL6-Pad2)")
    (add_net "Net-(TL7-Pad1)")
  )
  (net_class 50-ohm-chip ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.45)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +10V)
    (add_net +3V0)
    (add_net +3V3)
    (add_net +5V)
    (add_net +5V25)
  )
  (module aps_radar_lib:spartan_logo (layer B.Cu) (tedit 0)
    (at 154.1435 96.435211 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module aps_radar_lib:delta_logo (layer B.Cu) (tedit 0)
    (at 201.6835 96.4714 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module aps_radar_lib:SMA_Molex_Transition (layer F.Cu) (tedit 5E62ACF9)
    (at 216.07824 116.47122 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (zone_connect 2)
    (attr smd)
    (fp_text reference J8 (at 6.23474 4.35982) (layer F.SilkS) hide)
    (fp_text value Rx4 (at 6.97474 3.04982 180) (layer F.SilkS))
    (fp_text user "See Jason for proper keeoput" (at -0.05 9.05) (layer Cmts.User) hide)
    (fp_text user %R (at 2.775 6.975) (layer F.Fab))
    (pad 2 thru_hole rect (at 7.17225 3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 7.17225 0 180) (size 1.1555 1) (layers F.Mask)
      (net 3 GND) (zone_connect 1))
    (pad ~ smd rect (at 3.29725 0 180) (size 6.5945 1.77666) (layers F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole rect (at 7.17225 -3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 -3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 -4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 -2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers F.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 1 smd rect (at 7.5 0 180) (size 0.5 0.35) (layers F.Cu F.Mask)
      (net 28 /receiver_4/ANT_IN) (zone_connect 1))
    (pad ~ smd rect (at 6.5 0 180) (size 1.5 0.35) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad ~ smd rect (at 5.5 0 180) (size 0.5 0.35) (layers F.Cu)
      (zone_connect 1))
    (pad ~ smd rect (at 2.625 0 180) (size 5.25 1) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole circle (at 5.995 4.355 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 5.995 -4.405 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.42) (layers B.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers F.Cu F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_CuK_JS202011AQN_DPDT_Angled (layer F.Cu) (tedit 5A02FE31)
    (at 129.1535 71.3114 180)
    (descr "CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
    (tags "switch DPDT")
    (fp_text reference SW1 (at 5.41528 -1.88976) (layer F.SilkS) hide)
    (fp_text value PA_EN (at -3.13944 1.55448 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2.5 1.75) (layer F.Fab))
    (pad 6 thru_hole circle (at 5 3.3 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole circle (at 2.5 3.3 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 0 3.3 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 148 "Net-(SW1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_CuK_JS202011AQN_DPDT_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 170.8699 106.4306 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at -1.9812 0.0254 180) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C52-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 /receiver_4/IF1_RAW))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 172.5971 115.8032 180)
    (fp_text reference RV6 (at -0.0508 -3.3274 180) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999 180) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R25-Pad1)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 /RX4_I))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module aps_radar_lib:HMC-LP4 (layer F.Cu) (tedit 5E67DE1E)
    (at 126.36788 116.45706)
    (fp_text reference U20 (at -3.27438 -0.01566 90) (layer F.SilkS))
    (fp_text value HMC431 (at 0.15 3.65) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User) hide)
    (pad ~ smd roundrect (at -1.25 -1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 -1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.25 1.95 90) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 1.25 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad `9 smd roundrect (at -1.95 0.75 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 0.25 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.25 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.75 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -1.25 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -1.25 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.75 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.25 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.25 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.75 90) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 1.25 90) (size 0.15 0.65) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd rect (at 1.925 0) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.925 0) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.925) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 1.099) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 1.099) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 1.099) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 1.099) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 0.366) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 0.366) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 0.366) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 0.366) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -0.367) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -0.367) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -0.367) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -0.367) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -1.1) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -1.1) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -1.1) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 1.925) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -1.1) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 smd roundrect (at 0.6 0.6) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 0.6) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at 0.6 -0.6) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 -0.6) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd rect (at 0 0) (size 2.6 2.6) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.950001 -1.25 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 2 smd rect (at -1.950001 -0.750001 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 3 smd rect (at -1.950001 -0.25 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 4 smd rect (at -1.950001 0.25 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 5 smd rect (at -1.950001 0.750001 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 6 smd rect (at -1.950001 1.25 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 7 smd rect (at -1.25 1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 8 smd rect (at -0.750001 1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 9 smd rect (at -0.25 1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 10 smd rect (at 0.25 1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 11 smd rect (at 0.750001 1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 12 smd rect (at 1.25 1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 13 smd rect (at 1.950001 1.25 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 14 smd rect (at 1.950001 0.750001 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 15 smd rect (at 1.950001 0.25 90) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 16 smd rect (at 1.950001 -0.25 90) (size 0.22 0.699999) (layers F.Cu)
      (net 170 "Net-(TL13-Pad1)"))
    (pad 17 smd rect (at 1.950001 -0.750001 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 18 smd rect (at 1.950001 -1.25 90) (size 0.22 0.699999) (layers F.Cu))
    (pad 19 smd rect (at 1.25 -1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 20 smd rect (at 0.750001 -1.950001) (size 0.22 0.699999) (layers F.Cu)
      (net 69 "Net-(C86-Pad1)"))
    (pad 21 smd rect (at 0.25 -1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 22 smd rect (at -0.25 -1.950001) (size 0.22 0.699999) (layers F.Cu)
      (net 169 "Net-(TL12-Pad1)"))
    (pad 23 smd rect (at -0.750001 -1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 24 smd rect (at -1.25 -1.950001) (size 0.22 0.699999) (layers F.Cu))
    (pad 25 smd rect (at 0 0) (size 2.799999 2.799999) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:IC_Taper_0.25_0.35 (layer F.Cu) (tedit 5E69078D)
    (at 139.17324 97.92994 270)
    (fp_text reference TL14 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.43 0 270) (size 0.4 0.25) (layers F.Cu)
      (net 171 "Net-(TL14-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 62 /transmitter/ATTEN_OUT))
    (pad ~ smd rect (at 0.045 -0.0025 270) (size 1.3525 1) (layers F.Mask))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 170.6285 110.9464 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0.0562 -1.3844 270) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(R25-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 150.74228 79.00664 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U16 (at -2.98024 -0.05622 90) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 51 /RX1_I))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C71-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(R32-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C72-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 159.13028 79.02264 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U15 (at -3.11124 -0.09322 90) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 47 /RX1_Q))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C68-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R29-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C69-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 167.9335 109.9764 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U12 (at -3.075 -0.05 270) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 38 /RX4_I))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C53-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R25-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C54-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 159.40172 110.91692 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U11 (at -3.04552 -0.07678 270) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 34 /RX4_Q))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C50-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R22-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C51-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 150.93372 110.917 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U8 (at -2.6856 -0.09478 90) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 /RX3_I))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C35-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R18-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 159.35672 98.173 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U7 (at -2.7016 -0.09178 90) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 /RX3_Q))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C32-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R15-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C33-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 150.9285 98.161399 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 0.08 2.33 90) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX2_I))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R11-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 167.4835 79.0414 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -2.72 -0.08 90) (layer F.SilkS))
    (fp_text value OPA192 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /RX2_Q))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C14-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R8-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.4535 112.4414 90)
    (fp_text reference TL58 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.195 0.3625 90) (size 0.36 0.35) (layers F.Cu)
      (net 154 /transmitter/LO_4))
    (pad 2 smd rect (at 0.3675 -0.195 90) (size 0.35 0.3575) (layers F.Cu)
      (net 215 "Net-(TL52-Pad2)"))
    (pad ~ smd rect (at -0.08 -0.085 90) (size 1.25 1.25) (layers F.Mask))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.4535 85.8364 90)
    (fp_text reference TL57 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 90) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 90) (size 0.35 0.3575) (layers F.Cu)
      (net 214 "Net-(TL51-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 90) (size 0.36 0.35) (layers F.Cu)
      (net 152 /transmitter/LO_2))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.4585 99.5264)
    (fp_text reference TL56 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195) (size 0.35 0.3575) (layers F.Cu)
      (net 155 /transmitter/LO_3))
    (pad 1 smd rect (at -0.195 0.3625) (size 0.36 0.35) (layers F.Cu)
      (net 217 "Net-(TL54-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.4585 72.9314)
    (fp_text reference TL55 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195) (size 0.35 0.3575) (layers F.Cu)
      (net 153 /transmitter/LO_1))
    (pad 1 smd rect (at -0.195 0.3625) (size 0.36 0.35) (layers F.Cu)
      (net 216 "Net-(TL53-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.0685 104.8764 180)
    (fp_text reference TL54 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.195 0.3625 180) (size 0.36 0.35) (layers F.Cu)
      (net 217 "Net-(TL54-Pad1)"))
    (pad 2 smd rect (at 0.3675 -0.195 180) (size 0.35 0.3575) (layers F.Cu)
      (net 213 "Net-(TL4-Pad2)"))
    (pad ~ smd rect (at -0.08 -0.085 180) (size 1.25 1.25) (layers F.Mask))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.0685 78.2814 180)
    (fp_text reference TL53 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 180) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 180) (size 0.35 0.3575) (layers F.Cu)
      (net 211 "Net-(TL3-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 180) (size 0.36 0.35) (layers F.Cu)
      (net 216 "Net-(TL53-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.0635 107.0164 270)
    (fp_text reference TL52 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 212 "Net-(TL4-Pad3)"))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 215 "Net-(TL52-Pad2)"))
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 179.0635 80.4214 270)
    (fp_text reference TL51 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 214 "Net-(TL51-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 210 "Net-(TL3-Pad3)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 187.4185 72.9314 270)
    (fp_text reference TL50 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 209 "Net-(TL44-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 153 /transmitter/LO_1))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 187.4185 99.5214 270)
    (fp_text reference TL48 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 207 "Net-(TL38-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 155 /transmitter/LO_3))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 187.4235 86.2214 270)
    (fp_text reference TL47 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 206 "Net-(TL23-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 152 /transmitter/LO_2))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 187.4235 112.8314 270)
    (fp_text reference TL49 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 208 "Net-(TL41-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 154 /transmitter/LO_4))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.1185 80.4364 270)
    (fp_text reference TL46 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 205 "Net-(TL46-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 130 /receiver_1/IF2_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 188.6185 80.4364 270)
    (fp_text reference TL45 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 204 "Net-(TL45-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 132 /receiver_1/IF1_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.61206 74.20104 90)
    (fp_text reference TL44 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 90) (size 0.22 0.22) (layers F.Cu)
      (net 203 "Net-(TL44-Pad1)"))
    (pad 2 smd rect (at 0.61 0 90) (size 0.22 0.35) (layers F.Cu)
      (net 209 "Net-(TL44-Pad2)"))
    (pad ~ smd rect (at 0.055 0 90) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.1185 120.3364 270)
    (fp_text reference TL43 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 202 "Net-(TL43-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 126 /receiver_4/IF2_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 188.6185 120.3364 270)
    (fp_text reference TL42 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 201 "Net-(TL42-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 128 /receiver_4/IF1_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.6135 114.10032 90)
    (fp_text reference TL41 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 90) (size 0.22 0.22) (layers F.Cu)
      (net 200 "Net-(TL41-Pad1)"))
    (pad 2 smd rect (at 0.61 0 90) (size 0.22 0.35) (layers F.Cu)
      (net 208 "Net-(TL41-Pad2)"))
    (pad ~ smd rect (at 0.055 0 90) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.1185 107.0314 270)
    (fp_text reference TL40 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 199 "Net-(TL40-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 122 /receiver_3/IF2_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 188.6185 107.0314 270)
    (fp_text reference TL39 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 198 "Net-(TL39-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 124 /receiver_3/IF1_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.6135 100.7964 90)
    (fp_text reference TL38 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 90) (size 0.22 0.22) (layers F.Cu)
      (net 197 "Net-(TL38-Pad1)"))
    (pad 2 smd rect (at 0.61 0 90) (size 0.22 0.35) (layers F.Cu)
      (net 207 "Net-(TL38-Pad2)"))
    (pad ~ smd rect (at 0.055 0 90) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.1185 93.7414 270)
    (fp_text reference TL37 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 196 "Net-(TL37-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 118 /receiver_2/IF2_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 188.6185 93.7364 270)
    (fp_text reference TL24 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 195 "Net-(TL24-Pad1)"))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 120 /receiver_2/IF1_RAW))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 187.6135 87.49906 90)
    (fp_text reference TL23 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0 90) (size 0.22 0.22) (layers F.Cu)
      (net 194 "Net-(TL23-Pad1)"))
    (pad 2 smd rect (at 0.61 0 90) (size 0.22 0.35) (layers F.Cu)
      (net 206 "Net-(TL23-Pad2)"))
    (pad ~ smd rect (at 0.055 0 90) (size 1.3325 1) (layers F.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 150.3235 121.8914 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value IF_OUT (at 1.27 20.11 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RX2_Q))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /RX4_Q))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /RX2_I))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /RX4_I))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /RX1_Q))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RX3_Q))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /RX1_I))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /RX3_I))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 206.9635 71.2114)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 90.1535 71.2114)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 206.9635 121.6714)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 90.1535 121.6714)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP3 (layer F.Cu) (tedit 5E67DE3C)
    (at 199.69442 89.622 180)
    (fp_text reference U1 (at -3.32012 -1.35636 180) (layer F.SilkS))
    (fp_text value HMC717A (at 0.01 3.06 180) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -0.0025 1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad ~ smd roundrect (at 0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad 17 smd roundrect (at 0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at 0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd rect (at 0 0 180) (size 1.4732 1.4732) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 2 smd rect (at -1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 181 "Net-(TL25-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 3 smd rect (at -1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 4 smd rect (at -1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 smd rect (at -0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 6 smd rect (at -0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 7 smd rect (at 0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 8 smd rect (at 0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 4 "Net-(C2-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 9 smd rect (at 1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 10 smd rect (at 1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 11 smd rect (at 1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 185 "Net-(TL29-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 12 smd rect (at 1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 13 smd rect (at 0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 5 "Net-(C3-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 14 smd rect (at 0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 15 smd rect (at -0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 5 "Net-(C3-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 16 smd rect (at -0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 17 smd rect (at 0 0 180) (size 1.778 1.778) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP3 (layer F.Cu) (tedit 5E67DE3C)
    (at 199.69442 102.91934 180)
    (fp_text reference U5 (at -3.32012 -1.35636 180) (layer F.SilkS))
    (fp_text value HMC717A (at 0.01 3.06 180) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -0.0025 1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad ~ smd roundrect (at 0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad 17 smd roundrect (at 0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at 0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd rect (at 0 0 180) (size 1.4732 1.4732) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 2 smd rect (at -1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 182 "Net-(TL26-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 3 smd rect (at -1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 4 smd rect (at -1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 smd rect (at -0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 6 smd rect (at -0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 7 smd rect (at 0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 8 smd rect (at 0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 17 "Net-(C20-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 9 smd rect (at 1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 10 smd rect (at 1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 11 smd rect (at 1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 186 "Net-(TL30-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 12 smd rect (at 1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 13 smd rect (at 0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 18 "Net-(C21-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 14 smd rect (at 0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 15 smd rect (at -0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 18 "Net-(C21-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 16 smd rect (at -0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 17 smd rect (at 0 0 180) (size 1.778 1.778) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP3 (layer F.Cu) (tedit 5E67DE3C)
    (at 199.69442 116.22326 180)
    (fp_text reference U9 (at -3.32012 -1.35636 180) (layer F.SilkS))
    (fp_text value HMC717A (at 0.01 3.06 180) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -0.0025 1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad ~ smd roundrect (at 0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad 17 smd roundrect (at 0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at 0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd rect (at 0 0 180) (size 1.4732 1.4732) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 2 smd rect (at -1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 183 "Net-(TL27-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 3 smd rect (at -1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 4 smd rect (at -1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 smd rect (at -0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 6 smd rect (at -0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 7 smd rect (at 0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 8 smd rect (at 0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 30 "Net-(C38-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 9 smd rect (at 1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 10 smd rect (at 1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 11 smd rect (at 1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 187 "Net-(TL31-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 12 smd rect (at 1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 13 smd rect (at 0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 31 "Net-(C39-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 14 smd rect (at 0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 15 smd rect (at -0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 31 "Net-(C39-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 16 smd rect (at -0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 17 smd rect (at 0 0 180) (size 1.778 1.778) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP3 (layer F.Cu) (tedit 5E67DE3C)
    (at 199.69298 76.32398 180)
    (fp_text reference U13 (at -3.32012 -1.35636 180) (layer F.SilkS))
    (fp_text value HMC717A (at 0.01 3.06 180) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.45 0 180) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -0.0025 1.45 180) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 -0.525 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad ~ smd roundrect (at 0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.45 270) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.25 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.75 270) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad 17 smd roundrect (at 0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at 0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 -0.3433 180) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd rect (at 0 0 180) (size 1.4732 1.4732) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 2 smd rect (at -1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 184 "Net-(TL28-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 3 smd rect (at -1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 4 smd rect (at -1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 smd rect (at -0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 6 smd rect (at -0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 7 smd rect (at 0.25 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 8 smd rect (at 0.750001 1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 43 "Net-(C56-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 9 smd rect (at 1.45 0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 10 smd rect (at 1.45 0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 11 smd rect (at 1.45 -0.25 270) (size 0.22 0.799999) (layers F.Cu)
      (net 188 "Net-(TL32-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 12 smd rect (at 1.45 -0.750001 270) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 13 smd rect (at 0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 44 "Net-(C57-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 14 smd rect (at 0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 15 smd rect (at -0.25 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 44 "Net-(C57-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 16 smd rect (at -0.750001 -1.45 180) (size 0.22 0.799999) (layers F.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 17 smd rect (at 0 0 180) (size 1.778 1.778) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP4 (layer F.Cu) (tedit 5E67DE1E)
    (at 187.86852 90.62022 180)
    (fp_text reference U2 (at -3.77642 2.3808 180) (layer F.SilkS))
    (fp_text value HMC951A (at 0.15 3.65 180) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User) hide)
    (pad ~ smd roundrect (at -1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad `9 smd roundrect (at -1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 1.25 270) (size 0.15 0.65) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd rect (at 1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 smd roundrect (at 0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at 0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.6 2.6) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 2 smd rect (at -1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 6 "Net-(C10-Pad1)"))
    (pad 3 smd rect (at -1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 4 smd rect (at -1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 5 smd rect (at -1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 189 "Net-(TL33-Pad1)"))
    (pad 6 smd rect (at -1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 7 smd rect (at -1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 8 smd rect (at -0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 9 smd rect (at -0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 10 smd rect (at 0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 194 "Net-(TL23-Pad1)"))
    (pad 11 smd rect (at 0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 12 smd rect (at 1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 13 smd rect (at 1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 14 smd rect (at 1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 15 smd rect (at 1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 16 smd rect (at 1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 6 "Net-(C10-Pad1)"))
    (pad 17 smd rect (at 1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 18 smd rect (at 1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 19 smd rect (at 1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 20 smd rect (at 0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 196 "Net-(TL37-Pad1)"))
    (pad 21 smd rect (at 0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 22 smd rect (at -0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 23 smd rect (at -0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 195 "Net-(TL24-Pad1)"))
    (pad 24 smd rect (at -1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.799999 2.799999) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP4 (layer F.Cu) (tedit 5E67DE1E)
    (at 187.86852 103.91756 180)
    (fp_text reference U6 (at -3.77642 2.3808 180) (layer F.SilkS))
    (fp_text value HMC951A (at 0.15 3.65 180) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User) hide)
    (pad ~ smd roundrect (at -1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad `9 smd roundrect (at -1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 1.25 270) (size 0.15 0.65) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd rect (at 1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 smd roundrect (at 0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at 0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.6 2.6) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 2 smd rect (at -1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 19 "Net-(C25-Pad1)"))
    (pad 3 smd rect (at -1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 4 smd rect (at -1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 5 smd rect (at -1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 190 "Net-(TL34-Pad1)"))
    (pad 6 smd rect (at -1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 7 smd rect (at -1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 8 smd rect (at -0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 9 smd rect (at -0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 10 smd rect (at 0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 197 "Net-(TL38-Pad1)"))
    (pad 11 smd rect (at 0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 12 smd rect (at 1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 13 smd rect (at 1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 14 smd rect (at 1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 15 smd rect (at 1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 16 smd rect (at 1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 19 "Net-(C25-Pad1)"))
    (pad 17 smd rect (at 1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 18 smd rect (at 1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 19 smd rect (at 1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 20 smd rect (at 0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 199 "Net-(TL40-Pad1)"))
    (pad 21 smd rect (at 0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 22 smd rect (at -0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 23 smd rect (at -0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 198 "Net-(TL39-Pad1)"))
    (pad 24 smd rect (at -1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.799999 2.799999) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP4 (layer F.Cu) (tedit 5E67DE1E)
    (at 187.86852 117.22148 180)
    (fp_text reference U10 (at -3.77642 2.3808 180) (layer F.SilkS))
    (fp_text value HMC951A (at 0.15 3.65 180) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User) hide)
    (pad ~ smd roundrect (at -1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad `9 smd roundrect (at -1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 1.25 270) (size 0.15 0.65) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd rect (at 1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 smd roundrect (at 0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at 0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.6 2.6) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 2 smd rect (at -1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 32 "Net-(C43-Pad1)"))
    (pad 3 smd rect (at -1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 4 smd rect (at -1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 5 smd rect (at -1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 191 "Net-(TL35-Pad1)"))
    (pad 6 smd rect (at -1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 7 smd rect (at -1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 8 smd rect (at -0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 9 smd rect (at -0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 10 smd rect (at 0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 200 "Net-(TL41-Pad1)"))
    (pad 11 smd rect (at 0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 12 smd rect (at 1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 13 smd rect (at 1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 14 smd rect (at 1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 15 smd rect (at 1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 16 smd rect (at 1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 32 "Net-(C43-Pad1)"))
    (pad 17 smd rect (at 1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 18 smd rect (at 1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 19 smd rect (at 1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 20 smd rect (at 0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 202 "Net-(TL43-Pad1)"))
    (pad 21 smd rect (at 0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 22 smd rect (at -0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 23 smd rect (at -0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 201 "Net-(TL42-Pad1)"))
    (pad 24 smd rect (at -1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.799999 2.799999) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:HMC-LP4 (layer F.Cu) (tedit 5E67DE1E)
    (at 187.86708 77.3222 180)
    (fp_text reference U14 (at -3.77642 2.3808 180) (layer F.SilkS))
    (fp_text value HMC951A (at 0.15 3.65 180) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User) hide)
    (pad ~ smd roundrect (at -1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 -1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.25 1.95 270) (size 0.63 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad `9 smd roundrect (at -1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -1.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 -0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.25 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 0.75 270) (size 0.15 0.63) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.95 1.25 270) (size 0.15 0.65) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd rect (at 1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at -1.925 0 180) (size 0.762 2.9464) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 -1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 1.099 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 0.366 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -0.367 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 1.099 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at 0.366 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -0.367 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad ~ smd rect (at 0 1.925 180) (size 2.9464 0.762) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 25 thru_hole circle (at -1.1 -1.1 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 25 smd roundrect (at 0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at 0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd roundrect (at -0.6 -0.6 180) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.6 2.6) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 2 smd rect (at -1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 45 "Net-(C61-Pad1)"))
    (pad 3 smd rect (at -1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 4 smd rect (at -1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 5 smd rect (at -1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu)
      (net 192 "Net-(TL36-Pad1)"))
    (pad 6 smd rect (at -1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 7 smd rect (at -1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 8 smd rect (at -0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 9 smd rect (at -0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 10 smd rect (at 0.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 203 "Net-(TL44-Pad1)"))
    (pad 11 smd rect (at 0.750001 1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 12 smd rect (at 1.25 1.950001 180) (size 0.22 0.699999) (layers F.Cu))
    (pad 13 smd rect (at 1.950001 1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 14 smd rect (at 1.950001 0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 15 smd rect (at 1.950001 0.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 16 smd rect (at 1.950001 -0.25 270) (size 0.22 0.699999) (layers F.Cu)
      (net 45 "Net-(C61-Pad1)"))
    (pad 17 smd rect (at 1.950001 -0.750001 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 18 smd rect (at 1.950001 -1.25 270) (size 0.22 0.699999) (layers F.Cu))
    (pad 19 smd rect (at 1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 20 smd rect (at 0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 205 "Net-(TL46-Pad1)"))
    (pad 21 smd rect (at 0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 22 smd rect (at -0.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 23 smd rect (at -0.750001 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 204 "Net-(TL45-Pad1)"))
    (pad 24 smd rect (at -1.25 -1.950001 180) (size 0.22 0.699999) (layers F.Cu)
      (net 3 GND))
    (pad 25 smd rect (at 0 0 180) (size 2.799999 2.799999) (layers F.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 191.22076 76.5729)
    (fp_text reference TL36 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 159 /receiver_1/LNA_OUT))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 192 "Net-(TL36-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 191.2222 116.47218)
    (fp_text reference TL35 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 158 /receiver_4/LNA_OUT))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 191 "Net-(TL35-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 191.2222 103.16826)
    (fp_text reference TL34 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 157 /receiver_3/LNA_OUT))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 190 "Net-(TL34-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 191.2222 89.87092)
    (fp_text reference TL33 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 156 /receiver_2/LNA_OUT))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 189 "Net-(TL33-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 196.69016 76.5729 180)
    (fp_text reference TL32 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0 180) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 180) (size 0.22 0.35) (layers F.Cu)
      (net 159 /receiver_1/LNA_OUT))
    (pad 1 smd rect (at -0.5 0 180) (size 0.22 0.22) (layers F.Cu)
      (net 188 "Net-(TL32-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 196.6916 116.47218 180)
    (fp_text reference TL31 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0 180) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 180) (size 0.22 0.35) (layers F.Cu)
      (net 158 /receiver_4/LNA_OUT))
    (pad 1 smd rect (at -0.5 0 180) (size 0.22 0.22) (layers F.Cu)
      (net 187 "Net-(TL31-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 196.6916 103.16826 180)
    (fp_text reference TL30 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0 180) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 180) (size 0.22 0.35) (layers F.Cu)
      (net 157 /receiver_3/LNA_OUT))
    (pad 1 smd rect (at -0.5 0 180) (size 0.22 0.22) (layers F.Cu)
      (net 186 "Net-(TL30-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 196.6916 89.87092 180)
    (fp_text reference TL29 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0 180) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 180) (size 0.22 0.35) (layers F.Cu)
      (net 156 /receiver_2/LNA_OUT))
    (pad 1 smd rect (at -0.5 0 180) (size 0.22 0.22) (layers F.Cu)
      (net 185 "Net-(TL29-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 202.6787 76.57544)
    (fp_text reference TL28 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 42 "Net-(C55-Pad1)"))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 184 "Net-(TL28-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 202.68014 116.47472)
    (fp_text reference TL27 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 29 "Net-(C37-Pad1)"))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 183 "Net-(TL27-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 202.68014 103.1708)
    (fp_text reference TL26 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 16 "Net-(C19-Pad1)"))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 182 "Net-(TL26-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 202.68014 89.87346)
    (fp_text reference TL25 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -0.5 0) (size 0.22 0.22) (layers F.Cu)
      (net 181 "Net-(TL25-Pad1)"))
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59DE0611)
    (at 112.23146 75.79312)
    (descr "Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J9 (at 1.27508 16.38808 180) (layer F.SilkS))
    (fp_text value LMX2491_CONN (at 1.27 16.764) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 104 "Net-(J9-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 105 "Net-(J9-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 106 "Net-(J9-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 107 "Net-(J9-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 108 "Net-(J9-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 109 "Net-(J9-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 110 "Net-(J9-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 111 "Net-(J9-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 112 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:LP5900_NGF_6 (layer F.Cu) (tedit 5E66AE0C)
    (at 131.9825 105.3257 90)
    (fp_text reference U26 (at 2.9845 1.3081 90) (layer F.SilkS))
    (fp_text value LP5900-TL3.0 (at 0 2.625 270) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at -1.1557 -0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 +3V0) (solder_mask_margin 0.05))
    (pad 2 smd roundrect (at -1.1557 0 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 3 smd roundrect (at -1.1557 0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 4 smd roundrect (at 1.1557 0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 /power/5V0_PGD) (solder_mask_margin 0.05))
    (pad 5 smd roundrect (at 1.1557 0 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 6 smd roundrect (at 1.1557 -0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V) (solder_mask_margin 0.05))
    (pad 7 smd rect (at 0 0 90) (size 0.762 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin -0.09))
  )
  (module aps_radar_lib:HMC-LP3 (layer F.Cu) (tedit 5E65ADA5)
    (at 139.4247 103.662 90)
    (fp_text reference U17 (at -0.0762 -2.6416 270) (layer F.SilkS))
    (fp_text value HMC540S (at 0.01 3.06 90) (layer F.SilkS) hide)
    (pad 50 smd rect (at 1.45 0 90) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 50 smd rect (at -1.45 0 90) (size 0.8 1.95) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 50 smd rect (at 0 -1.45 90) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 50 smd rect (at -0.0025 1.45 90) (size 1.95 0.8) (layers F.Mask)
      (solder_paste_margin -0.2))
    (pad 17 thru_hole circle (at 0 0 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 0.525 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 0.525 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.525 -0.525 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.525 -0.525 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad ~ smd roundrect (at 0.75 1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.75 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 0.25 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.25 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -1.45 -0.75 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.75 -1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at -0.25 -1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.25 -1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 0.75 -1.45 180) (size 0.75 0.15) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.75 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 -0.25 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.25 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad ~ smd roundrect (at 1.45 0.75 180) (size 0.15 0.75) (layers F.Paste) (roundrect_rratio 0.5))
    (pad 17 smd roundrect (at 0.3433 0.3433 90) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 0.3433 90) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at 0.3433 -0.3433 90) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at -0.3433 -0.3433 90) (size 0.6366 0.6366) (layers F.Paste) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd rect (at 0 0 90) (size 1.4732 1.4732) (layers F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.45 -0.750001 180) (size 0.22 0.799999) (layers F.Cu)
      (net 61 +3V3) (solder_paste_margin_ratio -0.1))
    (pad 2 smd rect (at -1.45 -0.25 180) (size 0.22 0.799999) (layers F.Cu)
      (net 167 "Net-(TL10-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 3 smd rect (at -1.45 0.25 180) (size 0.22 0.799999) (layers F.Cu)
      (solder_paste_margin_ratio -0.1))
    (pad 4 smd rect (at -1.45 0.750001 180) (size 0.22 0.799999) (layers F.Cu)
      (net 57 "Net-(C75-Pad2)") (solder_paste_margin_ratio -0.1))
    (pad 5 smd rect (at -0.750001 1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (net 57 "Net-(C75-Pad2)") (solder_paste_margin_ratio -0.1))
    (pad 6 smd rect (at -0.25 1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (net 57 "Net-(C75-Pad2)") (solder_paste_margin_ratio -0.1))
    (pad 7 smd rect (at 0.25 1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (solder_paste_margin_ratio -0.1))
    (pad 8 smd rect (at 0.750001 1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (net 64 "Net-(C81-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 9 smd rect (at 1.45 0.750001 180) (size 0.22 0.799999) (layers F.Cu)
      (solder_paste_margin_ratio -0.1))
    (pad 10 smd rect (at 1.45 0.25 180) (size 0.22 0.799999) (layers F.Cu)
      (solder_paste_margin_ratio -0.1))
    (pad 11 smd rect (at 1.45 -0.25 180) (size 0.22 0.799999) (layers F.Cu)
      (net 168 "Net-(TL11-Pad1)") (solder_paste_margin_ratio -0.1))
    (pad 12 smd rect (at 1.45 -0.750001 180) (size 0.22 0.799999) (layers F.Cu)
      (solder_paste_margin_ratio -0.1))
    (pad 13 smd rect (at 0.750001 -1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (net 116 /~ATTEN_8DB) (solder_paste_margin_ratio -0.1))
    (pad 14 smd rect (at 0.25 -1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (net 115 /~ATTEN_4DB) (solder_paste_margin_ratio -0.1))
    (pad 15 smd rect (at -0.25 -1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (net 114 /~ATTEN_2DB) (solder_paste_margin_ratio -0.1))
    (pad 16 smd rect (at -0.750001 -1.45 90) (size 0.22 0.799999) (layers F.Cu)
      (net 113 /~ATTEN_1DB) (solder_paste_margin_ratio -0.1))
    (pad 17 smd rect (at 0 0 90) (size 1.778 1.778) (layers F.Cu)
      (net 3 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.601 83.1896)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R56 (at 0.0127 -0.9906) (layer F.SilkS))
    (fp_text value 68 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "Net-(R55-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.0897 83.6722 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R57 (at 0.0254 -0.9398 90) (layer F.SilkS))
    (fp_text value 18 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "Net-(R55-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(C93-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.0897 81.7037 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R55 (at 0.1143 -0.9271 90) (layer F.SilkS))
    (fp_text value 18 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 139 /transmitter/REF_OUT))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "Net-(R55-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:LMX2491RTWR (layer F.Cu) (tedit 5E659F31)
    (at 126.1659 90.8096 180)
    (fp_text reference U22 (at 2.8448 1.9685 90) (layer F.SilkS))
    (fp_text value LMX2491RTWR (at 0 3.38) (layer F.SilkS) hide)
    (pad 25 smd rect (at -0.675 0.675 180) (size 1.115 1.15) (layers F.Paste)
      (net 3 GND))
    (pad 25 smd rect (at 0.675 0.675 180) (size 1.115 1.15) (layers F.Paste)
      (net 3 GND))
    (pad 25 smd rect (at -0.675 -0.675 180) (size 1.115 1.15) (layers F.Paste)
      (net 3 GND))
    (pad 25 smd rect (at 0.675 -0.675 180) (size 1.115 1.15) (layers F.Paste)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.899999 -1.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 2 smd roundrect (at -1.899999 -0.750001 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 3 smd roundrect (at -1.899999 -0.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 4 smd roundrect (at -1.899999 0.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(C98-Pad2)") (solder_mask_margin 0.05))
    (pad 5 smd roundrect (at -1.899999 0.750001 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(C99-Pad2)") (solder_mask_margin 0.05))
    (pad 6 smd roundrect (at -1.899999 1.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC) (solder_mask_margin 0.05))
    (pad 7 smd roundrect (at -1.25 1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC) (solder_mask_margin 0.05))
    (pad 8 smd roundrect (at -0.750001 1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC) (solder_mask_margin 0.05))
    (pad 9 smd roundrect (at -0.25 1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(C93-Pad1)") (solder_mask_margin 0.05))
    (pad 10 smd roundrect (at 0.25 1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C94-Pad1)") (solder_mask_margin 0.05))
    (pad 11 smd roundrect (at 0.750001 1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 12 smd roundrect (at 1.25 1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /LMX_MOD) (solder_mask_margin 0.05))
    (pad 13 smd roundrect (at 1.899999 1.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 /transmitter/LMX_CE) (solder_mask_margin 0.05))
    (pad 14 smd roundrect (at 1.899999 0.750001 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 /transmitter/LMX_CLK) (solder_mask_margin 0.05))
    (pad 15 smd roundrect (at 1.899999 0.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 /transmitter/LMX_DATA) (solder_mask_margin 0.05))
    (pad 16 smd roundrect (at 1.899999 -0.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 /transmitter/LMX_LE) (solder_mask_margin 0.05))
    (pad 17 smd roundrect (at 1.899999 -0.750001 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /LMX_MUXOUT) (solder_mask_margin 0.05))
    (pad 18 smd roundrect (at 1.899999 -1.25 270) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC) (solder_mask_margin 0.05))
    (pad 19 smd roundrect (at 1.25 -1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC) (solder_mask_margin 0.05))
    (pad 20 smd roundrect (at 0.750001 -1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /LMX_TRIG1) (solder_mask_margin 0.05))
    (pad 21 smd roundrect (at 0.25 -1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /LMX_TRIG2) (solder_mask_margin 0.05))
    (pad 22 smd roundrect (at -0.25 -1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /transmitter/LMX_VCP) (solder_mask_margin 0.05))
    (pad 23 smd roundrect (at -0.750001 -1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 24 smd roundrect (at -1.25 -1.899999 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 179 "Net-(TL22-Pad1)") (solder_mask_margin 0.05))
    (pad 25 smd rect (at 0 0 180) (size 2.6 2.6) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad 25 thru_hole circle (at 0 1.05 180) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 25 thru_hole circle (at 0 0 180) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 25 thru_hole circle (at -1.05 0 180) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 25 thru_hole circle (at 1.05 0 180) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 25 thru_hole circle (at 0 -1.05 180) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.7242 92.3336 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C89 (at 2.0701 -0.0127 180) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.1974 94.1243 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C87 (at -0.0508 1.0033 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.3945 94.2386 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C84 (at 0 1.0541 270) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /transmitter/LMX_VCP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.0615 87.9878 45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C92 (at -1.052387 0.890742 225) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.6043 87.0758 45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C91 (at 0.314309 -0.835164 45) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.0803 87.0758 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C90 (at 1.3081 0.2032 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:IC_Taper_0.25_0.35 (layer F.Cu) (tedit 5E65291F)
    (at 127.4207 93.7364 270)
    (fp_text reference TL22 (at 0.01 1.125 270) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 270) (layer F.Fab))
    (pad ~ smd rect (at 0.045 -0.0025 270) (size 1.3525 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 54 /transmitter/LMX_CPOUT))
    (pad 1 smd rect (at -0.43 0 270) (size 0.4 0.25) (layers F.Cu)
      (net 179 "Net-(TL22-Pad1)"))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.8423 96.5373)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C76 (at 2.0447 0.0762 90) (layer F.SilkS))
    (fp_text value 0.68nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C76-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /transmitter/LMX_CPOUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.7798 92.486 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C100 (at 2.0574 -0.0254 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.5766 95.5086 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C97 (at 1.4478 -0.381 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.5766 94.5053 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C96 (at 1.4605 0.762 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.5766 96.5119 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C95 (at 0.3683 -1.1303) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 138.9802 109.8215 180)
    (fp_text reference TL21 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 180) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 180) (size 0.35 0.3575) (layers F.Cu)
      (net 178 "Net-(TL20-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 180) (size 0.36 0.35) (layers F.Cu)
      (net 56 /transmitter/VCO_OUT))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 136.8212 110.2152)
    (fp_text reference TL20 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195) (size 0.35 0.3575) (layers F.Cu)
      (net 178 "Net-(TL20-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625) (size 0.36 0.35) (layers F.Cu)
      (net 177 "Net-(TL20-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 132.2277 90.7499 270)
    (fp_text reference TL19 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 176 "Net-(TL18-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 77 /transmitter/LMX_FIN))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 132.6263 98.8195 90)
    (fp_text reference TL18 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 90) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 90) (size 0.35 0.3575) (layers F.Cu)
      (net 176 "Net-(TL18-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 90) (size 0.36 0.35) (layers F.Cu)
      (net 174 "Net-(TL17-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 134.6788 99.2043 270)
    (fp_text reference TL17 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 175 "Net-(TL17-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 174 "Net-(TL17-Pad1)"))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.8766 97.8073 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R40 (at 2.6543 0.254 180) (layer F.SilkS))
    (fp_text value 1.0k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C78-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 135.55628 116.01656 180)
    (fp_text reference TL16 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 180) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 180) (size 0.35 0.3575) (layers F.Cu)
      (net 166 "Net-(TL13-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 180) (size 0.36 0.35) (layers F.Cu)
      (net 173 "Net-(TL16-Pad1)"))
  )
  (module aps_radar_lib:wilkinson_3db (layer F.Cu) (tedit 5E6534B7)
    (at 170.3357 92.64819)
    (fp_text reference TL2 (at -0.01 -5.42) (layer F.SilkS) hide)
    (fp_text value wilkinson_3dB (at 0 5.47) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.87 -2.81) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.875 2.79) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.4 -2.85) (size 1.25 4.32) (layers F.Mask))
    (pad ~ smd rect (at 1.4275 2.845) (size 1.25 4.3) (layers F.Mask))
    (pad ~ smd rect (at -1.5 0) (size 1.25 10) (layers F.Mask))
    (pad ~ smd rect (at -0.04 -0.005) (size 1.7 10) (layers F.Mask))
    (pad 5 thru_hole circle (at 2.14 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6975 2.2725) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6925 1.6525) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.692595 2.946954 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.548162 3.686211 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.097432 4.289703 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.429579 4.638034 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.323264 4.662285 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.012151 4.357661 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.500788 3.784428 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 0.77 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 1.532 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 2.294 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 3.056 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.99998) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.14284) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 1.2857) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 0.42856) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -0.42858) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -1.28572) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -2.14286) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -3) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.680086 -2.951932) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.534732 -3.685272) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.085738 -4.283033) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.421934 -4.626952) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.325347 -4.648985) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.00826 -4.344772) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.491693 -3.774502) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.69 -1.675) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.685 -2.295) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -3.051) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -2.289) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -1.527) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -0.765) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad ~ smd roundrect (at 1.23 -0.3875) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.275))
    (pad ~ smd roundrect (at 1.23 0.39) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.35))
    (pad 3 smd rect (at 1.83 0.875) (size 0.3517 0.3517) (layers F.Cu)
      (net 150 "Net-(TL2-Pad3)"))
    (pad 2 smd rect (at 1.83 -0.8725) (size 0.3517 0.3517) (layers F.Cu)
      (net 151 "Net-(TL2-Pad2)"))
    (pad 1 smd rect (at -1.83 0.0025) (size 0.3517 0.3517) (layers F.Cu)
      (net 161 "Net-(TL1-Pad4)"))
  )
  (module aps_radar_lib:wilkinson_3db (layer F.Cu) (tedit 5E6534B7)
    (at 176.28378 79.34998)
    (clearance 0.1)
    (fp_text reference TL3 (at -0.01 -5.42) (layer F.SilkS) hide)
    (fp_text value wilkinson_3dB (at 0 5.47) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.87 -2.81) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.875 2.79) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.4 -2.85) (size 1.25 4.32) (layers F.Mask))
    (pad ~ smd rect (at 1.4275 2.845) (size 1.25 4.3) (layers F.Mask))
    (pad ~ smd rect (at -1.5 0) (size 1.25 10) (layers F.Mask))
    (pad ~ smd rect (at -0.04 -0.005) (size 1.7 10) (layers F.Mask))
    (pad 5 thru_hole circle (at 2.14 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6975 2.2725) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6925 1.6525) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.692595 2.946954 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.548162 3.686211 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.097432 4.289703 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.429579 4.638034 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.323264 4.662285 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.012151 4.357661 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.500788 3.784428 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 0.77 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 1.532 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 2.294 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 3.056 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.99998) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.14284) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 1.2857) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 0.42856) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -0.42858) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -1.28572) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -2.14286) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -3) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.680086 -2.951932) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.534732 -3.685272) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.085738 -4.283033) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.421934 -4.626952) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.325347 -4.648985) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.00826 -4.344772) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.491693 -3.774502) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.69 -1.675) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.685 -2.295) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -3.051) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -2.289) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -1.527) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -0.765) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad ~ smd roundrect (at 1.23 -0.3875) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.275))
    (pad ~ smd roundrect (at 1.23 0.39) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.35))
    (pad 3 smd rect (at 1.83 0.875) (size 0.3517 0.3517) (layers F.Cu)
      (net 210 "Net-(TL3-Pad3)"))
    (pad 2 smd rect (at 1.83 -0.8725) (size 0.3517 0.3517) (layers F.Cu)
      (net 211 "Net-(TL3-Pad2)"))
    (pad 1 smd rect (at -1.83 0.0025) (size 0.3517 0.3517) (layers F.Cu)
      (net 162 "Net-(TL3-Pad1)"))
  )
  (module aps_radar_lib:wilkinson_3db (layer F.Cu) (tedit 5E6534B7)
    (at 176.28378 105.9464)
    (fp_text reference TL4 (at -0.01 -5.42) (layer F.SilkS) hide)
    (fp_text value wilkinson_3dB (at 0 5.47) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.87 -2.81) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.875 2.79) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.4 -2.85) (size 1.25 4.32) (layers F.Mask))
    (pad ~ smd rect (at 1.4275 2.845) (size 1.25 4.3) (layers F.Mask))
    (pad ~ smd rect (at -1.5 0) (size 1.25 10) (layers F.Mask))
    (pad ~ smd rect (at -0.04 -0.005) (size 1.7 10) (layers F.Mask))
    (pad 5 thru_hole circle (at 2.14 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6975 2.2725) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6925 1.6525) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.692595 2.946954 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.548162 3.686211 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.097432 4.289703 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.429579 4.638034 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.323264 4.662285 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.012151 4.357661 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.500788 3.784428 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 0.77 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 1.532 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 2.294 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 3.056 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.99998) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.14284) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 1.2857) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 0.42856) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -0.42858) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -1.28572) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -2.14286) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -3) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.680086 -2.951932) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.534732 -3.685272) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.085738 -4.283033) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.421934 -4.626952) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.325347 -4.648985) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.00826 -4.344772) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.491693 -3.774502) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.69 -1.675) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.685 -2.295) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -3.051) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -2.289) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -1.527) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -0.765) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad ~ smd roundrect (at 1.23 -0.3875) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.275))
    (pad ~ smd roundrect (at 1.23 0.39) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.35))
    (pad 3 smd rect (at 1.83 0.875) (size 0.3517 0.3517) (layers F.Cu)
      (net 212 "Net-(TL4-Pad3)"))
    (pad 2 smd rect (at 1.83 -0.8725) (size 0.3517 0.3517) (layers F.Cu)
      (net 213 "Net-(TL4-Pad2)"))
    (pad 1 smd rect (at -1.83 0.0025) (size 0.3517 0.3517) (layers F.Cu)
      (net 163 "Net-(TL4-Pad1)"))
  )
  (module aps_radar_lib:wilkinson_3db (layer F.Cu) (tedit 5E6534B7)
    (at 135.74678 113.08794 90)
    (fp_text reference TL5 (at -0.01 -5.42 90) (layer F.SilkS) hide)
    (fp_text value wilkinson_3dB (at 0 5.47 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at 1.87 -2.81 90) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.875 2.79 90) (size 0.5 4.4) (layers F.Mask))
    (pad ~ smd rect (at 1.4 -2.85 90) (size 1.25 4.32) (layers F.Mask))
    (pad ~ smd rect (at 1.4275 2.845 90) (size 1.25 4.3) (layers F.Mask))
    (pad ~ smd rect (at -1.5 0 90) (size 1.25 10) (layers F.Mask))
    (pad ~ smd rect (at -0.04 -0.005 90) (size 1.7 10) (layers F.Mask))
    (pad 5 thru_hole circle (at 2.14 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6975 2.2725 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.6925 1.6525 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.692595 2.946954 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.548162 3.686211 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.097432 4.289703 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.429579 4.638034 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.323264 4.662285 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.012151 4.357661 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.500788 3.784428 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 0.77 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 1.532 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 2.294 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.6925 3.056 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.99998 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 2.14284 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 1.2857 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 0.42856 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -0.42858 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -1.28572 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -2.14286 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0 -3 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.680086 -2.951932 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.534732 -3.685272 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.085738 -4.283033 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 0.421934 -4.626952 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -0.325347 -4.648985 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.00826 -4.344772 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.491693 -3.774502 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.69 -1.675 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at 1.685 -2.295 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -3.051 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -2.289 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -1.527 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad 5 thru_hole circle (at -1.68 -0.765 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_paste_margin_ratio -0.1))
    (pad ~ smd roundrect (at 1.23 -0.3875 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.275))
    (pad ~ smd roundrect (at 1.23 0.39 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.35))
    (pad 3 smd rect (at 1.83 0.875 90) (size 0.3517 0.3517) (layers F.Cu)
      (net 177 "Net-(TL20-Pad1)"))
    (pad 2 smd rect (at 1.83 -0.8725 90) (size 0.3517 0.3517) (layers F.Cu)
      (net 175 "Net-(TL17-Pad2)"))
    (pad 1 smd rect (at -1.83 0.0025 90) (size 0.3517 0.3517) (layers F.Cu)
      (net 173 "Net-(TL16-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.25_0.35 (layer F.Cu) (tedit 5E65291F)
    (at 129.49418 116.2096)
    (fp_text reference TL13 (at 0.01 1.125 180) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 180) (layer F.Fab))
    (pad ~ smd rect (at 0.045 -0.0025) (size 1.3525 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0) (size 0.22 0.35) (layers F.Cu)
      (net 166 "Net-(TL13-Pad2)"))
    (pad 1 smd rect (at -0.43 0) (size 0.4 0.25) (layers F.Cu)
      (net 170 "Net-(TL13-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.25_0.35 (layer F.Cu) (tedit 5E65291F)
    (at 126.12018 113.21748 90)
    (fp_text reference TL12 (at 0.01 1.125 270) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 270) (layer F.Fab))
    (pad ~ smd rect (at 0.045 -0.0025 90) (size 1.3525 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 90) (size 0.22 0.35) (layers F.Cu)
      (net 68 "Net-(C85-Pad1)"))
    (pad 1 smd rect (at -0.43 0 90) (size 0.4 0.25) (layers F.Cu)
      (net 169 "Net-(TL12-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 139.1707 101.1347 90)
    (fp_text reference TL11 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0 90) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 90) (size 0.22 0.35) (layers F.Cu)
      (net 63 "Net-(C80-Pad1)"))
    (pad 1 smd rect (at -0.5 0 90) (size 0.22 0.22) (layers F.Cu)
      (net 168 "Net-(TL11-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.22_0.35 (layer F.Cu) (tedit 5E6528E8)
    (at 139.17578 106.3121 270)
    (fp_text reference TL10 (at 0.01 1.125 90) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 90) (layer F.Fab))
    (pad ~ smd rect (at 0.055 0 270) (size 1.3325 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 270) (size 0.22 0.35) (layers F.Cu)
      (net 55 "Net-(C74-Pad2)"))
    (pad 1 smd rect (at -0.5 0 270) (size 0.22 0.22) (layers F.Cu)
      (net 167 "Net-(TL10-Pad1)"))
  )
  (module aps_radar_lib:IC_Taper_0.25_0.35 (layer F.Cu) (tedit 5E65291F)
    (at 139.17578 92.07126 90)
    (fp_text reference TL15 (at 0.01 1.125 270) (layer F.SilkS) hide)
    (fp_text value ic_taper (at -0.025 -1.4575 270) (layer F.Fab))
    (pad ~ smd rect (at 0.045 -0.0025 90) (size 1.3525 1) (layers F.Mask))
    (pad 2 smd rect (at 0.61 0 90) (size 0.22 0.35) (layers F.Cu)
      (net 149 /transmitter/PA_OUT))
    (pad 1 smd rect (at -0.43 0 90) (size 0.4 0.25) (layers F.Cu)
      (net 172 "Net-(TL15-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 173.6235 105.7564 90)
    (fp_text reference TL9 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 90) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 90) (size 0.35 0.3575) (layers F.Cu)
      (net 164 "Net-(TL6-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 90) (size 0.36 0.35) (layers F.Cu)
      (net 163 "Net-(TL4-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 173.22426 91.5863 180)
    (fp_text reference TL8 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 180) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 180) (size 0.35 0.3575) (layers F.Cu)
      (net 151 "Net-(TL2-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 180) (size 0.36 0.35) (layers F.Cu)
      (net 165 "Net-(TL7-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 173.6185 79.5464)
    (fp_text reference TL7 (at -0.0875 -1.7825) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195) (size 0.35 0.3575) (layers F.Cu)
      (net 162 "Net-(TL3-Pad1)"))
    (pad 1 smd rect (at -0.195 0.3625) (size 0.36 0.35) (layers F.Cu)
      (net 165 "Net-(TL7-Pad1)"))
  )
  (module aps_radar_lib:mitered_bend_50 (layer F.Cu) (tedit 5E652D99)
    (at 173.2313 93.7199 270)
    (fp_text reference TL6 (at -0.0875 -1.7825 90) (layer F.SilkS) hide)
    (fp_text value mitered_bend (at 0.4575 1.895 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.08 -0.085 270) (size 1.25 1.25) (layers F.Mask))
    (pad 2 smd rect (at 0.3675 -0.195 270) (size 0.35 0.3575) (layers F.Cu)
      (net 164 "Net-(TL6-Pad2)"))
    (pad 1 smd rect (at -0.195 0.3625 270) (size 0.36 0.35) (layers F.Cu)
      (net 150 "Net-(TL2-Pad3)"))
  )
  (module aps_radar_lib:coupled_line_14db (layer F.Cu) (tedit 5E6529B0)
    (at 139.1707 82.8086 90)
    (fp_text reference TL1 (at 0.01 -1.32 90) (layer F.SilkS) hide)
    (fp_text value coupled_line_14db (at -0.0025 2.035 90) (layer F.SilkS) hide)
    (pad ~ smd rect (at -0.015 0.2625 90) (size 10 1.75) (layers F.Mask))
    (pad 1 smd rect (at -4.21 0.005 90) (size 0.351665 0.351665) (layers F.Cu)
      (net 149 /transmitter/PA_OUT))
    (pad 4 smd rect (at -4.2075 0.9 90) (size 0.351665 0.351665) (layers F.Cu)
      (net 161 "Net-(TL1-Pad4)"))
    (pad 2 smd rect (at 4.225 0.005 90) (size 0.351665 0.351665) (layers F.Cu)
      (net 103 /transmitter/TX_OUT))
    (pad 3 smd rect (at 4.2225 0.9025 90) (size 0.351665 0.351665) (layers F.Cu)
      (net 160 "Net-(R81-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 141.5837 78.6176)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R81 (at 2.33426 -0.04826) (layer F.SilkS))
    (fp_text value 50 (at 0 -1.27) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 160 "Net-(R81-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:VSSOP-8_3.0x3.0mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 126.458 102.5317 270)
    (descr "VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf")
    (tags "VSSOP-8 3.0 x 3.0")
    (attr smd)
    (fp_text reference U19 (at -3.00482 -2.9845 180) (layer F.SilkS))
    (fp_text value OPA192 (at 0.02 2.73 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.2 -0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.2 -0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C82-Pad1)"))
    (pad 6 smd rect (at 2.2 0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(R44-Pad1)"))
    (pad 5 smd rect (at 2.2 0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.2 0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -2.2 0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 54 /transmitter/LMX_CPOUT))
    (pad 2 smd rect (at -2.2 -0.325 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C78-Pad1)"))
    (pad 1 smd rect (at -2.2 -0.975 180) (size 0.45 1.45) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-8_3.0x3.0mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 112.6404 94.5688 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R75 (at -0.0127 -1.3208 90) (layer F.SilkS))
    (fp_text value 59.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(C119-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 110.30106 114.08108)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R76 (at 0.01524 -1.22936) (layer F.SilkS))
    (fp_text value 332k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(C120-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 112.6277 113.33432 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R77 (at 2.00152 0.39624 180) (layer F.SilkS))
    (fp_text value 63.4k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(C120-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.21266 113.32924 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R78 (at 0.01016 1.33096 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 145 "Net-(R78-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 /power/5V0_PGD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.93022 94.43164 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R79 (at -2.02184 0.04572) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 /power/5V25_PGD))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 +5V25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.43542 115.63556 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R80 (at 0 1.33096) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 /power/5V0_PGD))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 169.7685 71.5214 270)
    (fp_text reference RV1 (at 0.845 -3.485 90) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999 90) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R8-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /RX2_Q))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 155.0985 99.0064 180)
    (fp_text reference RV2 (at -1.58 -4.14 90) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R11-Pad1)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX2_I))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 163.52672 99.018 180)
    (fp_text reference RV3 (at -0.92678 3.3466 180) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R15-Pad1)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /RX3_Q))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 155.10372 111.762 180)
    (fp_text reference RV4 (at -1.57478 -4.0694 90) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R18-Pad1)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /RX3_I))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 163.57172 111.76192 180)
    (fp_text reference RV5 (at -0.29678 4.08052 90) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R22-Pad1)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 /RX4_Q))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 204.49536 116.47472)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 1.2pF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /receiver_4/ANT_IN))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(C37-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.13494 113.19068 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 3.02006 0.02286 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(C38-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 151.76372 114.712 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 2.195 0.05) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.94028 120.01294 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 2.63774 -0.09466 90) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C39-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 197.13494 122.14268 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C40 (at -2.07228 -0.04936) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C39-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 200.5736 120.01802 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C41 (at 2.13868 -0.27432) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C39-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 202.38716 119.81736 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C42 (at 2.79904 -0.15134 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C39-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 182.59294 116.5264 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C43 (at -3.20892 0.06056 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C43-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.34808 116.00062 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C44 (at -2.07772 -0.31242) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C43-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.35062 119.041 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C45 (at -2.08026 0.29972) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C43-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 194.67494 122.12268 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C46 (at -2.05228 -0.02016) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C43-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.87494 121.15068 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C47 (at -2.12 -0.25) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C43-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 191.34494 119.63068 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C48 (at -2.15 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C43-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.77672 107.37442 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C49 (at 1.96302 -0.25322) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C49-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /RX4_Q))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.5585 107.3614 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C50 (at 2.05052 -0.43322) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C50-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 160.23172 114.71192 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C51 (at 2.22948 -0.66178) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C51-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.3085 106.4339 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C52 (at 1.9845 -0.5722) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C52-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /RX4_I))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 165.1385 106.4239 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C53 (at -1.9475 0.085) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C53-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 168.7635 113.7714 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C54 (at 2.195 0.05 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C54-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 204.49392 76.57544)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C55 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 1.2pF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /receiver_1/ANT_IN))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(C55-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.1335 73.2914 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C56 (at 3.02006 0.02286 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C56-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.93884 80.11366 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C57 (at 2.63774 -0.09466 90) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C57-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 197.1335 82.2434 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C58 (at -2.0764 0.0254) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C57-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 200.57216 80.11874 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C59 (at 2.13868 -0.27432) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C57-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 202.38572 79.91808 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C60 (at 0.00762 -1.53924 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C57-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 182.5915 76.62712 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C61 (at -3.20892 0.06056 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C61-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.34664 76.10134 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C62 (at -2.07772 -0.31242) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C61-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.34918 79.14172 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C63 (at -2.08026 0.29972) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C61-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 194.6735 82.2234 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C64 (at -2.0564 -0.05) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C61-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.8735 81.2514 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C65 (at -2.12 -0.25) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C61-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 191.3435 79.7314 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C66 (at -2.15 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C61-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.50528 75.48014 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C67 (at 2.1225 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C67-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /RX1_Q))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.27028 75.46264 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C68 (at -0.09 -1.195 270) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(C68-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 159.96028 82.81764 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C69 (at 2.18876 -0.76322 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(C69-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.11728 75.46414 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C70 (at 2.1225 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(C70-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /RX1_I))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.0685 78.5864 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C71 (at -2.64 -0.015 270) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C71-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 151.57228 82.80164 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C72 (at 2.195 0.05) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(C72-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.9246 98.2264 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C73 (at -2.0828 -0.0889 90) (layer F.SilkS))
    (fp_text value 68pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /transmitter/LMX_CPOUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.9899 95.3054 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R74 (at 0.0381 -1.2827) (layer F.SilkS))
    (fp_text value 332k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(C119-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 +5V25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.34808 102.6967 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at -2.07772 -0.31242) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.35062 105.73708 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at -2.08026 0.29972) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 194.67494 108.81876 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at -2.03256 0.00524) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.87494 107.84676 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at -2.12 -0.25) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 191.34494 106.32676 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at -2.15 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.73172 94.6305 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 2.1225 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C31-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /RX3_Q))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.49672 94.613 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at -0.089999 -1.195 270) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C32-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 160.18672 101.968 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 2.2034 -0.16678) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C33-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 136.89134 120.93356 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R73 (at 2.03216 -0.08784 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 +3V0))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.30872 107.3745 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 2.1225 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C34-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /RX3_I))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.07372 107.357 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at -2.6644 0.05978 270) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C35-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 182.59294 103.22248 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at -3.20892 0.06056 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 204.49536 103.1708)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 1.2pF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /receiver_3/ANT_IN))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.13494 99.88676 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 3.02006 0.02286 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.94028 106.70902 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 2.63774 -0.09466 90) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 202.38716 106.51344 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0.00762 -1.53924 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 200.5736 106.7141 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 2.13868 -0.27432) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 197.13494 108.83876 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at -2.07796 0.02684) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 163.30028 79.86764 180)
    (fp_text reference RV7 (at -1.59322 -4.21876 90) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R29-Pad1)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 /RX1_Q))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module aps_radar_lib:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B0430E8)
    (at 154.91228 79.85164 180)
    (fp_text reference RV8 (at -1.60622 -4.23976 270) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.499999) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(R32-Pad1)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 51 /RX1_I))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
  )
  (module Button_Switch_THT:SW_CuK_JS202011AQN_DPDT_Angled (layer F.Cu) (tedit 5A02FE31)
    (at 96.6835 121.7814)
    (descr "CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
    (tags "switch DPDT")
    (fp_text reference SW2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value ON/OFF (at 4.28244 -1.71196) (layer F.SilkS) hide)
    (fp_text user %R (at 2.5 1.75) (layer F.Fab))
    (pad 6 thru_hole circle (at 5 3.3) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole circle (at 2.5 3.3) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 0 3.3) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 5 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 180 /power/+12V0_IN_CONN))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 193 /power/POWER_SW))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_CuK_JS202011AQN_DPDT_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 142.6505 90.3524)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value PA_DET (at -0.03048 -1.397) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 141 "Net-(R60-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 132.49558 79.3288)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 0.01524 -1.651 180) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 0 -1.50368) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 61 +3V3))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 101.54314 111.40392)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value 12V0_in (at 0 1.55) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 180 /power/+12V0_IN_CONN))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 123.77322 105.07424)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value 10V0 (at -1.31064 0.01016 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 84 +10V))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 103.97646 107.38564 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value 5V5 (at 0 1.55) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1 1) (layers F.Cu F.Mask)
      (net 85 /power/5V5_OUT))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 105.17534 95.97596 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value 5V5_PGD (at 2.40284 1.61036) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1 1) (layers F.Cu F.Mask)
      (net 143 /power/5V5_PGD))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 132.82578 109.09252)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value 3V0 (at 0.03556 -1.35636) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 86 +3V0))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 109.2749 97.8708 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at 0 -1.448 90) (layer F.SilkS) hide)
    (fp_text value 5V25 (at 1.41224 0) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1 1) (layers F.Cu F.Mask)
      (net 90 +5V25))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 109.29014 102.07196 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 -1.448 90) (layer F.SilkS) hide)
    (fp_text value 5V25_PGD (at -2.159 0.01524 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1 1) (layers F.Cu F.Mask)
      (net 147 /power/5V25_PGD))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 107.3445 110.67748 270)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 0 -1.448 90) (layer F.SilkS) hide)
    (fp_text value 5V0 (at 0 1.55 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1 1) (layers F.Cu F.Mask)
      (net 80 +5V))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 117.6735 114.8114 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value 5V0_PGD (at -0.04064 -1.55956) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1 1) (layers F.Cu F.Mask)
      (net 146 /power/5V0_PGD))
  )
  (module Oscillator:Oscillator_SMD_Abracon_ASDMB-4Pin_2.5x2.0mm (layer F.Cu) (tedit 5CA1C904)
    (at 126.9025 79.1002 180)
    (descr "Miniature Crystal Clock Oscillator Abracon ASDMB series, 2.5x2.0mm package, http://www.abracon.com/Oscillators/ASDMB.pdf")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference U18 (at 0.0381 2.2225) (layer F.SilkS))
    (fp_text value ASDMB-100MHz (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.825 -0.775 180) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C77-Pad1)"))
    (pad 3 smd rect (at 0.825 -0.775 180) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 139 /transmitter/REF_OUT))
    (pad 2 smd rect (at 0.825 0.775 180) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.825 0.775 180) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(JP5-Pad2)"))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_Abracon_ASDMB-4Pin_2.5x2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:QFN4-20-TQP5523 (layer F.Cu) (tedit 5E61BC38)
    (at 139.17578 95.00568 90)
    (descr "TQ5523 Landing pattern.")
    (tags TQ5523)
    (attr smd)
    (fp_text reference U21 (at -3.34772 -1.83388 180) (layer F.SilkS))
    (fp_text value TQP5523 (at 0 3.6 90) (layer F.Fab))
    (pad 21 smd rect (at 0 0 90) (size 2.7 2.7) (layers F.Cu)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 22 smd roundrect (at -0.6 -0.6 90) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 22 smd roundrect (at 0.6 -0.6 90) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 22 smd roundrect (at -0.6 0.6 90) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 22 smd roundrect (at 0.6 0.6 90) (size 1 1) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 21 smd rect (at 0 0 90) (size 2.5 2.5) (layers F.Mask)
      (net 3 GND) (solder_paste_margin -0.2))
    (pad 21 thru_hole circle (at 1.08 1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.08 0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.08 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.08 -0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.08 -1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0.54 1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0.54 0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0.54 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0.54 -0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0.54 -1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 -0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 -1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -0.54 1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -0.54 0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -0.54 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -0.54 -0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -0.54 -1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.08 1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.08 0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.08 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.08 -0.54 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.08 -1.08 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 20 smd roundrect (at -1 -1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)") (solder_mask_margin 0.05))
    (pad 19 smd roundrect (at -0.5 -1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)") (solder_mask_margin 0.05))
    (pad 18 smd roundrect (at 0 -1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)") (solder_mask_margin 0.05))
    (pad 17 smd roundrect (at 0.5 -1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 16 smd roundrect (at 1 -1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 15 smd roundrect (at 1.85 -1 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 14 smd roundrect (at 1.85 -0.5 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 13 smd roundrect (at 1.85 0 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 172 "Net-(TL15-Pad1)") (solder_mask_margin 0.05))
    (pad 12 smd roundrect (at 1.85 0.5 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 11 smd roundrect (at 1.85 1 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 10 smd roundrect (at 1 1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 141 "Net-(R60-Pad1)") (solder_mask_margin 0.05))
    (pad 9 smd roundrect (at 0.5 1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 8 smd roundrect (at 0 1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 7 smd roundrect (at -0.5 1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 6 smd roundrect (at -1 1.85 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 5 smd roundrect (at -1.85 1 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(SW1-Pad2)") (solder_mask_margin 0.05))
    (pad 4 smd roundrect (at -1.85 0.5 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 3 smd roundrect (at -1.85 0 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 171 "Net-(TL14-Pad1)") (solder_mask_margin 0.05))
    (pad 2 smd roundrect (at -1.85 -0.5 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 1 smd roundrect (at -1.85 -1 180) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
  )
  (module aps_radar_lib:LP5900_NGF_6 (layer F.Cu) (tedit 5E61C1DD)
    (at 135.5004 83.5452 90)
    (fp_text reference U23 (at -2.5062 0.7631 180) (layer F.SilkS))
    (fp_text value LP5900-TL3.3 (at 0 2.625 90) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at -1.1557 -0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3) (solder_mask_margin 0.05))
    (pad 2 smd roundrect (at -1.1557 0 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 3 smd roundrect (at -1.1557 0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 4 smd roundrect (at 1.1557 0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 /power/5V0_PGD) (solder_mask_margin 0.05))
    (pad 5 smd roundrect (at 1.1557 0 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 6 smd roundrect (at 1.1557 -0.649999 90) (size 0.6096 0.254) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V) (solder_mask_margin 0.05))
    (pad 7 smd rect (at 0 0 90) (size 0.762 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin -0.09))
  )
  (module aps_radar_lib:TPS82140SILR (layer F.Cu) (tedit 5E61CAF6)
    (at 102.62518 103.2048 90)
    (fp_text reference U24 (at -0.3556 -2.45364 90) (layer F.SilkS))
    (fp_text value TPS82140 (at -0.05 2.625 90) (layer F.SilkS) hide)
    (pad 9 smd roundrect (at 0 -0.525 90) (size 1.04 0.85) (layers F.Paste) (roundrect_rratio 0.1)
      (net 3 GND))
    (pad 9 smd roundrect (at 0 0.525 90) (size 1.04 0.85) (layers F.Paste) (roundrect_rratio 0.1)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.05 -0.974999 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 193 /power/POWER_SW) (solder_mask_margin 0.05))
    (pad 2 smd roundrect (at -1.05 -0.325001 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 180 /power/+12V0_IN_CONN) (solder_mask_margin 0.05))
    (pad 3 smd roundrect (at -1.05 0.325001 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 4 smd roundrect (at -1.05 0.974999 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.05))
    (pad 5 smd roundrect (at 1.05 0.974999 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.05))
    (pad 6 smd roundrect (at 1.05 0.325001 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 144 "Net-(R64-Pad2)") (solder_mask_margin 0.05))
    (pad 7 smd roundrect (at 1.05 -0.325001 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 142 "Net-(R61-Pad2)") (solder_mask_margin 0.05))
    (pad 8 smd roundrect (at 1.05 -0.974999 90) (size 0.599999 0.499999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 81 "Net-(C104-Pad1)") (solder_mask_margin 0.05))
    (pad 9 smd roundrect (at 0 0 90) (size 1.1 1.9) (layers F.Cu F.Mask) (roundrect_rratio 0.1)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 9 thru_hole circle (at 0 0 90) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu)
      (net 3 GND))
    (pad 9 thru_hole circle (at 0 -0.750001 90) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu)
      (net 3 GND))
    (pad 9 thru_hole circle (at 0 0.750001 90) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu)
      (net 3 GND))
  )
  (module aps_radar_lib:TPS7A4901_DGN_8 (layer F.Cu) (tedit 5E61C3F1)
    (at 117.6569 108.0181 270)
    (fp_text reference U25 (at 0.0635 2.8321 90) (layer F.SilkS))
    (fp_text value TPS7A49 (at 0.025 3.7 90) (layer F.SilkS) hide)
    (pad 9 thru_hole circle (at -0.55 -1.22 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 9 thru_hole circle (at 0.55 -1.22 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 9 thru_hole circle (at -0.55 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 9 thru_hole circle (at 0.55 0 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 9 thru_hole circle (at -0.55 1.22 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 9 thru_hole circle (at 0.55 1.22 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 3 GND))
    (pad 9 smd roundrect (at 0 0 270) (size 1.57 1.89) (layers F.Paste F.Mask) (roundrect_rratio 0.05)
      (net 3 GND))
    (pad 1 smd roundrect (at -2.213348 -0.974999 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 +10V) (solder_mask_margin 0.05))
    (pad 2 smd roundrect (at -2.213348 -0.325001 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(C110-Pad2)") (solder_mask_margin 0.05))
    (pad 3 smd roundrect (at -2.213348 0.325001 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 4 smd roundrect (at -2.213348 0.974999 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 5 smd roundrect (at 2.213348 0.974999 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 193 /power/POWER_SW) (solder_mask_margin 0.05))
    (pad 6 smd roundrect (at 2.213348 0.325001 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C105-Pad1)") (solder_mask_margin 0.05))
    (pad 7 smd roundrect (at 2.213348 -0.325001 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (solder_mask_margin 0.05))
    (pad 8 smd roundrect (at 2.213348 -0.974999 270) (size 1.327899 0.441) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 180 /power/+12V0_IN_CONN) (solder_mask_margin 0.05))
    (pad 9 smd roundrect (at 0 0 270) (size 2 3) (layers F.Cu) (roundrect_rratio 0.05)
      (net 3 GND))
  )
  (module aps_radar_lib:TPS7A9xDSKR (layer F.Cu) (tedit 5E61C826)
    (at 114.012 98.6709 270)
    (fp_text reference U27 (at -0.2921 -2.159 90) (layer F.SilkS))
    (fp_text value TPS7A90 (at -0.05 2.9 90) (layer F.SilkS) hide)
    (pad 11 smd roundrect (at 0 -0.5) (size 0.89 1.13) (layers F.Paste F.Mask) (roundrect_rratio 0.05)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 smd roundrect (at 0 0.5) (size 0.89 1.13) (layers F.Paste F.Mask) (roundrect_rratio 0.05)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at 0.35 0) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at 0 -0.75) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at -0.35 0) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at 0 0.75) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 smd roundrect (at 0 0 270) (size 1.2 2.000001) (layers F.Cu F.Mask) (roundrect_rratio 0.05)
      (net 3 GND))
    (pad 10 smd roundrect (at 1.15 -1.000003) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.07))
    (pad 9 smd roundrect (at 1.15 -0.500002) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.07))
    (pad 8 smd roundrect (at 1.15 -0.000003) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(C117-Pad1)") (solder_mask_margin 0.07))
    (pad 7 smd roundrect (at 1.15 0.499996) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 /power/5V5_PGD) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 1.15 0.999998) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at -1.15 0.999998) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 /power/5V25_PGD) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at -1.15 0.499996) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -1.15 -0.000003) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(C119-Pad2)") (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -1.15 -0.500002) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 +5V25) (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -1.15 -1.000003) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 +5V25) (solder_mask_margin 0.07))
  )
  (module aps_radar_lib:TPS7A9xDSKR (layer F.Cu) (tedit 5E61C826)
    (at 110.17914 110.19488 90)
    (fp_text reference U28 (at 0.61468 2.1336 90) (layer F.SilkS))
    (fp_text value TPS7A92 (at -0.05 2.9 90) (layer F.SilkS) hide)
    (pad 11 smd roundrect (at 0 -0.5 180) (size 0.89 1.13) (layers F.Paste F.Mask) (roundrect_rratio 0.05)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 smd roundrect (at 0 0.5 180) (size 0.89 1.13) (layers F.Paste F.Mask) (roundrect_rratio 0.05)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at 0.35 0 180) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at 0 -0.75 180) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at -0.35 0 180) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 thru_hole circle (at 0 0.75 180) (size 0.4 0.4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 11 smd roundrect (at 0 0 90) (size 1.2 2.000001) (layers F.Cu F.Mask) (roundrect_rratio 0.05)
      (net 3 GND))
    (pad 10 smd roundrect (at 1.15 -1.000003 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.07))
    (pad 9 smd roundrect (at 1.15 -0.500002 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.07))
    (pad 8 smd roundrect (at 1.15 -0.000003 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(C118-Pad1)") (solder_mask_margin 0.07))
    (pad 7 smd roundrect (at 1.15 0.499996 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 /power/5V5_PGD) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 1.15 0.999998 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at -1.15 0.999998 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 145 "Net-(R78-Pad2)") (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at -1.15 0.499996 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -1.15 -0.000003 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(C120-Pad2)") (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -1.15 -0.500002 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V) (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -1.15 -1.000003 180) (size 0.249999 0.599999) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V) (solder_mask_margin 0.07))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.0685 94.6014 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -2.3 0.045) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 151.7585 101.9564 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 2.195 0.05) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 197.10954 95.56682 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.09022 -0.02396) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 168.8585 75.4989 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0.2475 1.395 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C13-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /RX2_Q))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 191.34494 93.02942 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at -2.15 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.3035 94.6189 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 2.1225 -0.85) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C16-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RX2_I))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 164.6235 75.4814 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -0.09 -1.195 270) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 168.3135 82.8364 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 2.195 -0.215) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.13494 86.58942 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 3.02006 0.02286 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.94028 93.41168 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.63774 -0.09466 90) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 200.5736 93.41676 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.13868 -0.27432) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.553 107.599 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C83 (at -0.6096 -1.2319 90) (layer F.SilkS))
    (fp_text value 1.8nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C83-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.5403 110.8502 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C85 (at -0.0254 -1.2065 270) (layer F.SilkS))
    (fp_text value 0.82nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(C85-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.1344 113.0727)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C86 (at 0 -1.2065) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(C86-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 202.38716 93.2161 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.00762 -1.53924 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 182.59294 89.92514 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -3.20892 0.06056 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 122.8385 99.852 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C78 (at 2.2733 -0.0127 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C78-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.4689 107.1926 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C79 (at -0.0127 1.1938 90) (layer F.SilkS))
    (fp_text value 1.8nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 139.16816 99.52688 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C80 (at 0.08128 1.17094 90) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C80-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /transmitter/ATTEN_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.5035 101.8714 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C81 (at 0.955499 -1.415288 90) (layer F.SilkS))
    (fp_text value 330pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C81-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 128.6043 107.0021)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C82 (at -0.889 -1.1049) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C82-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.34808 89.39936 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.07772 -0.31242) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.35062 92.43974 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -2.08026 0.29972) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 194.64954 95.54682 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -2.07022 -0.04556) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.87494 94.54942 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -2.12 -0.25) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 139.17578 107.98254 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C74 (at 0.55626 1.24968 270) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(C74-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /transmitter/VCO_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.1298 106.5322 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C75 (at -0.1397 1.5748 90) (layer F.SilkS))
    (fp_text value 330pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(C75-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.2647 80.6623 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C77 (at -0.2286 -1.3716 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C77-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.3735 109.7714 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at -0.1 1.36 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 180 /power/+12V0_IN_CONN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 134.8527 80.0527 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C103 (at 0 1.4224 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 99.88198 100.15172 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C104 (at 2.23012 -0.889 180) (layer F.SilkS))
    (fp_text value 4.3nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C104-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.1395 112.51136)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C105 (at 2.96672 0.08636 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C105-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.9899 93.7306 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C119 (at -1.5621 1.4478) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(C119-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 +5V25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.30106 115.6254)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C120 (at -2.01676 1.41732) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(C120-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.8093 98.3661 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C121 (at 0.9779 -1.7145 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 90 +5V25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.55278 114.08616 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C122 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 107.6437 120.91356 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 12V0 (at 0.00216 1.8698 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 113.03074 120.91356 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 10V0 (at -0.02032 1.82372 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 118.7999 102.4936 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C110 (at 0.0508 1.2827) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(C110-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 +10V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.5634 101.9221 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C113 (at 0 -1.2192 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.1621 103.281 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C111 (at 2.8702 -0.0381 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 +10V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 106.94318 100.44636 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C112 (at 2.88036 -0.15748) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 85 /power/5V5_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.60866 107.2688 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C116 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 85 /power/5V5_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.15446 109.1992 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C114 (at 1.30556 -1.69672 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 +3V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 111.3069 98.9122 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C117 (at -1.1176 -1.4224 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(C117-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 109.8083 106.66936 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C118 (at -0.64516 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(C118-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.0214 102.3793 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C115 (at -0.86106 -1.80594) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 85 /power/5V5_OUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 132.808 83.596 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C108 (at 2.50444 -0.26162 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x11.9 (layer F.Cu) (tedit 5BCA39D0)
    (at 92.9935 103.7114 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic E12, 8.0x11.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C106 (at -5.19176 3.429 90) (layer F.SilkS))
    (fp_text value 68uF (at 0 5.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 3.475 0 180) (size 4.15 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.131579)
      (net 3 GND))
    (pad 1 smd roundrect (at -3.475 0 180) (size 4.15 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.131579)
      (net 180 /power/+12V0_IN_CONN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_8x11.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x11.9 (layer F.Cu) (tedit 5BCA39D0)
    (at 92.9989 94.1043 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic E12, 8.0x11.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C107 (at -3.9046 5.2229 180) (layer F.SilkS))
    (fp_text value DNP (at 0 5.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 3.475 0 180) (size 4.15 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.131579)
      (net 3 GND))
    (pad 1 smd roundrect (at -3.475 0 180) (size 4.15 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.131579)
      (net 180 /power/+12V0_IN_CONN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_8x11.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 118.26126 120.91356 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 5V5 (at -0.00984 1.80848 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 204.49536 89.87346)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 1.2pF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /receiver_2/ANT_IN))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 128.5916 110.4184)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C88 (at 1.34874 1.36652) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(C86-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.5474 88.9554 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C99 (at 0.1651 -0.8382 180) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(C99-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(C99-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 101.43138 107.29928 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0.01524 1.92024 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 180 /power/+12V0_IN_CONN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.8616 90.5556 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C98 (at -0.1651 -1.0287) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(C98-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /transmitter/LMX_FIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.0897 86.1106 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C93 (at 0.4445 -0.9271 270) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(C93-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(C93-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.4514 87.1647 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C94 (at 0.8128 1.0414) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C94-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C94-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 196.66244 92.26942)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at -0.1475 -1.17 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 133.74366 120.88356 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D6 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 0.00216 1.74984 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 138.77602 120.91356 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D7 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 3V0 (at -0.00784 1.75748 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 128.7059 120.92356 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D5 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 5V0 (at 0.01216 1.7476 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_Transition (layer F.Cu) (tedit 5E62ACF9)
    (at 216.07824 103.17178 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (zone_connect 2)
    (attr smd)
    (fp_text reference J7 (at 6.23474 4.37038) (layer F.SilkS) hide)
    (fp_text value Rx3 (at 6.97474 3.15038) (layer F.SilkS))
    (fp_text user "See Jason for proper keeoput" (at -0.05 9.05) (layer Cmts.User) hide)
    (fp_text user %R (at 2.775 6.975) (layer F.Fab))
    (pad 2 thru_hole rect (at 7.17225 3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 7.17225 0 180) (size 1.1555 1) (layers F.Mask)
      (net 3 GND) (zone_connect 1))
    (pad ~ smd rect (at 3.29725 0 180) (size 6.5945 1.77666) (layers F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole rect (at 7.17225 -3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 -3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 -4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 -2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers F.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 1 smd rect (at 7.5 0 180) (size 0.5 0.35) (layers F.Cu F.Mask)
      (net 15 /receiver_3/ANT_IN) (zone_connect 1))
    (pad ~ smd rect (at 6.5 0 180) (size 1.5 0.35) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad ~ smd rect (at 5.5 0 180) (size 0.5 0.35) (layers F.Cu)
      (zone_connect 1))
    (pad ~ smd rect (at 2.625 0 180) (size 5.25 1) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole circle (at 5.995 4.355 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 5.995 -4.405 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.42) (layers B.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers F.Cu F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_Transition (layer F.Cu) (tedit 5E62ACF9)
    (at 216.07824 89.87234 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (zone_connect 2)
    (attr smd)
    (fp_text reference J6 (at 6.23474 4.38094) (layer F.SilkS) hide)
    (fp_text value Rx2 (at 6.97474 3.10094) (layer F.SilkS))
    (fp_text user "See Jason for proper keeoput" (at -0.05 9.05) (layer Cmts.User) hide)
    (fp_text user %R (at 2.775 6.975) (layer F.Fab))
    (pad 2 thru_hole rect (at 7.17225 3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 7.17225 0 180) (size 1.1555 1) (layers F.Mask)
      (net 3 GND) (zone_connect 1))
    (pad ~ smd rect (at 3.29725 0 180) (size 6.5945 1.77666) (layers F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole rect (at 7.17225 -3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 -3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 -4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 -2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers F.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 1 smd rect (at 7.5 0 180) (size 0.5 0.35) (layers F.Cu F.Mask)
      (net 1 /receiver_2/ANT_IN) (zone_connect 1))
    (pad ~ smd rect (at 6.5 0 180) (size 1.5 0.35) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad ~ smd rect (at 5.5 0 180) (size 0.5 0.35) (layers F.Cu)
      (zone_connect 1))
    (pad ~ smd rect (at 2.625 0 180) (size 5.25 1) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole circle (at 5.995 4.355 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 5.995 -4.405 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.42) (layers B.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers F.Cu F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_Transition (layer F.Cu) (tedit 5E62ACF9)
    (at 139.1785 67.08915 270)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (zone_connect 2)
    (attr smd)
    (fp_text reference J4 (at 1.30048 -6.94436 90) (layer F.SilkS) hide)
    (fp_text value Tx (at 6.99225 3.085 90) (layer F.SilkS))
    (fp_text user "See Jason for proper keeoput" (at -0.05 9.05 90) (layer Cmts.User) hide)
    (fp_text user %R (at 2.775 6.975 90) (layer F.Fab))
    (pad 2 thru_hole rect (at 7.17225 3 270) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 7.17225 0 270) (size 1.1555 1) (layers F.Mask)
      (net 3 GND) (zone_connect 1))
    (pad ~ smd rect (at 3.29725 0 270) (size 6.5945 1.77666) (layers F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole rect (at 7.17225 -3 270) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 3.679306 270) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 -3.679306 270) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 270) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 -4.355 270) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 -2.38833 270) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 270) (size 5.08 2.42) (layers F.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 2.38833 270) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 1 smd rect (at 7.5 0 270) (size 0.5 0.35) (layers F.Cu F.Mask)
      (net 103 /transmitter/TX_OUT) (zone_connect 1))
    (pad ~ smd rect (at 6.5 0 270) (size 1.5 0.35) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad ~ smd rect (at 5.5 0 270) (size 0.5 0.35) (layers F.Cu)
      (zone_connect 1))
    (pad ~ smd rect (at 2.625 0 270) (size 5.25 1) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole circle (at 5.995 4.355 270) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 5.995 -4.405 270) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 270) (size 7.75 2.42) (layers B.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 270) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 270) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 270) (size 5.08 2.42) (layers F.Cu F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 123.52382 120.95356 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 5V25 (at 0 1.76276 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aps_radar_lib:SMA_Molex_Transition (layer F.Cu) (tedit 5E62ACF9)
    (at 216.07824 76.5729 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (zone_connect 2)
    (attr smd)
    (fp_text reference J5 (at 6.20474 -4.5185) (layer F.SilkS) hide)
    (fp_text value Rx1 (at 6.97474 -3.0785) (layer F.SilkS))
    (fp_text user "See Jason for proper keeoput" (at -0.05 9.05) (layer Cmts.User) hide)
    (fp_text user %R (at 2.775 6.975) (layer F.Fab))
    (pad 2 thru_hole rect (at 7.17225 3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 7.17225 0 180) (size 1.1555 1) (layers F.Mask)
      (net 3 GND) (zone_connect 1))
    (pad ~ smd rect (at 3.29725 0 180) (size 6.5945 1.77666) (layers F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole rect (at 7.17225 -3 180) (size 1.1555 5) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 3.875 -3.679306 180) (size 7.75 4) (drill 0.254) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 -4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 -2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 4.355 180) (size 5.08 2.42) (layers F.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.471 2.38833 180) (size 6.942 3) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 1 smd rect (at 7.5 0 180) (size 0.5 0.35) (layers F.Cu F.Mask)
      (net 41 /receiver_1/ANT_IN) (zone_connect 1))
    (pad ~ smd rect (at 6.5 0 180) (size 1.5 0.35) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad ~ smd rect (at 5.5 0 180) (size 0.5 0.35) (layers F.Cu)
      (zone_connect 1))
    (pad ~ smd rect (at 2.625 0 180) (size 5.25 1) (layers F.Cu F.Mask)
      (zone_connect 1))
    (pad 2 thru_hole circle (at 5.995 4.355 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 5.995 -4.405 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.42) (layers B.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers B.Cu B.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 3.875 4.355 180) (size 7.75 2.525) (layers F.Cu)
      (net 3 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.54 -4.405 180) (size 5.08 2.42) (layers F.Cu F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 166.4335 82.6314 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB3 (at -2.39 0.015) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C15-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.8785 101.7514 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB4 (at 0.045 -1.28 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C18-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 196.66244 105.56676)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB5 (at -0.1475 -1.17 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C21-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 193.62494 105.56676 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB6 (at 0.05 1.18 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C25-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.30672 101.763 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB7 (at -2.4184 -0.08322) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C33-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.88372 114.507 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB8 (at 0.045 -1.28 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C36-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 196.66244 118.87068)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB9 (at -0.1475 -1.17 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C39-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 193.62494 118.87068 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB10 (at 0.05 1.18 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C43-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.35172 114.50692 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB11 (at -2.40448 0.21178 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C51-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 166.8835 113.5664 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB12 (at -2.21 -0.625) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C54-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 196.661 78.9714)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB13 (at -0.1475 -1.17 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(C57-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 193.6235 78.9714 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB14 (at 0.05 1.18 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C61-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.08028 82.61264 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB15 (at -2.42376 0.37822 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(C69-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.69228 82.59664 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB16 (at 0.045 -1.28 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(C72-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.2647 77.6397 270)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB17 (at -0.0508 -1.3843 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C77-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.0615 104.4113 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB18 (at 2.9591 0.0635 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 +10V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C82-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.6292 96.1309 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB19 (at 2.9845 -0.4445) (layer F.SilkS))
    (fp_text value "120 ohm" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 +5V25))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /transmitter/LMX_VCP))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.4011 108.7293)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB20 (at 1.79324 0.02794 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 +3V0))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(C86-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.1113 95.2546 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB21 (at 2.9845 0.0127 180) (layer F.SilkS))
    (fp_text value "120 ohm" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.1113 93.7306 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB22 (at 2.9845 -0.0762) (layer F.SilkS))
    (fp_text value "120 ohm" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.2774 83.8246 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB23 (at -0.8128 -1.0795 90) (layer F.SilkS))
    (fp_text value "120 ohm" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.8141 83.8119 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB24 (at 1.8796 0.1524 180) (layer F.SilkS))
    (fp_text value "120 ohm" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.548747 86.823753 45)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB25 (at -0.235392 -1.157958 45) (layer F.SilkS))
    (fp_text value "120 ohm" (at 0 1.43 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 45) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.066 96.3014)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB26 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C100-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 89.38162 78.5614 270)
    (descr "Terminal Block TE 282834-4, 4 pins, pitch 2.54mm, size 10.620000000000001x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-4 pitch 2.54mm size 10.620000000000001x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J1 (at -2.72 1.49812 180) (layer F.SilkS))
    (fp_text value TRIG_MUX_OUT (at 3.81 4.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 2 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 99 /LMX_MOD))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 100 /LMX_MUXOUT))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 101 /LMX_TRIG2))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 102 /LMX_TRIG1))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 89.3335 111.4714 270)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J3 (at 5.16128 2.77876 180) (layer F.SilkS))
    (fp_text value POWER_IN (at 1.27 4.37 90) (layer F.SilkS) hide)
    (fp_text user %R (at 1.27 2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 180 /power/+12V0_IN_CONN))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 193.62494 92.26942 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB2 (at 0.05 1.18 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.92592 83.4944 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 1dB (at -0.0635 -2.8643 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 /~ATTEN_1DB))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.92592 79.561634 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 2dB (at -0.0635 -2.8643 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 /~ATTEN_2DB))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.92592 75.628868 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 4dB (at -0.0635 -2.8643 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 /~ATTEN_4DB))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.92592 71.6961 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 8dB (at -0.0635 -2.8643 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 /~ATTEN_8DB))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.92592 89.3364 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ~OSC_STBY (at -2.8448 1.1684) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(JP5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.2559 116.89644 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.032 -0.01524 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 /~ATTEN_1DB))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 140.913674 116.89644 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.032 -0.0254 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 /~ATTEN_2DB))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.571447 116.89644 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.032 0.04572) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 115 /~ATTEN_4DB))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 144.22922 116.89644 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.032 -0.01524 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 116 /~ATTEN_8DB))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 201.20494 86.57942 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -3.06324 -0.01778 180) (layer F.SilkS))
    (fp_text value 825 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 170.4127 75.4934 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.285 -1.315 90) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 /receiver_2/IF2_RAW))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.2285 75.4714 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0.735 1.325 90) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C13-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 170.1935 79.6864 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.3 90) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 153.846 94.6189 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -2.1225 0.2925) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 /receiver_2/IF1_RAW))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.6735 94.5914 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.14 -0.765) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C16-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.4335 102.6514 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 121 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 201.20494 99.87676 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -3.06324 -0.01778 180) (layer F.SilkS))
    (fp_text value 825 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C20-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.27422 94.6305 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -2.1225 0.2925) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 /receiver_3/IF2_RAW))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C31-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.10172 94.603 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 2.14 -0.765) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C31-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(C32-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.86172 102.663 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -2.53678 0.3316) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 153.85122 107.3745 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -2.1225 0.2925) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 /receiver_3/IF1_RAW))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C34-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.67872 107.347 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 2.14 -0.765) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C34-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C35-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.43872 115.407 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 201.20494 113.18068 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -3.06324 -0.01778 180) (layer F.SilkS))
    (fp_text value 825 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(C38-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.31922 107.37442 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -1.94802 -0.32428) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 /receiver_4/IF2_RAW))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C49-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.14672 107.34692 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 2.04552 0.18678) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C49-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C50-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.90672 115.40692 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(R22-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.6785 106.4064 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 2.0078 -0.3044) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C52-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C53-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 201.2035 73.2814 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at -1.35 -1.33 180) (layer F.SilkS))
    (fp_text value 825 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C56-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.04778 75.48014 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at -2.1225 0.2925) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 /receiver_1/IF2_RAW))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C67-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 157.87528 75.45264 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 2.14 -0.765) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C67-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(C68-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 162.63528 83.51264 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 "Net-(R29-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 153.65978 75.46414 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at -2.1225 0.2925) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 /receiver_1/IF1_RAW))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(C70-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.48728 75.43664 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 2.14 -0.765) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(C70-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C71-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.24728 83.49664 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 499 (at 0 1.430001) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(R32-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 72.15584 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at 0.0762 1.4732) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /LMX_TRIG1))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 73.77128)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at 0 1.40716) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 "Net-(J9-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 77.6524 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at -0.01524 1.40208) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /LMX_MUXOUT))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 "Net-(J9-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.2647 93.6036 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at 0.0254 1.4478 90) (layer F.SilkS))
    (fp_text value 1.2k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(C76-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 79.23228)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at -0.02032 1.38176) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 "Net-(J9-Pad3)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 82.87972 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R38 (at 0.02032 1.20396) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 /transmitter/LMX_CE))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(J9-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 84.44436)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R39 (at 0.01016 1.36144) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(J9-Pad5)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 88.00544 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R41 (at -0.01016 1.24968) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /LMX_MOD))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(J9-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.90762 89.57516)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R42 (at 0 1.34112) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(J9-Pad7)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 108.04554 94.45704 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R43 (at 0.47752 -1.22936 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(J9-Pad9)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.8037 102.5063 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R44 (at -0.0127 -1.2446 90) (layer F.SilkS))
    (fp_text value 1.24k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C78-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 "Net-(R44-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 88.0156)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R45 (at 0.0254 -1.25476) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /LMX_TRIG2))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(J9-Pad10)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 89.58024 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R46 (at 0 -1.36652) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(J9-Pad10)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.1151 107.599 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R47 (at 1.6256 0.0127) (layer F.SilkS))
    (fp_text value 8.2 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 "Net-(R44-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C83-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 84.43928 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R48 (at -0.01016 -1.31572) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(J9-Pad8)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 82.87464)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R49 (at 0 -1.27508) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 /transmitter/LMX_CLK))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(J9-Pad8)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.1151 110.84258 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R50 (at -2.34442 -1.8796 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C83-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(C85-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 79.2526 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R51 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 "Net-(J9-Pad4)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 77.64732)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R52 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 /transmitter/LMX_DATA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 "Net-(J9-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 73.79668 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R53 (at 0.01016 -1.37668) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 "Net-(J9-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.03434 72.1406)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R54 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 /transmitter/LMX_LE))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 "Net-(J9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.8291 84.0278 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R58 (at 0 1.2827 90) (layer F.SilkS))
    (fp_text value 51 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C94-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.0747 88.7014 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R59 (at -0.3288 1.22 180) (layer F.SilkS))
    (fp_text value 51 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(C99-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.64542 93.02194 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R60 (at 1.8542 -1.41478 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 141 "Net-(R60-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 101.79714 99.96884 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R61 (at -2.0066 0.2794 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 142 "Net-(R61-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 /power/5V5_PGD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.7999 104.0176 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R62 (at -1.2192 -1.8923 90) (layer F.SilkS))
    (fp_text value 86.6k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(C110-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 +10V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.2726 103.2556 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R63 (at -2.6289 0.0381 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(C110-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 104.12388 100.72068 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R64 (at -0.76698 -1.93548 90) (layer F.SilkS))
    (fp_text value 590k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 "Net-(R64-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 104.12378 99.15604)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R65 (at -0.00508 -1.18872) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 "Net-(R64-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.52358 96.59064 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R66 (at 2.73304 -0.0508) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 /power/5V5_PGD))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 105.57106 120.93356 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R67 (at -2.22216 -0.13244 180) (layer F.SilkS))
    (fp_text value 649 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 180 /power/+12V0_IN_CONN))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 111.09018 120.93356 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R68 (at 2.19216 -0.00668 180) (layer F.SilkS))
    (fp_text value 499 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 +10V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.28514 120.93356 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R69 (at 2.27216 0.00836 180) (layer F.SilkS))
    (fp_text value 274 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /power/5V5_OUT))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.6493 120.97356 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R70 (at -2.33216 -0.0442 180) (layer F.SilkS))
    (fp_text value 261 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(D4-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 +5V25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.7835 121.1714 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R71 (at 1.79 -0.04 180) (layer F.SilkS))
    (fp_text value 249 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.83866 120.90356 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R72 (at 1.97216 -0.01516 180) (layer F.SilkS))
    (fp_text value 165 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Revision 1.0" (at 191.2535 121.5914) (layer B.SilkS))
  (gr_text Group (at 177.1435 92.8014) (layer B.SilkS))
  (gr_text "\nMichigan State University" (at 192.6835 97.6314) (layer B.SilkS))
  (gr_text DELTA (at 193.0335 92.7014) (layer B.SilkS))
  (gr_text "Receiver 4" (at 185.6835 123.1614) (layer F.SilkS))
  (gr_text "Receiver 3" (at 185.6835 109.9614) (layer F.SilkS))
  (gr_text "Receiver 2" (at 185.6835 96.7414) (layer F.SilkS))
  (gr_text "Receiver 1" (at 185.6835 83.4114) (layer F.SilkS))
  (gr_text T1-T2-MUX-MOD (at 93.9435 82.4014 270) (layer F.SilkS))
  (gr_line (start 216.0835 69.5914) (end 216.0835 123.4714) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 85.3135 69.5914) (end 85.3135 123.4714) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 87.8135 67.0914) (end 213.5835 67.0914) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 87.8135 125.9714) (end 213.5835 125.9714) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 213.5835 69.5914) (end 216.0835 69.5914) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 213.5835 123.4714) (end 213.5835 125.9714) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 87.8135 123.4714) (end 85.3135 123.4714) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 87.8135 69.5914) (end 87.8135 67.0914) (angle -90) (layer Edge.Cuts) (width 0.01))
  (gr_text "PA ENABLE" (at 126.6535 75.1714 180) (layer F.SilkS))
  (gr_text "SYSTEM POWER" (at 99.0235 117.4114) (layer F.SilkS))
  (gr_text "OFF   ON" (at 99.0035 119.7214) (layer F.SilkS))
  (gr_text "ON   OFF" (at 126.6535 73.2414 180) (layer F.SilkS))
  (gr_text +12V (at 96.55554 112.7414 270) (layer F.SilkS))
  (gr_text "- +" (at 93.90886 112.7414 270) (layer F.SilkS))
  (gr_text "Tx Attenuation" (at 95.93482 77.633351 270) (layer F.SilkS))
  (zone (net 61) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 60)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.9863 106.8497) (xy 136.9863 105.7575) (xy 138.0785 104.6653) (xy 138.7897 104.6653) (xy 138.7897 105.5289)
        (xy 138.4722 105.5289) (xy 137.9896 106.0115) (xy 137.9896 106.8497)
      )
    )
  )
  (zone (net 75) (net_name "Net-(C100-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 65)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.6909 96.9183) (xy 135.6909 94.0227) (xy 135.2718 93.6036) (xy 135.2718 92.7908) (xy 136.3132 92.7908)
        (xy 136.3132 93.54645) (xy 136.5545 93.78775) (xy 136.5545 94.5942) (xy 136.8466 94.8863) (xy 137.6848 94.8863)
        (xy 137.6848 97.4414) (xy 136.8985 97.4414) (xy 136.5545 96.9183) (xy 136.5418 96.9183)
      )
    )
  )
  (zone (net 65) (net_name "Net-(C82-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 35)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.6076 104.70975) (xy 129.6076 105.73845) (xy 128.2868 107.7387) (xy 128.2233 107.7387) (xy 127.22 107.7387)
        (xy 126.5596 105.9226) (xy 126.5596 103.9922) (xy 127.0168 103.9922) (xy 127.0422 104.7161) (xy 127.2073 104.7161)
        (xy 127.8677 104.7161) (xy 127.8804 104.7161)
      )
    )
  )
  (zone (net 69) (net_name "Net-(C86-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 30)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.9914 114.8761) (xy 126.9914 114.01885) (xy 126.8517 113.87915) (xy 126.8644 108.234) (xy 127.1819 108.0689)
        (xy 128.1598 108.0689) (xy 128.3503 108.2467) (xy 128.3503 111.6122) (xy 127.8931 112.0694) (xy 127.8931 113.3648)
        (xy 127.2327 114.0252) (xy 127.2327 114.8761)
      )
    )
  )
  (zone (net 59) (net_name "Net-(C77-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 75)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.2454 79.3161) (xy 128.1598 79.3161) (xy 128.7186 78.7827) (xy 128.7186 77.9064) (xy 129.8489 77.9064)
        (xy 129.8489 80.3956) (xy 127.2454 80.3956)
      )
    )
  )
  (zone (net 57) (net_name "Net-(C75-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.047 104.7161) (xy 140.4661 104.7161) (xy 140.4661 103.8144) (xy 141.3551 103.8144) (xy 142.6505 105.1098)
        (xy 142.6505 106.2274) (xy 141.1773 106.2274) (xy 140.428 105.4781) (xy 140.047 105.4781)
      )
    )
  )
  (zone (net 64) (net_name "Net-(C81-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.4788 103.0397) (xy 141.2789 103.0397) (xy 141.7735 103.3314) (xy 143.0235 103.3414) (xy 143.0335 102.1914)
        (xy 141.4435 102.1714) (xy 140.809 102.7984) (xy 140.4788 102.7984)
      )
    )
  )
  (zone (net 61) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 70)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.4999 86.2884) (xy 132.1095 86.771) (xy 135.0178 86.8218) (xy 135.0051 85.0311) (xy 135.0051 84.3707)
        (xy 133.9891 84.358) (xy 132.00282 83.12356) (xy 131.96218 80.56324) (xy 133.37442 79.94856) (xy 133.37442 78.61252)
        (xy 130.8776 76.2681) (xy 128.6297 76.2681) (xy 128.6297 77.4365) (xy 130.0267 77.4365) (xy 130.0267 82.2371)
        (xy 128.7059 82.2371) (xy 128.7059 83.7484) (xy 131.1316 83.7484) (xy 131.538 84.1548) (xy 131.538 85.0057)
        (xy 131.4491 85.3867) (xy 131.4491 85.7042)
      )
    )
  )
  (zone (net 84) (net_name +10V) (layer F.Cu) (hatch edge 0.508)
    (priority 25)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.3935 106.4814) (xy 118.3935 105.0209) (xy 119.1174 104.297) (xy 119.1174 101.9856) (xy 121.6828 101.9856)
        (xy 121.6828 103.027) (xy 121.1621 103.0397) (xy 120.1715 103.96045) (xy 120.1715 105.3511) (xy 119.1047 106.4179)
        (xy 119.1047 106.4814)
      )
    )
  )
  (zone (net 180) (net_name /power/+12V0_IN_CONN) (layer F.Cu) (hatch edge 0.508)
    (priority 40)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.3935 109.5929) (xy 118.3935 110.9518) (xy 118.9142 111.4725) (xy 120.9635 111.446464) (xy 120.9635 110.096336)
        (xy 120.0318 109.5929)
      )
    )
  )
  (zone (net 90) (net_name +5V25) (layer F.Cu) (hatch edge 0.508)
    (priority 45)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3422 97.8454) (xy 114.3422 96.5373) (xy 115.0153 95.8642) (xy 115.0153 92.8924) (xy 116.17354 92.88224)
        (xy 116.52406 92.88224) (xy 116.9457 92.88224) (xy 119.5492 94.6196) (xy 119.5492 96.0547) (xy 122.6988 96.0547)
        (xy 123.3719 95.3816) (xy 124.6292 95.3816) (xy 124.6292 96.8675) (xy 121.378 96.8675) (xy 120.4001 97.8454)
      )
    )
  )
  (zone (net 85) (net_name /power/5V5_OUT) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.1804 103.3572) (xy 115.17278 103.3572) (xy 115.17278 106.2782) (xy 111.6498 109.42272) (xy 110.99448 109.41256)
        (xy 110.99194 108.52356) (xy 112.8055 107.1799) (xy 112.8055 104.97772) (xy 105.566516 104.981539) (xy 105.5665 107.2434)
        (xy 106.66378 107.97492) (xy 108.7161 107.97492) (xy 109.31046 108.44482) (xy 109.86926 108.43974) (xy 109.86926 109.36176)
        (xy 106.59266 109.36176) (xy 106.59266 109.3389) (xy 105.5665 109.3389) (xy 103.598 108.0689) (xy 103.59546 104.9828)
        (xy 103.29066 104.68308) (xy 103.29066 101.76716) (xy 104.23046 100.82736) (xy 104.23046 100.16188) (xy 108.16746 100.16188)
        (xy 108.16746 102.33104) (xy 109.33586 103.49944) (xy 112.4499 103.49944) (xy 113.7326 102.21674) (xy 113.7326 101.1093)
        (xy 114.3422 100.4997) (xy 114.3676 99.5472) (xy 115.1804 99.5472)
      )
    )
  )
  (zone (net 80) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.776 116.9189) (xy 104.785904 114.895614) (xy 104.7835 113.4439) (xy 108.8885 113.4514) (xy 108.891484 111.344035)
        (xy 109.125164 111.110355) (xy 109.968444 111.110355) (xy 109.968444 111.755515) (xy 110.186884 111.973955) (xy 110.21399 116.918605)
      )
    )
  )
  (zone (net 180) (net_name /power/+12V0_IN_CONN) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.50174 106.59316) (xy 102.60486 106.59316) (xy 102.60486 103.8906) (xy 101.37042 103.8906) (xy 100.50174 104.75928)
      )
    )
  )
  (zone (net 180) (net_name /power/+12V0_IN_CONN) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.125132 112.763557) (xy 90.6735 112.739243) (xy 92.75474 109.47352) (xy 92.769531 91.889003) (xy 96.74 91.8764)
        (xy 98.6935 91.8764) (xy 98.89646 101.8586) (xy 100.92846 103.8906) (xy 102.5185 103.88425) (xy 102.5185 104.63355)
        (xy 102.328 105.2114) (xy 102.328 106.6084) (xy 100.55 106.6084) (xy 100.2833 106.8878) (xy 100.2833 109.75292)
        (xy 101.23834 110.70796) (xy 102.52866 110.70796) (xy 104.41334 112.59264) (xy 104.40801 120.0414) (xy 104.9635 120.7814)
        (xy 106.519341 120.7964) (xy 106.503399 122.7514) (xy 100.523602 122.751401) (xy 100.5335 121.2314) (xy 100.5335 120.9114)
        (xy 100.537019 120.637794) (xy 95.949981 120.645006) (xy 90.6935 115.244734) (xy 88.110508 115.258066)
      )
    )
  )
  (zone (net 31) (net_name "Net-(C39-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.91494 118.16455) (xy 196.91494 120.0958) (xy 196.26494 120.8324) (xy 196.254494 121.741803) (xy 198.063307 121.751797)
        (xy 198.08494 120.8324) (xy 198.5813 120.1212) (xy 199.57792 119.75894) (xy 199.57792 118.6896) (xy 199.06484 118.17652)
        (xy 199.06484 117.2799) (xy 198.83116 117.2799) (xy 197.92946 118.1816)
      )
    )
  )
  (zone (net 31) (net_name "Net-(C39-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.8243 117.2672) (xy 199.8243 119.68274) (xy 203.10852 119.68274) (xy 203.10852 118.36702) (xy 200.38564 118.36702)
        (xy 200.09608 118.07746) (xy 200.09608 117.26974)
      )
    )
  )
  (zone (net 32) (net_name "Net-(C43-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.28102 117.60248) (xy 185.56982 117.60248) (xy 184.8535 118.73532) (xy 183.8735 118.73532) (xy 183.387932 117.99532)
        (xy 181.879068 117.99532) (xy 181.864846 116.87532) (xy 182.9635 116.87532) (xy 183.409663 116.23532) (xy 185.1835 116.23532)
        (xy 185.3735 116.34532) (xy 185.37678 117.06532) (xy 185.5495 117.37134) (xy 186.28102 117.37134)
      )
    )
  )
  (zone (net 32) (net_name "Net-(C43-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.57494 118.08068) (xy 189.57494 117.86068) (xy 190.65494 117.86068) (xy 190.85494 118.08068) (xy 193.815597 118.095681)
        (xy 193.814283 119.245679) (xy 194.4411 120.5784) (xy 195.394946 120.583698) (xy 195.376665 121.7722) (xy 194.1363 121.7722)
        (xy 193.334082 121.1147) (xy 192.315996 120.995798) (xy 192.284834 119.441463) (xy 191.048233 119.45068) (xy 190.16494 118.08068)
      )
    )
  )
  (zone (net 44) (net_name "Net-(C57-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.82286 77.36792) (xy 199.82286 79.78346) (xy 203.10708 79.78346) (xy 203.10708 78.46774) (xy 200.3842 78.46774)
        (xy 200.09464 78.17818) (xy 200.09464 77.37046)
      )
    )
  )
  (zone (net 43) (net_name "Net-(C56-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.82972 75.27496) (xy 199.04816 75.27242) (xy 199.04816 74.19546) (xy 199.5635 73.8214) (xy 200.8735 73.8214)
        (xy 200.863527 72.754889) (xy 198.436036 72.7414) (xy 198.43602 73.87288) (xy 198.5935 74.032845) (xy 198.5935 74.90412)
      )
    )
  )
  (zone (net 45) (net_name "Net-(C61-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.27958 77.7032) (xy 185.56838 77.7032) (xy 184.85206 78.83604) (xy 183.87206 78.83604) (xy 183.386492 78.09604)
        (xy 181.877628 78.09604) (xy 181.863406 76.97604) (xy 182.96206 76.97604) (xy 183.408223 76.33604) (xy 185.18206 76.33604)
        (xy 185.37206 76.44604) (xy 185.37534 77.16604) (xy 185.54806 77.47206) (xy 186.27958 77.47206)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.8243 90.66594) (xy 199.8243 93.08148) (xy 203.10852 93.08148) (xy 203.10852 91.76576) (xy 200.38564 91.76576)
        (xy 200.09608 91.4762) (xy 200.09608 90.66848)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.83116 88.57298) (xy 199.0496 88.57044) (xy 199.0496 87.49348) (xy 199.56494 87.11942) (xy 200.87494 87.11942)
        (xy 200.864967 86.052909) (xy 198.437476 86.03942) (xy 198.43746 87.1709) (xy 198.59494 87.330865) (xy 198.59494 88.20214)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C10-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.28102 91.00122) (xy 185.56982 91.00122) (xy 184.8535 92.13406) (xy 183.8735 92.13406) (xy 183.387932 91.39406)
        (xy 181.879068 91.39406) (xy 181.864846 90.27406) (xy 182.9635 90.27406) (xy 183.409663 89.63406) (xy 185.1835 89.63406)
        (xy 185.3735 89.74406) (xy 185.37678 90.46406) (xy 185.5495 90.77008) (xy 186.28102 90.77008)
      )
    )
  )
  (zone (net 18) (net_name "Net-(C21-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.8243 103.96328) (xy 199.8243 106.37882) (xy 203.10852 106.37882) (xy 203.10852 105.0631) (xy 200.38564 105.0631)
        (xy 200.09608 104.77354) (xy 200.09608 103.96582)
      )
    )
  )
  (zone (net 17) (net_name "Net-(C20-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.83116 101.87032) (xy 199.0496 101.86778) (xy 199.0496 100.79082) (xy 199.56494 100.41676) (xy 200.87494 100.41676)
        (xy 200.864967 99.350249) (xy 198.437476 99.33676) (xy 198.43746 100.46824) (xy 198.59494 100.628205) (xy 198.59494 101.49948)
      )
    )
  )
  (zone (net 19) (net_name "Net-(C25-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.28102 104.29856) (xy 185.56982 104.29856) (xy 184.8535 105.4314) (xy 183.8735 105.4314) (xy 183.387932 104.6914)
        (xy 181.879068 104.6914) (xy 181.864846 103.5714) (xy 182.9635 103.5714) (xy 183.409663 102.9314) (xy 185.1835 102.9314)
        (xy 185.3735 103.0414) (xy 185.37678 103.7614) (xy 185.5495 104.06742) (xy 186.28102 104.06742)
      )
    )
  )
  (zone (net 40) (net_name "Net-(C54-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.6235 113.4364) (xy 166.3235 113.4364) (xy 166.3235 112.0364) (xy 167.7335 112.0364) (xy 168.1935 111.5764)
        (xy 168.1935 110.4614) (xy 169.4485 110.4614) (xy 169.6235 110.6364)
      )
    )
  )
  (zone (net 53) (net_name "Net-(C72-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.43228 82.46664) (xy 149.13228 82.46664) (xy 149.13228 81.06664) (xy 150.54228 81.06664) (xy 151.00228 80.60664)
        (xy 151.00228 79.49164) (xy 152.25728 79.49164) (xy 152.43228 79.66664)
      )
    )
  )
  (zone (net 49) (net_name "Net-(C69-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.82028 82.48264) (xy 157.52028 82.48264) (xy 157.52028 81.08264) (xy 158.93028 81.08264) (xy 159.39028 80.62264)
        (xy 159.39028 79.50764) (xy 160.64528 79.50764) (xy 160.82028 79.68264)
      )
    )
  )
  (zone (net 14) (net_name "Net-(C18-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.6185 101.6214) (xy 149.3185 101.6214) (xy 149.3185 100.2214) (xy 150.7285 100.2214) (xy 151.1885 99.7614)
        (xy 151.1885 98.6464) (xy 152.4435 98.6464) (xy 152.6185 98.8214)
      )
    )
  )
  (zone (net 10) (net_name "Net-(C15-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.1735 82.5014) (xy 165.8735 82.5014) (xy 165.8735 81.1014) (xy 167.2835 81.1014) (xy 167.7435 80.6414)
        (xy 167.7435 79.5264) (xy 168.9985 79.5264) (xy 169.1735 79.7014)
      )
    )
  )
  (zone (net 27) (net_name "Net-(C36-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.62372 114.377) (xy 149.32372 114.377) (xy 149.32372 112.977) (xy 150.73372 112.977) (xy 151.19372 112.517)
        (xy 151.19372 111.402) (xy 152.44872 111.402) (xy 152.62372 111.577)
      )
    )
  )
  (zone (net 23) (net_name "Net-(C33-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.04672 101.633) (xy 157.74672 101.633) (xy 157.74672 100.233) (xy 159.15672 100.233) (xy 159.61672 99.773)
        (xy 159.61672 98.658) (xy 160.87172 98.658) (xy 161.04672 98.833)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C51-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.09172 114.37692) (xy 157.79172 114.37692) (xy 157.79172 112.97692) (xy 159.20172 112.97692) (xy 159.66172 112.51692)
        (xy 159.66172 111.40192) (xy 160.91672 111.40192) (xy 161.09172 111.57692)
      )
    )
  )
  (zone (net 30) (net_name "Net-(C38-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.83116 115.17424) (xy 199.0496 115.1717) (xy 199.0496 114.09474) (xy 199.56494 113.72068) (xy 200.87494 113.72068)
        (xy 200.864967 112.654169) (xy 198.437476 112.64068) (xy 198.43746 113.77216) (xy 198.59494 113.932125) (xy 198.59494 114.8034)
      )
    )
  )
  (zone (net 80) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.5507 104.5002) (xy 131.5507 103.535) (xy 132.0587 103.027) (xy 132.0587 102.3158) (xy 129.9251 102.3158)
        (xy 129.9251 103.9922)
      )
    )
  )
  (zone (net 80) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.9331 118.3432) (xy 196.7271 118.3432) (xy 196.7271 119.3846) (xy 197.0319 119.6894) (xy 197.0319 120.1212)
        (xy 196.7779 120.3752) (xy 194.5681 120.3752) (xy 193.9331 119.2068)
      )
    )
  )
  (zone (net 19) (net_name "Net-(C25-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.57494 104.77676) (xy 189.57494 104.55676) (xy 190.65494 104.55676) (xy 190.85494 104.77676) (xy 193.815597 104.791761)
        (xy 193.814283 105.941759) (xy 194.4411 107.27448) (xy 195.394946 107.279778) (xy 195.376665 108.46828) (xy 194.1363 108.46828)
        (xy 193.334082 107.81078) (xy 192.315996 107.691878) (xy 192.284834 106.137543) (xy 191.048233 106.14676) (xy 190.16494 104.77676)
      )
    )
  )
  (zone (net 18) (net_name "Net-(C21-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.91494 104.86063) (xy 196.91494 106.79188) (xy 196.26494 107.52848) (xy 196.254494 108.437883) (xy 198.063307 108.447877)
        (xy 198.08494 107.52848) (xy 198.5813 106.81728) (xy 199.57792 106.45502) (xy 199.57792 105.38568) (xy 199.06484 104.8726)
        (xy 199.06484 103.97598) (xy 198.83116 103.97598) (xy 197.92946 104.87768)
      )
    )
  )
  (zone (net 80) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.9331 105.03928) (xy 196.7271 105.03928) (xy 196.7271 106.08068) (xy 197.0319 106.38548) (xy 197.0319 106.81728)
        (xy 196.7779 107.07128) (xy 194.5681 107.07128) (xy 193.9331 105.90288)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C10-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.57494 91.47942) (xy 189.57494 91.25942) (xy 190.65494 91.25942) (xy 190.85494 91.47942) (xy 193.815597 91.494421)
        (xy 193.814283 92.644419) (xy 194.4411 93.97714) (xy 195.394946 93.982438) (xy 195.376665 95.17094) (xy 194.1363 95.17094)
        (xy 193.334082 94.51344) (xy 192.315996 94.394538) (xy 192.284834 92.840203) (xy 191.048233 92.84942) (xy 190.16494 91.47942)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.91494 91.56329) (xy 196.91494 93.49454) (xy 196.26494 94.23114) (xy 196.254494 95.140543) (xy 198.063307 95.150537)
        (xy 198.08494 94.23114) (xy 198.5813 93.51994) (xy 199.57792 93.15768) (xy 199.57792 92.08834) (xy 199.06484 91.57526)
        (xy 199.06484 90.67864) (xy 198.83116 90.67864) (xy 197.92946 91.58034)
      )
    )
  )
  (zone (net 80) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.9331 91.74194) (xy 196.7271 91.74194) (xy 196.7271 92.78334) (xy 197.0319 93.08814) (xy 197.0319 93.51994)
        (xy 196.7779 93.77394) (xy 194.5681 93.77394) (xy 193.9331 92.60554)
      )
    )
  )
  (zone (net 45) (net_name "Net-(C61-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.5735 78.1814) (xy 189.5735 77.9614) (xy 190.6535 77.9614) (xy 190.8535 78.1814) (xy 193.814157 78.196401)
        (xy 193.812843 79.346399) (xy 194.43966 80.67912) (xy 195.393506 80.684418) (xy 195.375225 81.87292) (xy 194.13486 81.87292)
        (xy 193.332642 81.21542) (xy 192.314556 81.096518) (xy 192.283394 79.542183) (xy 191.046793 79.5514) (xy 190.1635 78.1814)
      )
    )
  )
  (zone (net 44) (net_name "Net-(C57-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 55)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.9135 78.26527) (xy 196.9135 80.19652) (xy 196.2635 80.93312) (xy 196.253054 81.842523) (xy 198.061867 81.852517)
        (xy 198.0835 80.93312) (xy 198.57986 80.22192) (xy 199.57648 79.85966) (xy 199.57648 78.79032) (xy 199.0634 78.27724)
        (xy 199.0634 77.38062) (xy 198.82972 77.38062) (xy 197.92802 78.28232)
      )
    )
  )
  (zone (net 80) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads thru_hole_only (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.93166 78.44392) (xy 196.72566 78.44392) (xy 196.72566 79.48532) (xy 197.03046 79.79012) (xy 197.03046 80.22192)
        (xy 196.77646 80.47592) (xy 194.56666 80.47592) (xy 193.93166 79.30752)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 216.0835 104.9614) (xy 209.4835 104.9614) (xy 209.4835 101.3914) (xy 216.0835 101.3914)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 216.1335 91.6114) (xy 209.4835 91.6114) (xy 209.4835 88.0214) (xy 216.1335 88.0214)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 216.1935 78.3814) (xy 209.4835 78.3814) (xy 209.4835 74.7014) (xy 216.1935 74.7014)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.3035 66.9714) (xy 137.3035 73.6914) (xy 141.1335 73.6914) (xy 141.1335 66.9614)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.3185 67.09144) (xy 85.3185 125.97894) (xy 216.0885 125.97894) (xy 216.0885 67.09144)
      )
    )
  )
  (zone (net 80) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.3235 67.0914) (xy 85.3235 125.9789) (xy 216.0935 125.9789) (xy 216.0935 67.0914)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.3185 67.0914) (xy 85.3185 125.9789) (xy 216.0885 125.9789) (xy 216.0885 67.0914)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.325))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 216.0885 125.97894) (xy 85.3185 125.97894) (xy 85.3185 67.09144) (xy 216.0885 67.09144)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 216.0735 114.6514) (xy 216.0585 118.1614) (xy 209.4685 118.1614) (xy 209.4835 114.6514)
      )
    )
  )
)
